**3GPP TSG RAN WG1 #106-e R1-210xxxx**

**e-Meeting, August 16th – 27th, 2021**

|  |
| --- |
| **CHANGE REQUEST** |
|  |
|  | **38.213** | **CR** |  | **rev** |  | **Current version:** | **16.6.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Draft CR on SCell candidate beam detection |
|  |  |
| ***Source to WG:*** | Moderator (CATT) |
| ***Source to TSG:*** | RAN1 |
|  |  |
| ***Work item code:*** |  NR\_eMIMO-Core |  | ***Date:*** | 2021-08-19 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | In current 38.213, it is defined that UE should provide to its higher layer on whether UE identify at least one CSI-RS and/or SSB from q1. The “at least one CSI-RS and/or SSB” may imply UE identifies one CSI-RS and one SSB. But according to 38.321, the correct information should be whether UE identify one new beam. Thus it should be “at least one CSI-RS or SSB”. |
|  |  |
| ***Summary of change:*** | Clarify that for candidate beam detection, UE indicates whether it identifies at least one CSI-RS or SSB instead of one CSI-RS and one SSB. |
|  |  |
| ***Consequences if not approved:*** | UE behavior on candidate beam detection is unclear. |
|  |  |
| ***Clauses affected:*** | 6 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

### 6 Link recovery procedures

<unchanged part omitted>

For the PCell or the PSCell, upon request from higher layers, the UE provides to higher layers the periodic CSI-RS configuration indexes and/or SS/PBCH block indexes from the set  and the corresponding L1-RSRP measurements that are larger than or equal to the Qin,LR threshold.

For the SCell, upon request from higher layers, the UE indicates to higher layers whether there is at least one periodic CSI-RS configuration index or SS/PBCH block index from the set  with corresponding L1-RSRP measurements that are larger than or equal to the Qin,LR threshold, and provides the periodic CSI-RS configuration indexes and/or SS/PBCH block indexes from the set  and the corresponding L1-RSRP measurements that are larger than or equal to the Qin,LR threshold, if any.

<unchanged part omitted>