**3GPP TSG RAN WG1 #106bis-e R1-2109466**

**e-Meeting, October 11th – 19th, 2021**

**Agenda item:** 8.1.1

**Source:** Moderator (Samsung)

**Title:** Moderator summary for multi-beam enhancement

**Document for:** Discussion and Decision

## Introduction

In this summary, the term “item 1” refers to the first item in the Rel.17 NR FeMIMO WID, i.e. multi-beam enhancement:

|  |
| --- |
| 1. Enhancement on multi-beam operation, mainly targeting FR2 while also applicable to FR1:    1. Identify and specify features to facilitate more efficient (lower latency and overhead) DL/UL beam management for intra-cell and inter-cell scenarios to support higher UE speed and/or a larger number of configured TCI states:       1. Common beam for data and control transmission/reception for DL and UL, especially for intra-band CA       2. Unified TCI framework for DL and UL beam indication       3. Enhancement on signaling mechanisms for the above features to improve latency and efficiency with more usage of dynamic control signaling (as opposed to RRC)       4. For inter-cell beam management, a UE can transmit to or receive from only a single cell (i.e. serving cell does not change when beam selection is done). This includes L1-only measurement/reporting (i.e. no L3 impact) and beam indication associated with cell(s) with any Physical Cell ID(s)          1. The beam indication is based on Rel-17 unified TCI framework          2. The same beam measurement/reporting mechanism will be reused for inter-cell mTRP          3. This work shall only consider intra-DU and intra-frequency cases    2. Identify and specify features to facilitate UL beam selection for UEs equipped with multiple panels, considering UL coverage loss mitigation due to MPE, based on UL beam indication with the unified TCI framework for UL fast panel selection |

This summary includes the following:

* Observation and proposal
* Summary of current companies’ positions on each of the aspects within the category

## Summary of companies’ inputs

The listed issues are structured primarily to facilitate some progress on pending issues identified in the agreements (see Appendix A).

### Issue 1 (Rel.17 unified TCI framework – note: for intra-cell beam management)

Table 1 Summary: issue 1

|  |  |  |
| --- | --- | --- |
| **#** | **Issue** | **Companies’ views** |
| 1.1 | Offline proposal 1.A (below)  Note: The wording of proposal can be further refined (please describe in Table 2) | **Max 8 TCI codepoints in DCI (same as Rel.15/16):**   * **Support:** ZTE, vivo, Lenovo/MotM, CMCC, APT/FGI, Nokia/NSB, LG, Ericsson, Apple, OPPO, Intel, MTK, Fujitsu, Qualcomm, IDC, Spreadtrum, * **No (increase to 16):** Samsung   **Max total 128 configured TCI states (same as Rel.15/16):**   * **Support:** vivo, Lenovo/MotM, CMCC, Nokia/NSB, OPPO, MTK, Fujitsu, Qualcomm, IDC, Spreadtrum, * **No (increase to 256):** ZTE, Ericsson, Samsung, APT/FGI, LG, Intel |
| 1.2 | Offline proposal 1.B (below)  Note: The wording of proposal can be further refined (please describe in Table 2) | **Support**: Ericsson, Samsung, MTK, Intel (intra-cell only), AT&T, Apple, Intel, Spreadtrum, CMCC, ZTE, Fujitsu, Qualcomm, Sony, Lenovo/MotM,  **Not support**: |
| 1.3 | Offline proposal 1.C.1 and 1.C.2 (below)  Note: The wording of proposal can be further refined (please describe in Table 2) | **1.C.1:**   * **Support**: MTK, Samsung, ZTE, Intel, vivo, CMCC, Fujitsu, Lenovo/MotM, * **Not support**:   **1.C.2:**   * **Support**: MTK, Samsung, ZTE, Intel, vivo, CMCC, Fujitsu * **Not support**: |
| 1.4 | Offline proposal 1.D (below)  Note: If there is no consensus in removing the brackets, spec editor(s) will eventually assume that the bracketed text doesn’t exist in the agreement. | **Support**: vivo, NTT Docomo, Nokia/NSB, Samsung, Sony, Spreadtrum, MTK, Convida, Intel, vivo, CMCC, ZTE, Fujitsu, Lenovo/MotM, IDC,  **Not support**: Apple (replace “configured” by “CCs/BWPs at least within a band”) |
| 1.5 | Offline proposal 1.E (below)  Note: The wording of proposal can be further refined (please describe in Table 2) | **Support**: Spreadrum, MTK, Qualcomm, vivo, Intel, Samsung, CMCC, [ZTE], Fujitsu, Lenovo/MotM,  **Not support**: |
| 1.6 | Offline proposal 1.F (below)  Note: The wording of proposal can be further refined (please describe in Table 2) | **Support**: Ericsson (Opt 1), MTK, Intel (Opt2), Apple (Opt1), vivo, Spreadtrum, Samsung, CMCC, ZTE, Fujitsu, Lenovo/MotM, IDC,  **Not support**: |
| 1.7 | Offline proposal 1.G (below)  Note: The wording of proposal can be further refined (please describe in Table 2) | **Support**: OPPO, Lenovo/MotM, Fraunhofer IIS/HHI, Nokia/NSB, Samsung, MTK, Qualcomm, Intel, CMCC, Fujitsu, IDC  **Not support**: ZTE, vivo |
| 1.8 | Offline proposal 1.H (below)  Note: The wording of proposal can be further refined (please describe in Table 2) | **Support (RRC + MAC CE)**: ZTE, CATT, Nokia/NSB, Samsung, Qualcomm, MTK, CMCC, ZTE, Fujitsu, IDC  **Not support (RRC only)**: vivo, Intel, Ericsson, Spreadtrum |
| 1.9 | For separate TCI, UL TCI state pool  Alt1: Shared pool with joint/DL TCI state  Alt2: Separate pool  Note: Strictly speaking, this could be decided in RAN2 | **Alt1 (12)**: vivo, Spreadtrum, Samsung, Xiaomi, ZTE, Qualcomm, MTK, Convida, NTT Docomo, Intel, CATT, TCL  **Alt2 (10)**: CMCC, Ericsson, Futurewei, Huawei/HiSi, Fraunhofer IIS/HHI, IDC, Sony, Apple |
| 1.10 | Additional source RS type for DL QCL Type-D reference for DL common UE-dedicated reception on PDSCH and all/subset of CORESETs  Note: CSI-RS for tracking (TRS) and CSI-RS for BM have been agreed  Note: There are currently two interpretations on the agreement regarding CSI-RS for CSI: 1) Agreeing on reusing Rel-15/16 QCL rules implies CSI-RS for CSI is also agreed, 2) Only CSI-RS for tracking and BM were listed in the agreement, so CSI-RS for CSI is not yet agreed | SSB, with TRS as QCL Type-A source RS   * **Yes (4):** ZTE, Samsung, MTK, vivo * **No (8):** Spreadtrum, OPPO, Intel, Apple, Sony, Ericsson, Huawei/HiSi   SRS for BM, optionally with TRS as QCL Type-A source RS   * **Yes (8):** ZTE, IDC, Spreadtrum, Samsung, Convida, Nokia/NSB, vivo * **No (10):** Sony, OPPO, Fraunhofer IIS/HHI, MTK, Intel, Ericsson, Huawei/HiSi, LG |
| 1.11 | BFR enhancement for unified TCI:  X symbols after the UE receives the BFRR, the new/updated QCL source RS applies to both UE-dedicated PDCCH and PDSCH | **Yes**: Apple  **No**: |
| 1.12 | BFR enhancement for unified TCI: can BFD RS share the same indicated Rel-17 TCI state as UE-dedicated PDSCH/PDCCH? | **Yes**: NEC, NTT Docomo  **No**: |
|  |  |  |

Proposals 1.A – 1.F are taken from the final outcome of the offline discussion [1]:

* Proposal 1.B: Instead of using the final version from the FL, the format proposed by Apple is used with some refinement (marked red)

The following observation can be made:

* ...

Based on the above observation, the following moderator proposals can be made:

**Proposal 1.A**: On Rel.17 unified TCI framework, for Rel-17 unified TCI:

* For rhe number of configured TCI states (including joint TCI state(s), DL-only TCI state(s), UL-only TCI state(s), and/or DL-only+UL-only TCI state(s)), the largest configurable value is 128
* For the number of codepoints in the TCI field for DCI-based beam indication (hence the number of codepoints activated via MAC-CE-based TCI state activation), the largest configurable value is 8

**Proposal 1.B:** On Rel.17 unified TCI framework, for Rel-17 unified TCI:

* For DL channels/signals that do not share the same indicated Rel-17 TCI state as UE-dedicated reception on PDSCH/PDCCH (via Rel-17 MAC-CE/DCI TCI state update), all the QCL rules defined in section 5.1.5 in 38.214 are supported
  + Note: For CSI-RS used to provide QCL indication for non-UE dedicated channels, the CSI-RS should only be QCLed with SSB of the same PCID as that from the serving cell
* For DL channels/signals that share the same indicated Rel-17 TCI state as UE-dedicated reception on PDSCH/PDCCH (via Rel-17 MAC-CE/DCI TCI state update), only the following options on source RSs and QCL-Types are supported
  + Option 1: TRS is configured for QCL-TypeA ~~indication~~ source RS and CSI-RS for BM is configured for QCL-TypeD ~~indication~~ source RS
  + Option 2: TRS is configured for QCL-TypeA and QCL-TypeD ~~indication~~ source RS
  + Note: For inter-cell beam management, SSB with PCID different from that from the serving cell can be used as a QCL Type-D source RS for CSI-RS for BM and/or TRS

[Tables may be added on source-target relation for better clarity, e.g.

*For joint TCI and DL-only TCI*

|  |  |
| --- | --- |
| **Source RS (\*)** | **Target RS** |
| SSB | Periodic TRS |
| CSI-RS for BM |
| CSI-RS for CSI |
| Periodic TRS | AP TRS |
| CSI-RS for BM |
| CSI-RS for CSI |
| PDCCH/PDSCH DMRS |
| CSI-RS for BM | Periodic TRS |
| CSI-RS for BM |
| CSI-RS for CSI |
| PDCCH/PDSCH DMRS |
| CSI-RS for CSI | PDCCH/PDSCH DMRS |

*For UL-only TCI*

...

]

**Proposal 1.C.1**: On Rel.17 unified TCI framework, remove the brackets and clarify as indicated in red from the following *previous agreement*:

*On Rel-17 unified TCI framework, support common TCI state ID update and activation to provide common QCL information and/or common UL TX spatial filter(s) across a set of configured CCs:*

* *…*
* *Just as Rel.16, the source RS in the Rel-17 TCI state that provides QCL-TypeA ~~[or QCL-TypeB]~~ shall be in the same CC as the target channel or RS*
* *…*

**Proposal 1.C.2**: On Rel.17 unified TCI framework, the source RS in the Rel-17 TCI state that provides QCL-TypeA or QCL-TypeB shall be in the same CC as the target channel or RS

**Proposal 1.D**: On Rel.17 unified TCI framework, remove the brackets as indicated in red from the following *previous agreement*:

*For common TCI state ID update and activation to provide common QCL information at least for UE-dedicated PDCCH/PDSCH and/or common UL TX spatial filter(s) at least for UE-dedicated PUSCH/PUCCH across a set of ~~[~~configured~~]~~ CCs/BWPs:*

*...*

**Proposal 1.E**: On Rel.17 unified TCI framework, regarding the common TCI state ID update and activation for CA, the reference CC/BWP is the CC/BWP in which the common TCI state pool (list of TCI states) is configured.

* The details on how the PDSCH configuration (for each of those CCs/BWPs) contains a reference to the RRC-configured TCI state pool(s) in a reference BWP /CC are up to RAN2

**Proposal 1.F**: On path-loss measurement for Rel.17 unified TCI framework, a PL-RS (configured for path-loss calculation, already assumed periodic) is either a periodic CSI-RS or an SSB. When a periodic CSI-RS is used as a PL-RS, decide in RAN1#106bis-e between the two following options:

* Opt1. Only 1-port periodic CSI-RS is supported for PL-RS
* Opt2. Both 1- and 2-port periodic CSI-RS are supported for PL-RS

**Proposal 1.G**: On path-loss measurement for Rel.17 unified TCI framework, at least for discussion purposes, “beam alignment” also pertains to the following events:

* The PL-RS is identical to the QCL Type-D RS of UL TCI spatial relation RS
* The QCL Type-D RS of PL-RS is identical to the UL TCI spatial relation RS
* The QCL Type-D RS of PL-RS is identical to the QCL Type-D RS of UL TCI spatial relation RS

**Proposal 1.H**: On Rel.17 unified TCI framework, when the setting of (P0, alpha, closed loop index) for PUSCH, PUCCH, and/or SRS are associated with UL or (if applicable) joint TCI state per BWP:

* The multiple settings are configured via RRC
* Optionally, the association between a TCI state and one of the multiple settings, for each of the PUSCH, PUCCH, and/or SRS, is signaled via MAC-CE together with the MAC-CE-based TCI state activation

Table 2 Additional inputs: issue 1

|  |  |
| --- | --- |
| **Company** | **Input** |
| Mod V0 | **1) Check and update Table 1**  **2) Share your inputs on the above FL proposals** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

### Issue 2 (inter-cell beam management)

Table 3 Summary: issue 2

|  |  |  |
| --- | --- | --- |
| **#** | **Issue** | **Companies’ views** |
| 2.1 | Offline conclusion 2.A (below)  Note: The wording of proposal can be further refined (please describe in Table 4) | **Support**: Fujitsu  **Not support**: |
| 2.2 | Offline conclusion 2.B (below)  Note: The wording of proposal can be further refined (please describe in Table 4) | **Support**: Ericsson, Nokia/NSB, Spreadrum, MTK, LG, Qualcomm, Apple, MTK, Qualcomm, Samsung, Lenovo/MotM, OPPO, NEC, CATT, Sony, ZTE, Xiaomi, Huawei/HiSi, IDC  **Not support**: Futurewei, Intel, [NTT Docomo] |
| 2.3 | For separate DL/UL TCI, need to add restriction that the indicated DL TCI and UL TCI are associated with SSBs of a same physical cell ID? | **Yes:** OPPO, Nokia/NSB, Samsung, Intel, Apple  **No:** Ericsson, CMCC, Xiaomi, NTT Docomo |
| 2.4 | Supported value(s) of NMAX (the maximum number of RRC configured PCIs different from the serving cell for measurement/reporting)   * Alt1: NMAXis up to UE capability with candidate values of 1 and X.   + Note: X as agreed in AI 8.1.2.2   + When NMAXis configured to be X, the UE measures up to X PCIs different from the serving cell PCI   + Additional restriction may be added by RAN4 * Alt2. NMAX=1 | **Alt1:** Huawei/HiSi, Lenovo/MotM, Ericsson, CATT, CMCC, Samsung, Intel, NTT Docomo  **Alt2:** Spreadtrum, OPPO |
| 2.5 | Whether to support event-driven inter-cell beam reporting and if so the event definition   * Alt1. Support L1-based event-driven beam reporting for inter-cell beam management and inter-cell mTRP * Alt2. Support MAC CE based event-driven beam reporting for inter-cell beam management and inter-cell mTRP * Alt3. In Rel-17, event-driven beam reporting is not supported for inter-cell beam management and inter-cell mTRP | **Alt1**: Huawei/HiSi, Xiaomi, Intel, Sony, LG, Samsung  **Alt2**: ZTE, Lenovo/MotM, CATT, Xiaomi, NTT Docomo, Nokia/NSB, Apple, Qualcomm,  **Alt3**: OPPO, vivo, Ericsson, MTK |
| 2.6 | UCI design for L1-RSRP reporting: Reuse Rel-15 L1-RSRP table | **Yes:** Samsung  **No:** |
| 2.7 | UCI design for L1-RSRP reporting: For K>1, reuse (K-1) Rel-15 differential L1-RSRP() relative to the first L1-RSRP value | **Yes:** ZTE, Samsung  **No:** |
|  |  |  |

Proposals 2.A and 2.B are taken from the final outcome of the offline discussion [1].

The following observation can be made:

* 2.3: There is no consensus in adding the additional restriction
* 2.4: Alt1 represnets the super-majority view
* 2.5: Among the proponents of event-driven reporting, there is no consensus on whether to support L1-based or MAC-CE-based solution

Based on the above observation, the following moderator proposals can be made:

**Proposed conclusion 2.A**: On Rel-17 beam indication enhancements for inter-cell beam management, for the supported Rel-17 MAC-CE-based and/or DCI-based beam indication (at least using DCI formats 1\_1/1\_2 with and without DL assignment including the associated MAC-CE-based TCI state activation), the supported number of physical cell IDs different from that of the serving cell will be decided as a part of UE feature discussion.

**Proposed conclusion 2.B**: On Rel-17 enhancements for inter-cell beam management and inter-cell mTRP, for Rel-17 discussion purpose, the reception of signals other than SSBs from TRPs with PCIs different from the serving cell compared to that for serving cell is within one CP length.

**Proposed conclusion 2.C**: On Rel-17 beam indication enhancements for inter-cell beam management, for separate DL/UL TCI, there is no consensus in restricting the indicated DL TCI and UL TCI to be associated with SSBs of a same physical cell ID.

**Proposal 2.D**: On Rel-17 enhancements for inter-cell beam management and inter-cell mTRP, NMAX (the maximum number of RRC configured PCIs different from the serving cell for measurement/reporting) is up to UE capability with candidate values of 1 and X.

* Note: X as agreed in AI 8.1.2.2
* When NMAXis configured to be X, the UE measures up to X PCIs different from the serving cell PCI
* Additional restriction may be added by RAN4

**Proposed conclusion 2.E**: On Rel-17 enhancements for inter-cell beam management and inter-cell mTRP, there is no consensus in supporting event-driven inter-cell beam reporting

Table 4 Additional inputs: issue 2

|  |  |
| --- | --- |
| **Company** | **Input** |
| Mod V0 | **1) Check and update Table 3**  **2) Share your inputs on the above FL proposals** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

### Issue 3 (beam indication signaling medium)

Table 5 Summary: issue 3

|  |  |  |
| --- | --- | --- |
| **#** | **Issue** | **Companies’ views** |
| 3.1 | BAT (Y) for CA:   * Alt1: The first slot and the Y symbols are both determined on the carrier with the smallest SCS among the carrier(s) applying the beam indication * Alt2: The first slot and the Y symbols are both determined on the carrier with smallest SCS among the carrier(s) applying the beam indication and the UL carrier carrying the acknowledgment * Alt3: The first slot and the Y symbols are both determined on the UL carrier carrying the acknowledgment. | **Alt1**: OPPO, Lenovo/MotM, Ericsson, CATT, CMCC, Xiaomi, NTT Docomo, Nokia/NSB, Huawei/HiSi, Spreadtrum, MTK, Intel, Apple  **Alt2**: vivo, Samsung, APT/FGI  **Alt3**: ZTE, Sony |
| 3.2 | Whether to support different values of Y for different cases. If so, details | **Yes**: Samsung (multi-panel), Huawei/HiSi (multi-panel), MTK (panel-swicthing, inter-cell with time difference greater than CP)  **No**: OPPO |
| 3.3 | Further enhancements on ACK/NAK for DCI formats 1\_1/1\_2 with DL assignment when used for beam indication | **DCI ACK/NAK:** CATT, Apple, Xiaomi, Samsung, Intel (with higher priority for beam indication DCI ACK/NACK), ASUSTek  **DL assignment ACK/NAK, but only ACK can be used to confirm beam indication:** NEC, OPPO |
| 3.4 | Support for additional beam indication scheme for Rel-17 unified TCI framework beyond agreement to-date | **No additional beam indication scheme is supported:** CATT  **DCI formats 0\_1/0\_2 with UL grant (for UL-only TCI of separate DL/UL TCI)**: IDC, LG, Sony, MTK, Intel, Xiaomi, TCL  **New dedicated DCI format for beam indication**:  **Group-common DCI**: Sony, Intel  **When more than one TCI codepoints are activated by MAC CE, the activated TCI state(s) for the lowest codepoint is/are applied**: Huawei/HiSi, vivo (until DCI is indicated), Convida (after MAC CE activation) |
|  |  |  |

The following observation can be made:

* 3.1: Alt1 represmets the super-majority view
* 3.2: ... (need more views)

Based on the above observation, the following moderator proposals can be made:

**Proposal 3.A**: On Rel-17 DCI-based beam indication, regarding application time of the beam indication for CA, the first slot and the Y symbols are both determined on the carrier with the smallest SCS among the carrier(s) applying the beam indication.

Table 6 Additional inputs: issue 3

|  |  |
| --- | --- |
| **Company** | **Input** |
| Mod V0 | **1) Check and update Table 5**  **2) Share your inputs on the above FL proposals** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

### Issue 4 (MP-UE)

Table 7 Summary: issue 4

|  |  |  |
| --- | --- | --- |
| **#** | **Issue** | **Companies’ views** |
| 4.1 | Per RAN1#106-e agreement  **Scheme 1**: a panel entity corresponds to a reported CSI-RS and/or SSB resource index in a beam reporting instance (i.e. Opt1-1 per RAN1#104-bis-e agreement) ...  vs  **Scheme 2**: support UE reporting one of the following (to be down selected in RAN1#106bis-e):   * **Opt1**. A list of supported UL ranks (number of UL transmission layers) * **Opt2**. A list of supported number of SRS antenna ports * **Opt3**. A list of coherence types (as in Rel-15) indicating a subset of ports | **Scheme 1 (18)**: Huawei/HiSi, IDC, Spreadtrum, vivo, Fujitsu, Lenovo/MotM, Fraunhofer IIS/HHI, NTT Docomo, Sony, AT&T, Apple, LG, Qualcomm, ZTE, [Xiaomi]  **Scheme 2 (12)**: ZTE, Samsung, OPPO, CMCC, MTK, NTT Docomo, Nokia/NSB, [Ericsson, Intel, Apple], ZTE   * **Opt1**: MTK, [Intel] * **Opt2**: Nokia/NSB, OPPO * **Opt3**: Samsung, OPPO   **Do not support scheme 1**: Ericsson, Nokia/NSB  **Do not support Scheme 2**: CATT |
| 4.2 | Multiple SRS resource sets with different SRS #ports | **#SRS resource sets**   * **2**: Samsung, OPPO, Fraunhofer IIS/HHI * **3**: Samsung   **#SRS resources in each set:**   * **UE reporting**: vivo   **#SRS ports in each set**   * **1, 2, 4**: Samsung |
|  |  |  |

The following observation can be made:

* 4.1: Scheme 1 still represents the majority view. Among the proponents of Scheme 2, it is unclear if there is any convergence on the option (note that Scheme 2 includes 3 different schemes). Given the current situation, it seems proper to proceed with Scheme 1 (previously supported by some supporters of Scheme 2 as well).

Based on the above observation, the following moderator proposals can be made:

**Proposal 4.A**: On Rel.17 enhancements to facilitate UE-initiated panel activation and selection,

* A panel entity corresponds to a reported CSI-RS and/or SSB resource index in a beam reporting instance (i.e. Opt1-1 per RAN1#104-bis-e agreement)
  + The correspondence between a panel entity and a reported CSI-RS and/or SSB resource index is informed to NW
    - FFS: Detailed design of how to inform the correspondence to NW
  + Note: the correspondence between a CSI-RS and/or SSB resource index and a panel entity is determined by the UE (analogous to Rel-15/16)
* Support UE reporting of maximum number of SRS ports and coherence type for each panel entity as a UE capability
* Support multiple c odebook -based SRS resource sets with different maximum number of SRS ports
  + The indicated SRI is based on the SRS resources corresponding to one SRS resource set, where the SRS resource set should be aligned with the UE capability for the panel entity

Table 8 Additional inputs: issue 4

|  |  |
| --- | --- |
| **Company** | **Input** |
| Mod V0 | **1) Check and update Table 7**  **2) Share your input on the above FL proposals** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

### Issue 5 (MPE mitigation)

Table 9 Summary: issue 5

|  |  |  |
| --- | --- | --- |
| **#** | **Issue** | **Companies’ views** |
| 5.1 | Confirm working assumption on reporting M SSBRI(s)/CRI(s) together with N P-MPR(s) | **Yes**: ZTE, Samsung, CATT, CMCC, Xiaomi, Intel, NTT Docomo, Ericsson, Sony, Nokia/NSB, Apple, Qualcomm, LG  **No**: vivo (include panel ID) |
| 5.2 | Supported value(s) of N and M | Supported value(s) of N:   * **{1}**: Ericsson * **#beams {1,2,3,4 + UE cap}** (same as Rel-15/16 beam reporting): ZTE, Samsung, Sony, Nokia/NSB, Qualcomm * **Other** (specify):   + **#panels (2,3, or depends on UE cap)**: Spreadtrum, Lenovo/MotM, CATT, Xiaomi, LG   Supported value(s) of M:   * **Only 1**: ZTE, Samsung, Ericsson, CATT, Intel, NTT Docomo, Sony, Nokia/NSB, Apple, LG, Qualcomm * **Other** (specify):   + **M=#panels – N**: Spreadtrum |
| 5.3 | How to perform selection of N from a candidate SSB/CSI-RS resource pool and how the candidate resource pool is configured | Selection of N is based on:   * **TCI state quality**: OPPO * **TCI state group quality**: IDC * **L1-RSRP and P-MPR**: Ericsson, NTT Docomo, Qualcomm * **Virtual PHR**: Nokia/NSB   Candidate resource pool:   * **Configured via RRC**: CATT * **Configured via RRC using CSI report config**: Samsung, [Nokia/NSB] |
| 5.4 | Beam vs panel level | **Beam**: IDC, Sony, Nokia/NSB, Qualcomm  **Panel**: Huawei/HiSi, Spreadtrum, vivo, Lenovo/MotM, CATT, LG  **No need to discuss**: Ericsson |
|  |  |  |

The following observation can be made:

* 5.1, 5.2: Confirming the WA represents the super-majority view
  + M=1 represents the super-majority view
  + At least N=1 can be agreed, while the need for N={2, 3, 4} requires more discussion (also dependent on the outcome of issue 4)

Based on the above observation, the following proposal can be made:

**Proposal 5.A**: On Rel.17 enhancements to facilitate MPE mitigation, confirm the following working assumption as an agreement with the following refinement (highlighted in red):

* *For each P-MPR value, up to M SSBRI(s)/CRI(s), where the SSBRI(s)/CRI(s) is selected by the UE from a candidate SSB/CSI-RS resource pool (FFS: how to perform the selection)*
  + *~~FFS: The supported value(s) of M~~Support only M=1*

**Proposal 5.B**: On Rel.17 enhancements to facilitate MPE mitigation, support at least N=1

* Discuss and decide in RAN1#106bis-e whether to support N=2, 3, and/or 4

Table 10 Additional inputs: issue 5

|  |  |
| --- | --- |
| **Company** | **Input** |
| Mod V0 | **1) Check and update Table 10**  **2) Share your inputs on the above FL proposals** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

### Issue 6 (advanced beam refinement/tracking)

Table 11 Summary: issue 6

|  |  |  |
| --- | --- | --- |
| **#** | **Issue** | **Companies’ views on specific candidate schemes** |
| 6.1 | UE-initiated beam management:   * ALT1. UE -initiated (DL-only or DL/UL) beam selection, including the following options   + Opt1. The selected beam is reported by an event-triggered UE beam reporting via, e.g. UCI, MAC CE, UL CG, or Type 1/Type 2 CBRA/CFRA   + Opt2. The selected beam is reported by a legacy UE beam report (NW-configured)   + FFS on triggering condition and NW-indication of a beam group in which the UE is allowed to do the beam selection, e.g., the NW-indication via MAC-CE   + FFS: NW confirmation, e.g. if no NW beam selection command overwriting the selected beam is received in a time window after the report * ALT2. UE-initiated beam activation based on beam reporting   + The reported beam(s) are activated as active TCI/spatial relation RS(s) automatically w/o NW activation command after receiving gNB response signalling, e.g. DCI/MAC CE   + FFS: The reported beam is applied directly if the number of supported activated beam by the UE is one and/or after receiving gNB response signaling, or if no NW activation command overwrites the beam(s) activated by the report in a time window after the report * ALT3. UE -initiated UL-only beam selection considering potential misalignment between network and UE on the selected beams   + The UE can select an alternative beam from the other beams in the gNB -configured set containing more than one UL beam | **ALT1**:  **ALT2**:  **ALT3**: |
|  |  |  |

The following observation can be made:

* ...

Based on the above observation, the following proposal can be made:

**Proposal 6.A**: On Rel.17 enhancements to facilitate advanced beam refinement/tracking, [after more inputs/discussion]

Table 12 Additional inputs: issue 6

|  |  |
| --- | --- |
| **Company** | **Input** |
| Mod V0 | **1) Check and update Table 12** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# References

|  |  |  |  |
| --- | --- | --- | --- |
| 1 | R1-2109467 | Summary of offline discussion on unified TCI and inter-cell beam management | Moderator (Samsung) |
| 2 | R1-2108756 | Enhancements on multi-beam operation in Rel-17 | Huawei, HiSilicon |
| 3 | R1-2108796 | Enhancement on multi-beam operation | FUTUREWEI |
| 4 | R1-2108808 | Further Discussion on Enhancements for Multi-beam Operation | InterDigital, Inc. |
| 5 | R1-2108870 | Enhancements on Multi-beam Operation | ZTE |
| 6 | R1-2108895 | Enhancements on Multi-beam Operation | Spreadtrum Communications |
| 7 | R1-2108951 | Further discussion on multi beam enhancement | vivo |
| 8 | R1-2109029 | Enhancements on Multi-beam Operation | Fujitsu |
| 9 | R1-2109038 | Enhancements on Multi-beam Operation | OPPO |
| 10 | R1-2109103 | Enhancements on Multi-beam Operation | Lenovo, Motorola Mobility |
| 11 | R1-2109110 | Remaining issues on multi-beam enhancements | Ericsson |
| 12 | R1-2109122 | Discussion on multi-beam operation | NEC |
| 12 | R1-2109180 | Enhancements on multi-beam operation | TCL Communication Ltd. |
| 14 | R1-2109184 | Futher discussion on Rel-17 multi-beam operation | CATT |
| 15 | R1-2109270 | Enhancements on multi-beam operation | CMCC |
| 16 | R1-2109350 | Enhancements on multi-beam operation | Fraunhofer IIS, Fraunhofer HHI |
| 17 | R1-2109378 | Enhancements on multi-beam operation | Xiaomi |
| 18 | R1-2109468 | Multi-Beam Enhancements | Samsung |
| 19 | R1-2109543 | Enhancement on multi-beam operation | MediaTek Inc. |
| 20 | R1-2109591 | Enhancements to Multi-Beam Operations | Intel Corporation |
| 21 | R1-2109658 | Discussion on multi-beam operation | NTT DOCOMO, INC. |
| 22 | R1-2109772 | Further enhancement on multi-beam operation | Sony |
| 23 | R1-2109832 | Discussion of enhancements on multi-beam operation | FGI, Asia Pacific Telecom |
| 24 | R1-2109870 | Enhancements on Multi-beam Operation | Nokia, Nokia Shanghai Bell |
| 25 | R1-2109923 | Enhancements on Multi-Beam Operations | AT&T |
| 26 | R1-2110013 | Views on Rel-17 Beam Management enhancement | Apple |
| 27 | R1-2110077 | Enhancements on Multi-beam Operation | LG Electronics |
| 28 | R1-2110103 | Enhancements on Multi-beam Operation | Convida Wireless |
| 29 | R1-2110165 | Enhancements on Multi-beam Operation | Qualcomm Incorporated |
| 30 | R1-2108877 | Further details on Multi-beam and Multi-TRP operation | ZTE |
| 31 | R1-2109045 | Discussion on further enhancements for multi-beam operation | OPPO |
| 32 | R1-2109475 | Additional enhancements for multi-beam | Samsung |
|  |  |  |  |