**3GPP TSG-RAN WG1 Meeting #107-e R1-211xxxx**

**e-Meeting, Nov 11th – 19th, 2021**

**Agenda Item: 7.2.1**

**Source: Moderator (ZTE)**

**Title: FL summary on the maintenance of 2-step RACH**

**Document for: Discussion**

# Introduction

This document contains the summary of issues related to the maintenance of Rel-16 2-step RACH WI in RAN1#107-e meeting.

# Preparation phase discussion

The following CR is submitted to the maintenance of Rel-16 2-step RACH in RAN1#107-e.

|  |  |  |  |
| --- | --- | --- | --- |
| Issue # | Description | Affected spec | TDoc # |
| 1 | Editorial correction on the slot configuration of type-2 random access | TS38.213 | R1-2111357 |

To share the views on the necessity of the above issue, please fill in ‘Yes/No/Editorial’ to the table below.

|  |  |  |
| --- | --- | --- |
| Company | Issue #1 | Comments |
| Huawei | Ok | Thanks for spotting this. Can be concluded to be directly passed to Editor. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Email discussions

# Summary

The outcome of email discussion will be updated later.

# References

[1] R1-2111357 Editorial correction on the slot configuration of type-2 random access ZTE, Sanechips

# Appendix

List of proposals in the submitted contributions.

|  |  |
| --- | --- |
| TDoc | Proposals |
| R1-2111357, ZTE, Sanechips | ***Reason for change:*** RAR includes information of UL grant but successRAR does not include information of UL grant. The current description of spec includes editorial typo.***Summary of change:*** Revise “a RAR UL, fallbackRAR UL grant, or successRAR grant indicating to the UE” to “a RAR UL grant, fallbackRAR UL grant, or successRAR indicating to the UE”***Consequences if not approved:*** The description is not reasonable. ========CR to TS38.213=======11.1.1 UE procedure for determining slot format< Unchanged parts are omitted >- if an SFI-index field value in DCI format 2\_0 indicates the set of symbols of the slot as flexible and the UE detects a DCI format, a RAR UL grant, fallbackRAR UL grant, or successRAR indicating to the UE to transmit PUSCH, PUCCH, PRACH, or SRS in the set of symbols of the slot the UE transmits the PUSCH, PUCCH, PRACH, or SRS in the set of symbols of the slot- if an SFI-index field value in DCI format 2\_0 indicates the set of symbols of the slot as flexible, and the UE does not detect a DCI format indicating to the UE to receive PDSCH or CSI-RS, or the UE does not detect a DCI format, a RAR UL grant, fallbackRAR UL grant, or successRAR ~~grant~~ indicating to the UE to transmit PUSCH, PUCCH, PRACH, or SRS in the set of symbols of the slot, the UE does not transmit or receive in the set of symbols of the slot< Unchanged parts are omitted > |