**3GPP TSG RAN WG1 Meeting #107-e R1-210xxxx**

**Nov 11th – 19th, 2021**

**Agenda item: 7.2.2**

**Source: Moderator (Qualcomm Incorporated)**

**Title: Preparation phase email discussion for NR-U**

**Document for: Discussion and Decision**

# Introduction

The paper summarizes the preparation phase email discussion for contribution submitted to 7.2.2 on NR-U CR under the following email thread

* [107-e-Prep-AI7.2.2] Preparation phase for Rel-16 NR-U maintenance: Jing (Qualcomm)

# Issues identified

This section lists the issues discussed in submitted papers. I tried to put them under technical proposal or editorial proposal categories, but I might be wrong though.

Issues may need technical discussion:

|  |  |  |  |
| --- | --- | --- | --- |
| Issue ID | Brief summary | Summary document | Supporting document |
| T1 | Channel access updates for MIIT | [2] | [1]. CR for 37.213  [3]. CR for 38.212 |
| T2 | CG-UCI multiplexing condition | [4] | [4]. CR for 38.212 |
| T3 | Freq hopping for single/multi-PUSCH | [5], [8] | [9]. CR for 38.214 |
| T4 | Channel access for consecutive UL transmission | [6] | [7]. CR for 37.213 |
| T5 | Correction on unit of CP extension | [12] | [12]. CR for 38.211 |
| T6 | UL transmission in wideband operation | [13] | [13]. CR for 37.211 |
| T7 | Discussion on LS from RAN4 on measing CSI-RS during SCell activation | [14] |  |
| T8 | Changes of channel access procedure in TS 37.213 | [16] | [16]. CR for 37.213 |
| T9 | On additional PDSCH DM-RS dropping with double symbol | [17] | [17]. CR for 38.211 |

Issues more editorial in nature:

|  |  |  |  |
| --- | --- | --- | --- |
| Issue ID | Brief summary | Summary document | Supporting document |
| E1 | Correct IE name for availableRB-SetsToReleaseList | [10] | [10]. CR for 38.213 |
| E2 | Type 3 HARQ codebook construction, change “HARQ process number h” to “HARQ process h” | [11] | [11]. CR for 38.213 |
| E3 | Correction on usage of subCarrierSpacingCommon for unlicensed | [15] | [15]. CR for 38.213 |
| E4 | Correction on UL channel access procedure Type 2A/2B/2C | [18] | [18]. CR for 37.213 |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

# Discussion on which CR to treat

Please provide your view below. “Y” to discuss.

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Company | T1 | T2 | T3 | T4 | T5 | T6 | T7 | T8 | T9 |
| MTK | Y | Y | Y | Y | Y | Y | Y | Y | Y |
| Ericsson |  | Y (OK with 1st change) | Y |  |  | Y | N | Y |  |
| LG Electronics |  | Y (but the second change doesn’t seem to be needed) | Y |  | Y | Y |  | Y | Y |
| Transsion | Y | Y | Y |  |  | Y |  | Y | N |
| Huawei, HiSilicon | Y, comment below | Y, response to LG below | Y |  | Comment below | Y |  | Y | resolved in RAN1#104, |
| CAICT |  | Y | Y |  | Y | Y |  | Y | Y |
| ZTE, Sanechips | Y(specific CR can be further discussed) | Y(fine with 1st change, and not understand the motivation of 2nd change) | Y |  | Y(can be further clarified) | Y |  | Y | Y |
| Intel |  | Y | Y |  |  | Y | Y | Y | Y |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Company | E1 | E2 | E3 | E4 |
| MTK | Y | Y | Y | Y |
| Ericsson | Y | N | Y | N |
| LG Electronics | Y | Y | Y | Y |
| Transsion | Y | Y | Y | Y |
| Huawei, HiSilicon | Y | Y | Y | Comment below |
| CAICT | Y | Y | Y | Y |
| ZTE, Sanechips | Y | Y(but suggest to align name between different specs) | Y | Y |
| Intel | Y | Y | Y | Y |

Other comments:

|  |  |
| --- | --- |
| **Company Name** | **Comments** |
| MTK | For T9, we are trying to discuss the issue about additional PDSCH DM-RS dropping with double symbol. With the Rel-16 NR-U introduced Type B PDSCH duration :    In some condition, only the second symbol of an additional double-symbol DM-RS is out of bound according to current Rel-16 RAN1 spec, and it breaks the orthogonality of orthogonal cover code (OCC) applied on the DM-RS. As a result, we prefer to adopt Alt 1 below (drop both symbols when the second symbol of DMRS is out of bound) to avoid this kind of scenario. |
| Ericsson | T7: This issue has been discussed for 3 meetings now (one of them in Rel-15 maintenance) without consensus. We see little point in continuing the discussion which will end up with the same result. |
| Transsion | T9: This issue has been discussed and identified at the RAN1#104-e meeting, and the intention of the final CR R1-2102009 is the same as that of MTK. In current specification, “for all values of the PDSCH duration *l*d other than 2, 5, and 7 symbols, the UE is not expected to receive DM-RS beyond the (*l*d - 1):th symbol” means that for double-symbol DMRS, the UE is not expected to receive the two DM-RS symbols. The language “DM-RS” highlighted in yellow in current spec is for simplicity and to be consistent with the description in “if the PDSCH duration is 12 or 13 symbols, the UE is not expected to receive DM-RS mapped to symbol 12 or later in the slot”. Hence, we believe that this issue should not be discussed again. |
| MTK2 | Thanks Transsion for pointing out that T9 is already discussed before and had a corresponding CR R1-2102009. The information is very helpful to us. We agree with Transsion that T9 is **not** needed to be discussed again in RAN1 #107e. |
| Huawei, HiSilicon | **T1:** The new regulation for 2.4GHz, 5.1GHz and 5.8GHz in China was formally issued on Sept 8. It will take effect from Jan 1 2022. Current FBE mechanism did not conform to the regulation and should be resolved.  **T2:** As for the 2nd change, the current spec allocate all RE of PUSCH to CG-UCI, CSI-part- 1 and CSI-part-2. There is no space for CG-PUSCH.  **T5:** We think this correction is inaccurate as is used for defining the time interval on which the extension **time-continuous** signal is generated from the discrete samples using Tc. Therefore, should be also calculated in a time-continuous manner which also captures the gap duration accurately. Then, the calculation of the signal takes care of the Tc time unit.  **E4:** This clarifying editorial can be handled, if needed, without deletion |

# Reference

1. R1-2110822, Changes of channel access procedure in TS 37.213 according to MIIT regulation, Huawei, HiSilicon
2. R1-2110823, Discussion on the impact of MIIT consultation to channel access procedure, Huawei, HiSilicon
3. R1-2110824, Changes of channel access types tables in TS 38.212, Huawei, HiSilicon
4. R1-2110825, Corrections on CG-UCI multiplexing in TS38.212, Huawei, HiSilicon
5. R1-2110826, Discussion on the frequency hopping for single/multi PUSCH transmission, Huawei, HiSilicon
6. R1-2110974, Discussion on channel access procedures for consecutive UL transmissions, vivo
7. R1-2110975, Correction on channel access procedures for consecutive UL transmission(s), vivo
8. R1-2110977, Discussions on frequency hopping for PUSCH,PUCCH and SRS, vivo
9. R1-2110978, Draft CR on 38.214 on frequency hopping for multi-PUSCH scheduling by a single DCI, vivo
10. R1-2111082, Correction on slot configuration in TS 38.213, ZTE, Sanechips
11. R1-2111339, Correction on Type-3 HARQ-ACK codebook, OPPO
12. R1-2111340, Draft CR for correction on unit of CP extension, OPPO
13. R1-2111461, UL Transmissions in Wideband Operation, Ericsson, Nokia, NSB, LG Electronics, Qualcomm, Huawei, HiSilicon
14. R1-2111462, Discussion on LS from RAN4 on measing CSI-RS during SCell activation, Ericsson
15. R1-2111714, Correction on usage of subCarrierSpacingCommon for unlicensed, Samsung
16. R1-2111927, Changes of channel access procedure in TS 37.213, Huawei, HiSilicon
17. R1-2112294, On additional PDSCH DM-RS dropping with double symbol, MediaTek Inc.
18. R1-2112350, Correction on UL channel access procedure Type 2A/2B/2C , Lenovo, Motorola Mobility, ZTE, Sanechips, Xiaomi, Intel, OPPO