Companies are to share their inputs on the excel spreadsheet in /tsg\_ran/WG1\_RL1/TSGR1\_107-e/Inbox/drafts/8.1.1/RRC parameters/ herein.

## Inputs on version 00

Please share your inputs, if any, in the following table

Table 1 Inputs: Initial version

|  |  |
| --- | --- |
| **Company** | **Input** |
| ZTE | Regarding row 4 (tci-StateType), we think that it should be removed especially when we have the row 6.Regarding row 8 (p0\_Alpha\_CLIdPUCCHSet), it should be noted that there is no alpha for PUCCH, so we need to refresh the bullet as follows:

|  |  |  |  |
| --- | --- | --- | --- |
| p0~~\_Alpha~~\_CLIdPUCCHSet | new |   | UL PC parameters other than PLRS (Set of P0~~, alpha~~ and closed loop index): PUCCH  |

Similarly, for row 10, we have the update like: "p0\_Alpha\_CLIdPUSCHSet; p0~~\_Alpha~~\_CLIdPUCCHSet; p0\_Alpha\_CLIdSRSSet"Regarding row 17/18 (NeighbourCell\_Info, NeighbourCell\_Info\_ID), we prefer to reuse the same parameter of ‘AdditionalPCIInfo’ agreed in 8.1.2.2, rather than introducing a new one. The corresponding for row 13 is needed.Regarding row 35 (SourceRS-Info\_r17-PLRS), we have the following modification suggestion:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| [TCI-State\_r17 or new IE list for PSRS (typo?) in PUSCH\_Config] |   | SourceRS-Info\_r17-PLRS | new |   | ~~Source RS and QCL Info definition for~~ Rel-17path-loss measurement RS (PL-RS) |

 |
| Ericsson | Row 3 (tci-StateId\_r17): not needed. Since we have now agreed that the maximum number of joint TCI states is 128, tci\_StateId can be reusedRow 4: (tci-StateType): similar to ZTE, we think this is not needed.Row 7-9: combine into one structure. The same set of parameters would be used, only with different values for the different channels.Row 11 (InterCellBeamMetrics): Since CSI-SSB-ResourceSet is reused, there is no need to have a separate parameter. Besides, any combination of intra-cell and inter-cell measurements can be combined in one report.Row 17 (CSI-AssociatedReportConfigInfo): not needed, since tci\_StateId is reusedRow 18 (NZP-CSI-RS-Resource): not needed, since tci\_StateId is reusedRow 30 (NrofTCI-States\_r17): This is not an RRC parameter (that can be configured). This is part of “Multiplicity and type constraint definitions”. There are no candidate values, it is simply used to indicate the maximum length of lists in ASN.1. The description should state that it is the maximum number of TCI-State\_r17. The value should be 128, according to agreements. RAN2 typically starts the name with “max”Row 31 (NrofULTCI-States\_r17): This is not an RRC parameter (that can be configured). These are “Multiplicity and type constraint definitions”. There are no candidate values, it is simply used to indicate the maximum length of lists in ASN.1. The description should state that it is the maximum number of UL\_TCI-State\_r17. The value should be 64, according to agreements. RAN2 typically starts the name with “max”. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## Inputs on version xx

Please share your inputs, if any, in the following table

....