**3GPP TSG RAN WG1 Meeting #107 R1-21xxxxx**

**e-Meeting, November 11th – 19th, 2021**

**Agenda Item: 8.9**

**Source: Moderator (Huawei)**

**Title: Feature lead summary on 107-e-R17-RRC-NB-IoT-eMTC**

**Document for: Discussion and Decision**

# Introduction

In email discussion of RAN1#106bis-e, there were discussion on RRC parameters for the WI [1]. And the list of stable rows was endorsed in [2].

This documents provides the proposals and summary of discussions of the corresponding email discussion on RRC parameters.

[106bis-e-R17-RRC-NB-IoT-eMTC] Email discussion on Rel-17 RRC parameters for Rel-17 NB-IoT and eMTC – Yubo (Huawei)

The RRC parameter list is also attached: [RAN1#107-e\_Rel-17\_RRC\_NB-IoT\_eMTC\_v1.xlsx](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_107-e/Inbox/drafts/8.9/RRC/RAN1%23107-e_Rel-17_RRC_NB-IoT_eMTC_v1.xlsx).

# Discussion

## Support of 16-QAM for unicast in UL and DL for NB-IoT

**Issue 1-1: Configuration of PUR**

For the configuration of NPUSCH for PUR, the two rows below are marked as stable.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NB\_IOTenh4\_LTE\_eMTC6 | 16QAM for NB-IoT | 36.211, 36.213 | 　 | 　 | 　 | enable16QAM-ul in PUR-config-NB | New | enable 16QAM for NPUSCH in PUR procedure | Enable/disable the use of 16QAM for NPUSCH in PUR procedure | Enable | disable | Per UE | UE specific | 36.331 | According to the following agreement, the configurations are up to RAN2, including the MCS indices, RU indices and UL power control parameter: AgreementTo support 16-QAM for NPDSCH and NPUSCH in PUR procedure,• 16-QAM can be enabled/disabled by UE specific RRC signaling for NPDSCH and NPUSCH separately• The corresponding configurations and signaling details are up to RAN2 |
| NB\_IOTenh4\_LTE\_eMTC6 | 16QAM for NB-IoT | 36.211, 36.213 | 　 | 　 | 　 | enable16QAM-dl in PUR-config-NB | New | enable 16QAM for NPDSCH in PUR procedure | Enable/disable the use of 16QAM for NPDSCH in PUR procedure | Enable | disable | Per UE | UE specific | 36.331 | According to the following agreement, the configurations are up to RAN2, including the configuration of power allocation: AgreementTo support 16-QAM for NPDSCH and NPUSCH in PUR procedure,• 16-QAM can be enabled/disabled by UE specific RRC signaling for NPDSCH and NPUSCH separately• The corresponding configurations and signaling details are up to RAN2 |

Please input your comments for the above proposal:

|  |  |
| --- | --- |
| Companies | Comments |
|  |  |
|  |  |
|  |  |

**Issue 1-2: Configuration for downlink power allocation**

For the following rows for configuration of power allocation:

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NB\_IOTenh4\_LTE\_eMTC6 | 16QAM for NB-IoT | 36.213 | 　 | 　 | 　 | NPDSCH-NRS-PowerRatio | New | Power ratio of NPDSCH EPRE to NRS EPRE in symbols without NRS | the Power ratio of NPDSCH EPRE to NRS EPRE in symbols without NRS for standalone and guard-band deployments, or in symbols without NRS nor CRS for in-band deployments | FFS | 　 | Per UE | UE specific | 36.331 | Confirm working assumption:Working AssumptionFor downlink power allocation to support 16QAM:• For standalone and guard-band deployments:o One power ratio is signaled optionally§ NPDSCH EPRE to NRS EPRE in symbols without NRSo The same transmit power is assumed across different symbols.o If the signalling is not indicated, the legacy power allocation is used.§ i.e., the ratio of NPDSCH EPRE to NRS EPRE is 0dB for one NRS antenna port, and -3dB for two NRS antenna ports• UE specific signalling is used |
| NB\_IOTenh4\_LTE\_eMTC6 | 16QAM for NB-IoT | 36.213 | 　 | 　 | 　 | NPDSCH-NRS-PowerRatio-withCRS | New | Power ratio of NPDSCH EPRE to NRS EPRE in symbols with CRS | the Power ratio of NPDSCH EPRE to NRS EPRE in symbols with CRS for inband deployments | FFS | 　 | Per UE | UE specific | 36.331 | AgreementConfirm the following working assumption:For downlink power allocation to support 16QAM:• For inband deployments, a power ratio is signaled in addition to the signalling for standalone and guard-band deployments which in this case applies to “symbols with NRS” and “symbols without NRS nor CRS”. o the power ratio between NPDSCH EPRE and NRS EPRE in symbols with CRS is signalledo the signalling is UE specificNote: “symbols with NRS” and “symbols without NRS nor CRS” have the same power. |

There is following proposal

|  |  |
| --- | --- |
| Sourcing | Proposals |
| [3] | **Proposal 6: The value range for RRC parameter power ratio of NPDSCH EPRE to NRS EPRE in symbols without NRS should be {-6, -4.77, -3, -1.77, 0, 1, 2, 3} dB.** |

Please input your comments on the value range of the higher layer parameters for power allocation:

|  |  |
| --- | --- |
| Companies | Comments |
|  |  |
|  |  |
|  |  |

**Issue 1-3: Configuration for uplink power control**

This will be discussed once there’s new agreement.

**Issue 1-4: Others**

Please input your comments on issues other than the above ones:

|  |  |
| --- | --- |
| Companies | Comments |
|  |  |
|  |  |
|  |  |

## Support additional PDSCH scheduling delay for introduction of 14-HARQ processes in DL for eMTC

Please input your comments in below table:

|  |  |
| --- | --- |
| Companies | Comments |
|  |  |
|  |  |
|  |  |

## Support a maximum DL TBS of 1736 bits as a Rel-17 optional UE capability

Please input your comments in below table:

|  |  |
| --- | --- |
| Companies | Comments |
|  |  |
|  |  |
|  |  |

# Summary

# References

1. R1-2110650 Feature lead summary on 106bis-e-R17-RRC-NB-IoT-eMTC, Moderator (Huawei), RAN1#106bis-e, Oct., 11th-19th, 2021.
2. R1-2110572 Consolidated higher layers parameter list for Rel-17 LTE, Moderator (Ericsson), RAN1#106bis-e, Oct., 11th-19th, 2021.
3. R1-2110857 Support of 16QAM for unicast in UL and DL in NB-IoT Huawei, HiSilicon
4. R1-2111070 Discussion on 16QAM for NB-IoT ZTE, Sanechips
5. R1-2111133 Support of 16-QAM for NB-IoT Nokia, Nokia Shanghai Bell
6. R1-2111449 Support of 16-QAM for NB-IoT Qualcomm Incorporated
7. R1-2112001 Support 16QAM for NBIoT Lenovo, Motorola Mobility
8. R1-2112300 Discussion on CQI table and NPUSCH power control parameter for 16QAM MediaTek Inc.
9. R1-2112361 Support of 16-QAM for unicast in UL and DL in NB-IoT Ericsson
10. R1-2110858 Support of 14-HARQ processes in DL for HD-FDD MTC UEs Huawei, HiSilicon
11. R1-2111071 Remaining issues on 14-HARQ processes in DL for eMTC ZTE, Sanechips
12. R1-2111134 Support of 14-HARQ processes in DL for eMTC Nokia, Nokia Shanghai Bell
13. R1-2111450 Support of 14 HARQ processes and scheduling delay Qualcomm Incorporated
14. R1-2112362 Support of 14 HARQ processes in DL in LTE-MTC Ericsson
15. R1-2111939 Further considerations on Rel-17 NB-IoT and eMTC enhancements Huawei, HiSilicon
16. R1-2112363 On the support of 16-QAM for unicast in UL and DL in TDD NB-IoT Ericsson