## Inputs on version 00

Please share your inputs, if any, in the following table

Table 1 Inputs: Initial version

|  |  |
| --- | --- |
| **Company** | **Input** |
| vivo | **In section 6.12 add “can be” as highlighted below**An UE can be configured with multiple cells with different PCIs depending on capability however only one can be activate at a time.  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## Inputs on version xx

Please share your inputs, if any, in the following table

....