**3GPP TSG RAN WG1 Meeting #109-e R1-22xxxxx**

**e-Meeting, May 9 - 20, 2022**

**Agenda Item: 8.9**

**Source: Moderator (Huawei)**

**Title: Feature lead summary on 109-e-LTE-Rel17-NB-IoT-eMTC-01**

**Document for: Discussion and Decision**

# Introduction

This documents provides the proposals and summary of discussions of the following email discussion according to the inputs [2-5]. The detailed discussion in preparation phase can be found in [6].

[109-e-LTE-Rel17-NB-IoT-eMTC-01] Email discussion for Maintenance on support of 16-QAM, including Issue 1 and Issue 2 in FL summary R1-22xxxxx, – Yubo (Huawei)

* Discussion and decision by 5/14

# Discussion

## Issue 1: On whether and how to use the DwPTS in special subframes for NPDSCH with 16QAM

The proposals are summarized in the following table.

|  |  |
| --- | --- |
| Related contributions | Proposals |
| [2] | Text proposal to TS 36.211:  - On an NB-IoT carrier for which higher-layer parameter *operationModeInfo* indicates *inband-SamePCI* or *inband-DifferentPCI*, or higher-layer parameter *inbandCarrierInfo* is present, or on an NB-IoT carrier for *SystemInformationBlockType1-NB* for which *sib1-carrierInfo* indicates *non-anchor* and the value of the higher layer parameter *sib-GuardbandInfo* is set to *sib-GuardbandInbandSamePCI* or *sib-GuardbandinbandDiffPCI*, DwPTS in special subframe configuration 0 and 5 for normal cyclic prefix is not used for NPDCCH and NPDSCH transmission. DwPTS in special subframe configuration 9 for normal cyclic prefix is not used for NPDSCH transmission with 16QAM, when *NPDSCH-16QAM-Config-NB* is configured. |
| [4] | Text proposal to TS 36.211:  On an NB-IoT carrier for which higher-layer parameter *operationModeInfo* indicates *inband-SamePCI* or *inband-DifferentPCI*, or higher-layer parameter *inbandCarrierInfo* is present, or on an NB-IoT carrier for *SystemInformationBlockType1-NB* for which *sib1-carrierInfo* indicates *non-anchor* and the value of the higher layer parameter *sib-GuardbandInfo* is set to *sib-GuardbandInbandSamePCI* or *sib-GuardbandinbandDiffPCI*, DwPTS in special subframe configuration 0 and 5 for normal cyclic prefix is not used for NPDCCH and NPDSCH transmission, and when *npdsch-16QAM-Config-r17* is configured then DwPTS in special subframe configuration 9 for normal cyclic prefix is also not used for NPDSCH transmission. |
| [5] | **Proposal 1: It is up to the eNB to ensure that NPDSCH transmission on DwPTS using 16-QAM is self-decodable (e.g. coding rate lower than 0.932) by the UE after rate matching. There is no need for specification change.** |

As the background, the following was agreed in the last meeting on support of 16QAM for NPDSCH in TDD operation.

Agreement

* FDD/TDD differentiation is needed for FGs 1-1/1-2
  + DwPTS in special subframe configuration 9 for normal cyclic prefix is not used for NPDSCH transmission with 16QAM, when 16QAM is configured.

Please input your comments on whether a CR is needed on the use of DwPTS, and if your answer is yes, your comments to the CR proposed in [2] and [3].

|  |  |
| --- | --- |
| Companies | Comments |
|  |  |
|  |  |
|  |  |

## Issue 2: On the RRC configuration for NPDSCH 16QAM regarding power allocation in PUR procedure

The proposals are summarized in the following table.

|  |  |
| --- | --- |
| Related contributions | Proposals |
| [3] | Text proposal to TS 36.213:  If a UE is configured with higher layer parameters *npdsch-16QAM-Config* or *pur-DL-16QAM-Config* and *nrs-PowerRatio*,  - the ratio of NPDSCH EPRE to NRS EPRE among NPDSCH REs in symbols with NRS is given by for a cell with one NRS antenna port and for a cell with two NRS antenna ports, where is given by the parameter *nrs-PowerRatio*. |

In the preparation phase, there was some discussion on whether *npdsch-16QAM-Config* can refer to both connected mode and idle mode PUR procedure. In current 36.331 V17.0.0, the high layer parameters related to NPDSCH 16QAM are in the following IE:

NPDSCH-16QAM-Config-NB-r17 ::=SEQUENCE{

nrs-PowerRatio-r17 ENUMERATED {dB-6, dB-4dot77, dB-3, dB-1dot77, dB0, dB1, dB2, dB3} OPTIONAL,

nrs-PowerRatioWithCRS-r17 ENUMERATED {dB-6, dB-4dot77, dB-3, dB-1dot77, dB0, dB1, dB2, dB3} OPTIONAL -- Cond InBand

}

And for connected mode, the following configuration is used:

PhysicalConfigDedicated-NB-r13 ::= SEQUENCE {

*<unrelated parts omitted>*

[[ npusch-ConfigDedicated-v1700 NPUSCH-ConfigDedicated-NB-v1700 OPTIONAL, -- Need ON

npdsch-ConfigDedicated-v1700 SetupRelease {NPDSCH-16QAM-Config-NB-r17} OPTIONAL, -- Need ON

uplinkPowerControlDedicated-v1700 UplinkPowerControlDedicated-NB-v1700 OPTIONAL -- Cond npusch-16QAM

]]

}

And for PUR procedure in idle mode, the following configuration is used:

PUR-Config-NB-r16 ::= SEQUENCE {

*<unrelated parts omitted>*

[[

pur-PhysicalConfig-v1700 SEQUENCE {

pur-UL-16QAM-Config-r17 SetupRelease {PUR-UL-16QAM-Config-NB-r17} OPTIONAL, -- Need ON

pur-DL-16QAM-Config-r17 SetupRelease {NPDSCH-16QAM-Config-NB-r17} OPTIONAL -- Need ON

} OPTIONAL -- Need ON

]]

}

From the above IE, *npdsch-ConfigDedicated-v1700* is used to configure 16QAM for connected mode, and *pur-DL-16QAM-Config-r17* is used for PUR procedure, while both refer to NPDSCH-16QAM-Config-NB-r17 as the structure of the parameters. However, with the following field description, npdsch-16QAM-Config is the field identifier to configure 16QAM for connected mode, as that have used in RAN1 specs. It’s also noted that there’s some CR submitted to correct this inconsistency (e.g., R2-2206039).

| ***npdsch-16QAM-Config***  Activativation of 16QAM for DL, see TS 36.213 [23]. |
| --- |

Based on the above observation, it should be RAN2’s intention to use *npdsch-16QAM-Config* for connected configuration and *pur-DL-16QAM-Config-r17* for PUR procedure in idle mode.

Please input your comments to this issue and the related text proposal.

|  |  |
| --- | --- |
| Companies | Comments |
|  |  |
|  |  |
|  |  |

# Summary

TBD.

# References

1. RP-211340, “WID revision: Additional enhancements for NB-IoT and LTE-MTC”, Huawei, HiSilicon, RAN#92e, E-meeting, June 2021.
2. R1-2203223 On use of DwPTS for 16QAM NPDSCH in NB-IoT Huawei, HiSilicon
3. R1-2203631 Clarifications for DL power allocation for 16-QAM ZTE, Sanechips
4. R1-2204082 Support of 16-QAM for unicast in UL and DL in NB-IoT Ericsson
5. R1-2204878 Support of 16-QAM in NB-IoT TDD Nokia, Nokia Shanghai Bell
6. R1-2204878 Preparation phase discussion on 109-e-Prep-AI8.9 NB-IoT-eMTC Moderator (Huawei)