**3GPP TSG-RAN WG1 Meeting #110bis-eR1-221xxxx**

**e-Meeting, October 10– 19, 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **DRAFT CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.213** | **CR** | **xxxx** | **rev** |  | **Current version:** | **17.3.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Draft CR on handling SR and NACK-only collision | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Moderator (Huawei) | | | | | | | | | |
| ***Source to TSG:*** | R1 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_MBS-Core | | | | |  | ***Date:*** | | | 2022-10-13 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | To reflect the following agreement to clause 18 in TS38.213:  ***Agreement***  *It is up to UE implementation on which one to drop between SR or NACK-only when NACK-only collides with SR when UE would transmit PUCCH with HARQ-ACK according to the second reporting mode.* | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | It is up to UE implementation on which one to drop between SR or NACK-only when NACK-only collides with SR when UE would transmit PUCCH with HARQ-ACK according to the second reporting mode. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | It is unclear whether SR and NACK-only can collide and how UE handles the collision if it happens. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 18 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  |  | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  |  | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  |  | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

# 18 Multicast Broadcast Services

< Unchanged parts are omitted >

A UE can be configured per G-RNTI or per G-CS-RNTI, by *harq-FeedbackEnablerMulticast* with value set to 'enabled', to provide HARQ-ACK information for PDSCH receptions. When the UE is not provided *harq-FeedbackEnablerMulticast* for a G-RNTI or G-CS-RNTI, the UE does not provide HARQ-ACK information for respective PDSCH receptions. If a UE is provided *harq-FeedbackEnablerMulticast* with value set to 'dci-enabler' for a G-RNTI or a G-CS-RNTI, the UE determines whether or not to provide the HARQ-ACK information for PDSCH receptions based on an indication by the multicast DCI format associated with the G-RNTI or the G-CS-RNTI [4, TS 38.212].

If a UE would multiplex multicast HARQ-ACK information according to the second HARQ-ACK reporting mode with multicast HARQ-ACK information according to the first HARQ-ACK reporting mode, or unicast HARQ-ACK information, or CSI reports in a first PUCCH or in a PUSCH, as described in clauses 9 and 9.2.5, the UE provides the HARQ-ACK information according to the first HARQ-ACK reporting mode. For resolving an overlapping among a second PUCCH with HARQ-ACK information according to the second HARQ-ACK reporting mode and other PUCCHs or PUSCHs prior to multiplexing the HARQ-ACK information in a PUCCH or PUSCH when the UE is provided *moreThanOneNackOnlyMode*, the UE considers that the UE would transmit the second PUCCH using any PUCCH resource from the PUCCH resources associated with the second HARQ-ACK reporting mode when all values of the HARQ-ACK information are 'ACK'. If a UE would simultaneously transmit a first PUCCH with positive SR and a second PUCCH with HARQ-ACK with the same priority index according to the second HARQ-ACK reporting mode, it is up to UE implementation for the UE to transmit either the first PUCCH or the second PUCCH.

If a UE is provided multiple G-RNTIs or G-CS-RNTIs, a configuration for a HARQ-ACK codebook type applies to all G-RNTIs or G-CS-RNTIs.

< Unchanged parts are omitted >