**3GPP TSG RAN WG1 Meeting #102-e                     R1-200xxxx**

**e-Meeting, 17 – 28 August, 2020**

**Agenda Item: 7.2.2.2.2**

**Source: Charter Communications**

**Title: Draft [102-e-NR-unlic-NRU-InitAccessProc-01]**

**Document for: Discussion and Decision**

# Introduction

One email discussion has been sanctioned in RAN1#102-e on initial access procedures for Rel-16 NR-U based on contributions submitted to this meeting **Error! Reference source not found.**-[9]. This first discussion that aims to converge by 8/20 has the following scope:

[102-e-NR-unlic-NRU-InitAccessProc-01] Email discussion/approval on the following from R1-2006648 by 8/20; if necessary, endorse associated TPs by 8/26 – Amitav (Charter)

* (#2.5) Timing reference cell update to 38.213.
* (#3.1, #3.3) DCI Format 1\_0 bit-length alignment. Reflect LSB of SFN is not always in the DCI 1\_0 when RAR/msgB window is smaller than 10ms.
* (#4.1) Further clarifications on CSI-RS measurement averaging.
* Proposed conclusions (no spec impact):
  + For FBE mode, idle UE may transmit PRACH only within FFPs for which SSB, SIBs or paging are detected.
  + There is no requirement on the difference between the first and last candidate SS/PBCH block index of the SS/PBCH block burst within a discovery burst transmission window.
    - Note: This implies gNB can transmit multiple bursts of SS/PBCH blocks within a discovery burst transmission window.
* If necessary, reply LS from RAN1 to RAN4 is necessary based on R1-2003271 and R1-2005213

These issues have been selected based on the preparatory discussion summarized in [10].

# Company views

## (#2.1) Timing reference cell update to 38.213

Issue: in RAN4 LS (R1-2003272/R4-2005373) to RAN1, RAN4 provided the following information:

According to the UE transmit timing requirements (section 7.1, TS 38.133) in endorsed CR (R4-2005374), for the UE operating in scenario B or in scenario C, if a reference cell in a cell group (CG) is unavailable at the UE for more than 160 ms then the UE [can or shall] use any of the activated SCell(s) as its reference cell for deriving its transmit timing.

However, in current RAN1 specification, Clause 4.1 in TS 38.213 in particular, it says:

“For a serving cell without transmission of SS/PBCH blocks, a UE acquires time and frequency synchronization with the serving cell based on receptions of SS/PBCH blocks on the PCell, or on the PSCell, of the cell group for the serving cell.”

------------------------------------- < Start of TP#1 for Clause 4.1 of 38.213 > -------------------------------------

Synchronization procedures

4.1 Cell search

< Unchanged parts are omitted >

For operation without shared spectrum channel access, ~~F~~for a serving cell without transmission of SS/PBCH blocks, a UE acquires time and frequency synchronization with the serving cell based on receptions of SS/PBCH blocks on the PCell, or on the PSCell, of the cell group for the serving cell.

For operation with shared spectrum channel access, for a serving cell without transmission of SS/PBCH blocks, a UE acquires time and frequency synchronization with the serving cell based on receptions of SS/PBCH blocks on the PCell, or on the PSCell, or on any activated SCell if SS/PBCH blocks on the PCell or on the PSCell are unavailable as described in [10, TS 38.133], of the cell group for the serving cell.

-------------------------------------------------- < End of TP#1> -------------------------------------------------------

|  |  |
| --- | --- |
| **Company** | **Views** |
| Samsung | The impact to 38.213 can be simplified. Since 38.133 already specifies the condition to utilize a SCell for timing, 38.213 can simply refer to 38.133 to avoid any inconsistence between specs in the future. Here is an example we are thinking:  For a serving cell without transmission of SS/PBCH blocks, a UE acquires time and frequency synchronization with the serving cell based on receptions of SS/PBCH blocks on the PCell, or on the PSCell, or on a SCell if applicable as described in [10, TS 38.133], of the cell group for the serving cell. |
| Nokia/NSB | We support the simplified text proposed by Samsung, as it prevents from having in the future inconsistencies between 38.213 and 38.133 specifications, and we would propose the following update:  For a serving cell without transmission of SS/PBCH blocks, a UE acquires time and frequency synchronization with the serving cell based on receptions of SS/PBCH blocks on the PCell, or on the PSCell, or for operation with shared spectrum access on a SCell if applicable as described in [10, TS 38.133], of the cell group for the serving cell. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## (#3.1, #3.3) DCI Format 1\_0 bit-length alignment. Reflect LSB of SFN is not always in the DCI 1\_0 when RAR/msgB window is smaller than 10ms.

Issue: In current TS 38.212-g20, the number of DCI format 1\_0 bits except for “Frequency domain resource assignment” field is

- For operation in a cell with shared spectrum channel access

o 28 bits scrambled by RA-RNTI or MsgB-RNTI.

 Note: 4 + 1 + 5 + 2 + 2 + 14.

o 30 bits scrambled by other RNTI (C-RNTI, SI-RNTI, P-RNTI, TC-RNTI).

- For operation in a cell without shared spectrum channel access

o 28 bits scrambled by all RNTI.

The bits length for DCI format 1-0 by different RNTI should be the same. So the reserved bits for the DCI format 1\_0 with CRC scrambled by RA-RNTI for operation in a cell with shared spectrum channel access should be 16 and the reserved bits for the DCI format 1\_0 with CRC scrambled by MsgB-RNTI for operation in a cell with shared spectrum channel access should also be 16 [2].

------------------------------------- < Start of TP#2 for Clause 7.3.1.2.1 of 38.212 > -------------------------------

< Unchanged parts are omitted >

- Reserved bits – 14 bits for the DCI format 1\_0 with CRC scrambled by MsgB-RNTI for operation in a cell without shared spectrum channel access; otherwise 16 bits

< Unchanged parts are omitted >

-------------------------------------------------- < End of TP#2> --------------------------------------------------------

|  |  |
| --- | --- |
| **Company** | **Views** |
| Samsung | Do we still need the TP if TP#3 is adopted? |
| Nokia/NSB | Agreed with Samsung: if TP#3 is adopted TP#2 is not needed. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

Issue: RAN2 has made a new agreement regarding the inclusion of the SFN LSB bits in DCI and has sent a new LS to RAN1. The LS states the following:

RAN2 agreed that the gNB signals the SFN bits to the UE only if there is a risk of ambiguity, i.e. if the random access response window or the MSGB response window is larger than 10 ms. The RAR window is configured by *ra-ResponseWindow* or *ra-ResponseWindow-r16* and the MSGB response window is configured by *msgB-ResponseWindow-r16*.

Proposals [5]:

* 38.212 should state that the 2 SFN LSB bits are only included in DCI 1\_0 if either the RAR window or MsgB response window is configured to be larger than 10 ms
* Remove the text "if applicable" in 38.213, since it is now clear when the SFN LSB bits are included in DCI and that the UE must read them when they are included

--------------------------------- < Start of TP#3 for Clause 7.3.1.2.1 of 38.212 > -----------------------------------

\*\*\* Unchanged text omitted \*\*\*

The following information is transmitted by means of the DCI format 1\_0 with CRC scrambled by RA-RNTI or MsgB-RNTI:

- Frequency domain resource assignment – bits

-  is the size of CORESET 0 if CORESET 0 is configured for the cell and  is the size of initial DL bandwidth part if CORESET 0 is not configured for the cell

- Time domain resource assignment – 4 bits as defined in Clause 5.1.2.1 of [6, TS38.214]

- VRB-to-PRB mapping – 1 bit according to Table 7.3.1.2.2-5

- Modulation and coding scheme – 5 bits as defined in Clause 5.1.3 of [6, TS38.214], using Table 5.1.3.1-1

- TB scaling – 2 bits as defined in Clause 5.1.3.2 of [6, TS38.214]

- LSBs of SFN – 2 bits for the DCI format 1\_0 with CRC scrambled by MsgB-RNTI as defined in Clause 8.2A of [5, TS 38.213] if *msgB-responseWindow-r16* is configured to be larger than 10 ms; or 2 bits for the DCI format 1\_0 with CRC scrambled by RA-RNTI as defined in Clause 8.2 of [5, TS 38.213] for operation in a cell with shared spectrum channel access if *ra-ResponseWindow or ra-ResponseWindow-v1610* is configured to be larger than 10 ms; 0 bit otherwise

- Reserved bits – 14 bits for the DCI format 1\_0 with CRC scrambled by MsgB-RNTI if *msgB-responseWindow-r16* is configured to be larger than 10 ms; or 14 bits for the DCI format 1\_0 with CRC scrambled by RA-RNTI for operation in a cell with shared spectrum channel access if *ra-ResponseWindow or ra-ResponseWindow-v1610* is configured to be larger than 10 ms; otherwise 16 bits

\*\*\* Unchanged text omitted \*\*\*

-------------------------------------------------- < End of TP#3> --------------------------------------------------------

--------------------------------- < Start of TP#4 for Clause 8 of 38.213 > -----------------------------------

\*\*\* Unchanged text omitted \*\*\*

8.2 Random access response - Type-1 random access procedure

In response to a PRACH transmission, a UE attempts to detect a DCI format 1\_0 with CRC scrambled by a corresponding RA-RNTI during a window controlled by higher layers [11, TS 38.321]. The window starts at the first symbol of the earliest CORESET the UE is configured to receive PDCCH for Type1-PDCCH CSS set, as defined in Clause 10.1, that is at least one symbol, after the last symbol of the PRACH occasion corresponding to the PRACH transmission, where the symbol duration corresponds to the SCS for Type1-PDCCH CSS set as defined in Clause 10.1. The length of the window in number of slots, based on the SCS for Type1-PDCCH CSS set, is provided by *ra-ResponseWindow*.

If the UE detects the DCI format 1\_0 with CRC scrambled by the corresponding RA-RNTI and LSBs of a SFN field in the DCI format 1\_0, if included ~~and applicable~~, are same as corresponding LSBs of the SFN where the UE transmitted PRACH, and the UE receives a transport block in a corresponding PDSCH within the window, the UE passes the transport block to higher layers. The higher layers parse the transport block for a random access preamble identity (RAPID) associated with the PRACH transmission. If the higher layers identify the RAPID in RAR message(s) of the transport block, the higher layers indicate an uplink grant to the physical layer. This is referred to as random access response (RAR) UL grant in the physical layer.

If the UE does not detect the DCI format 1\_0 with CRC scrambled by the corresponding RA-RNTI within the window, or if the UE detects the DCI format 1\_0 with CRC scrambled by the corresponding RA-RNTI within the window and LSBs of a SFN field in the DCI format 1\_0, if included ~~and applicable~~, are not same as corresponding LSBs of the SFN where the UE transmitted PRACH, or if the UE does not correctly receive the transport block in the corresponding PDSCH within the window, or if the higher layers do not identify the RAPID associated with the PRACH transmission from the UE, the higher layers can indicate to the physical layer to transmit a PRACH. If requested by higher layers, the UE is expected to transmit a PRACH no later than  msec after the last symbol of the window, or the last symbol of the PDSCH reception, where  is a time duration of  symbols corresponding to a PDSCH processing time for UE processing capability 1 assuming  corresponds to the smallest SCS configuration among the SCS configurations for the PDCCH carrying the DCI format 1\_0, the corresponding PDSCH when additional PDSCH DM-RS is configured, and the corresponding PRACH. For , the UE assumes  [6, TS 38.214]. For a PRACH transmission using 1.25 kHz or 5 kHz SCS, the UE determines  assuming SCS configuration .

If the UE detects a DCI format 1\_0 with CRC scrambled by the corresponding RA-RNTI and LSBs of a SFN field in the DCI format 1\_0, if included ~~and applicable~~, are same as corresponding LSBs of the SFN where the UE transmitted the PRACH, and the UE receives a transport block in a corresponding PDSCH, the UE may assume same DM-RS antenna port quasi co-location properties, as described in [6, TS 38.214], as for a SS/PBCH block or a CSI-RS resource the UE used for PRACH association, as described in Clause 8.1, regardless of whether or not the UE is provided *TCI-State* for the CORESET where the UE receives the PDCCH with the DCI format 1\_0.

If the UE attempts to detect the DCI format 1\_0 with CRC scrambled by the corresponding RA-RNTI in response to a PRACH transmission initiated by a PDCCH order that triggers a contention-free random access procedure for the SpCell [11, TS 38.321], the UE may assume that the PDCCH that includes the DCI format 1\_0 and the PDCCH order have same DM-RS antenna port quasi co-location properties. If the UE attempts to detect the DCI format 1\_0 with CRC scrambled by the corresponding RA-RNTI in response to a PRACH transmission initiated by a PDCCH order that triggers a contention-free random access procedure for a secondary cell, the UE may assume the DM-RS antenna port quasi co-location properties of the CORESET associated with the Type1-PDCCH CSS set for receiving the PDCCH that includes the DCI format 1\_0.

A RAR UL grant schedules a PUSCH transmission from the UE. The contents of the RAR UL grant, starting with the MSB and ending with the LSB, are given in Table 8.2-1.

If the value of the frequency hopping flag is 0, the UE transmits the PUSCH without frequency hopping; otherwise, the UE transmits the PUSCH with frequency hopping.

The UE determines the MCS of the PUSCH transmission from the first sixteen indexes of the applicable MCS index table for PUSCH as described in [6, TS 38.214].

The TPC command value  is used for setting the power of the PUSCH transmission, as described in Clause 7.1.1, and is interpreted according to Table 8.2-2.

The CSI request field is reserved.

The ChannelAccess-CPext field indicates a channel access type and CP extension for operation with shared spectrum channel access [15, TS 37.213].

**Table 8.2-1: Random Access Response Grant Content field size**

|  |  |
| --- | --- |
| **RAR grant field** | **Number of bits** |
| Frequency hopping flag | 1 |
| PUSCH frequency resource allocation | 14, for operation without shared spectrum channel access  12, for operation with shared spectrum channel access |
| PUSCH time resource allocation | 4 |
| MCS | 4 |
| TPC command for PUSCH | 3 |
| CSI request | 1 |
| ChannelAccess-CPext | 0, for operation without shared spectrum channel access  2, for operation with shared spectrum channel access |

**Table 8.2-2: TPC Command  for PUSCH**

|  |  |
| --- | --- |
| **TPC Command** | **Value (in dB)** |
| 0 | -6 |
| 1 | -4 |
| 2 | -2 |
| 3 | 0 |
| 4 | 2 |
| 5 | 4 |
| 6 | 6 |
| 7 | 8 |

Unless the UE is configured a SCS, the UE receives subsequent PDSCH using same SCS as for the PDSCH reception providing the RAR message.

If the UE does not detect the DCI format 1\_0 with CRC scrambled by the corresponding RA-RNTI within the window, or if the UE detects the DCI format 1\_0 with CRC scrambled by the corresponding RA-RNTI within the window and the LSBs of a SFN field in the DCI format 1\_0, if included ~~and applicable~~, are not same as corresponding LSBs of the SFN where the UE transmitted the PRACH, or the UE does not correctly receive a corresponding transport block within the window, the UE procedure is as described in [11, TS 38.321].

8.2A Random access response - Type-2 random access procedure

In response to a transmission of a PRACH and a PUSCH, or to a transmission of only a PRACH if the PRACH preamble is mapped to a valid PUSCH occasion, a UE attempts to detect a DCI format 1\_0 with CRC scrambled by a corresponding MsgB-RNTI during a window controlled by higher layers [11, TS 38.321]. The window starts at the first symbol of the earliest CORESET the UE is configured to receive PDCCH for Type1-PDCCH CSS set, as defined in Clause 10.1, that is at least one symbol, after the last symbol of the PUSCH occasion corresponding to the PRACH transmission, where the symbol duration corresponds to the SCS for Type1-PDCCH CSS set. The length of the window in number of slots, based on the SCS for Type1-PDCCH CSS set, is provided by *msgB-ResponseWindow*.

In response to a transmission of a PRACH, if the PRACH preamble is not mapped to a valid PUSCH occasion, a UE attempts to detect a DCI format 1\_0 with CRC scrambled by a corresponding MsgB-RNTI during a window controlled by higher layers [11, TS 38.321]. The window starts at the first symbol of the earliest CORESET the UE is configured to receive PDCCH for Type1-PDCCH CSS set, as defined in Clause 10.1, that is at least one symbol, after the last symbol of the PRACH occasion corresponding to the PRACH transmission, where the symbol duration corresponds to the SCS for Type1-PDCCH CSS set. The length of the window in number of slots, based on the SCS for Type1-PDCCH CSS set, is provided by *msgB-ResponseWindow*.

If the UE detects the DCI format 1\_0, with CRC scrambled by the corresponding MsgB-RNTI and LSBs of a SFN field in the DCI format 1\_0, if included ~~applicable~~, are same as corresponding LSBs of the SFN where the UE transmitted PRACH, and the UE receives a transport block in a corresponding PDSCH within the window, the UE passes the transport block to higher layers. The higher layers indicate to the physical layer

- an uplink grant if the RAR message(s) is for fallbackRAR and a random access preamble identity (RAPID) associated with the PRACH transmission is identified, and the UE procedure continues as described in Clauses 8.2, 8.3, and 8.4 when the UE detects a RAR UL grant, or

- transmission of a PUCCH with HARQ-ACK information having ACK value if the RAR message(s) is for successRAR, where

- a PUCCH resource for the transmission of the PUCCH is indicated by PUCCH resource indicator field of 4 bits in the successRAR from a PUCCH resource set that is provided by *pucch-ResourceCommon*

- a slot for the PUCCH transmission is indicated by a PDSCH-to-HARQ\_feedback timing indicator field of 3 bits in the successRAR having a value from {1, 2, 3, 4, 5, 6, 7, 8} and, with reference to slots for PUCCH transmission having duration , the slot is determined as , where is a slot of the PDSCH reception and is as defined for PUSCH transmission in Table 6.1.2.1.1-5 of [6, TS 38.214]

- the UE does not expect the first symbol of the PUCCH transmission to be after the last symbol of the PDSCH reception by a time smaller than msec where is the PDSCH processing time for UE processing capability 1 [6, TS 38.214]

- for operation with shared spectrum channel access, a channel access type and CP extension [15, TS 37.213] for a PUCCH transmission is indicated by a ChannelAccess-CPext field in the successRAR

- the PUCCH transmission is with a same spatial domain transmission filter and in a same active UL BWP as a last PUSCH transmission

If the UE detects the DCI format 1\_0 with CRC scrambled by a C-RNTI and a transport block in a corresponding PDSCH within the window, the UE transmits a PUCCH with HARQ-ACK information having ACK value if the UE correctly detects the transport block or NACK value if the UE incorrectly detects the transport block and the time alignment timer is running [11, TS 38.321].

If the UE detects a DCI format 1\_0 with CRC scrambled by the corresponding MsgB-RNTI and receives a transport block within the window in a corresponding PDSCH, the UE may assume same DM-RS antenna port quasi co-location properties, as described in [6, TS 38.214], as for a SS/PBCH block the UE used for PRACH association, as described in Clause 8.1, regardless of whether or not the UE is provided *TCI-State* for the CORESET where the UE receives the PDCCH with the DCI format 1\_0.

The UE does not expect to be indicated to transmit the PUCCH with the HARQ-ACK information at a time that is prior to a time when the UE applies a TA command that is provided by the transport block. If the UE does not detect the DCI format 1\_0 with CRC scrambled by the corresponding MsgB-RNTI within the window, or if the UE detects the DCI format 1\_0 with CRC scrambled by the corresponding MsgB-RNTI within the window and LSBs of a SFN field in the DCI format 1\_0, if included ~~applicable~~, are not same as corresponding LSBs of the SFN where the UE transmitted the PRACH, or if the UE does not correctly receive the transport block in the corresponding PDSCH within the window, or if the higher layers do not identify the RAPID associated with the PRACH transmission from the UE, the higher layers can indicate to the physical layer to transmit only PRACH according to Type-1 random access procedure or to transmit both PRACH and PUSCH according to Type-2 random access procedure [11, TS 38.321]. If requested by higher layers, the UE is expected to transmit a PRACH no later than msec after the last symbol of the window, or the last symbol of the PDSCH reception, where is a time duration of symbols corresponding to a PDSCH processing time for UE processing capability 1 when additional PDSCH DM-RS is configured. For , the UE assumes [6, TS 38.214].

Unless the UE is configured a SCS, the UE receives subsequent PDSCH using same SCS as for the PDSCH reception providing the RAR message.

If the UE does not detect the DCI format 1\_0 with CRC scrambled by the corresponding MsgB-RNTI within the window, or if the UE detects the 1\_0 with CRC scrambled by the corresponding MsgB-RNTI within the window and LSBs of a SFN field in the DCI format 1\_0, if included ~~applicable~~, are not same as corresponding LSBs of the SFN where the UE transmitted the PRACH, or the UE does not correctly receive a corresponding transport block within the window, the UE procedure is as described in [11, TS 38.321].

\*\*\* Unchanged text omitted \*\*\*

-------------------------------------------------- < End of TP#4> --------------------------------------------------------

|  |  |
| --- | --- |
| **Company** | **Views** |
| Samsung | We are OK with TP for 38.212. The TP for 38.213 is not quite essential, if the TP for 38.212 is adopted. |
| Nokia/NSB | Related to the “If [included and] applicable” issue our proposal within R1-2006449 was simpler than TP#3/TP#4 (only 38.123 is impacted), but we see the proposal provided by the FL as equivalent, we therefore have no objection to adopt both TP#3 and TP#4, and we believe TP#4 should be definitely adopted, since it gets rid of the ambiguous “if applicable” wording.  Related to the “DCI 1\_0 reserved bits” issue we are fine with TP#3. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## (#4.1) Further clarifications on CSI-RS measurement averaging

Issue: there were discussions (not concluded) during the last RAN1 #101-e meeting about the following paragraph within TS 38.214, subclause 5.2.1.1:

For operation with shared spectrum channel access, the UE should not average CSI-RS measurements for channel estimation from occasions of an NZP CSI-RS (defined in [4, TS 38.211]) located in different DL transmissions burst (defined in [16, TS 37.213]).

There were two concerns raised with this paragraph:

- The “located in different DL transmission bursts” wording is written from the gNB perspective, but it was unclear for some how the UE can discriminate between “different DL transmission bursts”.

- The “not average CSI-RS” statement is not applicable to NZP CSI-RS for L1-RSRP, RLM, BFD, CBD and RRM, but only to RI-PMI-CQI, RI-il, RI-il-CQI, RI-CQI or RI-LI-PMI-CQI measurements.

------------------------------------- < Start of TP#5 for Clause 5.2.1.1 of 38.214 > ---------------------------------

5.2.1.1 Reporting settings

**\*\*\* Unchanged text is omitted \*\*\***

For operation with shared spectrum channel access and if the higher layer parameter *reportQuantity* is set to 'cri-RI-PMI-CQI', 'cri-RI-LI-PMI-CQI', 'cri-RI-i1', 'cri-RI-CQI' or 'cri-RI-i1-CQI', the UE should not average CSI-RS measurements for channel estimation from occasions of an NZP CSI-RS (defined in [4, TS 38.211]) located in different DL transmissions which satisfies any of the following conditions:

* gap among the different DL transmissions is greater than if the UE does not detect a DCI format 2\_0 that indicates a channel occupancy duration which overlaps the occasions of the NZP CSI-RS

the DL transmissions are in different detected channel occupancy durations

**\*\*\* Unchanged text is omitted \*\*\***

-------------------------------------------------- < End of TP#5> --------------------------------------------------------

|  |  |
| --- | --- |
| **Company** | **Views** |
| Samsung | We are OK with the TP.  One minor editorial change on the indent format:  For operation with shared spectrum channel access and if the higher layer parameter *reportQuantity* is set to 'cri-RI-PMI-CQI', 'cri-RI-LI-PMI-CQI', 'cri-RI-i1', 'cri-RI-CQI' or 'cri-RI-i1-CQI', the UE should not average CSI-RS measurements for channel estimation from occasions of an NZP CSI-RS (defined in [4, TS 38.211]) located in different DL transmissions which satisfies any of the following conditions:   * gap among the different DL transmissions is greater than if the UE does not detect a DCI format 2\_0 that indicates a channel occupancy duration which overlaps the occasions of the NZP CSI-RS * the DL transmissions are in different detected channel occupancy durations |
| Nokia/NSB | We are fine with the first updated part of the TP related to *reportQuantity*. Regarding the remaining updates we don’t think they are needed; as indicated in our contribution R1-2006449 how the UE can discriminate “different DL transmission bursts” is already know and defined within NR-U Rel-16 specifications; adding the proposed text may lead in the future to inconsistencies between specs. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## Proposed conclusions (no spec impact)

### FBE RO

* For FBE mode, idle UE may transmit PRACH only within FFPs for which SSB, SIBs or paging are detected.

|  |  |
| --- | --- |
| **Company** | **Views** |
| Samsung | We are supportive of the proposed conclusion. |
| Nokia/NSB | We also support the proposed conclusion. 😊 |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

### SS/PBCH block burst within a discovery burst transmission window

* There is no requirement on the difference between the first and last candidate SS/PBCH block index of the SS/PBCH block burst within a discovery burst transmission window.
  + Note: This implies gNB can transmit multiple bursts of SS/PBCH blocks within a discovery burst transmission window.

|  |  |
| --- | --- |
| **Company** | **Views** |
| Samsung | We are supportive of the proposed conclusion. |
| Nokia/NSB | We also support the proposed conclusion. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## Necessity of LS reply to RAN4 based on R1-2003271 and R1-2005213

Issue: is a separate reply LS from RAN1 to RAN4 needed, given RAN2’s feedback in R1-2005213 regarding UE declaring beam failure due to LBT failures during active TCI switching?

|  |  |
| --- | --- |
| **Company** | **Views** |
| Samsung | Procedure wise a response LS seems necessary since there is an action point from the original RAN4 LS. RAN1 can send a simple one to confirm RAN2’s feedback. |
| Nokia/NSB | As indicated within our contribution R1-2006449 we are fine with both ways (Reply LS sent or not sent).  Note: In the case we agree to send a Reply LS to RAN4 Nokia volunteers to draft the Reply LS. Otherwise we would suggest to capture a conclusion stating that a Reply LS to RAN4 will not be sent because our (RAN1) statement is the same as RAN2 R1-2005213 LS. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# References

1. R1-2005334 Remaining issues on initial access procedure for NR-U vivo
2. R1-2005601 Remaining issues on the initial access procedure for NR-U ZTE, Sanechips
3. R1-2005756 TPs on DCI reserved bits length in NR-U NEC
4. R1-2005810 Maintenance on initial access procedures Huawei, HiSilicon
5. R1-2005915 Enhancements to initial access procedures Ericsson
6. R1-2006021 Discussion on the remaining issues of enhancements to initial access procedure OPPO
7. R1-2006096 Initial access procedures for NR-U Samsung
8. R1-2006449 On Enhancements to Initial Access Procedures for NR-U Nokia, Nokia Shanghai Bell
9. R1-2006764 TP for Initial access and mobility procedures for NR-U Qualcomm Incorporated
10. R1-2006648 Feature lead summary on for initial access procedures enhancements Charter Communications