**3GPP TSG RAN WG1 #102-e R1-20xxxxx**

**e-Meeting, August 17th – 28th, 2020**

**Agenda Item:** 7.2.2.2.5

**Source:** Moderator (LG Electronics)

**Title:** Summary of email discussion [102-e-NR-unlic-NRU-WB]

**Document for:** Discussion and decision

# Introduction

[102-e-NR-unlic-NRU-WB] Email discussion/approval on the following until 8/19; if necessary, endorse remaining TPs by 8/25 – Seonwook (LGE)

* Editorial changes and discussion on whether/how to reflect previous RAN1 conclusion for CORESET misconfiguration
	+ RRC parameter name alignment (freqMonitorLocations-r16, intraCellGuardBandsDL-r16, intraCellGuardBandsUL-r16) (Issue 8 in [10])
	+ Whether/how to clarify indices of RB set and GB in TS 38.214 Section 7 (Issue 8 in [10])
	+ Whether/how to reflect previous RAN1 conclusion for CORESET mis-configuration (Issue 7 in [10])

This email discussion [102-e-NR-unlic-NRU-WB] is to discuss the following issues identified from [10].

* Issue A (Issue 7 in [10]): Whether/how to reflect previous RAN1 conclusion for CORESET mis-configuration
* Issue B (Issue 8 in [10]): Editorial changes

# Issue A: Whether/how to reflect previous RAN1 conclusion for CORESET mis-configuration

## <Background>

In RAN1#101-e meeting, the following conclusion was made for CORESET configuration.

|  |
| --- |
| Conclusion:When a configured RB set contains different size of RBs than RB set 0 within the active DL BWP, UE does not expect a CORESET configuration which has CORESET resource not confined within any of the RB set indicated by *freqMonitorLocations-r16*. |

## <Proposals in contributions>

As described in [10], at least following three alternatives are identified about whether/how to reflect the above conclusion in the specification.

* Alt 1: The above conclusion is specified using the TP provided in [2] as a starting point.
* Alt 2: More generalized statement needs to be specified, e.g., UE does not expect any RE of a CORESET to overlap with any RE determined as intra-cell guard bands.
* Alt 3: No need to specify such a mis-configuration of CORESET.

## <1st round comments>

Companies are encouraged to express preference among above three alternatives.

|  |  |
| --- | --- |
| Company | Comments |
| LG Electronics | Alt 2 |
|  |  |

# Issue B: Editorial changes

## <Proposals in contributions>

As described in [10], companies suggested the following editorial changes.

* Alignment of name of RRC parameters (*freqMonitorLocations-r16, intraCellGuardBandsDL-r16, intraCellGuardBandsUL-r16*)
* There can be some ambiguity since the same index s is used to index intra-cell guard bands and RB sets, even though the number of guard bands is one less than the number of RB sets. This can be easily corrected by using different indices.
* The formatting of the variables in this section is not consistent with other specs, e.g., 38.211. Subscripts and superscripts should not be in italics, e.g., $N\_{ BWP,i}^{start,μ}$ should be $N\_{BWP,i}^{start,μ}$ and $RB\_{N\_{RB-set}-1,x}^{end,μ}$ should be $RB\_{N\_{RB-set}-1,x}^{end,μ}$. These can be highlighted and left to the editor to correct.

**<TS 38.213 Section 10.1>**

|  |
| --- |
| 10.1 UE procedure for determining physical downlink control channel assignment < Unchanged parts are omitted >For each CORESET in a DL BWP of a serving cell, a respective *frequencyDomainResources* provides a bitmap. - if a CORESET is not associated with any search space set configured with *freqMonitorLocations-r16*, the bits of the bitmap have a one-to-one mapping with non-overlapping groups of 6 consecutive PRBs, in ascending order of the PRB index in the DL BWP bandwidth of $N\_{RB}^{BWP}$ PRBs with starting common RB position $N\_{BWP}^{start}$, where the first common RB of the first group of 6 PRBs has common RB index $6⋅\left⌈N\_{BWP}^{start}/6\right⌉$ if *rb-Offset-r16* is not provided, or the first common RB of the first group of 6 PRBs has common RB index $N\_{BWP}^{start}+N\_{RB}^{offset}$ where $N\_{RB}^{offset}$ is provided by *rb-Offset-r16.* - if a CORESET is associated with at least one search space set configured with *freqMonitorLocations-r16*, the first $N\_{RBG,set0}^{size}$ bits of the bitmap have a one-to-one mapping with non-overlapping groups of 6 consecutive PRBs, in ascending order of the PRB index in each RB set $k$ in the DL BWP bandwidth of $N\_{RB}^{BWP}$ PRBs with starting common RB position $RB\_{s0+k,DL}^{start,μ} $ [6, TS 38.214], where the first common RB of the first group of 6 PRBs has common RB index $RB\_{s0+k,DL}^{start,μ}+N\_{RB}^{offset}$ and *k* is indicated by *freqMonitorLocations-r16* if provided for a search space set; otherwise, $k=0$. $N\_{RBG,set0}^{size}=\left⌊(N\_{RB,set0}^{size}-N\_{RB}^{offset})/6\right⌋$, $N\_{RB,set0}^{size}$ is a number of available PRBs in the RB set 0 for the DL BWP, and $N\_{RB}^{offset}$ is provided by *rb-Offset-r16* or $N\_{RB}^{offset}=0$ if *rb-Offset-r16* is not provided.< Unchanged parts are omitted >For each DL BWP configured to a UE in a serving cell, the UE is provided by higher layers with $S\leq 10$ search space sets where, for each search space set from the $S$ search space sets, the UE is provided the following by *SearchSpace*: - a search space set index $s$, $0<s<40$ , by *searchSpaceId* - an association between the search space set$ s$ and a CORESET $p$ by *controlResourceSetId* - a PDCCH monitoring periodicity of $k\_{s}$ slots and a PDCCH monitoring offset of $o\_{s}$ slots, by *monitoringSlotPeriodicityAndOffset*- a PDCCH monitoring pattern within a slot, indicating first symbol(s) of the CORESET within a slot for PDCCH monitoring, by *monitoringSymbolsWithinSlot* - a duration of $T\_{s}<k\_{s}$ slots indicating a number of slots that the search space set $s$ exists by *duration* - a number of PDCCH candidates $M\_{s}^{(L)}$ per CCE aggregation level $L$ by *aggregationLevel1*, *aggregationLevel2*, *aggregationLevel4*, *aggregationLevel8*, and *aggregationLevel16*, for CCE aggregation level 1, CCE aggregation level 2, CCE aggregation level 4, CCE aggregation level 8, and CCE aggregation level 16, respectively- an indication that search space set $s$ is either a CSS set or a USS set by *searchSpaceType* - if search space set $s$ is a CSS set - an indication by *dci-Format0-0-AndFormat1-0* to monitor PDCCH candidates for DCI format 0\_0 and DCI format 1\_0 - an indication by *dci-Format2-0* to monitor one or two PDCCH candidates, or to monitor one PDCCH candidate per RB set if the UE is provided *freqMonitorLocations-r16* for the search space set, for DCI format 2\_0 and a corresponding CCE aggregation level- an indication by *dci-Format2-1* to monitor PDCCH candidates for DCI format 2\_1- an indication by *dci-Format2-2* to monitor PDCCH candidates for DCI format 2\_2- an indication by *dci-Format2-3* to monitor PDCCH candidates for DCI format 2\_3- an indication by *dci-Format2-4* to monitor PDCCH candidates for DCI format 2\_4- an indication by *dci-Format2-6* to monitor PDCCH candidates for DCI format 2\_6- if search space set $s$ is a USS set, an indication by *dci-Formats* to monitor PDCCH candidates either for DCI format 0\_0 and DCI format 1\_0, or for DCI format 0\_1 and DCI format 1\_1, or an indication by *dci-Formats-Rel16* to monitor PDCCH candidates for DCI format 0\_0 and DCI format 1\_0, or for DCI format 0\_1 and DCI format 1\_1, or for DCI format 0\_2 and DCI format 1\_2, or, if a UE indicates a corresponding capability, for DCI format 0\_1, DCI format 1\_1, DCI format 0\_2, and DCI format 1\_2, or for DCI format 3\_0, or for DCI format 3\_1, or for DCI format 3\_0 and DCI format 3\_1 - a bitmap by *freqMonitorLocations-r16*, if provided, to indicate an index of one or more RB sets for the search space set $s$, where the MSB $k$ in the bitmap corresponds to RB set $k-1$ in the DL BWP. For RB set $k$ indicated in the bitmap, the first PRB of the frequency domain monitoring location confined within the RB set is given by $RB\_{s0+k,DL}^{start,μ}+N\_{RB}^{offset}$, where $RB\_{s0+k,DL}^{start,μ}$ is the index of first common RB of the RB set $k$ [6, TS 38.214], and $N\_{RB}^{offset}$ is provided by *rb-Offset-r16* or $N\_{RB}^{offset}=0$ if *rb-Offset-r16* is not provided. For each RB set with a corresponding value of 1 in the bitmap, the frequency domain resource allocation pattern for the monitoring location is determined based on the first $N\_{RBG, set 0}^{size}$ bits in *frequencyDomainResources* provided by the associated CORESET configuration. |

**<TS 38.214 Section 7>**

|  |
| --- |
| 7 UE procedures for transmitting and receiving on a carrier with intra-cell guard bandsFor operation with shared spectrum channel access, when the UE is configured with any of *intraCellGuardBandsUL-r16* for UL carrier and *intraCellGuardBandsDL-r16* for DL carrier, the UE is provided with $\_{}\_{}$ intra-cell guard bands on a carrier, each defined by start CRB and size in number of CRBs, $ \_{}^{}$ and$ GB\_{ r,x}^{size,μ}$, provided by higher layer parameters *startCRB-r16* and *nrofCRBs-r16*, respectively, where $ r\in \left\{0,1,…,N\_{RB-set,x}-2\right\}$. The subscript *x* is set to DL and UL for the downlink and uplink, respectively. Where there is no risk of confusion, the subscript *x* can be dropped. The intra-cell guard bands separate $\_{}\_{}$RB sets, each defined by start and end CRB, $RB\_{ s,x}^{start,μ} $and$RB\_{ s,x}^{end,μ}$, respectively. UE does not expect that *nrofCRBs-r16* is configured with non-zero value smaller than the applicable intra-cell guard bands as specified in [8, TS 38.101-1] corresponding to $μ$ and carrier size$\_{}^{}$. UE determines$RB\_{ 0,x}^{start,μ}=N\_{grid,x}^{start,μ}$, $RB\_{N\_{RB-set}-1,x}^{end,μ}=$$\_{}^{}\_{}^{}$, and the remaining start and end CRBs for $ s\in \left\{1,…,N\_{RB-set,x}-2\right\}$ as $ RB\_{ s,x}^{end,μ}=N\_{grid,x}^{start,μ}+GB\_{ s,x}^{start,μ}-1$ and$\_{}^{}\_{}^{}\_{}^{}\_{}^{}$. The RB set with index *s* consists of $ \_{}^{}\_{}^{}$ resource blocks where $ \_{}^{}\_{}^{}\_{}^{}\_{}^{}\_{}^{}\_{}^{}$. When the UE is not configured with *intraCellGuardBandsUL-r16,* the UE determines the CRB indices for the intra-cell guard band(s), if any, and corresponding RB set(s) according to the nominal intra-cell guard band and RB set pattern as specified in [8, TS 38.101-1] corresponding to $μ$ and carrier size$\_{}^{}$. When the UE is not configured with *intraCellGuardBandsDL-r16,* the UE determines the CRB indices for the intra-cell guard band(s), if any, and corresponding RB set(s) according to the nominal intra-cell guard band and RB set pattern as specified in [8, TS 38.101-1] corresponding to $μ$ and carrier size$\_{}^{}$. For either or both DL and UL, if the nominal intra-cell guard band and RB set pattern as specified in [8, TS 38.101-1] contains no intra-cell guard bands, the number of RB sets for the carrier is$\_{}$.For a carrier, the UE expects $ \_{}^{}\_{}^{}\_{}^{}\_{}^{}$, and $\_{}^{}\_{}^{}\_{}^{}\_{}^{}\_{}^{}\_{}^{}$ where $0\leq s0\leq s1\leq \_{}\_{}-1$for a BWP *i* configured by *BWP-DownlinkCommon* or *BWP-DownlinkDedicated* for the DL BWP, or *BWP-UplinkCommon* or *BWP-UplinkDedicated* for the UL BWP. Within the BWP *i*, RB sets are numbered in increasing order from 0 to $\_{}^{}\_{}^{}$ where $\_{}^{}\_{}^{}$ is the number of RB sets contained in the BWP *i* and RB set 0 within the BWP *i* corresponds to RB set $s0$ in the carrier and RB set $\_{}^{}\_{}^{}$ within the BWP *i* corresponds to RB set $s1$ in the carrier.When a UE is provided with *nrofCRBs-r16=*0 for all intra-cell guard band(s) on a carrier, the UE is indicated that no intra-cell guard-bands are configured for the carrier, and expects $\_{}\_{}>1$. For $μ=0$, the UE expects the number of RBs within a RB set is between 100 and 110. For $μ=1$, the UE expects the number of RBs within a RB set is between 50 and 55 except for at most one RB set which may contain 56 RBs. |

## <1st round comments>

Companies are encouraged to express whether the above TPs are acceptable or not.

|  |  |
| --- | --- |
| Company | Comments |
|  |  |
|  |  |

# Conclusion

# Reference

1. R1-2005538 Remaining issue on wideband operation Fujitsu
2. R1-2005604 Remaining issues on the wideband operation for NR-U ZTE, Sanechips
3. R1-2005813 Maintenance on the wideband operation procedures Huawei, HiSilicon
4. R1-2005829 Text proposals for wideband operation for NR-U Lenovo, Motorola Mobility
5. R1-2005906 Remaining issues on Wideband operation in NR-U Nokia, Nokia Shanghai Bell
6. R1-2005918 Wideband operation Ericsson
7. R1-2006024 Discussion on the remaining issues of wide-band operations OPPO
8. R1-2006556 Remaining corrections for wideband operation for NR-U Sharp
9. R1-2006767 TP for Wideband operation for NR-U operation Qualcomm Incorporated
10. R1-2006967 Summary on maintenance of wide-band operation for NR-U Moderator (LG Electronics)

# Appendix: Text proposals corresponding to Issues A and B

## Issue A

### From ZTE [2],

|  |
| --- |
| ---------------------------------------------- < Start of TP#1 for 38.213 [1]> --------------------------------------------10.1 UE procedure for determining physical downlink control channel assignment < Unchanged parts are omitted >For each CORESET in a DL BWP of a serving cell, a respective *frequencyDomainResources* provides a bitmap. - if a CORESET is not associated with any search space set configured with *freqMonitorLocation-r16*, the bits of the bitmap have a one-to-one mapping with non-overlapping groups of 6 consecutive PRBs, in ascending order of the PRB index in the DL BWP bandwidth of $N\_{RB}^{BWP}$ PRBs with starting common RB position $N\_{BWP}^{start}$, where the first common RB of the first group of 6 PRBs has common RB index $6⋅\left⌈N\_{BWP}^{start}/6\right⌉$ if *rb-Offset-r16* is not provided, or the first common RB of the first group of 6 PRBs has common RB index $N\_{BWP}^{start}+N\_{RB}^{offset}$ where $N\_{RB}^{offset}$ is provided by *rb-Offset-r16.* - if a CORESET is associated with at least one search space set configured with *freqMonitorLocation-r16*, the first $N\_{RBG,set0}^{size}$ bits of the bitmap have a one-to-one mapping with non-overlapping groups of 6 consecutive PRBs, in ascending order of the PRB index in each RB set $k$ in the DL BWP bandwidth of $N\_{RB}^{BWP}$ PRBs with starting common RB position $RB\_{s0+k,DL}^{start,μ} $ [6, TS 38.214], where the first common RB of the first group of 6 PRBs has common RB index $RB\_{s0+k,DL}^{start,μ}+N\_{RB}^{offset}$ and *k* is indicated by *freqMonitoringLocations-r16* if provided for a search space set; otherwise, $k=0$. $N\_{RBG,set0}^{size}=\left⌊(N\_{RB,set0}^{size}-N\_{RB}^{offset})/6\right⌋$, $N\_{RB,set0}^{size}$ is a number of available PRBs in the RB set 0 for the DL BWP, and $N\_{RB}^{offset}$ is provided by *rb-Offset-r16* or $N\_{RB}^{offset}=0$ if *rb-Offset-r16* is not provided.For each RB set $k$, the UE does not expect the common RB $RB\_{s0+k,DL}^{start,μ}+N\_{RB}^{offset}$ + $6∙N\_{RBG, set 0}^{size}$ is not in the RB set $k$.< Unchanged parts are omitted >-------------------------------------------------- < End of text proposal> ---------------------------------------------------- |

## Issue B

### From ZTE [2],

|  |
| --- |
| **Proposal 2: Correct the parameters in TS 38.213 to align with the parameter “*freqMonitorLocations-r16*” in TS 38.331, and the TP#2 can be adopted.**---------------------------------------------- < Start of TP#2 for 38.213 [1]> --------------------------------------------10.1 UE procedure for determining physical downlink control channel assignment < Unchanged parts are omitted >For each CORESET in a DL BWP of a serving cell, a respective *frequencyDomainResources* provides a bitmap. - if a CORESET is not associated with any search space set configured with *freqMonitorLocations-r16*, the bits of the bitmap have a one-to-one mapping with non-overlapping groups of 6 consecutive PRBs, in ascending order of the PRB index in the DL BWP bandwidth of $N\_{RB}^{BWP}$ PRBs with starting common RB position $N\_{BWP}^{start}$, where the first common RB of the first group of 6 PRBs has common RB index $6⋅\left⌈N\_{BWP}^{start}/6\right⌉$ if *rb-Offset-r16* is not provided, or the first common RB of the first group of 6 PRBs has common RB index $N\_{BWP}^{start}+N\_{RB}^{offset}$ where $N\_{RB}^{offset}$ is provided by *rb-Offset-r16.* - if a CORESET is associated with at least one search space set configured with *freqMonitorLocations-r16*, the first $N\_{RBG,set0}^{size}$ bits of the bitmap have a one-to-one mapping with non-overlapping groups of 6 consecutive PRBs, in ascending order of the PRB index in each RB set $k$ in the DL BWP bandwidth of $N\_{RB}^{BWP}$ PRBs with starting common RB position $RB\_{s0+k,DL}^{start,μ} $ [6, TS 38.214], where the first common RB of the first group of 6 PRBs has common RB index $RB\_{s0+k,DL}^{start,μ}+N\_{RB}^{offset}$ and *k* is indicated by *freqMonitor~~ing~~Locations-r16* if provided for a search space set; otherwise, $k=0$. $N\_{RBG,set0}^{size}=\left⌊(N\_{RB,set0}^{size}-N\_{RB}^{offset})/6\right⌋$, $N\_{RB,set0}^{size}$ is a number of available PRBs in the RB set 0 for the DL BWP, and $N\_{RB}^{offset}$ is provided by *rb-Offset-r16* or $N\_{RB}^{offset}=0$ if *rb-Offset-r16* is not provided.< Unchanged parts are omitted >- if search space set $s$ is a CSS set - an indication by *dci-Format0-0-AndFormat1-0* to monitor PDCCH candidates for DCI format 0\_0 and DCI format 1\_0 - an indication by *dci-Format2-0* to monitor one or two PDCCH candidates, or to monitor one PDCCH candidate per RB set if the UE is provided *freqMonitorLocations-r16* for the search space set, for DCI format 2\_0 and a corresponding CCE aggregation level- an indication by *dci-Format2-1* to monitor PDCCH candidates for DCI format 2\_1- an indication by *dci-Format2-2* to monitor PDCCH candidates for DCI format 2\_2- an indication by *dci-Format2-3* to monitor PDCCH candidates for DCI format 2\_3- an indication by *dci-Format2-4* to monitor PDCCH candidates for DCI format 2\_4- an indication by *dci-Format2-6* to monitor PDCCH candidates for DCI format 2\_6< Unchanged parts are omitted >- a bitmap by *freqMonitorLocations-r16*, if provided, to indicate an index of one or more RB sets for the search space set $s$, where the MSB $k$ in the bitmap corresponds to RB set $k-1$ in the DL BWP. For RB set $k$ indicated in the bitmap, the first PRB of the frequency domain monitoring location confined within the RB set is given by $RB\_{s0+k,DL}^{start,μ}+N\_{RB}^{offset}$, where $RB\_{s0+k,DL}^{start,μ}$ is the index of first common RB of the RB set $k$ [6, TS 38.214], and $N\_{RB}^{offset}$ is provided by *rb-Offset-r16* or $N\_{RB}^{offset}=0$ if *rb-Offset-r16* is not provided. For each RB set with a corresponding value of 1 in the bitmap, the frequency domain resource allocation pattern for the monitoring location is determined based on the first $N\_{RBG, set 0}^{size}$ bits in *frequencyDomainResources* provided by the associated CORESET configuration.< Unchanged parts are omitted >-------------------------------------------------- < End of text proposal> ----------------------------------------------------**Proposal 3: Correct the parameters in TS 38.214 to align with the parameters “*intraCellGuardBandsDL-r16*” and “*intraCellGuardBandsUL-r16*” in TS 38.331, and the TP#3 can be adopted.**---------------------------------------------- < Start of TP#3 for 38.214 [3]> --------------------------------------------7 UE procedures for transmitting and receiving on a carrier with intra-cell guard bandsFor operation with shared spectrum channel access, when the UE is configured with any of *intraCellGuardBandsUL-r16* for UL carrier and *intraCellGuardBandsDL-r16* for DL carrier, the UE is provided with $N\_{RB-set,x}-1 $ intra-cell guard bands on a carrier, each defined by start CRB and size in number of CRBs, $GB\_{ s,x}^{start,μ} $ and $GB\_{ s,x}^{size,μ} $, provided by higher layer parameters *startCRB-r16* and *nrofCRBs-r16*, respectively. The subscript *x* is set to DL and UL for the downlink and uplink, respectively. Where there is no risk of confusion, the subscript *x* can be dropped. The intra-cell guard bands separate $N\_{RB-set,x} $RB sets, each defined by start and end CRB, $RB\_{ s,x}^{start,μ} $and $RB\_{ s,x}^{end,μ}$, respectively. UE does not expect that *nrofCRBs-r16* is configured with non-zero value smaller than the applicable intra-cell guard bands as specified in [8, TS 38.101-1] corresponding to $μ$ and carrier size $N\_{grid,x}^{size,μ}$. UE determines $RB\_{ 0,x}^{start,μ}=N\_{grid,x}^{start,μ}$, $RB\_{N\_{RB-set}-1,x}^{end,μ}=N\_{grid,x}^{start,μ}+N\_{grid,x}^{size,μ}-1$, and the remaining start and end CRBs as $RB\_{ s,x}^{end,μ}=N\_{grid,x}^{start,μ}+GB\_{ s,x}^{start,μ}-1$ and $RB\_{ s+1,x}^{start,μ}=N\_{grid,x}^{start,μ}+GB\_{ s,x}^{start,μ}+GB\_{ s,x}^{size,μ}$. The RB set *s* consists of $ RB\_{s,x}^{size,μ}$ resource blocks where $ RB\_{s,x}^{size,μ}=RB\_{ s,x}^{end,μ}-RB\_{ s,x}^{start,μ}+1$. When the UE is not configured with *intraCellGuardBandsUL-r16,* the UE determines the CRB indices for the intra-cell guard band(s), if any, and corresponding RB set(s) according to the nominal intra-cell guard band and RB set pattern as specified in [8, TS 38.101-1] corresponding to $μ$ and carrier size $N\_{grid,x}^{size,μ}$. When the UE is not configured with *intraCellGuardBandsDL-r16,* the UE determines the CRB indices for the intra-cell guard band(s), if any, and corresponding RB set(s) according to the nominal intra-cell guard band and RB set pattern as specified in [8, TS 38.101-1] corresponding to $μ$ and carrier size $N\_{grid,x}^{size,μ}$. For either or both DL and UL, if the nominal intra-cell guard band and RB set pattern as specified in [8, TS 38.101-1] contains no intra-cell guard bands, the number of RB sets for the carrier is $N\_{RB-set,x}=1$.For a carrier, the UE expects $ N\_{ BWP,i}^{start,μ}=RB\_{ s0,x}^{start,μ}$, and $N\_{ BWP,i}^{size,μ}=RB\_{ s1,x}^{end,μ}-RB\_{ s0,x}^{start,μ}+1$ where $0\leq s0\leq s1\leq N\_{RB-set,x}-1$for a BWP *i* configured by *BWP-DownlinkCommon* or *BWP-DownlinkDedicated* for the DL BWP, or *BWP-UplinkCommon* or *BWP-UplinkDedicated* for the UL BWP. Within the BWP *i*, RB sets are numbered in increasing order from 0 to $N\_{RB-set,x}^{BWP}-1$ where $N\_{RB-set,x}^{BWP}$ is the number of RB sets contained in the BWP *i* and RB set 0 within the BWP *i* corresponds to RB set $s0$ in the carrier and RB set $N\_{RB-set,x}^{BWP}-1$ within the BWP *i* corresponds to RB set $s1$ in the carrier.When a UE is provided with *nrofCRBs-r16=*0 for all intra-cell guard band(s) on a carrier, the UE is indicated that no intra-cell guard-bands are configured for the carrier, and expects $N\_{RB-set,x}>1$. For $μ=0$, the UE expects the number of RBs within a RB set is between 100 and 110. For $μ=1$, the UE expects the number of RBs within a RB set is between 50 and 55 except for at most one RB set which may contain 56 RBs.-------------------------------------------------- < End of text proposal> ---------------------------------------------------- |

### From Lenovo [4],

|  |
| --- |
| -----------------------------------------------< BEGIN TEXT PROPOSAL >-------------------------------------------------7 UE procedures for transmitting and receiving on a carrier with intra-cell guard bandsFor operation with shared spectrum channel access, when the UE is configured with any of *intraCellGuardBandsUL-r16* for UL carrier and *intraCellGuardBandsDL-r16* for DL carrier, the UE is provided with $N\_{RB-set,x}-1 $ intra-cell guard bands on a carrier, each defined by start CRB and size in number of CRBs, $GB\_{ s,x}^{start,μ} $ and $GB\_{ s,x}^{size,μ} $, provided by higher layer parameters *startCRB-r16* and *nrofCRBs-r16*, respectively. The subscript *x* is set to DL and UL for the downlink and uplink, respectively. Where there is no risk of confusion, the subscript *x* can be dropped. The intra-cell guard bands separate $N\_{RB-set,x} $RB sets, each defined by start and end CRB, $RB\_{ s,x}^{start,μ} $and $RB\_{ s,x}^{end,μ}$, respectively. UE does not expect that *nrofCRBs-r16* is configured with non-zero value smaller than the applicable intra-cell guard bands as specified in [8, TS 38.101-1] corresponding to $μ$ and carrier size $N\_{grid,x}^{size,μ}$. UE determines $RB\_{ 0,x}^{start,μ}=N\_{grid,x}^{start,μ}$, $RB\_{N\_{RB-set}-1,x}^{end,μ}=N\_{grid,x}^{start,μ}+N\_{grid,x}^{size,μ}-1$, and the remaining start and end CRBs as $RB\_{ s,x}^{end,μ}=N\_{grid,x}^{start,μ}+GB\_{ s,x}^{start,μ}-1$ and $RB\_{ s+1,x}^{start,μ}=N\_{grid,x}^{start,μ}+GB\_{ s,x}^{start,μ}+GB\_{ s,x}^{size,μ}$. The RB set *s* consists of $ RB\_{s,x}^{size,μ}$ resource blocks where $ RB\_{s,x}^{size,μ}=RB\_{ s,x}^{end,μ}-RB\_{ s,x}^{start,μ}+1$. When the UE is not configured with *intraCellGuardBandsUL-r16,* the UE determines the CRB indices for the intra-cell guard band(s), if any, and corresponding RB set(s) according to the nominal intra-cell guard band and RB set pattern as specified in [8, TS 38.101-1] corresponding to $μ$ and carrier size $N\_{grid,x}^{size,μ}$. When the UE is not configured with *intraCellGuardBandsDL-r16,* the UE determines the CRB indices for the intra-cell guard band(s), if any, and corresponding RB set(s) according to the nominal intra-cell guard band and RB set pattern as specified in [8, TS 38.101-1] corresponding to $μ$ and carrier size $N\_{grid,x}^{size,μ}$. For either or both DL and UL, if the nominal intra-cell guard band and RB set pattern as specified in [8, TS 38.101-1] contains no intra-cell guard bands, the number of RB sets for the carrier is $N\_{RB-set,x}=1$.For a carrier, the UE expects $ N\_{ BWP,i}^{start,μ}=RB\_{ s0,x}^{start,μ}$, and $N\_{ BWP,i}^{size,μ}=RB\_{ s1,x}^{end,μ}-RB\_{ s0,x}^{start,μ}+1$ where $0\leq s0\leq s1\leq N\_{RB-set,x}-1$ for a BWP *i* configured by *BWP-DownlinkCommon* or *BWP-DownlinkDedicated* for the DL BWP, or *BWP-UplinkCommon* or *BWP-UplinkDedicated* for the UL BWP. Within the BWP *i*, RB sets are numbered in increasing order from 0 to $N\_{RB-set,x}^{BWP}-1$ where $N\_{RB-set,x}^{BWP}$ is the number of RB sets contained in the BWP *i* and RB set 0 within the BWP *i* corresponds to RB set $s0$ in the carrier and RB set $N\_{RB-set,x}^{BWP}-1$ within the BWP *i* corresponds to RB set $s1$ in the carrier.When a UE is provided with *nrofCRBs-r16=*0 for all intra-cell guard band(s) on a carrier, the UE is indicated that no intra-cell guard-bands are configured for the carrier, and expects $N\_{RB-set,x}>1$. For $μ=0$, the UE expects the number of RBs within a RB set is between 100 and 110. For $μ=1$, the UE expects the number of RBs within a RB set is between 50 and 55 except for at most one RB set which may contain 56 RBs.-----------------------------------------------< END TEXT PROPOSAL >------------------------------------------------- |

### From Ericsson [6],

|  |
| --- |
| ---------------------------------------------- Text Proposal (TP#1) for 38.214, Section 7 ----------------------------------------\*\*\* Unchanged text omitted \*\*\*7 UE procedures for transmitting and receiving on a carrier with intra-cell guard bandsNote to editor: to be consistent with other specs, e.g., 38.211, the subscripts/superscripts in the highlighted variables should be formatted so they are not italicized, e.g., $N\_{ BWP,i}^{start,μ}$ should be $N\_{BWP,i}^{start,μ}$ and $RB\_{N\_{RB-set}-1,x}^{end,μ}$ should be $RB\_{N\_{RB-set}-1,x}^{end,μ}$.For operation with shared spectrum channel access, when the UE is configured with any of *intraCellGuardBandUL-r16* for UL carrier and *intraCellGuardBandDL-r16* for DL carrier, the UE is provided with $N\_{RB-set,x}-1 $ intra-cell guard bands on a carrier, each defined by start CRB and size in number of CRBs, $GB\_{r,x}^{start,μ}$ $GB\_{ s,x}^{start,μ} $ and $GB\_{r,x}^{size,μ}$ $GB\_{ s,x}^{size,μ} $, provided by higher layer parameters *startCRB-r16* and *nrofCRBs-r16*, respectively, where $r\in \left\{0,1,…,N\_{RB-set,x}-2\right\}$. The subscript *x* is set to DL and UL for the downlink and uplink, respectively. Where there is no risk of confusion, the subscript *x* can be dropped. The intra-cell guard bands separate $N\_{RB-set,x} $RB sets, each defined by start and end CRB, $RB\_{ s,x}^{start,μ} $and $RB\_{ s,x}^{end,μ}$, respectively. UE does not expect that *nrofCRBs-r16* is configured with non-zero value smaller than the applicable intra-cell guard bands as specified in [8, TS 38.101-1] corresponding to $μ$ and carrier size $N\_{grid,x}^{size,μ}$. UE determines $RB\_{ 0,x}^{start,μ}=N\_{grid,x}^{start,μ}$, $RB\_{N\_{RB-set}-1,x}^{end,μ}=N\_{grid,x}^{start,μ}+N\_{grid,x}^{size,μ}-1$, and the remaining start and end CRBs for $s\in \left\{1,…,N\_{RB-set,x}-2\right\} $as $RB\_{ s,x}^{end,μ}=N\_{grid,x}^{start,μ}+GB\_{ s,x}^{start,μ}-1$ and $RB\_{ s+1,x}^{start,μ}=N\_{grid,x}^{start,μ}+GB\_{ s,x}^{start,μ}+GB\_{ s,x}^{size,μ}$. The RB set with index *s* consists of $ RB\_{s,x}^{size,μ}$ resource blocks where $ RB\_{s,x}^{size,μ}=RB\_{ s,x}^{end,μ}-RB\_{ s,x}^{start,μ}+1$. When the UE is not configured with *intraCellGuardBandUL-r16,* the UE determines the CRB indices for the intra-cell guard band(s), if any, and corresponding RB set(s) according to the nominal intra-cell guard band and RB set pattern as specified in [8, TS 38.101-1] corresponding to $μ$ and carrier size $N\_{grid,x}^{size,μ}$. When the UE is not configured with *intraCellGuardBandDL-r16,* the UE determines the CRB indices for the intra-cell guard band(s), if any, and corresponding RB set(s) according to the nominal intra-cell guard band and RB set pattern as specified in [8, TS 38.101-1] corresponding to $μ$ and carrier size $N\_{grid,x}^{size,μ}$. For either or both DL and UL, if the nominal intra-cell guard band and RB set pattern as specified in [8, TS 38.101-1] contains no intra-cell guard bands, the number of RB sets for the carrier is $N\_{RB-set,x}=1$.For a carrier, the UE expects $ N\_{ BWP,i}^{start,μ}=RB\_{ s0,x}^{start,μ}$, and $N\_{ BWP,i}^{size,μ}=RB\_{ s1,x}^{end,μ}-RB\_{ s0,x}^{start,μ}+1$ where $0\leq s0\leq s1\leq N\_{RB-set,x}-1$for a BWP *i* configured by *BWP-DownlinkCommon* or *BWP-DownlinkDedicated* for the DL BWP, or *BWP-UplinkCommon* or *BWP-UplinkDedicated* for the UL BWP. Within the BWP *i*, RB sets are numbered in increasing order from 0 to $N\_{RB-set,x}^{BWP}-1$ where $N\_{RB-set,x}^{BWP}$ is the number of RB sets contained in the BWP *i* and RB set 0 within the BWP *i* corresponds to RB set $s0$ in the carrier and RB set $N\_{RB-set,x}^{BWP}-1$ within the BWP *i* corresponds to RB set $s1$ in the carrier.When a UE is provided with *nrofCRBs-r16=*0 for all intra-cell guard band(s) on a carrier, the UE is indicated that no intra-cell guard-bands are configured for the carrier, and expects $N\_{RB-set,x}>1$. For $μ=0$, the UE expects the number of RBs within a RB set is between 100 and 110. For $μ=1$, the UE expects the number of RBs within a RB set is between 50 and 55 except for at most one RB set which may contain 56 RBs.\*\*\* Unchanged text omitted \*\*\*----------------------------------------------------------- End Text Proposal ----------------------------------------------------------- |