**3GPP TSG RAN WG1 #102-e R1-200xxxx**

**August 17th – 28th, 2020**

**Agenda item:** 7.2.4.4

**Source:** Moderator (Qualcomm)

**Title:** Email Discussion for In-device Coexistence Aspects in NR-V2X

**Document for:** Discussion and Decision

# Introduction

This document provides a summary of the email discussion [102-e-NR- 5G\_V2X\_NRSL-InDevice-Coex-01]:

[102-e-NR- 5G\_V2X\_NRSL-InDevice-Coex-01] Email discussion/approval regarding

* processing time for prioritization of LTE sidelink and NR sidelink (Issue #1 in the summary)

by 8/20, followed by potential TPs, also including

* issue #2 (to start after 8/20) regarding capturing the agreement on prioritization of multiple overlapping transmissions between NR sidelink and LTE sidelink

by 8/25 – Gabi (Qualcomm)

# Discussion on Issue #1: Prioritization Timeline

The first issue to discuss is the value of UE processing time when performing prioritization between LTE sidelink and NR sidelink. TS 38.213 discusses the prioritization procedure in subclause 16.2.4.1 and uses the variable *T* to reference the processing time [1]:

16.2.4.1 Simultaneous NR and E-UTRA transmission/reception

If a UE

- would transmit a first channel/signal using E-UTRA radio access and a second channel/signal using NR radio access, and

- a transmission of the first channel/signal would overlap in time with a transmission of the second channel/signal, and

- the priorities of the two channels/signals are known to the UE msec prior to the start of the earlier of the two transmissions

the UE transmits only the channel/signal with the higher priority as determined by the SCI formats scheduling the transmissions or, in case of a S-SS/PSBCH block or a sidelink synchronization signal using E-UTRA radio access, as indicated by higher layers or, in case of PSFCH, equal to the priority of the corresponding PSSCH.

If a UE

- would respectively transmit or receive a first channel/signal using E-UTRA radio access and receive or transmit a second channel/signal using NR radio access, and

- a transmission or reception of the first channel/signal would respectively overlap in time with a reception or transmission of the second channel/signal, and

- the priorities of the two channels/signals are known to the UE msec prior to the start of the earlier transmission or reception

the UE transmits or receives only the channel/signal with the higher priority as determined by the SCI formats scheduling the transmissions or, in case of a S-SS/PSBCH block or a sidelink synchronization signal using E-UTRA radio access, as indicated by higher layers or, in case of PSFCH, equal to the priority of the corresponding PSSCH

Some contributions discussed this issue and proposed solutions on how to complete specification regarding the value *T* [2][3][4][5].

## Initial Discussion

Potential values for UE processing time based on company submissions are:

* Alt 1: , where is 2ms +1 slot, i.e. {3, 5, 9, 17} slots for {15, 30, 60, 120} kHz sub-carrier spacing, respectively. This is based on the maximum value required to prepare an NR sidelink transmission.
* Alt 2: ms, based on the maximum value required to prepare an LTE sidelink transmission.
* Alt 3: ms based on the maximum inter-module communication delay.
* Alt 4: Leave up to UE implementation.
* Alt 5: Others.

Table 1 Company views on values for T

|  |  |  |
| --- | --- | --- |
| Company | Option | Comments |
| OPPO | Alt 4 | In NR V2X, or is the preparation time for encoding PSCCH / PSSCH and 4ms in LTE without considering the inter-module communication delay. But for the case of cross-RAT prioritization, the inter-module delay can vary from 0 to up to 20ms depending on UE capability reporting of a timing delay. Therefore, it would be difficult to impose a single timing requirement ms prior to the start of the earlier transmission or reception. Furthermore, the issue of ms in cross-RAT prioritization is related to in-device coexistence and therefore does not impact to other UEs or network scheduling. Also, in many instances it is agreed when the priorities of both LTE and NR sidelink transmissions are not known to both RATs prior to time of transmission, it is then up to UE implementation to handle the overlap.  So based on the above, it is not critical to define a value for ms in the spec and it can be leave it to UE implementation. |
| LG Electronics | Alt 3 | First of all, the exact meaning of “T msec prior to” in the specification should be clarified. To be specific, which of followings is correct?   * (a) Timing at which each module knows its priority **before** exchanging the priority information between different modules * (b) Timing at which a module knows both its own priority and that of another module **after** exchanging the priority information between different modules   In case of (a), when defining T value, the inter-module communication delay should be taken into account. Since the maximum value of X was defined as 20ms in the agenda of NR Uu controlling LTE SL, T value can be set to 20ms. |
| CATT |  | We think LGE raise a good question, the exact meaning of T msce should be clarified.  In case of b) we think 4ms is enough.  In case of a), the additional timing should be introduced due to inter-module coordination. However, we think the 20ms is too large for in-device coexistence. For example, in pre-crash use case, the maximum latency is 20ms, which will be impossible to perform in-device coexistence due to such a large T value. |
| vivo | Alt 2 | Firstly, it is our understanding anyway a time limit to differentiate the long- and short- term TDM operations is needed and should be specified, otherwise, a UE may declare support of short-term TDM with a processing time of minutes or hours, which is totally meaningless. This processing time is also needed for testing. So we think Alt 4 is not acceptable.  Regarding LG’s question, our understanding is interpretation b). With this understanding, Alt 2 (i.e., based on the preparation time of LTE) is more suitable than Alt 1, considering that the processing time should be applicable to both NR and LTE modules. In the case of interpretation a), Alt 3 (20ms) is acceptable to us. |
| Ericsson | Alt 4 | In our view, the value T is subject to the processing time restriction of the UE and its value does not impact the functionality of other UEs. Therefore, we propose to leave the value T up to UE implementation. |
| ZTE, Sanechips | Alt 4 | The parameter T may be related to UE processing capability. It is also an internal implementation consequence whose different values do not lead to different spec logics and different UE behaviors. In addition, it seems all first three Alternatives above have good reasons. So we prefer to leave T up to UE implementation.  In our view, how to interpret “T prior to…” as mentioned by LGE also depends on how the inter-module communication is done inside UE implementation. So Alt-4 does not require RAN1 to decide which interpretation should be mandated. |
| Futurewei | Alt 4 | We do not see a system benefit in specifying the parameter T. Consequently, it can be left up to the implementation |
| Huawei, HiSilicon | Alt 4 | We haven’t see any necessary and benefit to specify the detailed values of T. This is purely UE implementation issue. |
| Qualcomm | Alt 3 | We agree with LG, CATT, and Vivo that the answer depends on the reference point for T. 20 ms is sufficient to address both interpretations in LG’s list; whereas 4 ms would only apply for Interpretation (b). Therefore, while we think that a value less than 20ms could be selected, it is simplest to go with 20 ms at this point. |
| NTT DOCOMO | Alt 2 or Alt 3 | We share the view with vivo, that short-term TDM with a large processing time should be prohibited. In our understanding, short-term TDM could have impact on gNB scheduling, or other UE’s NR transmission requesting HARQ feedback. So Alt 4 is not good, and at least maximum value should be defined. Actual value supported by each UE can be up to UE implementation. |
| NEC | Alt 2 | 20ms is the max inter-module communication delay which is not proper for some UEs.  Besides, we think 4ms for encoding PSCCH / PSSCH is what we need to consider. Regarding the inter-module delay, wording ''*the priorities of the two channels/signals are known to the UE T msec prior to the start of the earlier of the two transmissions*'' has the precondition ''known'', which already includes the inter-module delay in our view. |

# Discussion on Issue 2

[This discussion will commence after August 20th]

# References

1. 3GPP TS 38.213 V16.2.0, NR, Physical Layer Procedures for Control (Release 16).
2. R1-2005744, “Discussion on essential corrections in in-device coexistence,” LG Electronics.
3. R1-2006438, “Correction for in-device coexistence in SL,” Ericsson.
4. R1-2006771, “In-device Coexistence between LTE and NR sidelink,” Qualcomm Incorporated.
5. R1-2006869, “Discussion on processing time restriction for in-device coexistence,” ASUSTeK.