Title: Summary on SRS evaluation methodology

# Remaining issues on evaluation methodology

Prior to RAN1#102e, an offline discussion has been conducted in RAN1 NR reflector on the evaluation methodology for SRS enhancements [1]. The following three proposals are the outcome of this discussion.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***EVM Proposal 1:*** *LLS is used to evaluate SRS enhancements in Rel-17 FeMIMO, while SLS can be used additionally for evaluating data throughput for a given SRS design.*  ***EVM Proposal 2:*** *Adopt the following LLS assumptions at least for SRS enhancements on coverage/capacity in Rel-17.*   |  |  | | --- | --- | | **Parameter** | **Value** | | Metric | UL/DL BLER or throughput  Note: Other metrics like MSE can be considered optionally. | | Baseline | Rel-15 SRS + FG 10-11. Companies to state the detailed configuration used as baseline scheme.  FFS: converged baseline(s). | | Carrier frequency, SCS, System BW | FR1: 3.5GHz or 4GHz, 30kHz, 20, 40 or 100 MHz  FR2: 30 GHz, 120kHz | | Channel model | CDL-B or CDL-C in TR 38.901 with 30ns or 300ns delay spread as baseline  Note: other delay spread is not precluded.  FFS: whether and how to define scenario  FFS: whether and how to use CDL in MU-MIMO | | UE speed | 3km/h , 30km/h or 120km/h | | Number of UE antennas | 1T4R, 2T4R or 4T4R | | Number of gNB antennas | 32T32R or 64T64R | | UE antenna configuration | FR1: omni as baseline   * + FFS: whether direction can also be considered for more than 2 antennas   FR2: directional | | Rank, precoder and MCS | Precoder is adaptive. Rank/MCS can be adaptive or fixed. | | Precoding granularity | Fixed: 2, 4 or wideband for DL, wideband for UL. | | SRS periodicity | Companies to state the used SRS periodicity.  Note: SRS triggering may be aperiodic. | | SRS Comb | Comb 2 or 4 | | SRS frequency hopping | Companies to state whether SRS frequency hopping is enabled and the hopping pattern if so. | | DL SNR | Companies to state the used difference between DL SNR and UL SNR   * + FFS detailed values | | Phase coherency | Companies to state whether the phase coherency in time domain is modelled and if so, how. |   ***EVM Proposal 3:*** *Adopt the following SLS assumptions at least for SRS capacity enhancements in Rel-17.*   |  |  | | --- | --- | | **Parameter** | **Value** | | Metric | DL throughput | | Baseline | Rel-15 SRS + FG 10-11. Companies to state the detailed configuration used as baseline scheme. | | SRS error modelling | Table A.1-2 of TR 36.897 | | SRS periodicity | Companies to state the simulated SRS periodicity.  Note: SRS triggering may be aperiodic | | Carrier frequency, SCS and system bandwidth | 3.5GHz, 30KHz and 20MHz/40MHz/100MHz as baseline | | Number of gNB antennas | (*M*, *N*, *P*, *M*g,*N*g; *M*p, *N*p) = (8,8,2,1,1,4,8). (dH,dV) = (0.5, 0.8)λ | | Number of UE antennas | 1T4R, 2T4R or 4T4R | | Traffic model | FTP 1 or FTP 3 | | Handover margin | 3dB | | Scenario | UMi/UMa with 200m ISD.  Note: UMa with 500m ISD can also be considered. | |

Several contributions submitted to RAN1#102e propose to refine the three proposals.

## EVM proposal 1

Qualcomm proposes to update EVM proposal 1 as

* *LLS is used to evaluate SRS enhancements in Rel-17 FeMIMO, while SLS can be used additionally for evaluating data throughput and utilized SRS resources for a given SRS capacity enhancement design*

Companies’ views are collected as follows.

|  |  |
| --- | --- |
| **Company** | **View** |
| Rapporteur’s assessment | In SLS, SRS resource utilization can be reflected in data throughput. For example, for a given number of UEs in a cell, a particular scheme with larger overhead reduces the number of UEs which can be multiplexed in a slot. Then to accommodate SRS transmission for all the UEs in a cell, a larger SRS periodicity is required, which reduces data throughput due to larger CSI latency. Hence to investigate the overall impact of SRS overhead/capacity, data throughput is critical and sufficient to be the metric in SLS. |
|  |  |

## EVM proposal 2

The following updates are proposed by companies on EVM proposal 2.

* Baseline
  + Samsung proposes to remove “FG 10-11” in baseline.
* Carrier frequency
  + Qualcomm proposes to remove “3.5GHz” and “FR2”.
* DL/UL prioritization
  + Qualcomm proposes to prioritize DL over UL.
  + Nokia proposes to prioritize UL over DL.
* UE antenna configuration
  + CATT proposes to consider directional antennas additionally for more than 2 antennas in FR1.
  + Samsung and ZTE propose not to consider directional antennas for FR1.
* SRS periodicity
  + Samsung propose to remove “Note: SRS triggering may be aperiodic.”
* Scenario and angular scaling
  + ZTE proposes to add “Companies to state whether angle scaling is performed, and if so, the desired angle spread and mean angle”.
* Difference between UL SNR and DL SNR
  + ZTE and Ericsson suggest to let companies to state one signal value. The value may depend on link budget analysis.
* Phase coherency modeling
  + Alt 1 (Qualcomm): for per SRS port
  + Alt 2 (Qualcomm): for per SRS port
  + Alt 3 (CATT): Phase noise model as in R1-165685

Companies’ views on the above are collected as follows.

|  |  |
| --- | --- |
| **Company** | **View** |
| Rapporteur’s assessment | * Baseline   + Rel-16 UE capability discussion for NR-U has concluded FG 10-11 can also be applied on licensed band. Hence it should be included in the baseline. * Carrier frequency   + FR2 or DL in 3.5GHz has global interest for operators’ deployment. It’s better not to disallow companies to conduct evaluation for them. * DL/UL prioritization   + Based on offline discussion prior to RAN1#102e and the submitted contributions, it’s impossible to prioritize one link to another. There are good points on both sides. DL may have more gain based on accurate CSI, while UL has more urgent need to enhance coverage. Hence it’s better not to prioritize any link in evaluation. * UE antenna configuration   + The current situation is to use omni antennas as baseline for FR1, as it is more useful for FR1. On the other hand, this does not preclude companies to evaluate directional antennas for FR1. Hence it is suggested to keep the current EVM proposal of having omni as baseline. * SRS periodicity   + The intention of the note is not to preclude companies to evaluate the utilization of aperiodic SRS for capacity coverage enhancement. Hence it seems fine to keep it. * Scenario and angular scaling   + Angle scaling reflects the angular spread and allows simulator to generate different angles for different UEs. Hence it is suggested to add “Companies to state whether angle scaling is performed, and if so, the desired angle spread and mean angle”. With this, we can remove the two FFS bullets in channel model. * Difference between UL SNR and DL SNR   + We can keep the current proposal to let companies report the difference and remove the FFS bullet. The reported value may depend on gNB/UE Tx power, noise figure, number of antennas, bandwidth, etc.. * Phase coherency modeling   + It’s better to align the modeling of phase coherency if it is used. Companies’ input on the three alternatives are encouraged. |
|  |  |

## EVM proposal 3

The following update is proposed on EVM proposal 3.

* Traffic model
  + Qualcomm proposes to add full buffer in the traffic model.

Companies’ views on the above are collected as follows.

|  |  |
| --- | --- |
| **Company** | **View** |
| Rapporteur’s assessment | * Traffic model   + Burst model like FTP is closer to what we have in real network, esp. considering interference, MU paring, etc. caused by on-demand scheduling. Hence it is suggested keep FTP models only. |
|  |  |

# References

[1] Offline email discussion on FeMIMO evaluation methodology: Item 3