**3GPP TSG RAN WG1 #102-e R1-200xxxx**

**e-Meeting, 17th - 28th August, 2020**

**Agenda item:** 8.12

**Source:** Moderator (CMCC)

**Title:** Phase 2 moderator summary on NR Multicast and Broadcast Services

**Document for:** Discussion/decision

# Introduction

As announced by chairman, one email thread is planned to discuss high-level aspects for NR MBS in this meeting.

[102-e-NR-MBS-01] Email discussion/approval using R1-2007001 as a starting point, focusing on high-level aspects – Fei (CMCC)

* By 8/19 – Classification of high priority/medium priority items for this e-Meeting
* By 8/24 – high priority items
* By 8/27 - medium priority items

The initial moderator summary is provided in R1-2007001 which can be found in the inbox. The issues in the summary are classified into two tiers.

The first tier issues are the ones for the high level concept and can be considered as starting point for this meeting, which are summarized in table 1 below and the details can be found in section 2 in R1-2007001.

The second tier issues are low priority issues and are mainly the ones for details or further step issues set up on the conclusion of the first tier issues, which are targeted to be discussed in the following meeting but some of them can also be discussed in this meeting upon the first tier issues are concluded. The summary and the details for the second tier issues can be found in section 3 in R1-2007001.

**Table 1: The first tier issues**

|  |  |
| --- | --- |
| **Sub-agenda** | **Issues (summary in section 2 in R1-2007001)** |
| Group scheduling for RRC\_CONNECTED UEs | **Issue 1 (Question 1 in R1-2007001)**: Regarding the two high level group scheduling mechanisms, i.e., group-common PDCCH based group scheduling and UE-specific PDCCH based group scheduling, whether down selection is needed or both of them can be considered for MBS for RRC\_CONNECTED UEs? |
| **Issue 2 (Question 2 in** **R1-2007001)**: Please share your views on the following two alternatives for frequency resource configuration for MBS for RRC\_CONNECTED UEs.• Alternative 1: Introduce a MBS specific BWP• Alternative 2: Define a MBS common frequency resource confined within UE’s active BWP. |
| **Issue 3 (Question 3 in** **R1-2007001)**: Whether the simultaneous operation with unicast reception in the WID means a UE is required to receive multicast PDSCH and unicast PDSCH simultaneously in one slot? If the answer is YES, which multiplexing type(s) of simultaneous reception of unicast PDSCH and multicast PDSCH in a slot can be supported in NR MBS? e.g., TDM, FDM, SDM. |
| Reliability improvement for RRC\_CONNECTED UEs | **Issue 4 (Proposal 1 in R1-2007001, with little update)**: For RRC\_CONNECTED UEs, HARQ-ACK feedback is supported for multicast without additional evaluation for it, i.e., no evaluation is needed to justify whether HARQ-ACK feedback is needed. |
| **Issue 5 (Proposal 2 in R1-2007001, with little update)**: For RRC\_CONNECTED UEs, consider following reliability improvement mechanisms for MBS.• CSI feedback, FFS whether modification is needed on top of existing CSI feedback mechanism for unicast• PDSCH repetition, FFS whether spec impact is implied |
| **Issue 6 (Question 4 in R1-2007001, with little update)**: Whether a common evaluation methodology and assumptions are necessary for NR MBS? If the answer is YES, what’s the purpose of the evaluation? And what’s your suggestion on the common evaluation methodology and assumptions? |
| Basic functions for MBS for RRC\_IDLE/RRC\_INACTIVE UEs | **Issue 7 (Proposal 3 in R1-2007001)**: For UE in IDLE/INACTIVE state, the frequency resource for PTM transmission is• Alt 1: Initial BWP• Alt 2: Configured with larger size to cover initial BWP• Alt 3: Configured to be within initial BWP |
| **Issue 8 (Proposal 4 in R1-2007001)**: Multi-beam/beam-sweeping operation is supported for PTM in IDLE/INACTIVE state. |

According to Chairman’s guidance, this email thread will be organized in three phases:

* Phase 1: by 8/19, classification of high priority/medium priority items for this e-Meeting based on the summarized first tier issues.
* Phase 2: by 8/24, discuss and conclude the high priority items.
* Phase 3: by 8/27, discuss and conclude the medium priority items.

In phase 1, based on companies’ views, the following high/medium priority items have been classified for this meeting:

* High priority:
	+ Issue 1/4/6
* Medium priority:
	+ Issue 2/3/5

For phase 2, companies are invited to provide their views on the high priority issues for this e-Meeting in section 3. Moderator will provide the observation and proposal on the high priority issues in section 2 based on companies’ inputs.

# Observation and Proposal for Phase 2

Moderator will provide the observation and proposal based on companies’ input in section 3.

# Companies’ Views on high priority issues in Phase 2

***Group scheduling mechanisms for RRC\_CONNECTED UEs***

Based on companies’ submitted contributions, two group scheduling mechanisms were proposed. The first is group-common PDCCH based group scheduling, which is similar to LTE SC-PTM transmission. In this mechanism, CRC of PDCCH is scrambled by a common RNTI (e.g., G-RNIT) and the PDSCH is also scrambled by the common RNTI. Nine companies proposed to consider this mechanism for MBS.

The second is UE-specific PDCCH based group scheduling. In this mechanism, CRC of PDCCH is scrambled by C-RNTI, but different PDCCHs schedule a group common PDSCH for a group of UEs. From UE’s perspective, it is the same as unicast transmission. Three companies proposed to also consider this mechanism.

One company proposed to also consider sub-G-RNTI PDCCH based group scheduling, in which sub-G-RNTI can be used to scramble a sub-group common PDCCH for a small group scheduling. This mechanism seems to fall into group-common PDCCH based group scheduling in high level, if any difference, the details can be considered in later stage.

|  |  |
| --- | --- |
| **group scheduling mechanisms** | **Companies** |
| Option 1: group-common PDCCH based group scheduling | Huawei, Nokia, QC, Convida, ZTE, Intel, CATT, CMCC, LG |
| Option 2: UE-specific PDCCH based group scheduling | CMCC, vivo, CATT |

**[High priority] Issue 1 (Question 1 in R1-2007001)**: *Regarding the two high level group scheduling mechanisms, i.e., group-common PDCCH based group scheduling and UE-specific PDCCH based group scheduling, whether down selection is needed or both of them can be considered for MBS for RRC\_CONNECTED UEs?*

Please share your views and comments in the table.

|  |  |
| --- | --- |
| **Company** | **Comment** |
| TD Tech, Chengdu TD Tech | Support Option 1 : group-common PDCCH based group schedulingComments on option 2:The PDSCH for unicast is bit-scrambled by C-RNTI. The group common PDSCH is impossible to be entirely same as the PDSCH for unicast.When the number of UEs is large, the PDCCH resource consumed becomes larger than the PDCCH resource used for beam-sweeping in Option 1.  |
| vivo | We think both of them can be considered for MBS for RRC\_CONNECTED UEs for the following reasons:1. group-common PDCCH based group scheduling can be a basic scheduling mechanism, considering there may be quite lots of UEs in an MBS group, this mechanism is beneficial for PDCCH overhead reduction. But this mechanism will introduce many efforts when HARQ-ACK feedback is supported.
2. UE-specific PDCCH based group scheduling can also be used in some cases, for example, the case that number of MBS UEs is medium and the MBS service reliability requirement is high, i.e., HARQ-ACK is needed for the service. In this case, there is no has no PDCCH blocking issue. Then UE-specific PDCCH can benefit from scheduling and HARQ-ACK feedback perspective as summarized in the following table.

In our view, group-common PDCCH mechanism will have large spec impact / standardization effort for HARQ-ACK feedback, multiplexing / prioritization between multicast and unicast, etc. It is more suitable for an MBS with no HARQ-ACK feedback or with only group-specific NACK only feedback. UE-specific PDCCH mechanism can the minimize spec impact / standardization effort for these aspects and is a good scheduling scheme for MBS PDSCH retransmission. Therefore, no down select is needed.Table 1 Comparisons of groupcast PDCCH and unicast PDCCH

|  |  |  |
| --- | --- | --- |
|  | group-common PDCCH | UE-specific PDCCH |
| PDCCH overhead | Low  | high |
| Search space configuration | Larger spec impact | No spec impact |
| DCI size alignment | If DCI 1\_1/1\_2 is used, it may have impact on DCI size alignmentIf DCI 2\_x is used, other group common DCI need to align the DCI payload size with it, which may reduce the PDCCH performance | Same as unicast PDSCH, no additional impact |
| Impact on HARQ-ACK feedback | PUCCH resource | Hard to indicate orthogonal PUCCH resources due to the same PRI value.  |
| HARQ-ACK feedback timing | Same timing, all UEs in an MBS group will feed back HARQ-ACK in the same slot, resulting PUCCH overload and collision  |
| TPC | Difficult to indicate different UEs’ TPC using one single DC |
| Impacts when considering simultaneous receptions of MBS PDSCH and unicast PDSCH  | DAI | Separating DAI counting for groupcast PDSCH and uncast PDSCH |
| HARQ-ACK Codebook | Separate or joint HARQ-ACK codebook needs to be discussed/specified |
| if separate codebook for MBS PDSCH and unicast PDSCH, multiplexing/prioritization of different codebooks needs to be discussed |
| RNTI | if UE is interested in multiple MBS services, UE needs to monitor a PDCCH with multiple g-RNTIs |

 |
| CMCC | Both group-common PDCCH based group scheduling and UE-specific PDCCH based group scheduling can be supported for MBS for RRC\_CONNECTED UEs.It is noteworthy that the decision on which group scheduling mechanism should be supported should not only consider the overhead of PDCCH, but also the other aspects, e.g., the standization effort or spec impact to support HARQ-ACK feedback if it is supported, the PUCCH resource utilization efficiency for HARQ-ACK feedback, etc.From the comparison in the following table, we can see that, on the one hand, the PDCCH overhead of UE-specific PDCCH based scheme is larger than that of group common PDCCH based scheme, on the other hand, the standardization efforts for UE-specific PDCCH based scheme to support ACK-NACK based HARQ feedback is much less than group common PDCCH based scheme.

|  |  |  |
| --- | --- | --- |
|  | Group common PDCCH based scheme | UE-specific PDCCH based scheme |
| PDCCH overhead | Small  | **Larger** |
| PUCCH resource configuration for HARQ-ACK | **Less configuration flexibility, less PUCCH resource utilization efficiency and larger spec impact*** For ACK/NACK feedback, network needs to configure orthogonal PUCCH resources for UEs in the same group by RRC so that a single PRI field in DCI can optionally be used to select separate PUCCH resource for each UE. This will cause that NW has to reserve a certain amount of dedicated PUCCH resources for multicast transmission which cannot be shared with unicast transmission.
* Separate PUCCH resource configurations for multicast and unicast may be needed, which will introduce additional spec impact.
 | More Flexible, more efficiency and little spec impact* The same as for unicast.
 |
| HARQ-ACK multiplexing for multicast and unicast / HARQ-ACK codebook construction | **More complicated and large spec impact*** If HARQ-ACK multiplexing for multicast and unicast in a slot is supported, the joint codebook construction procedure is much more complicated and will induce more spec impact whether for semi-static or dynamic HARQ-ACK codebook.
* If HARQ-ACK multiplexing for multicast and unicast in a slot is not supported, HARQ-ACK for multicast or unicast has to be dropped which may impact the performance, or it has to be based on network implementation to avoid collision of HARQ-ACK feedback for multicast and unicast, which will introduce additional scheduling restriction.
 | NO spec impact* Can reuse Rel-15/Rel-16 HARQ codebook construction procedure.
 |

Considering the pros and cons of these two group scheduling schemes, we think they can be used for different use cases. * For the case with relatively less number of UEs in a MBS group (but multicast still has advantage on spectral efficiency compared with unicast transmission), it is more suitable to use UE-specific PDCCH group scheduling together with ACK/NACK based HARQ-ACK feedback to improve reliability with little spec impact and managable PDCCH / PUCCH overhead.
* For the case with large number of UEs in a MBS group, it is more suitable to use group common PDCCH scheduling for which NACK only based HARQ-ACK feedback can be used to improve reliability with small PDCCH / PUCCH overhead.

Therefore, we think both two group scheudling mechanisms can be supported. |
| LG | We think that group scheduling with G-RNTI is beneficial for the newtork especially when multiple UEs interested in a service can receive same TBs of the service via same time/frequency resources. However, it would not be always possible for certain UEs. Thus, it is also good to consider UE specific scheduling with C-RNTI. |
| Nokia | For RRC Connected mode UEs, in general we prefer option 1, because of the lower downlink signaling overhead. However, we can envisage of some scenarios where option 2 may also be beneficial to support additional feedback from certain UEs. In those scenarios, the UE could be configured with an additional USS to support additional UE specific reliability information. |
| ZTE | We suggest to support group-common PDCCH only.Compared with UE-specific PDCCH, group-common PDCCH can save lots of resources as all UEs in one group share the same PDCCH. Besides, for broadcast for RRC\_IDLE/RRC\_INACTIVE UEs, only group-common PDCCH (or more specifically, cell-common PDCCH) can be applied. It is preferred to keep commonality between broadcast and multicast. That is, group-common PDCCH needs to be supported anyway considering broadcast service scheduling, and more standardization work will be needed for additional support for UE-specific PDCCH. We would also like to mention that the UE-specific PDCCH based solution may have RAN2 impact. Based on our understanding, UE MAC layer needs to know the G-RNTI (corresponding to a type of service/logical channel) of each PDSCH. If UE-specific PDCCH based solution is introduced, then how can the network indicate the G-RNTI to the UE?  |
|  |  |

***Reliability improvement mechanisms for RRC\_CONNECTED UEs***

Based on companies’ submitted contributions, three reliability improvement mechanisms have more supporters than others as illustrated in the following table, including HARQ-ACK feedback, CSI feedback and PDSCH repetition.

Regarding HARQ-ACK feedback, nine companies suggested to support it for at least multicast for RRC\_CONNECTED state, some companies [Huawei, HiSilicon] have submitted some simulation results for justifying the benefits of HARQ-ACK feedback, one company proposed to study the potential gain and standardization impact for HARQ-ACK feedback,

Regarding CSI-feedback, six companies proposed that CSI feedback can be supported to improve reliability. Four of them [CMCC][VIVO][CATT][ZTE] think the existing CSI-RS configuration and CSI feedback mechanism for unicast can be directly used for MBS without additional spec impact. Two of them [QC][E///] think some modifications may be needed.

Regarding PDSCH repetition, some of the proponents think the existing PDSCH repetition mechanism for unicast can be reused for MBS.

Regarding multi-beam/beam sweeping operation, two companies [Sony, CATT] mentioned it in the sub-agenda for reliability improvement. Beam sweeping was also raised in some contributions for RRC\_IDLE/INACTIVE UEs and two other companies [ZTE, LG] also raised similar issue for group scheduling, it can be discussed later in which sub-agenda it should be discussed.

Each of other potential mechanisms only have one proponent, including conservative scheduling based on network implementation, multi-DCI based M-TRP transmission and HARQ-based time-interleaving.

|  |  |
| --- | --- |
| **Reliability improvement mechanisms** | **Companies** |
| HARQ-ACK feedback | CMCC, Huawei, OPPO, vivo, CATT, Convida, QC, E///, Samsung, Nokia  |
| CSI feedback | CMCC, E///, CATT, vivo, QC, ZTE |
| PDSCH repetition | CMCC, ZTE, Intel, vivo, LG, Nokia |
| Multi-beam/beam sweeping operation  | CATT, Sony  |
| Conservative scheduling (network implementation) | ZTE, Nokia |
| Multi-DCI based M-TRP transmission | LG |
| HARQ-based time-interleaving | BBC |

 **[High priority] Issue 4 (Proposal 1 in R1-2007001, with little update)**: *For RRC\_CONNECTED UEs, HARQ-ACK feedback is supported for multicast without additional evaluation for it, i.e., no evaluation is needed to justify whether HARQ-ACK feedback is needed.*

Please share your views and comments in the table.

|  |  |
| --- | --- |
| **Company** | **Comment** |
| TD Tech and Chengdu TD Tech | The views and comments of ours are listed in the table below.

|  |  |
| --- | --- |
| **Reliability improvement mechanisms** | **Companies: TD Tech and Chengdu TD Tech** |
| HARQ-ACK feedback | supported |
| CSI feedback | Comments: The further discussion and simulation are needed to make the decision. |
| PDSCH repetition | Supported |
| Multi-beam/beam sweeping operation  | Supported |
| Conservative scheduling (network implementation) | Comments: The further discussion and simulation results are needed to make the decision. |
| Multi-DCI based M-TRP transmission | Comments: The further discussion and simulation results are needed to make the decision. |
| HARQ-based time-interleaving | Comments: The further discussion and simulation results are needed to make the decision. |

 |
| vivo | We support the proposal.Diffentent from LTE, NR MBS support many use cases, and some case, such as V2X or Industry applications have very high reliabiility requirement, e.g. 99.9999%. It is impossible to meet this requirement simply using link adaption based on CSI feedback only or automatic repetition. Considering this perspective, HARQ-ACK is anyway needs to be supported. No evaluation is needed to justify this considering the limited TU for MBS WI.Table 1. Requirements for different MBS use cases

|  |  |  |
| --- | --- | --- |
| MBS use cases | Latency | Reliability |
| V2X | 5-100ms | 90% to 99.9999% |
| Live Video | 150ms | 99.9% |
| IOT Software update | Latency Tolerant | Higher reliability is beneficial |
| Industry applications | 0.5ms | 99.9999% |

 |
| CMCC | Support the proposal.* In Rel-13 LTE SC-PTM, simulations had been carried out to evaluate the gain of HARQ-ACK feedback and justify that HARQ-ACK can improve the reliability. The evaluations for SC-PTM aimed at supporting multicast/broadcast service for group communications as defined in 3GPP TS 22.468 and mission critical push to talk as defined in 3GPP TS 22.179, which are consistent with the requirement mentioned in the WID of NR MBS. In addition, considering both R17 NR MBS and LTE SC-PTM aim to support single cell multicast/broadcast, we think the evaluation results and observation for HARQ-ACK feedback in LTE SC-PTM are also applicable for R17 NR MBS.
* In addition, NR MBS also aims to support more services which may require much higher reliability, e.g., V2X applications. The higher reliability the service requires, the more adavatages can be expected from HARQ-ACK feedback.

Therefore, we think the HARQ-ACK feedback should be supported for CONNECTED UEs, and no additional evaluation is needed to justify whether to support it. |
| LG | If legacy UE specific scheduling is used for a multicast TB, it can already support HARQ-ACK feedback. Thus, HARQ-ACK feedback can be supported for multicast without additional evaluation at least for UE specific scheduling. |
| Nokia | Additional evaluation for HARQ-ACK is desirable, preferably with some minimum reliability to target.In our view, there are many variants of HARQ-ACK feedback that could be supported. We would like to see evaluations of these techniques compared against each other (justifying a common set of simulation assumptions) and against some minimum reliability targets.Subject to those evaluations, RAN1 can then make an informed decision about the support of HARQ-ACK. |
| ZTE | We suggest to evaluate the potential gain for HARQ-ACK for NR MBS first.In LTE SC-PTM, some preliminary evaluations on spectrum efficiency between ‘SC-PTM with CQI and HARQ ACK/NACK feedback’ and ‘SC-PTM with CQI feedback only and eOLLA’ had been done. Conclusions were made in TR 36.890 as follows.

|  |
| --- |
| Conclusions...SC-PTM performance in terms of spectral efficiency was evaluated by the simulations. The performance analysis results in the following conclusions:- Link adaptation allowed by the availability of UL feedback provides significant gains when the number of receiving UEs is rather small and decreases with increasing group size. HARQ with retransmissions can further improve the spectral efficiency in some scenarios but these improvements are small. It has not been concluded whether the gains provided by HARQ and retransmission are worth of the increased complexity of the system.  |

For NR MBS, the deployment scenarios have changed compared with LTE SC-PTM. The simulation assumptions, e.g., frequency, bandwidth, traffic model and antenna configuration, etc., should be updated accordingly.It is questionable on whether/under which conditions/how much gain can be achieved by supporting HARQ-ACK feedback under the new simulation assumptions. So some more careful evaluations on the gain of supporting HARQ-ACK feedback in NR MBS can be done prior to specific mechanism design. With more careful evaluation, companies can even compare the potential performance gain between different HARQ-ACK solutions, which is also beneficial to subsequent technical discussion if HARQ-ACK is supported. |
|  |  |

***Evaluation***

Regarding evaluation, four companies have contributions on evaluation in the “Others” sub-agenda. One company [ZTE] provided the evaluation results to support CSI feedback, one company [Huawei] provided the evaluation results to support HARQ-ACK feedback, one company [Nokia] proposed the methodology and assumptions for evaluation of different UL feedback schemes, and one company [E///] proposed the methodology and assumptions for evaluation of different PTM features.

Before we discuss a common evaluation methodology and assumptions, we need to first determine the purpose of the evaluation campaign.

**[High priority] Issue 6 (Question 4 in R1-2007001, with little update)**: *Whether a common evaluation methodology and assumptions are necessary for NR MBS? If the answer is YES, what’s the purpose of the evaluation? And what’s your suggestion on the common evaluation methodology and assumptions?*

Please share your views and comments in the table.

|  |  |
| --- | --- |
| **Company** | **Comment** |
| TD Tech and Chengdu TD Tech | The related simulaiton is needed to prove the corresponding method is nessesary for the NR MBS. The simulation assumptions shall be discussed to ensure that the simulation results from the different companies can be compared with each other. |
| vivo | From our understanding, a common evaluation methodology and assumptions are not necessary for NR MBS. As above proposed, HARQ-ACK for MBS should be supported without evaluation. Then, the motivation to spend much time to do evaluation is not clear to us. |
| CMCC | Not necessary.As the FL summary about reliability improvement mechanisms for RRC\_CONNECTED UEs above, HARQ-ACK feedback, CSI feedback and PDSCH repetition are three major mechanisms. * For HARQ-ACK feedback, as our comment in issue 4, no evaluation is needed to justify whether HARQ-ACK feedback is needed.
* For CSI feedback and PDSCH repetition, they are also efficient ways to improve reliability, and we think the spec impact is small and even none.

Therefore, we think there is no strong motivation to do any evaluation for NR MBS, and all these three reliability improvement mechanisms can be supported. |
| LG | Some assumptions for evaluations are already provided by a few companies in AI 8.12.5. Thus, it seems good to have common evaluation methodology and assumptions to justify a certain solution, if we cannot easily draw the benefit of the solution or reach an agreement on support of it. |
| Nokia | Yes, to enable a fair, efficient and meaningful comparison of different reliability techniques from different companies. Note, as part of these assumptions/methodology, we would like to see a baseline unicast scenario defined, to allow differences between different simulations to be more readily identified. |
| ZTE | Yes. As mentioned in our tdoc x5437, there are different candidate mechanisms to improve the reliability of NR MBS, e.g., HARQ-ACK, CSI feedback and repetition. The simulation results can further guide the subsequent discussion on whether/how to support reliability improvement. Further, the simulation results can provide some useful information for the operators who are interested in the MBS, e.g., which mechanism to deploy in the practical network if multiple mechanisms are specified for reliability improvement.Regarding the common evaluation methodology and assumptions, we have the following comments.* Using system-level simulations
* The Rural and Dense-Urban scenarios can be evaluated considering the main target use cases of Public safety and Mission critical.
* Full buffer or periodic deterministic traffic model can be used.
* Spectral efficiency or user experienced data rate can be considered as the performance metric.
* The details of the simulation assumptions can be fully discussed in the following e-mail discussion.
 |
|  |  |

# Appendix A: Second tier issues summarized in R1-2007001

**Table A.1: Summary of second tier issues of group scheduling for RRC\_CONNECTED UEs**

|  |  |
| --- | --- |
| **Second tier issues** | **Possible questions or proposals** |
| 3.1.1 Configuration of group scheduling for multicast/broadcast | Question: Whether broadcast and multicast need to be differentiated for RRC\_CONNECTED UEs? If the answer is YES, whether the same configuration mechanism of group scheduling for Broadcast is applied for both RRC\_CONNECTED UEs and RRC\_IDLE/INACTIVE UEs? |
| Proposal: For RRC\_CONNECTED UEs, at least part of the parameters for multicast configuration is received by dedicated RRC signaling. |
| 3.1.2.1 CORESET configuration for MBS | Proposal: For group common PDCCH based group scheduling and a MBS common frequency resource configured with in UE’s active DL BWP, the CORESET is configured within the MBS common frequency resource. |
| Proposal: For group common PDCCH based group scheduling and a MBS common frequency resource configured with in UE’s active DL BWP, the CORESET for MBS is configured per BWP. |
| 3.1.2.2 Search space configuration for MBS | Proposal: Consider the following options for search space configuration for MBS for RRC\_CONNECTED UEs:• Option 1: CSS (existing CSS type or new defined CSS type)• Option 2: USS |
| 3.1.2.3 DCI format for MBS | Proposal: Consider the following options for DCI format for MBS for RRC\_CONNECTED UEs:• Option 1: DCI format 1\_0• Option 2: DCI format 1\_1• Option 3: DCI format 2\_x• Option 4: New DCI format |
| 3.1.2.4 Blind decoding related issues | Proposal: The maximum number of monitored PDCCH candidates and non-overlapped CCEs per slot are not increased for MBS. |
| Proposal: Keep the “3+1” DCI size budget for MBS with group common PDCCH based group scheduling. |
| 3.1.2.5 Multi-beam/beam sweeping operation | Proposal: Support multi-beam/beam sweeping operation for MBS PDCCH/PDSCH for RRC\_CONNECTED UEs. |
| 3.1.3 Simultaneous operation with unicast reception | Proposal: The UE is expected to process maximum two transport blocks for simultaneous reception of unicast PDSCH and multicast PDSCH. |
| 3.1.4 Other issues | Proposal: Support DL SPS for MBS for RRC\_CONNECTED UEs. |
| Proposal: Support multi-layer MIMO for MBS PDSCH for RRC\_CONNECTED UEs. |
| Question: Whether modifications are needed for QCL framework in order to support MBS transmission? |
| Proposal: Introduce a new reception type of PDCCH and PDSCH for MBS for RRC\_CONNECTED UEs, if group common PDCCH based group scheduling is supported. |
| Question: Whether to support receiving MBS service on a Scell? |
| Question: Whether to support SFBC for MBS? |

**Table A.2: Summary of second tier issues of reliability improvement for RRC\_CONNECTED UEs**

|  |  |
| --- | --- |
| **Second tier issues** | **Possible questions or proposals** |
| 3.2.1 HARQ-ACK feedback | Proposal: Consider the following two alternatives for HARQ-ACK feedback for RRC\_CONNECTED UEs:* Alternative 1: ACK/NACK based HARQ-ACK feedback
* Alternative 2: NACK-only based HARQ-ACK feedback
 |
| Proposal: HARQ-ACK feedback for NR MBS should be RRC configurable if it is supported for RRC\_CONNECTED UEs. |
| Proposal: Both PTM-based and PTP-based retransmissions can be supported for NR MBS for RRC\_CONNECTED UEs. |
| Question: Whether multiplexing of HARQ-ACK of unicast and multicast transmission should be supported for UEs receiving both unicast and multicast service. |
| Question: Whether prioritization of HARQ-ACK of unicast and multicast transmission should be supported for UEs receiving both unicast and multicast service. |
| 3.2.2 CSI feedback | Proposal: Consider to support following schemes for NR MBS:* Option 1: Single port transmission
* Option 2: Open-loop spatial multiplexing
* Option 3: Closed-loop spatial multiplexing
 |
| 3.2.3 Other issues | Question: Whether it is needed to discuss the reliability requirements for NR MBS from RAN1 perspective? If the answer is YES, then whether the reliability requirements are RRC state dependent and whether the reliability requirements for multicast and broadcast traffic are the same or not? |
| Question: If it is decided to discuss the reliability requirements for NR MBS in RAN1, then how to define the reliability requirements? |

**Table A.3: Summary of second tier issues of MBS for RRC\_IDLE/RRC\_INACTIVE UEs**

|  |  |
| --- | --- |
| **Second tier issues** | **Possible proposals** |
| CORESET for PTM | For UE in IDLE/INACTIVE state, the CORESET for PTM is * Alt 1: CORESET0
* Alt 2: Configurable
 |
| Search space for PTM | For UE in IDLE/INACTIVE state, the search space for PTM is * Alt 1: One(s) of existing common search space
* Alt 2: A new type of CSS set
 |
| Multi-beam operation | Monitoring occasions for PTM is associated with SSB. |
| HARQ-ACK | Whether HARQ-ACK feedback is supported for PTM for UE in IDLE/INACTIVE state:Alt 1: Supported but NACK onlyAlt 2: Not supported |
| Search spaces for SIBx/MCCH if defined | Search spaces for SIBx/MCCH needs to be discussed.  |
| MCS table and number of layers | MCS table to be used and how many layers are used should be configured |

# Appendix B: Summary of Phase 1 discussion

Seventeen companies have provided their views on the classification of priorities for this meeting in phase 1 discussion. The statistics are shown in the table below.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | Issue 1(Question 1 in R1-2007001) | Issue 2(Question 2 in R1-2007001) | Issue 3(Question 3 in R1-2007001) | Issue 4(Proposal 1 in R1-2007001) | Issue 5(Proposal 2 in R1-2007001) | Issue 6(Question 4 in R1-2007001) | Issue 7(Proposal 3 in R1-2007001) | Issue 8(Proposal 4 in R1-2007001) |
| # High | 17 | 8 | 7 | 14 | 6 | 9 | 2 | 2 |
| # Medium |  | 8 | 10 | 3 | 11 | 7 | 7 | 6 |
| # Low |  | 1 |  |  |  | 1 | 8 | 9 |

The following observations can be drawn from companies’ views:

* Issue 1/4/6: More than half of the companies think these three issues should be high priority items.
* Issue 2/3/5: Less than half of the companies think these three issues should be high priority items, but almost all of the companies think they should be at least medium priority items.
* Issue 7/8: About half of the companies think these issues should be low priority. It is explicitly mentioned in Chairman’s notes that no plan to treat 8.12.3 in this meeting.

Based on the above observation, the following proposal is made on the classification of high/medium priority items for this meeting:

**Proposal: The following high/medium priority items are classified for this meeting:**

* **High priority:**
	+ **Issue 1/4/6**
* **Medium priority:**
	+ **Issue 2/3/5**

# References

1. R1-2007001 FL summary on NR Multicast and Broadcast Services Moderator (CMCC)
2. RP-193248 New WID proposal: NR Multicast and Broadcast Services
3. RP-201038 Revised WID: Core part: NR multicast and broadcast services
4. R1-2005249 Resource configuration and group scheduling for RRC\_CONNECTED UEs Huawei, HiSilicon
5. R1-2005406 Discussion on mechanisms to support group scheduling for RRC\_CONNECTED UEs vivo
6. R1-2005436 Mechanisms to Support Group Scheduling for RRC\_CONNECTED UEs ZTE
7. R1-2005531 Group Scheduling Mechanisms to Support 5G Multicast / Broadcast Services for RRC\_CONNECTED Ues Nokia, Nokia Shanghai Bell
8. R1-2005589 Considerations on MBMS group scheduling for RRC\_CONNECTED UEs Sony
9. R1-2005693 Discussion on group scheduling mechanism for RRC\_CONNECTED UEs in MBS CATT
10. R1-2005898 Group Scheduling for NR-MBS Intel Corporation
11. R1-2006013 Group scheduling for NR Multicast and Broadcast Services OPPO
12. R1-2006173 On Mechanisms to support group scheduling for RRC\_CONNECTED UEs Samsung
13. R1-2006233 Discussion on group scheduling mechanisms in NR MBS CMCC
14. R1-2006320 Support of group scheduling for RRC\_CONNECTED UEs LG Electronics
15. R1-2006631 On group scheduling mechanism for NR multicast and broadcast Convida Wireless
16. R1-2006830 Views on group scheduling for Multicast RRC\_CONNECTED UEs Qualcomm Incorporated
17. R1-2006918 Mechanism for group scheduling of RRC\_CONNECTED UEs in NR Ericsson
18. R1-2005250 Mechanisms to improve reliablity for RRC\_CONNECTED UEs Huawei, HiSilicon
19. R1-2005407 Discussion on mechanisms to improve reliability for RRC\_CONNECTED UEs vivo
20. R1-2005437 Mechanisms to Improve Reliability for RRC\_CONNECTED UEs ZTE
21. R1-2005532 Mechanisms for 5G Multicast / Broadcast Reliability Improvements for RRC\_CONNECTED Ues Nokia, Nokia Shanghai Bell
22. R1-2005590 Considerations on MBMS reliability for RRC\_CONNECTED UEs Sony
23. R1-2005694 Discussion on reliability improvement mechanism for RRC\_CONNECTED UEs in MBS CATT
24. R1-2005899 Mechanisms to Improve Reliability for NR-MBS Intel Corporation
25. R1-2006014 UL feedback for RRC-CONNECTED UEs in MBMS OPPO
26. R1-2006174 On Mechanisms to improve reliability for RRC\_CONNECTED Ues Samsung
27. R1-2006234 Discussion on reliability improvement in NR MBS CMCC
28. R1-2006321 Mechanisms to improve reliability of Broadcast/Multicast service LG Electronics
29. R1-2006632 On reliability enhancement for NR multicast and broadcast Convida Wireless
30. R1-2006831 Views on UE feedback for Multicast RRC\_CONNECTED UEs Qualcomm Incorporated
31. R1-2006863 HARQ-based time-interleaving for NR Multicast/Broadcast BBC
32. R1-2006919 Mechanisms to improve reliability for RRC\_CONNECTED UEs receiving PTM transmission Ericsson
33. R1-2005272 Discussion on multicast support for IDLE/INACTIVE UEs Huawei, HiSilicon
34. R1-2005408 Discussion on basic functions for broadcast/multicast for RRC\_IDLE/RRC\_INACTIVE UEs vivo
35. R1-2005438 Basic Functions for Broadcast or Multicast for RRC\_IDLE or RRC\_INACTIVE UEs ZTE
36. R1-2005533 Basic Functions for Broadcast / Multicast for RRC\_IDLE / RRC\_INACTIVE Ues Nokia, Nokia Shanghai Bell
37. R1-2005695 Discussion on basic functions for broadcast/multicast for RRC\_IDLE/RRC\_INACTIVE UEs CATT
38. R1-2006015 Discussion on enhancements for IDLE and INACTIVE state UEs OPPO
39. R1-2006175 On Basic functions for broadcast/multicast for RRC\_IDLE/RRC\_INACTIVE UEs Samsung
40. R1-2006235 Discussion on NR MBS in RRC\_IDLE RRC\_INACTIVE states CMCC
41. R1-2006322 Basic function for broadcast/multicast LG Electronics
42. R1-2006832 Views on group scheduling for Multicast RRC\_IDLE/INACTIVE UEs Qualcomm Incorporated
43. R1-2006920 Basic functions for broadcast/multicast for RRC\_IDLE/RRC\_INACTIVE UEs Ericsson
44. R1-2005439 Preliminary Simulation Results of Rel-17 MBS ZTE
45. R1-2005534 Simulation assumptions and evaluation scenarios for 5G Multicast Services Nokia, Nokia Shanghai Bell
46. R1-2006016 PUCCH resource allocation for UL feedback in MBMS OPPO
47. R1-2006236 On R17 NR MBS WI CMCC
48. R1-2006410 Performance evaluation of HARQ for NR multicast Huawei, HiSilicon
49. R1-2006658 Other issues for Rel-17 MBS vivo
50. R1-2006861 MIMO support in NR Multicast/Broadcast BBC
51. R1-2006921 Assumptions for Performance Evaluations of NR-MBS Ericsson