3GPP TSG RAN WG1 #104-e R1-21xxxxx

**e-Meeting, January 25th – February 5th, 2021**

**Agenda item: 7.2.12**

**Source: Moderator (China Telecom)**

**Title: [104-e-NR-TxSwitching-01] Summary of email discussion on maintenance of Rel-16 uplink Tx switching**

**Document for: Discussion and Decision**

# Introduction

In [1], maintenance issues are summarized for Rel-16 uplink Tx switching. As per the guidance of Chairman, following issues are identified for email discussion/approval during RAN1 #104 e-meeting:

[104-e-NR-TxSwitching-01] Email discussion/approval on corrections regarding – till 1/29, Jianchi (China Telecom)

* Issue#1: Clarification on the ambiguity issue on SCS in TS 38.214
* Issue#2: Align the RRC parameters in TS 38.214 with TS 38.331
* Issue#3: Clarification on the Maximum data rate in TS 38.306
* Issue#4: Clarification of Tswitch in TS 38.213
* Issue#6: Clarification on the state of Tx chains for SRS antenna switching

and how to handle the following proposal (as a conclusion in Chairman’s notes?)

* For Rel-16 inter-band UL CA, SUL and EN-DC, if uplink Tx switching is configured on two uplinks, the case where SRS carrier switching is configured on a third uplink is not supported.
  + No spec impact.

This contribution is the summary of email discussion/approval on maintenance of Rel-16 uplink Tx switching.

# Discussion

## Issue#1: Clarification on the ambiguity issue on SCS in TS 38.214

This issue has been discussed for several meetings, but no progress has been made.

The last version of TP in RAN1#103e is as follows:

|  |
| --- |
| 6.1.6 Uplink switching  **< unchanged text omitted>**  The UE does not expect to perform more than one uplink switching in a slot with *µUL* = max (*µUL,1, µUL,2*), where the *µUL,1* corresponds to the subcarrier spacing of the active UL BWP of one uplink transmitted before the switching gap and the *µUL,2* corresponds to the subcarrier spacing of the active UL BWP of the other uplink transmitted after the switching gap.  **< unchanged text omitted>** |

In this meeting, R1-2100087 provided two alternatives:

|  |
| --- |
| **TP Alt.1**  The UE does not expect to perform more than one uplink switching in a slot with *µUL* = max(*µUL, 1, µUL, 2*), where the *µUL, 1* corresponds to the subcarrier spacing of the active UL BWP of one uplink carrier and the *µUL, 2* corresponds to the subcarrier spacing of the active UL BWP of the other uplink carrier. |

|  |
| --- |
| **TP Alt.2**  The UE does not expect to perform more than one uplink switching in a slot with *µUL* = max(*µUL, 1, µUL, 2*), where the *µUL, 1* corresponds to the subcarrier spacing of the active UL BWP of one uplink carrier after the switching gap and the *µUL, 2* corresponds to the subcarrier spacing of the active UL BWP of the other uplink carrier after the switching gap. |

Companies are invited to provide views on the above TPs.

|  |  |
| --- | --- |
| **Companies** | **Comments** |
| CATT | Ok with TP Alt.1, but not TP Alt.2. |
|  |  |
|  |  |

## Issue#2: Align the RRC parameters in TS 38.214 with TS 38.331

R1-2100117 proposed the following TP to align the RRC parameters of TS 38.214 and TS 36.331.

|  |
| --- |
| 1. 6.1.6.1 Uplink switching for EN-DC   **< unchanged text omitted>**  - when the UE is configured with *tdm-PatternConfig-r15* or by *~~tdm-PatternConfig-r16~~ tdm-PatternConfig2*  - for the E-UTRA subframes designated as uplink by the configuration, the UE assumes the operation state in which one-port E-UTRA uplink can be transmitted.  - for the E-UTRA subframes other than the ones designated as uplink by the configuration, the UE assumes the operation state in which two-port NR uplink can be transmitted.  **< unchanged text omitted>** |

Companies are invited to provide views on the above TP.

|  |  |
| --- | --- |
| **Companies** | **Comments** |
|  |  |
|  |  |
|  |  |

## Issue#3: Clarification on the Maximum data rate in TS 38.306

R1-2101445 proposed to adopt the following revision of the note for the maximum data rate.

|  |
| --- |
| NOTE 2:  For UL Tx switching ~~between carriers in cell(s)~~, only the supported MIMO layer combination ~~across carriers~~ that results in the highest combined data rate is counted for the cell(s) in the supported maximum UL data rate. |

R1-2101554 proposed to adopt the following revision of the note for the maximum data rate.

|  |
| --- |
| NOTE 2:  For UL Tx switching between two cells, only the supported MIMO layer combination across the two cells that results in the highest combined data rate is counted for those cells in the supported maximum UL data rate. |

Companies are invited to provide views on the above TPs.

|  |  |
| --- | --- |
| **Companies** | **Comments** |
| CATT | The TP from R1-2101445 is more generic and covers the case that more than two cells are configured with UL Tx switching. |
|  |  |
|  |  |

## Issue#4: Clarification of *Tswitch* in TS 38.213

R1-2101738 proposed the following TP to TS 38.213.

|  |
| --- |
| 9.2.5 UE procedure for reporting multiple UCI types  **< unchanged text omitted>**  - if there is an aperiodic CSI report multiplexed in a PUSCH in the group of overlapping PUCCHs and PUSCHs, is not before a symbol with CP starting after after a last symbol of  - any PDCCH with the DCI format scheduling an overlapping PUSCH, and  - any PDCCH scheduling a PDSCH, or SPS PDSCH release, or providing a DCI format 1\_1 indicating SCell dormancy, or a DCI format 1\_1 indicating a request for a Type-3 HARQ-ACK codebook report without scheduling PDSCH, with corresponding HARQ-ACK information in an overlapping PUCCH in the slot  where corresponds to the smallest SCS configuration among the SCS configuration of the PDCCHs, the smallest SCS configuration for the group of the overlapping PUSCHs, and the smallest SCS configuration of CSI-RS associated with the DCI format scheduling the PUSCH with the multiplexed aperiodic CSI report, and for , for and for . is defined in [6, TS 38.214] and it is applied only if of table 5.4-1 in [6, TS 38.214] is applied to the determination of .  - , , , , , and are defined in [6, TS 38.214], and and are defined in [4, TS 38.211].  **< unchanged text omitted>** |

Companies are invited to provide views on the above TP.

|  |  |
| --- | --- |
| **Companies** | **Comments** |
|  |  |
|  |  |
|  |  |

## Issue#6: Clarification on the state of Tx chains for SRS antenna switching

**Proposal:**

* In the Y-symbol gap between SRS transmissions defined by Table 6.2.1.2-1 in 38.214, the UE is assumed to operate with the same number of ports as before and after the gap.

Companies are invited to provide views on the above proposal.

|  |  |
| --- | --- |
| **Companies** | **Comments** |
| CATT | Ok with the proposal. |
|  |  |
|  |  |

## Discussion on the conclusion on CA based SRS switching

**Proposed conclusion:**

* For Rel-16 inter-band UL CA, SUL and EN-DC, if uplink Tx switching is configured on two uplinks, the case where SRS carrier switching is configured on a third uplink is not supported.
  + No spec impact.

Companies are invited to provide views on the above proposal.

|  |  |
| --- | --- |
| **Companies** | **Comments** |
| CATT | We would like to understand the proposal more. A UE configured with UL Tx switching on CC1 and CC2, are configured with SRS carrier switching between CC3 and CC4. The proposed conclusion ruled out such configuration. Is that the intention? |
|  |  |
|  |  |

# References

1. R1-2101782, Summary of Rel-16 uplink Tx switching, Moderator (China Telecom), RAN1#104-e, January 25th – February 5th, 2021.
2. R1-2100087, Remaining issues of Rel-16 UL Tx Switching, ZTE, RAN1#104-e, January 25th – February 5th, 2021.
3. R1-2100117, Text Proposals for Tx Switching between Two Uplink Carriers, OPPO, RAN1#104-e, January 25th – February 5th, 2021.
4. R1-2101445, Remaining issues for 1Tx-2Tx switching, Qualcomm Incorporated, RAN1#104-e, January 25th – February 5th, 2021.
5. R1-2101554, Maintenance for Rel-16 UL Tx Switching, Ericsson, RAN1#104-e, January 25th – February 5th, 2021.
6. R1-2101738, Discussion on the remaining problems of supporting Tx switching between two uplink carriers, Huawei, HiSilicon, RAN1#104-e, January 25th – February 5th, 2021.

# Appendix

|  |  |
| --- | --- |
| **Companies** | **Views** |
| **ZTE(R1-2100087)** | ***Proposal 1****: Adopt TP Alt.1 or Alt.2 for 38.214 UL Tx switching.*   |  | | --- | | **TP Alt.1**  The UE does not expect to perform more than one uplink switching in a slot with *µUL* = max(*µUL, 1, µUL, 2*), where the *µUL, 1* corresponds to the subcarrier spacing of the active UL BWP of one uplink carrier and the *µUL, 2* corresponds to the subcarrier spacing of the active UL BWP of the other uplink carrier. |  |  | | --- | | **TP Alt.2**  The UE does not expect to perform more than one uplink switching in a slot with *µUL* = max(*µUL, 1, µUL, 2*), where the *µUL, 1* corresponds to the subcarrier spacing of the active UL BWP of one uplink carrier after the switching gap and the *µUL, 2* corresponds to the subcarrier spacing of the active UL BWP of the other uplink carrier after the switching gap. | |
| **OPPO(R1-2100117)** | 1. 6.1.6.1 Uplink switching for EN-DC   **< unchanged text omitted>**  - when the UE is configured with *tdm-PatternConfig-r15* or by *~~tdm-PatternConfig-r16~~ tdm-PatternConfig2*  - for the E-UTRA subframes designated as uplink by the configuration, the UE assumes the operation state in which one-port E-UTRA uplink can be transmitted.  - for the E-UTRA subframes other than the ones designated as uplink by the configuration, the UE assumes the operation state in which two-port NR uplink can be transmitted.  **< unchanged text omitted>** |
| **Qualcomm(R1-2101445)** | **Proposal 1: In the prioritization for SRS switching considers the state of carriers configured with UL Tx switching jointly. As an example, if SRS switching is configured between CC2 and CC3 then in the prioritization the state of CC1 also needs to be considered if CC1 and CC2 are configured with UL Tx switching.**  **Proposal 2: Define requirements allowing dropping transmissions on a CC due to SRS transmission on another CC, even if this CC is not configured with SRS switching, as long as the CC is configured with UL Tx switching.**  **Proposal 3: Choose one of the following options:**   * **During the SRS transmission on CC3 and the interruption time caused by RF tuning, UE is not expected to be scheduled or configured with other transmission requiring UL Tx switching** * **Define rules on the order in which the UE state vs. dropping decisions are being made**   **Proposal 4: When the UE transmits SRS with Tx switching according to capability ‘xTyR’ on a CC, the UE is assumed to be in an UL Tx switching state supporting at least x ports on that CC.**  **Proposal 5: RAN1 should discuss and decide whether to introduce further capability with which a UE can indicate that 1TyR is counted as 2 ports on the CC supporting 2-port transmission.**  **Proposal 6: In the Y-symbol gap between SRS transmissions defined by Table 6.2.1.2-1 in 38.214, the UE is assumed to operate with the same number of ports as before and after the gap.**  **Proposal 7: Adopt the following revision of the note for the maximum data rate:**  NOTE 2:  For UL Tx switching ~~between carriers in cell(s)~~, only the supported MIMO layer combination ~~across carriers~~ that results in the highest combined data rate is counted for the cell(s) in the supported maximum UL data rate. |
| **Ericsson(R1-2101554)** | **Proposal** 1: NOTE 2 in the TP agreed for 38.306, section 4.1.2 is updated as follows:  NOTE 2:  For UL Tx switching between two cells, only the supported MIMO layer combination across the two cells that results in the highest combined data rate is counted for those cells in the supported maximum UL data rate. |
| **Huawei, HiSilicon(R1-2101738)** | 9.2.5 UE procedure for reporting multiple UCI types  **< unchanged text omitted>**  - if there is an aperiodic CSI report multiplexed in a PUSCH in the group of overlapping PUCCHs and PUSCHs, is not before a symbol with CP starting after after a last symbol of  - any PDCCH with the DCI format scheduling an overlapping PUSCH, and  - any PDCCH scheduling a PDSCH, or SPS PDSCH release, or providing a DCI format 1\_1 indicating SCell dormancy, or a DCI format 1\_1 indicating a request for a Type-3 HARQ-ACK codebook report without scheduling PDSCH, with corresponding HARQ-ACK information in an overlapping PUCCH in the slot  where corresponds to the smallest SCS configuration among the SCS configuration of the PDCCHs, the smallest SCS configuration for the group of the overlapping PUSCHs, and the smallest SCS configuration of CSI-RS associated with the DCI format scheduling the PUSCH with the multiplexed aperiodic CSI report, and for , for and for . is defined in [6, TS 38.214] and it is applied only if of table 5.4-1 in [6, TS 38.214] is applied to the determination of .  - , , , , , and are defined in [6, TS 38.214], and and are defined in [4, TS 38.211].  **< unchanged text omitted>** |