**3GPP TSG-RAN WG1 Meeting #104-e *R1-210xxxx***

**e-Meeting, January 25th – February 5th, 2021**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **38.213** | **CR** |  | **rev** |  | **Current version:** | **16.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Corrections related to prioritization between uplink and sidelink |
|  |  |
| ***Source to WG:*** | Moderator (LG Electroincs) |
| ***Source to TSG:*** | R1 |
|  |  |
| ***Work item code:*** | 5G\_V2X\_NRSL |  | ***Date:*** | 2021-02-05 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | 1. Prioritization between sidelink and PUCCH associated with the random access is not specified in the current speicfication.
2. Prioritization between PUCCH carrying SL HARQ-ACK reporting and PSFCH or S-SSB reception is not specified in the current specification.
 |
|  |  |
| ***Summary of change:*** | 1. PUCCH transmission for the response of MsgB and Msg4 is prioritized over SL transmission(s).
2. Prioritization between PUCCH carrying SL HARQ-ACK reporting and PSFCH or S-SSB reception are specified by reusing the rule for PSFCH or S-SSB transmission.
 |
|  |  |
| ***Consequences if not approved:*** | 1. The UE behavior remains incompete when PUCCH associated with random access overlaps with sidelink and the random access procedure may not be terminated properly.
2. The UE procedure remains incomplete in the collision between PUCCH carrying SL HARQ-ACK reporting and PSFCH or S-SSB reception.
 |
|  |  |
| ***Clauses affected:*** | 16.2.4.3.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ... |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\* Unchanged text is omitted \*\*\*

16.2.4.3.1 Prioritizations for sidelink and uplink transmissions/receptions

A UE performs prioritization between SL transmissions/receptions and UL transmissions after performing the procedures described in Clause 9.2.5 and in Clause 6.1 of [6, TS 38.214].

\*\*\* Unchanged text is omitted \*\*\*

A PRACH transmission, or a PUSCH scheduled by an UL grant in a RAR and its retransmission, or a PUSCH for Type-2 random access procedure and its retransmission, or a PUCCH indicated by successRAR, or a PUCCH scheduled by a DCI format 1\_0 with CRC scrambled by a corresponding TC-RNTI has higher priority than a SL transmission or reception.

A PUCCH transmission with a sidelink HARQ-ACK information report has higher priority than a SL transmission if a priority value of the PUCCH is smaller than a priority value of the SL transmission. The priority value of the PUCCH transmission is as described in Clause 16.5. If the priority value of the PUCCH transmission is larger than the priority value of the SL transmission, the SL transmission has higher priority.

A PUCCH transmission with a sidelink HARQ-ACK information report has higher priority than a PSFCH/S-SS/PSBCH block reception if a priority value of the PUCCH is smaller than a priority value of the SL reception. If the priority value of the PUCCH transmission is larger than the priority value of the PSFCH/S-SS/PSBCH block reception, the SL reception has higher priority.

\*\*\* Unchanged text is omitted \*\*\*