3GPP TSG RAN WG1 #104-e R1-210xxxx

e-Meeting, January 25th – February 5th, 2021

Source: Moderator (OPPO)

Title: Discussions on Issue MT.1

Agenda Item: 7.2.6

Document for: Discussion and Decision

The Issue of MT.1

The UE capability of out-of-order operation of PUSCH/PDCCH in mTRP is specified by the feature group 16-2a-3 in R1-2100113:

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 16-2a-3 | Out-of-order operation for UL | 1. Support out-of-order operation for PDCCH to PUSCH | 16-2a | Yes | N/A |  | Per band | No | No |  | Note: “Same closed loop index for power control across PUSCHs associated with different CORESETPoolIndex values is not supported by a UE indicating the support of this feature” | Optional with capability signalling |

OPPO (R1-2100113), ZTE (R1-2100281) and Huawei/HiSi (R1-2101256) explained in their tdoc that the note added here could cause some critical issues.

* The note would result in that in FR1, the system can not schedule PUSCHs by PDCCH of different CORESETPoolIndex value to a UE supporting the UE capability of 16-2a-3. Because typically in FR1, only one SRS resource is configured for PUSCH transmission and there is no SRI field in DCI. Thus, a same default closed loop index is always applied to all the PUSCH transmissions.
* To make the system work, the note seems to mandate the gNB to implement two different close loops based on UE capability reporting, no matter whether gNB needs 16-2a-3 functionality.

To resolve that issue, OPPO, ZTE and Huawei/HiSi proposed different solutions or TPs:

* OPPO and ZTE proposed to specify in 38.213 that when the DCI does not have SRI field or when SRI-PUSCH-PowerControl is not provided (i.e., only one default closed-loop index is assumed as specified in current spec), the UE would assume different closed loop index for PUSCHs towards different TRPs.
* ZTE and Huawei/HiSi proposed to capture the scheduling restriction imposed by that Note in the spec even through they proposed different TPs.

## **Round#1 discussion**

Based on the proposals by OPPO/ZTE/HW, here is the initial proposal for MT.1

**Proposal: For issue MT.1:**

* **In Section 7.1.1 of 38.213, for the case when DCI does not have SRI field or SRI-PUSCH-PowerControl is not provided, we clarify that the PUSCHs scheduled by PDCCH of different CORESETPoolindex are associated with different default closed loop index**
* **In section 6.1 of 38.214, we capture the restriction described by the note of FG 16-2a-3 into the description of PUSCH out-order-operation.**

The TP for 38.213:

|  |
| --- |
| **7.1.1 UE behaviour**\*\*\* Unchanged text is omitted \*\*\*-  if the UE is configured with *twoPUSCH-PC-AdjustmentStates* and  if the UE is not configured with *twoPUSCH-PC-AdjustmentStates* or if the PUSCH transmission is scheduled by a RAR UL grant as described in Clause 8.3- For a PUSCH (re)transmission configured by *ConfiguredGrantConfig*, the value of  is provided to the UE by *powerControlLoopToUse*- If the UE is provided *SRI-PUSCH-PowerControl*, the UE obtains a mapping between a set of values for the SRI field in a DCI format scheduling the PUSCH transmission and the  value(s) provided by *sri-PUSCH-ClosedLoopIndex* and determines the  value that is mapped to the SRI field value- If the PUSCH transmission is scheduled by a DCI format that does not include an SRI field, or if an *SRI-PUSCH-PowerControl* is not provided to the UE, *l*=1 if the PUSCH is scheduled by a PDCCH received in a CORESET which is configured with *CORESETPoolIndex* equal to 1 and othersiwe - If the UE obtains one TPC command from a DCI format 2\_2 with CRC scrambled by a TPC-PUSCH-RNTI, the  value is provided by the closed loop indicator field in DCI format 2\_2 |

The TP for 38.214:

|  |
| --- |
| **6.1 UE procedure for transmitting the physical uplink shared channel**\*\*\* Unchanged text is omitted \*\*\*If a UE is configured by higher layer parameter *PDCCH-Config* that contains two different values of *CORESETPoolIndex* in *ControlResourceSet* for the active BWP of a serving cell and PDCCHs that schedule two non-overlapping in time domain PUSCHs are associated to different *ControlResourceSets* having different values of *CORESETPoolIndex,* for any two HARQ process IDs in a given scheduled cell, if the UE is scheduled to start a first PUSCH transmission starting in symbol *j* by a PDCCH associated with a value of *CORESETpoolIndex* ending in symbol *i*, the UE can be scheduled to transmit a PUSCH starting earlier than the end of the first PUSCH by a PDCCH associated with a different value of *CORESETpoolIndex* that ends later than symbol *i* and the UE is expected to be provided with a closed loop index for that PUSCH different from the closed loop index of the first PUSCH.\*\*\* Unchanged text is omitted \*\*\* |

If you have comments, please input below

|  |  |
| --- | --- |
| Company | comments |
| QC | There are two different/ unrelated issues lumped together here.Issue 1: DCI does not have SRI field.Issue 2: Restriction imposed by the note on the network.Do not support the proposal for Issue 1. The scenario mentioned by OPPO (SRI field not configured) is not just related to closed loop index. If SRI field is not configured, how does the UE obtain P0, alpha, PL-RS? How does the UE obtain precoding (TPMI for CB-based, SRS resources for NCB-based). This seems to be a big surgery to Rel. 16. If PUSCHs are to be transmitted to different TRPs, SRI field should be always configured and DCI format 0\_1 should be used, which solves all the problems mentioned by OPPO. Regarding Issue 2, we do not see how the TP alleviates the issue. Is the intention here only to capture the note in 38.214? We do see why this is critical. The note is captured already and is part of NR specification. It is not critical to repeat the same in 38.214. We are open to discuss actual solutions to address the issue, but the suggested TP above is not for this purpose. |
|  |  |
|  |  |
|  |  |