**Proposal 4.1**: On Rel.17 enhancement for facilitating fast uplink panel selection, for discussion purposes, a panel entity corresponds to one or more RS resources:

* For CSI/beam reporting, the RS is an RS associated with measurement and/or reporting
* For beam indication, the RS is a source RS for UL TX spatial filter information
* [Note: For one RS, the corresponding panel entity may not be consistent and is up to UE implementation]
* [FFS: Whether the one or more RS resources can correspond to one or more RS resource set(s)]
* [FFS: Whether panel entity is not consistent or not for one RS source
* FFS: Whether panel entity is up to UE implementation or not]

**Proposal 5.1**: On Rel.17 enhancements to facilitate MPE mitigation, decide in RAN1#104bis-e whether to support at least one the following (not necessarily, but can be, in one reporting instance):

* {Rel.16 P-MPR based (beam/panel-level)} + {A}, where A is either Opt1A, Opt1B, Opt1C, or Opt1D:
	+ Option 1A: Virtual PHR or a modified version associated with each activated UL TCI or, if applicable, joint TCI
	+ Option 1B: {SSBRI(s)/CRI(s) and/or panel indication}
	+ Option 1C: {SSBRI(s)/CRI(s) and/or panel indication} + virtual PHR or a modified version associated with each of the reported SSBRI(s)/CRI(s) and/or panel indication (if configured)
	+ Option 1D: No additional reporting quantity
* {SSBRI(s)/CRI(s) and/or panel indication} + {A}, where A is either Opt2A, Opt2B, Opt2A+ Opt2B, or Option 2C
	+ Option 2A: L1-RSRP [L1-SINR] or a modified version that accounts for MPE effect associated with each of the reported SSBRI(s)/CRI(s) and/or panel indication (if configured)
		- FFS: How panel-level L1-RSRP [L1-SINR] is reported if L1-RSRP [L1-SINR] is associated with panel
		- FFS: Whether/how to account for MPE effect in L1-RSRP [L1-SINR] report, e.g. by using scaled L1-RSRP [L1-SINR]
		- FFS: Whether/how to enhance existing beam reporting format to support Option 2A
	+ Option 2B: Virtual PHR or a modified version associated with each of the reported SSBRI(s)/CRI(s) and/or panel indication (if configured)
	+ Option 2C: No additional reporting quantity