[104-e-NR-R17-SL-03] Email discussion on 8.11.2 (remaining issues for sidelink evaluation methodology update for power saving) – Teng (CATT)

* 1st check point: Jan 28
* 2nd check point: Feb 3

This document is used to discuss the issues raised during the 1st round of discussion, which is considered to be necessary for further discussion and determination.

# Definition of different profiles for V2V/V2P/P2V

1 contribution proposes to define separate profiles for P2V, V2P and mixture case. In order to guarantee that the simulation results of companies can be compared with each other, 3 profiles are proposed with corresponding parameters.

* Profile 1-P2V: Evaluation on partial sensing.
* Profile 2-V2P: Evaluation on DRX.
* Profile 3-Mixture with P2V/V2P/V2V: Evaluation on co-existence of PUE and VUE with different RA schemes in the same resource pool.

Based on the clarification during GTW, companies agreed to further discuss on the definition of the profiles for V2V/V2P/P2V. I would like to use the proposal in R1-2100143 as the starting point of this discussion. Companies are welcome to provide comments about it.

***FL Proposal:***

* *The following profiles are defined:*
	+ *Profile 1: P2V-only;*
	+ *Profile 2: V2P-only;*
	+ *Profile 3: Mixture of P2V, V2P and V2V.*

|  |  |  |  |
| --- | --- | --- | --- |
|  | **P2V Only** | **V2P Only** | **Mixture(P2V,V2P,V2V)** |
| **Sidelink frequency (GHz)** | 6 | 6 | 6 |
| **Traffic models** | Periodic: Traffic model for P-UE’s transmission specified in TS 36.885−The message size is fixed at 300 bytes and transmission frequency is 1 Hz −‘100ms’ latency requirement−100% vehicles generate packets.Aperiodic: Aperiodic Model 1 specified in TR37.885 with following changes:−Inter-packet arrival time: 250 ms + an exponential random variable with the mean of 250 ms−Packet size: Uniformly random in the range between 200 bytes and 800 bytes with the quantization step of 200 bytes−Latency requirement: 100 ms−100% vehicles generate packets.Note:All PUEs use the same traffic for simplicity.Periodic and aperiodic traffic are simulated separately. | Periodic: Medium intensity; [50] ms inter-packet arrival, [50]% vehicles generate packets.Aperiodic: Medium intensity, 100% vehicles generate packets.Note:All VUEs use the same traffic for simplicityPeriodic and aperiodic traffic are simulated separately. | Periodic traffic for VUE: Medium intensity; [50] ms inter-packet arrival, [50]% vehicles generate packets.Aperiodic traffic for VUE: Medium intensity, 100% vehicles generate packets.Periodic traffic for PUE:Traffic model for P-UE’s transmission specified in TS 36.885−The message size is fixed at 300 bytes and transmission frequency is 1 Hz −‘100ms’ latency requirement−100% vehicles generate packets.Aperiodic traffic for PUE:Aperiodic Model 1 specified in TR37.885 with following changes:−Inter-packet arrival time: 250 ms + an exponential random variable with the mean of 250 ms−Packet size: Uniformly random in the range between 200 bytes and 800 bytes with the quantization step of 200 bytes−Latency requirement: 100 ms−100% vehicles generate packets.Note:All PUEs use the same traffic for simplicity.All VUEs use the same traffic for simplicityThe traffic model of V2P and V2V is same for simplicity |
| **Cast type** | Broadcast  | 33%, 33%, 34% vehicles generate unicast, multicast, broadcast packets, respectively. | VUE: 33%, 33%, 34% vehicles generate unicast, multicast, broadcast packets, respectively.PUE: Broadcast |
| **Simulation environment, UE drop and mobility** | Urban: Option AAmount of PUE: 500All PUEs are dropped in 9 grids | Urban: Option AAmount of PUE: 500All PUEs are dropped in 9 grids | Urban: Option AAmount of PUE: 500All PUEs are dropped in 9 grids |
| **Channel model** | As defined | As defined | As defined |
| **SL simulation bandwidth (MHz)** | 20 MHz  | 20 MHz  | 40 MHz  |
| **Resource selection scheme** | Full sensingPartial sensingRandom selectionEach scheme is simulated separately (To compare with each other) | Full sensing (As a background to evaluate different DRX schemes) | VUE: Full sensingPUE: Random selection or partial sensingNote: All VUEs use the same resource selection scheme for simplicityAll PUEs use the same resource selection scheme for simplicity |

**Round 1 comment on 1/27 – 1.29**

**Q1: Do you think it necessary to define the profile for P2V/V2P/V2V? (Y/N)**

**Q2: If Q1 is Yes, do you support all the three profiles, or some of them? (Profile 1/2/3)**

**Q3: If Q1 is Yes, and Q2 is also supported, please provide your suggested profiles below the comments table.**

|  |  |  |  |
| --- | --- | --- | --- |
| **Company** | **Q1** | **Q2** | **Views** |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

[Company name 1]

|  |  |  |  |
| --- | --- | --- | --- |
|  | **P2V-only** | **V2P-only** | **Mixture of P2V/V2P/V2V** |
|  |  |  |  |

[Company name 2]

|  |  |  |  |
| --- | --- | --- | --- |
|  | **P2V-only** | **V2P-only** | **Mixture of P2V/V2P/V2V** |
|  |  |  |  |

[Company name 3]

|  |  |  |  |
| --- | --- | --- | --- |
|  | **P2V-only** | **V2P-only** | **Mixture of P2V/V2P/V2V** |
|  |  |  |  |