[104-e-NR-R17-SL-03] Email discussion on 8.11.2 (remaining issues for sidelink evaluation methodology update for power saving) – Teng (CATT)

* 1st check point: Jan 28
* 2nd check point: Feb 3

This document is used to discuss the issues raised during the 1st round of discussion, which is considered to be necessary for further discussion and determination.

# Definition of different profiles for V2V/V2P/P2V

1 contribution proposes to define separate profiles for P2V, V2P and mixture case. In order to guarantee that the simulation results of companies can be compared with each other, 3 profiles are proposed with corresponding parameters.

* Profile 1-P2V: Evaluation on partial sensing.
* Profile 2-V2P: Evaluation on DRX.
* Profile 3-Mixture with P2V/V2P/V2V: Evaluation on co-existence of PUE and VUE with different RA schemes in the same resource pool.

Based on the clarification during GTW, companies agreed to further discuss on the definition of the profiles for V2V/V2P/P2V. I would like to use the proposal in R1-2100143 as the starting point of this discussion. Companies are welcome to provide comments about it.

***FL Proposal:***

* *The following profiles are defined:*
	+ *Profile 1: P2V-only;*
	+ *Profile 2: V2P-only;*
	+ *Profile 3: Mixture of P2V, V2P and V2V.*

|  |  |  |  |
| --- | --- | --- | --- |
|  | **P2V Only** | **V2P Only** | **Mixture(P2V,V2P,V2V)** |
| **Sidelink frequency (GHz)** | 6 | 6 | 6 |
| **Traffic models** | Periodic: Traffic model for P-UE’s transmission specified in TS 36.885−The message size is fixed at 300 bytes and transmission frequency is 1 Hz −‘100ms’ latency requirement−100% vehicles generate packets.Aperiodic: Aperiodic Model 1 specified in TR37.885 with following changes:−Inter-packet arrival time: 250 ms + an exponential random variable with the mean of 250 ms−Packet size: Uniformly random in the range between 200 bytes and 800 bytes with the quantization step of 200 bytes−Latency requirement: 100 ms−100% vehicles generate packets.Note:All PUEs use the same traffic for simplicity.Periodic and aperiodic traffic are simulated separately. | Periodic: Medium intensity; [50] ms inter-packet arrival, [50]% vehicles generate packets.Aperiodic: Medium intensity, 100% vehicles generate packets.Note:All VUEs use the same traffic for simplicityPeriodic and aperiodic traffic are simulated separately. | Periodic traffic for VUE: Medium intensity; [50] ms inter-packet arrival, [50]% vehicles generate packets.Aperiodic traffic for VUE: Medium intensity, 100% vehicles generate packets.Periodic traffic for PUE:Traffic model for P-UE’s transmission specified in TS 36.885−The message size is fixed at 300 bytes and transmission frequency is 1 Hz −‘100ms’ latency requirement−100% vehicles generate packets.Aperiodic traffic for PUE:Aperiodic Model 1 specified in TR37.885 with following changes:−Inter-packet arrival time: 250 ms + an exponential random variable with the mean of 250 ms−Packet size: Uniformly random in the range between 200 bytes and 800 bytes with the quantization step of 200 bytes−Latency requirement: 100 ms−100% vehicles generate packets.Note:All PUEs use the same traffic for simplicity.All VUEs use the same traffic for simplicityThe traffic model of V2P and V2V is same for simplicity |
| **Cast type** | Broadcast  | 33%, 33%, 34% vehicles generate unicast, multicast, broadcast packets, respectively. | VUE: 33%, 33%, 34% vehicles generate unicast, multicast, broadcast packets, respectively.PUE: Broadcast |
| **Simulation environment, UE drop and mobility** | Urban: Option AAmount of PUE: 500All PUEs are dropped in 9 grids | Urban: Option AAmount of PUE: 500All PUEs are dropped in 9 grids | Urban: Option AAmount of PUE: 500All PUEs are dropped in 9 grids |
| **Channel model** | As defined | As defined | As defined |
| **SL simulation bandwidth (MHz)** | 20 MHz  | 20 MHz  | 40 MHz  |
| **Resource selection scheme** | Full sensingPartial sensingRandom selectionEach scheme is simulated separately (To compare with each other) | Full sensing (As a background to evaluate different DRX schemes) | VUE: Full sensingPUE: Random selection or partial sensingNote: All VUEs use the same resource selection scheme for simplicityAll PUEs use the same resource selection scheme for simplicity |

**Round 1 comment on 1/27 – 1.29**

**Q1: Do you think it necessary to define the profile for P2V/V2P/V2V? (Y/N)**

**Q2: If Q1 is Yes, do you support all the three profiles, or some of them? (Profile 1/2/3)**

**Q3: If Q1 is Yes, and Q2 is also supported, please provide your suggested profiles below the comments table.**

|  |  |  |  |
| --- | --- | --- | --- |
| **Company** | **Q1** | **Q2** | **Views** |
| vivo | comment | comment | It would be good to limit the variations between results from different sources. The problem of these profiles for P2V-only and V2P-only is on the interference link. For example, in P2V-only profile, the only interference / collision sources are TX from other PUEs. Such modelling is too optimistic to get a meaningful observation. Thus, at least V2V should be modelled together for P2V case, while P2P should be modelled together for V2P case, in order to have meaningful results.But then the P2V and V2P profiles require a similar cost of simulations as mixture profiles, and become questionable why we should define these two profiles. Note that it is also possible to evaluate the P2V and V2P performance in a single mixture scenario. |
| **Qualcomm** | **No** |  | **In our view, companies can select their scenario(s) of interest and perform evaluations. There is no need to start an alignment effort at this point.** |
| OPPO | YES | YES | We support the above three profiles. The scenario of P2V only is used to evaluate the performance of different partial sensing algorithms in a relatively ideal scenario. In the meanwhile, the scenario of V2P only is used to evaluate the performance of different DRX schemes. Finally, the mixture scenario is the most complicated one. Considering the workload of simulation, we have to make some assumptions for simplicity, e.g., all of VUEs have the same traffic model and only perform one type of RA schemes in one simulation. |
| ZTE,Sanechips | Yes | Yes | See table below. |
| CATT, GOHIGH | Yes | Some of them | For P2V evaluation, we think at least P2V+V2V should be evaluated. In P2V only cases with current evaluation assumption, the resources for P-UE transmission is over-provided, maybe all the partial sensing schemes could achieve better and similar performance gain. For V2P evaluation, similar with P2V, we think at least V2P+V2V should be evaluated.  |
| Huawei, HiSilicon | No |  | We think companies can select the scenarios and perform evaluations they prefer. No common profile is needed. |
| Fujitsu | Yes | See comments | It would be convenient to compare simulation results from different companies with a uniform profile.Aside from the above three profiles, profile for P2P should also be defined. In RAN#90e, the Rel.17 sidelink WID was updated to consider the impact of sidelink DRX when specifying power saving resource allocation (e.g., partial sensing). One of the major impacts of DRX on partial sensing is expected to be in P2P use case. Without the P2P scenario, the evaluation of DRX impact would be incomplete.  |
| Samsung | Comment | Comment | Having the three simulation profiles is OK, but the details should follow previous agreements. There is no need to repeat the details in the table that have been previously agreed.  |

[ZTE,Sanechips]

|  |  |  |  |
| --- | --- | --- | --- |
|  | **P2V-only** | **V2P-only** | **Mixture of P2V/V2P/V2V** |
| **Cast type** | Broadcast  | All VUEs use the same cast type for simplicityOptional: 33%, 33%, 34% vehicles generate unicast, multicast, broadcast packets, respectively. | PUE: BroadcastAll VUEs use the same cast type for simplicityOptional: 33%, 33%, 34% vehicles generate unicast, multicast, broadcast packets, respectively. |
|  |  |  |  |

***Observations on the 1st round of discussion:***

* Totally 8 companies replied on the definition of profile.
	+ 2 companies [Qualcomm, Huawei, HiSilicon] do not prefer to have this profile.
	+ 2 companies [vivo, Samsung] think it is good to have a profile for simulation results comparison among companies. [vivo] think that V2P and P2V requires similar consumptions in mixture scenarios. [Samsung] think that there is no necessary to copy the agreements into such a table as duplicated work.
	+ 4 companies [OPPO, ZTE/Sanechips, CATT/GOHIGH, Fujitsu] support to have such a simulation profile for better comparison on the results. Following to address some comments:
		- P2V-only, V2P-only should consider V2V. Without V2V, purely P2V-only or V2P-only is to optimized for evaluation, which cannot reflect the practical scenarios.
		- P2P is also another important scenario. However, the evaluation should follow the agreements on P2P during last two meetings. It is all up to companies’ option for evaluation. Additional discussion on how to involve P2P in the simulation is not expected.

**[FL]**

The intention of having a simulation profile is good, which is to be used for better comparison on the evaluation results from different companies by applying the same parameters/scenarios. No additional evaluation workload is expected to be introduced to companies’ current simulation work, especially at this stage. The evaluations should follow the agreements, and companies can also select additional scenario(s) they are interested for evaluations.

This profile is that it can be a guidance of evaluation work for future results comparison rather than an extra burden. I would like to suggest companies to update the following profiles based on the agreements and their preference of evaluation assumptions.

**Updated proposal (1.29)**

***FL Proposal:***

* *The following profiles are defined:*

|  |  |  |  |
| --- | --- | --- | --- |
|  | **P2V Only** | **V2P Only** | **Mixture(P2V,V2P,V2V)** |
| **Sidelink frequency (GHz)** | 6 | 6 | 6 |
| **Traffic models** | Periodic: Traffic model for P-UE’s transmission specified in TS 36.885−The message size is fixed at 300 bytes and transmission frequency is 1 Hz −‘100ms’ latency requirement−100% vehicles generate packets.Aperiodic: Aperiodic Model 1 specified in TR37.885 with following changes:−Inter-packet arrival time: 250 ms + an exponential random variable with the mean of 250 ms−Packet size: Uniformly random in the range between 200 bytes and 800 bytes with the quantization step of 200 bytes−Latency requirement: 100 ms−100% vehicles generate packets.Note:All PUEs use the same traffic for simplicity.Periodic and aperiodic traffic are simulated separately. | Periodic: Medium intensity; [50] ms inter-packet arrival, [50]% vehicles generate packets.Aperiodic: Medium intensity, 100% vehicles generate packets.Note:All VUEs use the same traffic for simplicityPeriodic and aperiodic traffic are simulated separately. | Periodic traffic for VUE: Medium intensity; [50] ms inter-packet arrival, [50]% vehicles generate packets.Aperiodic traffic for VUE: Medium intensity, 100% vehicles generate packets.Periodic traffic for PUE:Traffic model for P-UE’s transmission specified in TS 36.885−The message size is fixed at 300 bytes and transmission frequency is 1 Hz −‘100ms’ latency requirement−100% vehicles generate packets.Aperiodic traffic for PUE:Aperiodic Model 1 specified in TR37.885 with following changes:−Inter-packet arrival time: 250 ms + an exponential random variable with the mean of 250 ms−Packet size: Uniformly random in the range between 200 bytes and 800 bytes with the quantization step of 200 bytes−Latency requirement: 100 ms−100% vehicles generate packets.Note:All PUEs use the same traffic for simplicity.All VUEs use the same traffic for simplicityThe traffic model of V2P and V2V is same for simplicity |
| **Cast type** | Broadcast  | All VUEs use the same cast type for simplicityOptional: 33%, 33%, 34% vehicles generate unicast, multicast, broadcast packets, respectively. | PUE: BroadcastAll VUEs use the same cast type for simplicityOptional: 33%, 33%, 34% vehicles generate unicast, multicast, broadcast packets, respectively. |
| **Simulation environment, UE drop and mobility** | Urban: Option AAmount of PUE: 500All PUEs are dropped in 9 grids | Urban: Option AAmount of PUE: 500All PUEs are dropped in 9 grids | Urban: Option AAmount of PUE: 500All PUEs are dropped in 9 grids |
| **Channel model** | As defined | As defined | As defined |
| **SL simulation bandwidth (MHz)** | 20 MHz  | 20 MHz  | 40 MHz  |
| **Resource selection scheme** | Full sensingPartial sensingRandom selectionEach scheme is simulated separately (To compare with each other) | Full sensing (As a background to evaluate different DRX schemes) | VUE: Full sensingPUE: Random selection or partial sensingNote: All VUEs use the same resource selection scheme for simplicityAll PUEs use the same resource selection scheme for simplicity |

**Round 2 comments 1/29-2/2**

|  |  |
| --- | --- |
| **Company** | **Views** |
| vivo | As commented before, the proposed P2V and V2P profiles are meaningless given only impractical interference modelling. The mixture profile is somewhat better, but still not representing, given the broadcast traffic is simulated for PUE. Moreover, all the profiles here are for V2X scenarios. Then the evaluation results may be meaningful for public safety/commercial. Thus, we start to doubt the benefit of these profiles, and do not support this proposal. |
| Qualcomm | We do not support this proposal. In addition to issues raised by vivo, we would like to emphasize that there had been other proposals by the companies to include other scenarios for evaluation; however, they were not included on the basis that the companies could consider other scenarios too and report their assumptions. We think, for consistency, the same approach can be taken here.  |
|  |  |
|  |  |
|  |  |

[Company name 1]

|  |  |  |  |
| --- | --- | --- | --- |
|  | **P2V-only** | **V2P-only** | **Mixture of P2V/V2P/V2V** |
|  |  |  |  |

[Company name 2]

|  |  |  |  |
| --- | --- | --- | --- |
|  | **P2V-only** | **V2P-only** | **Mixture of P2V/V2P/V2V** |
|  |  |  |  |

[Company name 3]

|  |  |  |  |
| --- | --- | --- | --- |
|  | **P2V-only** | **V2P-only** | **Mixture of P2V/V2P/V2V** |
|  |  |  |  |