**3GPP TSG RAN WG1 Meeting #104bis-e R1-21xxxxx**

**E-meeting, April 12th – April 20th, 2021**

**Agenda Item: 7.1**

**Source: Moderator (Huawei)**

**Title: Summary of [104b-e-NR-7.1CRs-07]: Correction on out-of-order HARQ operation in 38.214**

**Document for: Discussion and Decision**

# Introduction

This document is created to collect company views on the proposed changes in [1].

# Discussion

In Rel-15, a UE is not expected to handle out-of-order PDSCH/HARQ operation, i.e. a later PDSCH has an earlier HARQ-ACK feedback and a later PDCCH schedules an earlier PUSCH transmission. However, the out-of-order PDSCH/HARQ and out-of-order PUSCH operation can be supported by a Rel-16 UE supporting multi-DCI based multi-TRP.

## Issue 1#: Out-of-order PDSCH/HARQ operation

In section 5.1 of TS 38.214 v16.5.0, the second paragraph implies that out-of-order PDSCH/HARQ operation is not allowed in any case since there is no condition for this restriction. The text highlighted in yellow and cyan are for the case where two PDSCH are associated with the HARQ-ACK codebook of same and different priority respectively.

## 5.1 UE procedure for receiving the physical downlink shared channel

[…]

A UE shall upon detection of a PDCCH with a configured DCI format 1\_0, 1\_1 or 1\_2 decode the corresponding PDSCHs as indicated by that DCI. For any HARQ process ID(s) in a given scheduled cell, the UE is not expected to receive a PDSCH that overlaps in time with another PDSCH. The UE is not expected to receive another PDSCH for a given HARQ process until after the end of the expected transmission of HARQ-ACK for that HARQ process, where the timing is given by Clause 9.2.3 of [6]. In a given scheduled cell, the UE is not expected to receive a first PDSCH and a second PDSCH, starting later than the first PDSCH, with its corresponding HARQ-ACK assigned to be transmitted on a resource ending before the start of a different resource for the HARQ-ACK assigned to be transmitted for the first PDSCH, where the two resources are in different slots for the associated HARQ-ACK transmissions, each slot is composed of symbols [4] or a number of symbols indicated by *subslotLengthForPUCCH* if provided, and the HARQ-ACK for the two PDSCHs are associated with the HARQ-ACK codebook of the same priority. In a given scheduled cell, the UE is not expected to receive a first PDSCH, and a second PDSCH, starting later than the first PDSCH, with its corresponding HARQ-ACK assigned to be transmitted on a resource ending before the start of a different resource for the HARQ-ACK assigned to be transmitted for the first PDSCH if the HARQ-ACK for the two PDSCHs are associated with HARQ-ACK codebooks of different priorities. For any two HARQ process IDs in a given scheduled cell, if the UE is scheduled to start receiving a first PDSCH starting in symbol *j* by a PDCCH ending in symbol *i*, the UE is not expected to be scheduled to receive a PDSCH starting earlier than the end of the first PDSCH with a PDCCH that ends later than symbol *i*. In a given scheduled cell, for any PDSCH corresponding to SI-RNTI, the UE is not expected to decode a re-transmission of an earlier PDSCH with a starting symbol less than *N* symbols after the last symbol of that PDSCH, where the value of *N* depends on the PDSCH subcarrier spacing configuration *μ,* with *N*=13 for *μ*=0, *N*=13 for *μ*=1, *N*=20 for *μ*=2, and *N*=24 for *μ*=3.

This is in conflict with a latter description (paragraph 14) for multi-DCI based multi-TRP case where out-of-order PDSCH/HARQ operation is allowed as highlighted in yellow below

## 5.1 UE procedure for receiving the physical downlink shared channel

[…]

If a UE is configured by higher layer parameter *PDCCH-Config* that contains two different values of *coresetPoolIndex* in *ControlResourceSet*, the UE may expect to receive multiple PDCCHs scheduling fully/partially/non-overlapped PDSCHs in time and frequency domain. The UE may expect the reception of full/partially-overlapped PDSCHs in time, only when PDCCHs that schedule two PDSCHs are associated to different *ControlResourceSets* having different values of *coresetPoolIndex*. For a *ControlResourceSet* without *coresetPoolIndex*, the UE may assume that the *ControlResourceSet* is assigned with *coresetPoolIndex* as 0. When the UE is scheduled with full/partially/non-overlapped PDSCHs in time and frequency domain, the full scheduling information for receiving a PDSCH is indicated and carried only by the corresponding PDCCH, the UE is expected to be scheduled with the same active BWP and the same SCS. When the UE is scheduled with full/partially-overlapped PDSCHs in time and frequency domain, the UE can be scheduled with at most two codewords simultaneously. When PDCCHs that schedule two PDSCHs are associated to different *ControlResourceSets* having different values of *coresetPoolIndex,* the following operations are allowed:

- For any two HARQ process IDs in a given scheduled cell, if the UE is scheduled to start receiving a first PDSCH starting in symbol *j* by a PDCCH associated with a value of *coresetPoolIndex* ending in symbol *i*, the UE can be scheduled to receive a PDSCH starting earlier than the end of the first PDSCH with a PDCCH associated with a different value of *coresetPoolIndex* that ends later than symbol *i*.

- In a given scheduled cell, the UE can receive a first PDSCH in slot *i*, with the corresponding HARQ-ACK assigned to be transmitted in slot *j*, and a second PDSCH associated with a value of *coresetPoolIndex* different from that of the first PDSCH starting later than the first PDSCH with its corresponding HARQ-ACK assigned to be transmitted in a slot before slot *j*.

There is a need to add a condition for the case when out-of-order PDSCH/HARQ operation is not allowed at the beginning of section 5.1, i.e. it is not allowed unless specified in the other part of the specification.

## Issue 2#: Out-of-order PUSCH operation

In section 6.1 of TS 38.214 (paragraph 5), the current specification implies that out-of-order PUSCH operation is not allowed in any case.

6.1 UE procedure for transmitting the physical uplink shared channel

[…]

A UE shall upon detection of a PDCCH with a configured DCI format 0\_0, 0\_1 or 0\_2 transmit the corresponding PUSCH as indicated by that DCI. Upon detection of a DCI format 0\_1 or 0\_2 with '*UL-SCH indicator*' set to '0' and with a non-zero '*CSI request*' where the associated *reportQuantity* in *CSI-ReportConfig* set to '*none*' for all CSI report(s) triggered by '*CSI request*' in this DCI format 0\_1 or 0\_2, the UE ignores all fields in this DCI except the '*CSI request*' and the UE shall not transmit the corresponding PUSCH as indicated by this DCI format 0\_1 or 0\_2. When the UE is scheduled with multiple PUSCHs by a DCI, HARQ process ID indicated by this DCI applies to the first PUSCH, as described in clause 6.1.2.1, HARQ process ID is then incremented by 1 for each subsequent PUSCH(s) in the scheduled order, with modulo 16 operation applied. For any HARQ process ID(s) in a given scheduled cell, the UE is not expected to transmit a PUSCH that overlaps in time with another PUSCH. For any two HARQ process IDs in a given scheduled cell, if the UE is scheduled to start a first PUSCH transmission starting in symbol *j* by a PDCCH ending in symbol *i*, the UE is not expected to be scheduled to transmit a PUSCH starting earlier than the end of the first PUSCH by a PDCCH that ends later than symbol *i*. The UE is not expected to be scheduled to transmit another PUSCH by DCI format 0\_0, 0\_1 or 0\_2 scrambled by C-RNTI or MCS-C-RNTI for a given HARQ process until after the end of the expected transmission of the last PUSCH for that HARQ process.

This is in conflict with a later description (paragraph 6) for multi-DCI based multi-TRP case where out-of-order PUSCH operation is allowed.

6.1 UE procedure for transmitting the physical uplink shared channel

[…]

If a UE is configured by higher layer parameter *PDCCH-Config* that contains two different values of *coresetPoolIndex* in *ControlResourceSet* for the active BWP of a serving cell and PDCCHs that schedule two non-overlapping in time domain PUSCHs are associated to different *ControlResourceSets* having different values of *coresetPoolIndex,* for any two HARQ process IDs in a given scheduled cell, if the UE is scheduled to start a first PUSCH transmission starting in symbol *j* by a PDCCH associated with a value of *coresetPoolIndex* ending in symbol *i*, the UE can be scheduled to transmit a PUSCH starting earlier than the end of the first PUSCH by a PDCCH associated with a different value of *coresetPoolIndex* that ends later than symbol *i*.

There is a need to add a condition for the case when out-of-order PUSCH operation is not allowed at the beginning of section 6.1, i.e. it is not allowed unless specified in the other part of the specification.

# Company views

**Q1: Do you agree with changes proposed for issue 1? If not, why?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree or not** | **Comment** |
| vivo | agree |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q2: Do you agree with changes proposed for issue 2? If not, why?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree or not** | **Comment** |
| vivo | agree |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Conclusions

To be updated based on the discussion

# References

1. R1-2103744 Correction on out-of-order HARQ operation in 38.214 Huawei, HiSilicon

# Appendix: Proposed CR in R1-2101275

5.1 UE procedure for receiving the physical downlink shared channel

For downlink, a maximum of 16 HARQ processes per cell is supported by the UE. The number of processes the UE may assume will at most be used for the downlink is configured to the UE for each cell separately by higher layer parameter *nrofHARQ-ProcessesForPDSCH*, and when no configuration is provided the UE may assume a default number of 8 processes.

A UE shall upon detection of a PDCCH with a configured DCI format 1\_0, 1\_1 or 1\_2 decode the corresponding PDSCHs as indicated by that DCI. For any HARQ process ID(s) in a given scheduled cell, the UE is not expected to receive a PDSCH that overlaps in time with another PDSCH. The UE is not expected to receive another PDSCH for a given HARQ process until after the end of the expected transmission of HARQ-ACK for that HARQ process, where the timing is given by Clause 9.2.3 of [6]. Unless specified otherwise, in a given scheduled cell, the UE is not expected to receive a first PDSCH and a second PDSCH, starting later than the first PDSCH, with its corresponding HARQ-ACK assigned to be transmitted on a resource ending before the start of a different resource for the HARQ-ACK assigned to be transmitted for the first PDSCH, where the two resources are in different slots for the associated HARQ-ACK transmissions, each slot is composed of symbols [4] or a number of symbols indicated by *subslotLengthForPUCCH* if provided, and the HARQ-ACK for the two PDSCHs are associated with the HARQ-ACK codebook of the same priority. Unless specified otherwise, in a given scheduled cell, the UE is not expected to receive a first PDSCH, and a second PDSCH, starting later than the first PDSCH, with its corresponding HARQ-ACK assigned to be transmitted on a resource ending before the start of a different resource for the HARQ-ACK assigned to be transmitted for the first PDSCH if the HARQ-ACK for the two PDSCHs are associated with HARQ-ACK codebooks of different priorities. For any two HARQ process IDs in a given scheduled cell, if the UE is scheduled to start receiving a first PDSCH starting in symbol *j* by a PDCCH ending in symbol *i*, the UE is not expected to be scheduled to receive a PDSCH starting earlier than the end of the first PDSCH with a PDCCH that ends later than symbol *i*. In a given scheduled cell, for any PDSCH corresponding to SI-RNTI, the UE is not expected to decode a re-transmission of an earlier PDSCH with a starting symbol less than *N* symbols after the last symbol of that PDSCH, where the value of *N* depends on the PDSCH subcarrier spacing configuration *μ,* with *N*=13 for *μ*=0, *N*=13 for *μ*=1, *N*=20 for *μ*=2, and *N*=24 for *μ*=3.

< Unchanged parts are omitted >

6.1 UE procedure for transmitting the physical uplink shared channel

PUSCH transmission(s) can be dynamically scheduled by an UL grant in a DCI, or the transmission can correspond to a configured grant Type 1 or Type 2. The configured grant Type 1 PUSCH transmission is semi-statically configured to operate upon the reception of higher layer parameter of *configuredGrantConfig* including *rrc-ConfiguredUplinkGrant* without the detection of an UL grant in a DCI. The configured grant Type 2 PUSCH transmission is semi-persistently scheduled by an UL grant in a valid activation DCI according to Clause 10.2 of [6, TS 38.213] after the reception of higher layer parameter *configuredGrantConfig* not including *rrc-ConfiguredUplinkGrant*. If *configuredGrantConfigToAddModList* is configured, more than one configured grant configuration of configured grant Type 1 and/or configured grant Type 2 may be active at the same time on an active BWP of a serving cell.

For the PUSCH transmission corresponding to a Type 1 configured grant or a Type 2 configured grant activated by DCI format 0\_0 or 0\_1, the parameters applied for the transmission are provided by *configuredGrantConfig* except for *dataScramblingIdentityPUSCH*, *txConfig*, *codebookSubset*, *maxRank*, *scaling* of *UCI-OnPUSCH,* which are provided by *pusch-Config*. For the PUSCH transmission corresponding to a Type 2 configured grant activated by DCI format 0\_2, the parameters applied for the transmission are provided by *configuredGrantConfig* except for *dataScramblingIdentityPUSCH*, *txConfig*, *codebookSubsetDCI-0-2*, *maxRankForDCI-Format0-2*, *scaling* of *UCI-OnPUSCH*, *resourceAllocationType1GranularityDCI-0* provided by *pusch-Config*.If the UE is provided with *transformPrecoder* in *configuredGrantConfig*, the UE applies the higher layer parameter *tp-pi2BPSK*, if provided in *pusch-Config*, according to the procedure described in Clause 6.1.4 for the PUSCH transmission corresponding to a configured grant.

For the PUSCH retransmission scheduled by a PDCCH with CRC scrambled by CS-RNTI with NDI=1, the parameters in *pusch-Config* are applied for the PUSCH transmission except for *p0-NominalWithoutGrant, p0-PUSCH-Alpha, powerControlLoopToUse,* *pathlossReferenceIndex* described in Clause 7.1 of [6, TS 38.213], *mcs-Table, mcs-TableTransformPrecoder* described in Clause 6.1.4.1 and *transformPrecoder* described in Clause 6.1.3.

For a UE configured with two uplinks in a serving cell, PUSCH retransmission for a TB on the serving cell is not expected to be on a different uplink than the uplink used for the PUSCH initial transmission of that TB.

A UE shall upon detection of a PDCCH with a configured DCI format 0\_0, 0\_1 or 0\_2 transmit the corresponding PUSCH as indicated by that DCI. Upon detection of a DCI format 0\_1 or 0\_2 with '*UL-SCH indicator*' set to '0' and with a non-zero '*CSI request*' where the associated *reportQuantity* in *CSI-ReportConfig* set to '*none*' for all CSI report(s) triggered by '*CSI request*' in this DCI format 0\_1 or 0\_2, the UE ignores all fields in this DCI except the '*CSI request*' and the UE shall not transmit the corresponding PUSCH as indicated by this DCI format 0\_1 or 0\_2. When the UE is scheduled with multiple PUSCHs by a DCI, HARQ process ID indicated by this DCI applies to the first PUSCH, as described in clause 6.1.2.1, HARQ process ID is then incremented by 1 for each subsequent PUSCH(s) in the scheduled order, with modulo 16 operation applied. For any HARQ process ID(s) in a given scheduled cell, the UE is not expected to transmit a PUSCH that overlaps in time with another PUSCH. Unless specified otherwise, for any two HARQ process IDs in a given scheduled cell, if the UE is scheduled to start a first PUSCH transmission starting in symbol *j* by a PDCCH ending in symbol *i*, the UE is not expected to be scheduled to transmit a PUSCH starting earlier than the end of the first PUSCH by a PDCCH that ends later than symbol *i*. The UE is not expected to be scheduled to transmit another PUSCH by DCI format 0\_0, 0\_1 or 0\_2 scrambled by C-RNTI or MCS-C-RNTI for a given HARQ process until after the end of the expected transmission of the last PUSCH for that HARQ process.

If a UE is configured by higher layer parameter *PDCCH-Config* that contains two different values of *coresetPoolIndex* in *ControlResourceSet* for the active BWP of a serving cell and PDCCHs that schedule two non-overlapping in time domain PUSCHs are associated to different *ControlResourceSets* having different values of *coresetPoolIndex,* for any two HARQ process IDs in a given scheduled cell, if the UE is scheduled to start a first PUSCH transmission starting in symbol *j* by a PDCCH associated with a value of *coresetPoolIndex* ending in symbol *i*, the UE can be scheduled to transmit a PUSCH starting earlier than the end of the first PUSCH by a PDCCH associated with a different value of *coresetPoolIndex* that ends later than symbol *i*.