**3GPP TSG RAN WG1#104bis-e R1-2nnnnnn**

**e-Meeting, April 12th – 20th, 2021**

**Agenda Item: 7.2.2**

**Source: Moderator (Lenovo)**

**Title: Email discussion/approval [104b-e-NR-NRU-01] on DL signals and channels**

**Document for: Discussion, Decision**

# Scope of Discussion

This document summarises the discussion on the following topics:

[104b-e-NR-NRU-01] Email discussion/approval on DL signals and channels until Apr-16 – Alex (Lenovo)

* DL-A1, DL-B3 (editorial), DL-D1

# Topic DL-A: PDCCH Monitoring

## Issue DL-A1 (R1-2102786): Maximum size of switchTriggerToAddModList-r16 and switchTriggerToReleaseList-r16

|  |
| --- |
| Background:  ***FL Note: Please refer to the detailed background given in R1-2102786.*** |
| Proposal:  **To align 38.213 and 38.331 with RAN1's original intention, request RAN2 to increase the maximum size of the lists switchTriggerToAddModList-r16 and switchTriggerToReleaseList-r16 to maxNrofAggregatedCellsPerCellGroup (i.e., max 16 instead of 4).** |

|  |  |
| --- | --- |
| Company | Comments |
|  |  |
|  |  |

# Topic DL-B: CSI Measurement, Report

## Issue DL-B3 (R1-2103335): CSI measurement across DL bursts

|  |
| --- |
| Background:  ***FL Note: Please refer to the detailed background given in R1-2103335.*** |
| Proposal:  **Adopt the following text proposal in TS 38.214 Clause 5.2.1.4.2.**   |  | | --- | | For operation with shared spectrum channel access, if the UE is configured with a *CSI-ReportConfig* with higher layer parameter *reportQuantity* set to 'cri-RI-PMI-CQI ', 'cri-RI-i1', 'cri-RI-i1-CQI', 'cri-RI-CQI' or 'cri-RI-LI-PMI-CQI', the UE shall derive:  - the CSI parameters without averaging two or more instances of any periodic or semi-persistent *nzp-CSI-RS-Resources* in the corresponding *NZP-CSI-RS-ResourceSet* for channel measurement or for interference measurement located in different DL transmissions,  - the instances of the *nzp-CSI-RS-Resources* are not in the same channel occupancy duration indicated by DCI format 2\_0, if the UE is provided at least one of *SlotFormatIndicator* or co*-DurationList*; or  - the instances of the *nzp-CSI-RS-Resources* occur within a set of consecutive symbols which are not all occupied by PDSCH(s) and/or aperiodic CSI-RS(s) indicated by DCI formats and, if any, the corresponding PDCCH(s), if the UE is neither provided with *CO-DurationPerCell* nor *SlotFormatIndicator*, but is provided with *csi-RS-ValidationWith-DCI*  - the interference measurements for computing CSI value based on periodic/semi-persistent CSI-IM measured only in OFDM symbol(s) that fulfill the same conditions under which the UE is expected to receive periodic/semi-persistent CSI-RS as described in Clause 11.1 and Clause 11.1.1 of [6, TS 38.213]. | |

|  |  |
| --- | --- |
| Company | Comments |
|  |  |
|  |  |

# Topic DL-D: Missing description of PDCCH features for shared spectrum in TS38.300

## Issue DL-D1 (R1-2102326): Missing description of PDCCH features for shared spectrum in TS38.300

|  |
| --- |
| Background:  The functionalities of physical downlink control channels (PDCCH) are described in section 5.2.3 of TS38.300. However, the new features introduced in NR-U Rel-16 were not reflected in the description, which results incompleteness of the specification. The missing features includes:   * Indicating Available RB set * Indicating COT duration * Trigger search space set group switching * Indicating CG-DFI indication * Triggering one-shot HARQ codebook feedback |
| Proposal:  ***Add description of PDCCH features introduced for shared spectrum operation in TS38.300.*** TP#4: in TS38.300 5.2.3 Physical downlink control channels  The Physical Downlink Control Channel (PDCCH) can be used to schedule DL transmissions on PDSCH and UL transmissions on PUSCH, where the Downlink Control Information (DCI) on PDCCH includes:  - Downlink assignments containing at least modulation and coding format, resource allocation, and hybrid-ARQ information related to DL-SCH;  - Uplink scheduling grants containing at least modulation and coding format, resource allocation, and hybrid-ARQ information related to UL-SCH.  In addition to scheduling, PDCCH can be used to for  - Activation and deactivation of configured PUSCH transmission with configured grant;  - Activation and deactivation of PDSCH semi-persistent transmission;  - Notifying one or more UEs of the slot format;  - Notifying one or more UEs of the PRB(s) and OFDM symbol(s) where the UE may assume no transmission is intended for the UE;  - Transmission of TPC commands for PUCCH and PUSCH;  - Transmission of one or more TPC commands for SRS transmissions by one or more UEs;  - Switching a UE's active bandwidth part;  - Initiating a random access procedure;  - Indicating the UE(s) to monitor the PDCCH during the next occurrence of the DRX on-duration;  - In IAB context, indicating the availability for soft symbols of an IAB-DU.  - Triggering one shot HARQ-ACK codebook feedback  - Notifying one or more UEs of the available RB sets, COT duration and search space set group switching for shared spectrum operation.  - Indicating downlink feedback information for configured grant PUSCH (CG-DFI) for shared spectrum operation  A UE monitors a set of PDCCH candidates in the configured monitoring occasions in one or more configured COntrol REsource SETs (CORESETs) according to the corresponding search space configurations.  A CORESET consists of a set of PRBs with a time duration of 1 to 3 OFDM symbols. The resource units Resource Element Groups (REGs) and Control Channel Elements (CCEs) are defined within a CORESET with each CCE consisting a set of REGs. Control channels are formed by aggregation of CCE. Different code rates for the control channels are realized by aggregating different number of CCE. Interleaved and non-interleaved CCE-to-REG mapping are supported in a CORESET.  Polar coding is used for PDCCH.  Each resource element group carrying PDCCH carries its own DMRS.  QPSK modulation is used for PDCCH. |

|  |  |
| --- | --- |
| Company | Comments |
|  |  |
|  |  |