**3GPP TSG RAN WG1 #104b-e R1-2103217**

**e-Meeting, April 12th – 20th, 2021**

**Agenda item:** 7.2.6

**Source:** Moderator (Samsung)

**Title:** Summary for Rel.16 NR eMIMO maintenance

**Document for:** Discussion and Decision

1. Introduction

The moderator summary of the maintenance-related issues raised in the submitted contributions for Rel.16 NR\_eMIMO maintenance is given below. The listed maintenance issues are under the usual designations:

* LP: low-PAPR RS
* MB: Multi-beam operation
* MT: Multi-TRP
* MU: Type-II enhancement for MU-CSI
* UL: UL full power transmission

An initial assessment on each of the issues is given (but can be revised based on the outcome of the discussion during the preparation week). The assessment will be used as a basis to select four issues (per chairman instruction) for further discussion in the upcoming weeks.

* *High priority (H):* this includes high-priority item (essential, pending issues, broken spec components) and proposed editorial changes that either enhance the clarity of the specs or correct mistakes
  + *H2:* The proposal can be endorsed without discussion (i.e. unless pointed out otherwise, the moderator will propose to the chair that the proposal be endorsed thereby not counted toward the four-thread quota). It can be merged with any of the assigned threads without any further discussion. This includes TPs associated with previous agreements.
* *Non-essential (N)*: this includes all other purposes such as spec optimization and low priority issues
* *Editorial (E)*: this includes editorial issues that will be handled as editorial CRs (to be communicated to the editors/chairs) and thereby not counted toward the four-thread quota

1. Maintenance issues

The issues are summarized in the following table:

**Table 1 Summary**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **#** | **Issue (summary)** | **Companies** | **Initial assessment** | **Company inputs (if any)** |
| MB.1 | RRC parameter misalignment in TS 38.213 and TS 38.214 with regards to *enableDefaultBeamPL-ForPUSCH0-0-r16*  FL: needed | CATT, Vivo | E |  |
| MB.2 | Fixing a typo in clause 7.2.1 of TS 38.213: ‘with with’ 🡪 ‘with’  FL: needed | CATT | E |  |
| MB.3 | Current TS38.213 could be misinterpreted that multi-CC simultaneous TCI update cannot be applied to CORESET#0 (i.e. p=0) because CORESET index p starts from 1 in the same paragraph (either 0<p<12 or 0<p<16). TP proposes to include p=0 for the multi-CC simultaneous TCI update to be aligned with the related MAC-CE description.    FL: discussed in pre-phase of last several meetings but not treated. Even though current text in TS38.213 does not explicitly preclude p=0, it is true that it could be implicitly precluded by the value range of p described in the same paragraph. | Vivo | H |  |
| MB.4 | 1. For multi-CC simultaneous TCI update, clarify which BWP’s tci-States-ToAddModList is applied to CORESET#0.  2. If TCI state of active BWP is applied for CORESET #0, conclude that UE does not expect to receive TCI state indication for CORESET #0 when the BWP(s) containing CORESET #0 is inactive.  FL: discussed in pre-phase of last meeting. According to TS38.321, it seems clear that the TCI list is from active BWP of the CC. Motivation of the second proposal is unclear. | Vivo | N |  |
| MB.5 | Paragraph indentation and wording modification (Proposal4 of R1-2102946)  FL: Paragraph indentation seems needed while wording modification seems not. | Vivo | E (only paragraph indentation) |  |
| MB.6 | Clarifying PL-RS selection for Type-2 CG-PUSCH based on one of the following interpretations:  •Interpretation 1: The PL-RS for Type-2 CG-PUSCH is always based on the one indicated by SRI in activating DCI  •Interpretation 2: The PL-RS for Type-2 CG-PUSCH is based on the lasted PL-RS associated with the SRI  FL: current spec seems support Interpretation 1 only as the MAC-CE is only for updating ‘mapping’ | Apple | N |  |
| MB.7 | Clarify that SSB cannot be used for BFD (R1-2102374)  FL: This was proposed multiple times and suggest at least a conclusion should be made. | OPPO | H |  |
| MB.8 | Clarify SCS for 28 symbols (R1-2102657, TP1/2)  FL: Although this was discussed in last meeting without any consensus, it is better to fix this issue with regard to potential ambiguity. | ZTE | H |  |
| MB.9 | Update CORESETPoolIndex to be 0 after BFR (R1-2102657, TP3)  FL: This was proposed multiple times and suggest at least a conclusion should be made. | ZTE | H |  |
| MB.10 | Add a condition (when spCell-BFR-CBRA is ‘true’) to apply new beam to PUCCH after CBRA based BFR (R1-2102946)  FL: This is based on RAN2’s agreement in last meeting. | vivo | E |  |
| MB.11 | Define BFD RS selection to avoid ambiguity of BFD RS counting for FG 16-1g (R1-2103084)  FL: There is a potential ambiguity for UE FG 16-1g counting if BFD RS selection rule is unclear. | Apple | H |  |
| MB.12 | Add time duration definition for CPU occupation for L1-SINR computation (R1-2103402)  FL: It seems the time duration definition for CPU occupation for L1-SINR is missing in current spec. | Huawei/HiSilicon | H |  |
|  | |  | | |
| MT.1 | R1-2102596 suggested that the title description of Table 5.1.2.1-2 is not proper for URLLC scheme 4 since scheme 4 uses “RepetitionNumber-r16” but the table title uses “*pdsch-AggregationFactor*”. Thus, it suggested to use a separate table for scheme 4.  FL: this was discussed in pre-phase in last meeting, some companies commented that the suggested change does not change the spec interpretation. | CATT | N |  |
| MT.2 | R1-2102596 explained that in current specification, out-of-order operation for PDSCH to HARQ-ACK can be supported only in slot-level granularity. R1-2102596 proposed to update the text to support out-of-order operation for PDSCH to TDMed HARQ-ACK within a slot.  FL: this has been proposed multiple times. Suggest to discuss to at least make an conclusion. | CATT | H |  |
| MT.3 | The issues of default TCI state:   * R1-2102658 proposed to extend the default TCI state mapping mechanism specified for TDMSchemeA to all the other single-DCI PDSCH transmission schemes. * R1-2102947 proposed to specify the mapping between default TCI states and frequency sources of scheme 2a/2b * R1-2102947 proposes to specify default TCI state for cross-carrier scheduling for mTRP. * R1-2103218 propose to specify the default TCI state of PDSCH of cross-carrier in S-DCI based mTRP. * R1-2103673 suggested to discuss the default TCI state of mTRP in cross-carrrier scheduling.   FL: That issue has been discussed multiple time in previous meetings but no conclusion. | ZTE, vivo, Samsung, ASUSTEK | N |  |
| MT.4 | R1-2102373 proposes to clarify in 38.214 that the UE does not expect to receive single-DCI mTRP TCI state activation MAC CE when multi-DCI mTRP is configured.  FL: it is a good clarification in 214. | OPPO | H |  |
| MT.5 | For multi-DCI based M-TRP transmission, UE needs to determine whether is larger than or not. But the description in 213 does not align with that. According to the description in current 213, reader would understand that the SCS configuration μ only corresponds to the active DL BWPs of the scheduling cells, and the deactivated cells (without active DL BWP) are not counted for the comparison. Proposal 2 in R1-2102373 provided TP to fix that.  FL: this is needed. It looks like the current text description in 213 change the UE behavior wrongly. | OPPO | H |  |
| MT.6 | R1-2102947 proposes TP to specify the case when PUCCH of CSI/SR/LRR does not overlap with two HARQ-ACK PUCCHs.  FL: this issue has been proposed by multiple times. We can discuss and make an conclusion | vivo | H |  |
| MT.7 | R1-2102947 proposes to conclude that UE does not expect to be scheduled a PDSCH overlapping with a PDCCH associated to CORESET having different CORESETPoolIndex from the scheduling PDCCH  FL: During pre-phase in last meeting, 9 companies thought it is H but 4 companies thought it is N. | vivo | H |  |
| MT.8 | The issue of radio link monitoring in mTRP:   * Apple (R1-2103085) proposed to enhance the method of UE determining RLM RS in M-DCI mTRP system by adding Lmax = 8.   FL: was proposed multiple time and suggest to discuss it at least for a conclusion | Apple | H |  |
| MT.9 | The issue of sub-slot HARQ vs m-DCI mTRP transmission.  R1-2103085 proposes to make conclusion on the following two issues:   * whether UE supports sub-slot based HARQ-ACK PUCCH when UE is configured with Multi-DCI based Multi-TRP operation. * whether UE supports two HARQ-ACK codebooks with different priorities when UE is configured with Multi-DCI based Multi-TRP operation   R1-2103433 suggests to limit the number of PUCCH transmission for m-DCI based mTRP HARQ when sub-slot PUCCH or two PUCCH configurations are configured with m-DCI mTRP transmission.  FL: The issue of m-DCI mTRP HARQ transmission vs sub-slot based HARQ is important. Suggest to discuss and make conclusion on that | Apple, Nokia | H |  |
| MT.10 | R1-2103145 proposes to reset the PDSCH beam to qnew during BFR in single-DCI based mTRP system  FL: This was proposed couple of times. Whether to reset the beam of PDSCH to qnew was discussed a lot in rel15/rel16 PCell and SCell. | Qualcomm | N |  |
| MT.11 | R1-2103145 proposes to specify the BD/CCE limit when NR-DC and multi-DCI mTRP are configured  FL: This was discussed in pre-phase in a few previous meetings. Some companies commented that it is not essential issue. We might discuss it and make a conclusion on that | Qualcomm | H |  |
| MT.12 | The issue of SPS PDSCH transmission in mTRP:   * R1-2103145 proposed to clarify that the RV sequence used across multiple repetitions in schemes 2b, 3, and 4 is based on setting rvid=0. * R1-2103218 proposed to Extend the single-DCI M-TRP dynamic grant PDSCH transmission schemes to include SPS PDSCH for enhanced PDSCH reliability for URLLC service types * R1-2103551 proposed CR to specify the RV values for DL DPSCH SPS in S-DCI mTRP   FL: it was discussed in pre-phase in previous meeting and some companies thought that is it is not essential to rel16 and maybe for later release. In last meeting, 4 companies support it as H but 5 companies suggested this is N | Qualcomm, Samsung, Ericsson | N |  |
| MT.13 | R1-2103218 proposes to Introduce a parameter X which can be corresponding to or can include a DCI decoding delay time for default TCI states of the single-DCI multi-TRP PDSCH repetition. UE applies the first TCI state to a receive symbols before decoding DCI. The value of X can be specified by one of the following candidates  FL: the threshold *timeDurationForQCL* already consider the DCI decoding latency. | Samsung | N |  |
| MT.14 | The issue of PT-RS in NC-JT:  R1-2103552 suggested that the current PT-RS power allocation for NC-JT does not take the muted RE into account when 2 PT-RS ports are configured. Thus, R1-2103552 proposes to update PT-RS power allocation in Table 4.1-2 of 38.214 v16.4.0 to reflect additional power boosting for NC-JT when 2 PT-RS ports are configured and also proposed a new table for 38.214.  FL: suggest to discuss it | Ericsson | H |  |
|  | | | | |
| UL.1 | ***ul-FullPwrMode2-TPMIGroup-r16***  Indicates the UE supported TPMI group(s) which delivers full power. The capability signalling comprises the following values:  - *twoPorts-r16* indicates a 2-bit bitmap  - *fourPortsNonCoherent-r16* indicates one of the TPMI groups {~~G~~g0-3}  - *fourPortsPartialCoherent-r16* indicates one of the TPMI groups (~~G~~g0-6)  UE indicates support of this feature shall also indicate support of *ul-FullPwrMode2-MaxSRS-ResInSet.*  NOTE 1: When a full coherent UE operates in mode 2, it reports TPMIs the same as a partial-coherent UE.  NOTE 2: For 4 port partial-coherent or full-coherent UE, UE can only report: 2-port {2-bit bitmap} or/and one of 4-port non-coherent {G0~G3} or/and one of 4-port partial-coherent {G0~G6}  For 4 port non-coherent UE, UE can only report: 2-port {2-bit bitmap} or/and one of 4-port non-coherent {G0~G3}  For 2 port UE, UE can report: 2-port {2-bit bitmap}}  NOTE 3: A UE that supports this feature must report at least one of the values.  FL: TP for 38.306, should be discussed in RAN2 and make necessary correction according the previous LS from RAN1 | Samsung | E (RAN2) |  |

1. Discussion and proposal

From the inputs shared by participating companies during the preparation phase, the following **observation** can be made:

* The following issues can be handled as E (a part of editorial CR):
* The following issues can be handled as H2 (editorial TPs that can be agreed without further email discussion, including capturing previous agreements)
* The following issues can be designated as H (requiring discussion and additional agreements/conclusions):

In light of the above observations, the moderator makes the following **proposals**:

* Continue discussion on 4 threads:
  + Thread 1 (moderator ...) Maintenance and TPs for Multi-beam 1: addressing
  + Thread 2 (moderator ...) Maintenance for Multi-TRP 1: addressing

# References

|  |  |  |  |
| --- | --- | --- | --- |
| 1 | R1-2102373 | Text proposals for M-TRP transmission | OPPO |
| 2 | R1-2102374 | Corrections for SCell BFR | OPPO |
| 3 | R1-2102595 | Maintenance of Multi-beam enhancement operation | CATT |
| 4 | R1-2102596 | Maintenance of Multi-TRP transmission | CATT |
| 5 | [R1-2102657](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_104b-e/Docs/R1-2102657.zip) | Maintenance of multi-beam operation | ZTE |
| 6 | [R1-2102658](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_104b-e/Docs/R1-2102658.zip) | Maintenance of Multi-TRP enhancements | ZTE |
| 7 | [R1-2102946](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_104b-e/Docs/R1-2102946.zip) | Maintenance on multi beam related issues | vivo |
| 8 | [R1-2102947](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_104b-e/Docs/R1-2102947.zip) | Maintenance on multi TRP | vivo |
| 9 | [R1-2103084](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_104b-e/Docs/R1-2103084.zip) | Remaining issues on Rel-16 beam management enhancement | Apple |
| 10 | [R1-2103085](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_104b-e/Docs/R1-2103085.zip) | Remaining issues on Rel-16 Multi-TRP enhancement | Apple |
| 11 | R1-2103145 | Remaining Issues on Multi-TRP Enhancements | Qualcomm Incorporated |
| 12 | R1-2103218 | On Rel.16 multi-TRP/panel transmission | Samsung |
| 13 | [R1-2103219](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_104b-e/Docs/R1-2103219.zip) | On UL full power transmission and multi-beam | Samsung |
| 14 | [R1-2103395](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_104b-e/Docs/R1-2103395.zip) | Corrections on the precoding for PUSCH | Huawei, HiSilicon |
| 15 | [R1-2103402](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_104b-e/Docs/R1-2103402.zip) | Correction on CPU occupation rules for L1-SINR reporting | Huawei, HiSilicon |
| 16 | [R1-2103433](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_104b-e/Docs/R1-2103433.zip) | Maintenance of Rel-16 Multi-TRP operation | Nokia, Nokia Shanghai Bell |
| 17 | R1-2103551 | Draft CR on DL SPS based PDSCH repetitions | Ericsson |
| 18 | R1-2103552 | Maintenance for single-DCI based multi-TRP in Rel-16 | Ericsson |
| 19 | R1-2103673 | Interoperation between cross-carrier scheduling and multiple TRPs | ASUSTEK COMPUTER (SHANGHAI) |