3GPP TSG-RAN WG1 Meeting #103b-e draft R1- 21NNNNN

e-Meeting, April 12th – 20th, 2021

**Source: Moderator (Ericsson)**

**Title: Output #1 for email discussion [104-be-NR-Pos-02]**

**Agenda item: 7.2.8**

**Document for: Discussion and Decision**

1. Introduction

This contribution documents the output of email discussion [104b-e-NR-Pos-02] triggered by the following Chairman’s decision and based on the feature lead summary for AI 7.2.8[TBD,[3]:

[104b-e-NR-Pos-02] Email discussion/approval on the following until Apr-16 – Florent (Ericsson)

* Aspect #3: Maintaining multiple pathloss estimates
* Aspect #4: Clarification on UE Rx-Tx time difference measurements
1. List of Remaining Opens on NR Positioning

## Aspect #3: Maintaining multiple pathloss estimates for SRS for positioning

### Feature Lead Summary

In [1], it is noticed that specification is not clear with respect to UE capability for support of simultaneous pathloss estimates per serving cell and across all serving cells. It is proposed to address the following points:

1. The fact that UE may not indicate the capability (“may” is added in front of “indicates”)
2. Maximum number of pathloss estimates per serving cell
3. UE behavior/capability for pathloss estimates across all cells

It is proposed to adopt the following text proposal for the pathloss estimates that the UE can simultaneously maintain for SRS-Pos in section 7.3.1 of 38.213:

|  |
| --- |
| Section 7.3.1 of 38.213*----------------------------------------Start of Text Proposal for 38.213-----------------------------------------*7.3.1 UE behaviour*-----------------------------------------------------* unrelated part omitted *--------------------------------* The UE may indicate a capability for up to sixteen pathloss estimates that the UE can simultaneously maintain for all SRS resource sets provided by *SRS-PosResourceSet* per serving cell in addition to the up to four pathloss estimates that the UE maintains per serving cell for PUSCH/PUCCH transmissions and for SRS transmissions configured by *SRS-Resource*.The UE may indicate a capability for up to sixteen pathloss estimates that the UE can simultaneously maintain for all SRS resource sets provided by *SRS-PosResourceSet* across all cells in addition to the up to four pathloss estimates that the UE maintains per serving cell for PUSCH/PUCCH transmissions and for SRS transmissions configured by *SRS-Resource*. *-------------------------------------------------------End of Text Proposal -------------------------------------------* |

### first round of comments

Companies are encouraged to provide their view on the TP in the table below

|  |  |
| --- | --- |
| Company | Comment |
| Huawei/HiSilicon | Not necessary for the whole TP.It is common in the specification that some UE features that are self-explanatory in TS 38.306 introduced by RAN1 do not necessarily have a full description RAN1 specs. |
| vivo | WE don’t see any confusion or misinterpretation on current specification wording and think no need to have this TP as that would duplicate from UE feature list. |
| QC | We are OK to change the “indicates” to “may indicate”, and generally the changes in the 1st paragraph. With regards to the 2nd paragraph, we also tend to believe that 38.306 seems to be good enough, but we are OK to capture it if there is majority view.From 38.306:*- maxNumberPathLossEstimatePerServing-r16 indicates the maximum number of pathloss estimates that the UE can simultaneously maintain for all the SRS resource sets for positioning per serving cell in addition to the up to four pathloss estimates that the UE maintains per serving cell for the PUSCH/PUCCH/SRS transmissios. The UE shall include this field if the UE supports any of olpc-SRS-PosBasedOnPRS-Serving-r16, olpc-SRS-PosBasedOnSSB-Neigh-r16 and olpc-SRS-PosBasedOnPRS-Neigh-r16. Otherwise, the UE does not include this field.* |
| Nokia/NSB | Same view as Huawei and vivo.  |
| ZTE | Similar view as QC. |

## Aspect #4: Clarification on UE Rx-Tx time difference measurements

### Feature Lead Summary

In [2], it is noticed that agreed UE capabilities are not correctly captured in current specification 38.214 for the following aspects:

* According to FG13-11a, it should be UE’s capability to support measurements derived on one or more DL PRS resource/resource sets which may be in different positioning frequency layers for SRS transmitted in a single CC. However, the current specification in TS 38.214 doesn’t mention that UE should report this capability, and all the measurements should correspond to SRS transmitted in a single CC.
* According to FG 13-11, the following aspects are not captured in the current specification, which may cause ambiguity to understand this FG.
* Different UE Rx–Tx time difference measurements are based on different DL PRS resources or DL PRS resource sets.
* Up to 4 UE Rx–Tx time difference measurements are based on DL PRS resources associated with the same TRP.
* Up to 4 UE Rx–Tx time difference measurements are based on DL PRS resources associated with the same positioning frequency layer.

To address above aspects, the following TP is provided in [4]:

|  |
| --- |
| clause 5.1.6.5 of TS 38.2145.1.6.5 PRS reception procedure===========================**Unchanged parts omitted** ============================The UE may be configured to measure and report, subject to UE capability, up to 4 DL RSTD measurements per pair of *dl-PRS-ID* with each measurement between a different pair of DL PRS resources or DL PRS resource sets within the DL PRS configured for those *dl-PRS-ID*. The up to 4 measurements being performed on the same pair of *dl-PRS-ID* and all DL RSTD measurements in the same report use a single reference timing. The UE may be configured to measure and report, subject to UE capability, up to 8 DL PRS-RSRP measurements on different DL PRS resources associated with the same *dl-PRS-ID*. When the UE reports DL PRS-RSRP measurements from one DL PRS resource set, the UE may indicate which DL PRS-RSRP measurements associated with the same higher layer parameter *nr-DL-PRS-RxBeamIndex* [17, TS 37.355] have been performed using the same spatial domain filter for reception if for each *nr-DL-PRS-RxBeamIndex* reported there are at least 2 DL PRS-RSRP measurements associated with it within the DL PRS resource set.The UE may be configured to measure and report, subject to UE capability, up to 4 UE Rx-Tx time difference measurements based on DL PRS resources associated with the same *dl-PRS-ID* and the same positioning frequency layer, and corresponding to a single configured SRS resource or resource set for positioning. Different measurements correspond to different received DL PRS resources or resource sets, which can be in different positioning frequency layers corresponding to SRS transmitted in a single carrier, subject to UE capability. ========================== **Unchanged parts omitted** ============================= |

### first round of comments

Companies are encouraged to provide their view on the TP in the table below

|  |  |
| --- | --- |
| Company | Comment |
| Huawei/HiSilicon | We see the value of clarifying that the 4 UE Rx – Tx time difference are from the same TRP on a positioning frequency layer. However, the second half needs some fine-tuning.Changes suggested below:The UE may be configured to measure and report, subject to UE capability, up to 4 UE Rx-Tx time difference measurements based on DL PRS resources associated with the same *dl-PRS-ID* and the same positioning frequency layer, and corresponding to a single configured SRS resource or resource set for positioning. The UE may be configured to measurement and report, subject to UE capability, UE Rx – Tx time difference measurements based on DL PRS resources or resource sets in different positioning frequency layers for SRS transmitted in a single CC. |
| vivo | We don’t see any critical or essential problem of existing specification wording. As we commented toward aspect#3, we prefer not to duplicate from UE feature list.On the suggested clarification w.r.t. the same PFL, our understanding on the word ‘can’ in “Each measurement corresponds to a single received DL PRS resource or resource set which can be in different positioning frequency layers” covers both same or different PFL.  |
| QC | OK with HW’s revision, with a minor change on top, as shown below with red:The UE may be configured to measure and report, subject to UE capability, up to 4 UE Rx-Tx time difference measurements based on DL PRS resources associated with the same *dl-PRS-ID* and the same positioning frequency layer, and corresponding to a single configured SRS resource or resource set for positioning. The UE may be configured to ~~measurement~~ measure and report, subject to UE capability, UE Rx – Tx time difference measurements based on DL PRS resources or resource sets in different positioning frequency layers for SRS transmitted in a single CC. |
| Nokia/NSB | We don’t really see how the change suggested by HW/QC above changes the spec. While we agree that the change, if accepted, makes the spec correct we also think it is correct now. Could a proponent explain how the current spec might be misinterpreted?  |
| ZTE | We can accept original TP or the TP revised by Huawei and QC. As we described in our tDoc, for your convenience, the justifications are listed and amended as below,* According to FG13-11a, it should be UE’s capability to support measurements derived on one or more DL PRS resource/resource sets which may be in different positioning frequency layers for SRS transmitted in a single CC. However, the current specification in TS 38.214 doesn’t mention that UE should report this capability, and all the measurements should correspond to SRS transmitted in a single CC.
* According to FG 13-11, the following aspects are not captured in the current specification, which may cause ambiguity to understand this FG.
* Different UE Rx–Tx time difference measurements are based on different DL PRS resources or DL PRS resource sets. For DL-RSTD and DL-AOD, it’s clearly stated in current specification that different measurements are based on different DL PRS resources or DL PRS resource sets, so it would be better to clarify this in Multi-RTT.Otherwise, it’s not clear what the meaning of this capability.
* Up to 4 UE Rx–Tx time difference measurements are based on DL PRS resources associated with the same TRP. The similar descriptions are also stated in current specification for DL-RSTD and DL-AOD,so it would be better to clarify this in Multi-RTT.Otherwise, it’s not clear what the meaning of this capability.
* Up to 4 UE Rx–Tx time difference measurements are based on DL PRS resources associated with the same positioning frequency layer. The note in FG13-11 should be captured to avoid ambiguity.
 |

# Conclusion

TBD

1. References
2. [R1-2102597](file:///C%3A%5C%5CUsers%5C%5Cwanshic%5C%5COneDrive%20-%20Qualcomm%5C%5CDocuments%5C%5CStandards%5C%5C3GPP%20Standards%5C%5CMeeting%20Documents%5C%5CTSGR1_104b%5C%5CDocs%5C%5CR1-2102597.zip) Discussion and TP on remaining issues in NR positioning CATT
3. [R1-2102659](file:///C%3A%5C%5CUsers%5C%5Cwanshic%5C%5COneDrive%20-%20Qualcomm%5C%5CDocuments%5C%5CStandards%5C%5C3GPP%20Standards%5C%5CMeeting%20Documents%5C%5CTSGR1_104b%5C%5CDocs%5C%5CR1-2102659.zip) Maintenance of NR positioning support ZTE
4. R1-210zzzz Feature Leads Summary for NR Positioning Maintenance – AI 7.2.8