**3GPP TSG RAN WG1 #106-e R1-210xxxx**

**e-Meeting, August 16th – 27th, 2021**

**Agenda item:** 8.1.1

**Source:** Moderator (Samsung)

**Title:** Moderator summary#6 for multi-beam enhancement: ROUND 5

**Document for:** Discussion and Decision

## Introduction

In this summary, the term “item 1” refers to the first item in the Rel.17 NR FeMIMO WID, i.e. multi-beam enhancement:

|  |
| --- |
| 1. Enhancement on multi-beam operation, mainly targeting FR2 while also applicable to FR1:    1. Identify and specify features to facilitate more efficient (lower latency and overhead) DL/UL beam management for intra-cell and inter-cell scenarios to support higher UE speed and/or a larger number of configured TCI states:       1. Common beam for data and control transmission/reception for DL and UL, especially for intra-band CA       2. Unified TCI framework for DL and UL beam indication       3. Enhancement on signaling mechanisms for the above features to improve latency and efficiency with more usage of dynamic control signaling (as opposed to RRC)       4. For inter-cell beam management, a UE can transmit to or receive from only a single cell (i.e. serving cell does not change when beam selection is done). This includes L1-only measurement/reporting (i.e. no L3 impact) and beam indication associated with cell(s) with any Physical Cell ID(s)          1. The beam indication is based on Rel-17 unified TCI framework          2. The same beam measurement/reporting mechanism will be reused for inter-cell mTRP          3. This work shall only consider intra-DU and intra-frequency cases    2. Identify and specify features to facilitate UL beam selection for UEs equipped with multiple panels, considering UL coverage loss mitigation due to MPE, based on UL beam indication with the unified TCI framework for UL fast panel selection |

This summary includes the following:

* Observation and proposal
* Summary of current companies’ positions on each of the aspects within the category

## Summary of companies’ inputs

The listed issues are structured primarily to facilitate some progress on pending issues identified in the agreements (see Appendix A).

### Issue 1 (Rel.17 unified TCI framework – note: for intra-cell beam management)

(no more for this meeting)

### Issue 2 (inter-cell beam management)

**Proposal 2.E**: On Rel.17 L1-RSRP multi-beam measurement/reporting enhancements for inter-cell beam management and inter-cell mTRP, select NMAX (the maximum number of RRC configured TRP(s) with different PCIs from the serving cell for measurement/reporting) from the following alternatives (to be decided in RAN1#106bis-e):

* Alt1: NMAX is up to UE capability with candidate values of 1 and X.
  + Note: X as agreed in AI 8.1.2.2
  + When NMAX is configured to be X, the UE measures up to X PCIs different from the serving cell PCI
* Alt2. NMAX  = 1

Table 1 Additional inputs: FL proposal

|  |  |
| --- | --- |
| **Company** | **Input** |
| Mod V0 | **1) Share your inputs on the above FL proposal** |
|  |  |
|  |  |
|  |  |

### Issue 3 (beam indication signaling medium)

(no more for this meeting)

### Issue 4 (MP-UE)

Table 2 Summary: issue 4

|  |  |
| --- | --- |
| Proposal 4.A V2 | **Support/ok**: LG, Sony, Samsung, Lenovo/MotM, Qualcomm, Apple, MTK, ZTE, IDC, LG, CMCC, vivo, NTT Docomo, Spreadtrum, Xiaomi, Fraunhofer IIS/HHI  **Concern**: Ericsson, OPPO, CATT, Nokia/NSB |
| Proposal 4.A V3 (proposed by Ericsson during GTW) | **Support/ok**:  **Concern**: |

**Proposal 4.A V2**: On Rel.17 enhancements to facilitate UE-initiated panel activation and selection:

* A panel entity corresponds to a reported CSI-RS and/or SSB resource index in a beam reporting instance (i.e. Opt1-1 per RAN1#104-bis-e agreement)
  + The correspondence between a panel entity and a reported CSI-RS and/or SSB resource index is informed to NW
    - FFS: Detailed design of how to inform the correspondence to NW
  + Note: the correspondence between a CSI-RS and/or SSB resource index and a panel entity is determined by the UE (analogous to Rel-15/16)
* Support UE reports maximum number of SRS ports for each panel entity
* Support multiple codebook-based SRS resource sets with different maximum number of UL MIMO layers
  + The indicated SRI is based on the SRS resources corresponding to one SRS resource set, where the SRS resource set should be aligned with the UE capability for the panel entity

**OR**

**Proposal 4.A V3**: On Rel.17 enhancements to facilitate UE-initiated panel activation and selection:

* Include in the CSI report, the maximum number of supported number of SRS antenna ports corresponding to the reported SSBRI/CRI
* Support multiple codebook-based SRS resource sets with different maximum number of UL MIMO layers
  + The indicated SRI is based on the SRS resources corresponding to one SRS resource set, where the SRS resource set should be aligned with the UE capability for the panel entity

Table 3 Additional inputs: issue 4

|  |  |
| --- | --- |
| **Company** | **Input** |
| Mod V0 | **1) Check and update Table 2 based on the two alternative proposals (4.A V2 vs 4.A V3).**  **2) Summarize your concern, if any, on a proposal you are against** |
|  |  |
|  |  |

### Issue 5 (MPE mitigation)

(no more for this meeting)

### Issue 6 (advanced beam refinement/tracking)

**Proposal 6.A**: On Rel-17 enhancements to facilitate advanced beam refinement/tracking, in Rel-17, further focus study (including down-selection) and, if needed, specification effort on Opt 1-A as agreed in RAN1#105-e (UE-initiated beam selection/activation based on beam measurement and/or reporting, without beam indication or activation from NW) comprising:

* UE-initiated (DL-only or DL/UL) beam selection, including the following options
  + Opt1. The selected beam is reported by an event-triggered UE beam reporting via, e.g. UCI, MAC CE, PRACH, UL CG, or CBRA/CFRA
  + Opt2. The selected beam is reported by a legacy UE beam report (NW-configured)
  + FFS on NW-indication of a beam group in which the UE is allowed to do the beam selection, e.g., the NW-indication via MAC-CE
* UE-initiated beam activation based on beam reporting
  + The reported beam(s) are activated as active TCI/spatial relation RS(s) automatically w/o NW activation command after receiving gNB response signaling
  + FFS: The reported beam is applied directly if the number of supported activated beam by the UE is one and/or after receiving gNB response signaling
* UE-initiated UL-only beam selection
  + The UE can select an alternative beam from the other beams in the gNB-configured set containing more than one UL beam

Table 4 Summary: issue 6

|  |  |
| --- | --- |
| Proposal 6.A | **Support/ok**: ZTE, Qualcomm, Samsung, Apple, IDC, LG, NTT Docomo, CATT, MTK,  **Concern**: Ericsson |

Table 5 Additional inputs: issue 6

|  |  |
| --- | --- |
| **Company** | **Input** |
| Mod V0 | **1) Update table 4 if needed**  **2) Please share your inputs, if any, on proposal 6.A** |
|  |  |
|  |  |
|  |  |
|  |  |

# References

|  |  |  |  |
| --- | --- | --- | --- |
| 1 | R1-2106864 | Summary of offline discussion on unified TCI and inter-cell beam management | Moderator (Samsung) |
| 2 | R1-2106463 | Enhancements on multi-beam operation in Rel-17 | Huawei, HiSilicon |
| 3 | R1-2106541 | Enhancements on Multi-beam Operation | ZTE |
| 4 | R1-2106571 | Further discussion on multi beam enhancement | vivo |
| 5 | R1-2106640 | Remaining Details on Enhancements for Multi-beam Operation | IDC, Inc. |
| 6 | R1-2106666 | Enhancements on Multi-beam Operation | Lenovo, Motorola Mobility |
| 7 | R1-2106685 | Enhancements on Multi-beam Operation | Spreadtrum Communications |
| 8 | R1-2106789 | Further enhancement on multi-beam operation | Sony |
| 9 | R1-2106864 | Moderator summary for multi-beam enhancement | Moderator (Samsung) |
| 10 | R1-2106865 | Multi-Beam Enhancements | Samsung |
| 11 | R1-2106935 | Discussions on enhancements on multi-beam operation | CATT |
| 12 | R1-2107029 | Enhancements on Multi-beam Operation | Fujitsu |
| 13 | R1-2107085 | Enhancement on multi-beam operation | FUTUREWEI |
| 14 | R1-2107143 | Discussion on multi-beam operation | NEC |
| 15 | R1-2107203 | Enhancements on Multi-beam Operation | OPPO |
| 16 | R1-2107297 | Discussion of enhancements on multi-beam operation | FGI, Asia Pacific Telecom |
| 17 | R1-2107323 | Enhancements on Multi-beam Operation | Qualcomm Incorporated |
| 18 | R1-2107390 | Enhancements on multi-beam operation | CMCC |
| 19 | R1-2107464 | Enhancements on multi-beam operation | Fraunhofer IIS, Fraunhofer HHI |
| 20 | R1-2107485 | Enhancement on multi-beam operation | MTK Inc. |
| 21 | R1-2107570 | Enhancements to Multi-Beam Operations | Intel Corporation |
| 22 | R1-2107628 | Enhancements on Multi-beam Operation | Ericsson |
| 23 | R1-2107689 | Enhancements on Multi-beam operations | AT&T |
| 24 | R1-2107718 | Views on Rel-17 Beam Management enhancement | Apple |
| 25 | R1-2107814 | Enhancements on Multi-beam Operation | LG Electronics |
| 26 | R1-2107838 | Discussion on multi-beam operation | NTT DOCOMO, INC. |
| 27 | R1-2107893 | Enhancements on multi-beam operation | Xiaomi |
| 28 | R1-2108019 | Enhancements on Multi-beam Operation | Convida Wireless |
| 29 | R1-2108052 | Enhancements on Multi-beam Operation | Nokia, Nokia Shanghai Bell |
| 30 | R1-2106548 | Further details on Multi-beam and Multi-TRP operation | ZTE |
| 31 | R1-2106671 | HARQ feedback of SPS PDSCH reception in multi-DCI based multiple TRPs | Lenovo, Motorola Mobility |
| 32 | R1-2106872 | Additional enhancements for multi-beam | Samsung |
| 33 | R1-2107210 | Discussion on further enhancements for multi-beam operation | OPPO |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |