**3GPP TSG RAN WG1 #108-e R1-22xxxxx**

**e-Meeting, February 21 – March 3, 2022**

**Title:** Draft LS on use of CQI table for NB-IoT DL 16QAM

**Response to:**

**Release:** Rel-17

**Work Item:** NB\_IOTenh4\_LTE\_eMTC6-Core

**Source:** RAN1

**To:** RAN2

**CC:**

**Contact Person:**

**Name:**  Yubo Yang

**E-mail Address:** yangyubo1@huawei.com

**1. Overall Description:**

RAN1 has discussed the use of CQI table for downlink 16QAM and has achieved the following agreements:

|  |
| --- |
| Agreement* When 16QAM is configured, the new CQI table is used.

Note: There’s no consensus in RAN1 on the use of legacy CQI table when 16-QAM is configured   |

**2. Actions:**

**To RAN2**

**ACTION:**

RAN1 would like to respectfully request RAN2 to take the above information into account in the future work.

**3. Date of Next TSG-RAN WG1 Meetings:**

TSG-RAN WG1 Meeting #108-e 21st Feb. – 3rd Mar. 2022 e-Meeting

TSG-RAN WG1 Meeting #109-e 16th May – 27th May 2022 e-Meeting