**3GPP TSG-RAN WG1 Meeting #112bR1-23xxxxx**

**e-meeting, April May 17 – 26, 2023**

|  |
| --- |
| *CR-Form-v12.2* |
| **DRAFT CHANGE REQUEST** |
|  |
|  | **38.211** | **CR** | **xxxx** | **rev** | **-** | **Current version:** | **17.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Introduction of additional PRS configurations [1symbol\_PRS] |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** | TEI18 |  | ***Date:*** | 2023-03-23 |
|  |  |  |  |  |
| ***Category:*** | B |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Additional PRS configurations agreed for Rel-18 |
|  |  |
| ***Summary of change:*** | Adding PRS configurations |
|  |  |
| ***Consequences if not approved:*** | No support for the new PRS configurations |
|  |  |
| ***Clauses affected:*** | 7.4.1.7.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

##### 7.4.1.7.3 Mapping to physical resources in a downlink PRS resource

For each downlink PRS resource configured, the UE shall assume the sequence  is scaled with a factor and mapped to resources elements according to

when the following conditions are fulfilled:

- the resource element is within the resource blocks occupied by the downlink PRS resource for which the UE is configured;

- the symbol is not used by any SS/PBCH block used by a serving cell for downlink PRS transmitted from the same serving cell or any SS/PBCH block from a non-serving cell whose time frequency location is provided to the UE by higher layers for downlink PRS transmitted from the same non-serving cell;

- the slot number satisfies the conditions in clause 7.4.1.7.4.

and where

- the antenna port

- is the first symbol of the downlink PRS within a slot and given by the higher-layer parameter *dl-PRS-ResourceSymbolOffset*;

- the size of the downlink PRS resource in the time domain is given by the higher-layer parameter *dl-PRS-NumSymbols*;

- the comb size is given by the higher-layer parameter *dl-PRS-CombSizeN-AndReOffset* for a downlink PRS resource configured for RTT-based propagation delay compensation, otherwise by the higher-layer parameter *dl-PRS-CombSizeN* such that the combination is one of {1, 2}, {2, 2},{4, 2}, {6, 2}, {12, 2}, {1, 4}, {4, 4}, {12, 4}, {1, 6}, {6, 6}, {12, 6}, {1, 12} and {12, 12}*;*

- the resource-element offset is obtained from the higher-layer parameter *dl-PRS-CombSizeN-AndReOffset*;

- the quantity is given by Table 7.4.1.7.3-1.

If the downlink PRS resource is configured for RTT based propagation delay compensation as described in clause 9 of [6, TS 38.214], the reference point for is subcarrier 0 in common resource block 0; Otherwise, the reference point for is the location of the point A of the positioning frequency layer, in which the downlink PRS resource is configured where point A is given by the higher-layer parameter *dl-PRS-PointA*.

Table 7.4.1.7.3-1: The frequency offset as a function of .

|  |  |
| --- | --- |
|  | Symbol number within the downlink PRS resource  |
| 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 |
| 2 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| 4 | 0 | 2 | 1 | 3 | 0 | 2 | 1 | 3 | 0 | 2 | 1 | 3 |
| 6 | 0 | 3 | 1 | 4 | 2 | 5 | 0 | 3 | 1 | 4 | 2 | 5 |
| 12 | 0 | 6 | 3 | 9 | 1 | 7 | 4 | 10 | 2 | 8 | 5 | 11 |