# RAN1 AGREEMENTS with MAC-CE IMPACT FOR SUB-AGENDA 9.2.1

#### **RAN1 Meeting #116**

N/A

#### **RAN1 Meeting #116-bis**

N/A

#### **RAN1 Meeting #117**

N/A

# RAN1 AGREEMENTS with MAC-CE IMPACT FOR SUB-AGENDA 9.2.2

#### **RAN1 Meeting #116**

N/A

#### **RAN1 Meeting #116-bis**

N/A

#### **RAN1 Meeting #117**

N/A

# RAN1 AGREEMENTS with MAC-CE IMPACT FOR SUB-AGENDA 9.2.3

#### **RAN1 Meeting #116**

N/A

#### **RAN1 Meeting #116-bis**

N/A

#### **RAN1 Meeting #117**

N/A

# RAN1 AGREEMENTS with MAC-CE IMPACT FOR SUB-AGENDA 9.2.4

#### **RAN1 Meeting #116**

N/A

#### **RAN1 Meeting #116-bis**

N/A

#### **RAN1 Meeting #117**

**Agreement**

For the association between PL offset and joint/UL TCI state, support the following

* Alt1b: One PL offset value is configured in a joint or UL TCI state by RRC, where different PL offset values can be configured to different joint or UL TCI states. A MAC CE can update the PL offset value(s) for joint or UL TCI state(s).

**“MAC-CE impact: MAC-CE updates the PL offset value(s) configured in one or more joint TCI states or UL TCI states”**