23GPP TSG-RAN WG2 Meeting #109bis-e R2-2004001

**Electronic, 20 April – 30 April 2020**

Agenda Item:

Source: Session chair (CMCC)

Title: Proposals for approval

Document for: Approval

Based on the progress of [801] Open issues on MDT, the session chair would like to propose to agree the following proposals:

Proposal 1: mobilityState field in included only when the serving cell broadcasts speedStateReselectionPars in SIB2.

Proposal 2: For capturing the measurement quantities included in the logged MDT, re-use the existing IE MeasQuantityResults and if required, add a text in the field description of the IE MeasQuantityResults, e.g. sinr is not included when it is used for MDT.

Proposal 3: Change the wording from

“When the UE resumes the RRC connection in one new NG-RAN, the last serving NG-RAN can propagate the logged MDT configuration to the new NG-RAN.”

To:

 ”When the UE resumes the RRC connection in one new NG-RAN, the new NG-RAN can configure the MDT configuration for the UE, only if the signalling based logged MDT was received by the new NG-RAN from the previous NG-RAN or AMF. It is not required to propagate the management based logged MDT configuration.”

Companies are invited to show opinion on the above agreements. Only add your company name into the table if and only you don’t agree with the proposals.

|  |  |
| --- | --- |
|  | Company name who objects the proposal |
| P1 |  |
| P2 |  |
| P3 |  |