**3GPP TSG-RAN WG2 Meeting #110-e DRAFT R2-2005811**

**Online, 01 – 11 June 2020**

**Title: [DRAFT]** LS on Detail MIMO MAC CE operations

**Response to:** -

**Release:** Release 16

**Work Item:** NR\_eMIMO-Core

**Source:** Samsung [TSG RAN WG2]

**To:** RAN1

**Cc:** -

**Contact Person:**

#### Name: Seungri Jin

E-mail Address: seungri.jin@samsung.com

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**Attachments:** -

**1. Overall Description:**

**1) Issue 1: Restrictions on DCI format 1\_2**

According to RAN1 LS (R2-2006057\_ R1-2004808), RAN1 provided the answers for the RAN2’s questions regarding the applicability of DCI format 1\_2 for NR eMIMO features as below.

|  |
| --- |
| **5)** **DCI format 1\_2 applicability to features introduced in NR\_eMIMO WI**  The IE ControlResourceSet includes both tci-PresentInDCI and tci-PresentInDCI-ForDCI-Format1-2. Currently both parameters can be configured in all or some CORESETs of the UE and these CORESETs may be configured with CORESETPoolIndex (mPDCCH mTRP). Further, eMIMO WI introduced a new TCI state mapping MAC CE in TS 38.321 6.1.3.24 where two TCI states can be mapped to one DCI codepoint. Currently, there is no limitation which DCI format this new MAC CE in TS 38.321 6.1.3.24 applies to.  **Q5-1)** Can the UE be configured with both DCI format 1\_1 and DCI format 1\_2 with TCI field, either in the same or different CORESETs? And can the value of tci-PresentInDCI-ForDCI-Format1-2 be different in different CORESETs?  **[Answer]: Yes to both questions.**  **Q5-2)** Can the UE be configured with mPDCCH mTRP (have at least on CORESET with CORESETPoolIndex=1) and the parameter tci-PresentInDCI-ForDCI-Format1-2?  **[Answer]: Yes.**  **Q5-3)** Does the Enhanced TCI state MAC CE in TS 38.321 6.1.3.24 apply to DCI1\_2?  **[Answer]: Yes.** |

RAN2 understand that both DCI format 1\_1 and DCI format 1\_2 can be configured and used at the same CORESET. However, RAN2 think that handling/mapping of codepoints for activated TCI states which are indicated by MAC CE (i.e. TCI State Indication for UE-specific PDCCH MAC CE or Enhanced TCI States Activation/Deactivation for UE-specific PDSCH MAC CE) to DCI format 1\_2 is not clear when the number of codepoints in the TCI field of DCI format 1\_2 is less than the maximum number of codepoints in the TCI field of DCI format 1\_1.

RAN2 believes that some restrictions on TCI states codepoints mapping when the number of codepoints in the TCI field of DCI format 1\_2 is less than the maximum number of codepoints in the TCI field of DCI format 1\_1 can be clarified in RAN1 specifications.

**Question 1:** Could RAN1 specify the restrictions on TCI states codepoints mapping when the number of codepoints in the TCI field of DCI format 1\_2 is less than the maximum number of codepoints in the TCI field of DCI format 1\_1 can be clarified in RAN1 specifications?

**2) Issue 2: Functionality of Serving cell set based SRS spatial relation indication MAC CE**

According to RAN1 LS (R2-2004251\_R1-2002798), RAN1 provided the answers for the RAN2’s questions regarding the functionality of Serving cell set based SRS spatial relation indication MAC CE as below.

|  |
| --- |
| **Question 4.** RAN2 would like to ask RAN1 whether the intention is to activate per SRS resource set or per SRS resource. Further, if per SRS resource, whether RAN1 sees any issues in indicating spatial relation, potentially different, for more than one resource in one MAC CE in order to save overhead.  **Answer 4.**  RAN1 understands that the intention of the agreement is to support activating the independent spatial relations for SRS resource(s) in an SRS resource set.  Furthermore, RAN1 see no issue in using one MAC CE (to save overhead) to activate/deactivate spatial relations for >1 SRS resources from an SRS resource set. |

RAN2 confused whether this MAC CE should support activate/deactivate SRS transmission or this MAC CE only indicates the SRS spatial relations which are applied for all configured serving cell set (i.e. setting which spatial relation is used for SRS without affecting whether the SRS is transmitted). RAN2 understanding is that the intended functionality of this MAC CE is to indicate the SRS spatial relations which are applied for all configured serving cell set. RAN2 determined not to add A/D field in this MAC CE based on this understanding.

**Question 2:** Is it correct understanding that the intended functionality of the Serving cell set based SRS spatial relation indication MAC CE is to indicate the SRS spatial relations which are applied for all configured serving cell set?

In addition, RAN2 want to know whether the functionality of this MAC CE can be applied to SUL carrier as well. RAN2 assumed this MAC CE is also used to indicate the SRS spatial relations in SUL configuration because RAN1 didn’t provide the need of the restrictions in case of SUL configuration.

**Question 3:** Is it correct understanding that the Serving cell set based SRS spatial relation indication MAC CE can be used to indicate the SRS spatial relations in SUL configuration?

**2. Actions:**

**To RAN1.**

**ACTION:** RAN2 respectfully asks RAN1 to answer the above questions.

**3. Date of Next TSG-RAN WG2 Meetings:**

3GPP RAN2#111 24 – 28 August 2020 eMeeting