**3GPP T****SG-RAN WG2 Meeting #111-e R2-200xxxx**

**Electronic Meeting, 17th – 28th August 2020**

**Agenda item: 6.1.3**

**Source: vivo**

**Title: Report of [AT111-e][023][NR16]** **NG-ENDC capability (vivo)**

**Document for: Discussion and Decision**

# 1 Introduction

This contribution is to report the discussion and the result of the following offline discussion in RAN2#111-e Meeting [1]:

* [AT111-e][023][NR16] NG-ENDC capability (vivo)

Scope: Treat R2-2008080, R2-2008081, R2-2008082

Deadline: Short UE cap

# 2 Discussion

In the last RAN2 meeting, whether the reported UE capabilities related to L1/L2 features for EN-DC can be also re-used for the case of NGEN-DC had been warmly discussed. In the end, it was agreed to clarify the support of NGEN-DC for UE capabilities [2].

The following contributions were submitted to clarify the support of NGEN-DC for the newly added Rel-16 LTE/NR UE capabilities and two specific Rel-15 UE capabilities (i.e. *v2x-EUTRA* and *pdcp-DuplicationSRB*) that were not discussed in the previous offline discussion.

R2-2008080 Clarification on the extended capability of NGEN-DC vivo CR Rel-16 36.306 16.1.0 1784 - F NR\_newRAT-Core

R2-2008081 Clarification on the extended capability of NGEN-DC vivo CR Rel-16 38.306 16.1.0 0402 - F NR\_newRAT-Core

R2-2008082 Clarification on the extended capability of NGEN-DC vivo CR Rel-15 38.306 15.10.0 0403 - F NR\_newRAT-Core

## 2.1 Rel-16 LTE clarification on the support of NGEN-DC

The capability *nr-HO-ToEN-DC-r16* was introduced in Rel-16. To clarify that this capability can be also re-used for the NGEN-DC scenario, the 36.306 CR in R2-2008080 [3] proposes the following revision to the description of *nr-HO-ToEN-DC-r16*.

|  |
| --- |
| *nr-HO-ToEN-DC-r16*  This field indicates whether the UE supports inter-RAT handover from NR to (NG)EN-DC while NR-DC or NE-DC is not configured as defined in TS 37.340 [38]. It is mandatory to support inter-RAT handover from NR to (NG)EN-DC if the UE supports (NG-RAN) E-UTRA NR Dual Connectivity. |

**Question 1: Do companies agree to capture the proposed clarification for NGED-DC in the description of *nr-HO-ToEN-DC-r16*?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments, if any** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.2 Rel-16 NR clarification on the support of NGEN-DC

Same as the motivation described in section 2.1, the 38.306 CR in R2-2008081 [4] proposes to clarify the description of the following capabilities:

* *ULTxSwitchingBandPair-r16*
* *uplinkTxSwitching-OptionSupport-r16*
* *handoverInterF*
* *nr-HO-ToEN-DC-r16*
* *measurementEnhancement-r16*
* *demodulationEnhancement-r16*

The corresponding changes are given below:

***BandCombinationList* parameters:**

| **Definitions for parameters** | **Per** | **M** | **FDD-TDD**  **DIFF** | **FR1-FR2**  **DIFF** |
| --- | --- | --- | --- | --- |
| ***ULTxSwitchingBandPair-r16***  Indicates UE supports dynamic UL Tx switching in case of inter-band CA, SUL, and (NG)EN-DC as defined in TS 38.214 [12], TS 38.101-1 [2] and TS 38.101-3 [4]. The capability signalling comprises of the following parameters:  - *bandIndexUL1-r16* and *bandIndexUL2-r16* indicate the band pair on which UE supports dynamic UL Tx switching. *bandindexUL1*/*bandindexUL2* xx refers to the xxth band entry in the band combination. UE shall indicate support for 2-layer UL MIMO capabilities at least on one of the indicated two bands for UL Tx switching, and only the band where UE supports 2-layer UL MIMO capability can work as carrier2 as defined in TS 38.101-1 [2] and TS 38.101-3 [4].  - *uplinkTxSwitchingPeriod-r16* indicates the length of UL Tx switching period per pair of UL bands per band combination when dynamic UL Tx switching is configured, as specified in TS 38.101-1 [2] and TS 38.101-3 [4]. UE shall not report the value n210us for EN-DC band combinations. n35us represents 35 us, n140us represents 140us, and so on, as specified in TS 38.101-1 [2] and TS 38.101-3 [4].  - *uplinkTxSwitching-DL-Interruption-r16* indicates that DL interruption on the band will occur during UL Tx switching, as specified in TS 38.133 [5] and in TS 36.133 [27]. UE is not allowed to set this field for the band combination of SUL band+TDD band, for which no DL interruption is allowed.  Field encoded as a bit map, where bit N is set to "1" if DL interruption on band N will occur during uplink Tx switching as specified in TS 38.133 [5] and in TS 36.133 [27]. The leading / leftmost bit (bit 0) corresponds to the first band of this band combination, the next bit corresponds to the second band of this band combination and so on. The capability is not applicable to the following band combinations, in which DL reception interruption is not allowed:  - TDD+TDD CA with the same UL-DL pattern  - TDD+TDD EN-DC with the same UL-DL pattern | BC | FD | N/A | FR1 only |
| ***uplinkTxSwitching-OptionSupport-r16***  Indicates which option is supported for dynamic UL Tx switching for inter-band UL CA and (NG)EN-DC. *switchedUL* represents option 1 as specified in TS 38.214 [12], *dualUL* represents option 2 as specified in TS 38.214 [12], *both* represents both option 1 and option2 as specified in TS 38.214 [12]. UE shall not report the value *both* for (NG)EN-DC case. The field is mandatory for inter-band UL CA and (NG)EN-DC case where UE supports dynamic UL Tx switching. | BC | CY | N/A | FR1 only |

***MeasAndMobParameters*:**

| **Definitions for parameters** | **Per** | **M** | **FDD-TDD DIFF** | **FR1-FR2 DIFF** |
| --- | --- | --- | --- | --- |
| ***handoverInterF***  Indicates whether the UE supports inter-frequency HO. It indicates the support for inter-frequency HO from the corresponding duplex mode if this capability is included in *fdd-Add-UE-NR-Capabilities* or *tdd-Add-UE-NR-Capabilities*. It indicates the support for inter-frequency HO from the corresponding frequency range if this capability is included in *fr1-Add-UE-NR-Capabilities* or *fr2-Add-UE-NR-Capabilities*. This field only applies to NR SA/NR-DC/NE-DC (e.g. PCell handover). For PSCell change when (NG)EN-DC/NR-DC is configured, this feature is mandatory supported. | UE | Yes | Yes | Yes |

**Inter-RAT parameters:**

| **Definitions for parameters** | **Per** | **M** | **FDD-TDD DIFF** |
| --- | --- | --- | --- |
| ***nr-HO-ToEN-DC-r16***  Indicates whether the UE supports inter-RAT handover from NR to (NG)EN-DC while NR-DC or NE-DC is not configured as defined in TS 36.306 [15]. It is mandated if the UE supports (NG)EN-DC. | UE | CY | No |

**High speed parameters:**

| **Definitions for parameters** | **Per** | **M** | **FDD-TDD**  **DIFF** | **FR1-FR2**  **DIFF** |
| --- | --- | --- | --- | --- |
| ***measurementEnhancement-r16***  Indicates whether the UE supports the enhanced intra-NR and inter-RAT E-UTRAN measurement requirements to support high speed up to 500 km/h as specified in TS 38.133 [5]. This field applies to MN configured measurement enhancement when MR-DC is not configured and SN configured measurement enhancement when (NG)EN-DC is configured. | UE | TBD | No | FR1 only |
| ***demodulationEnhancement-r16***  Indicates whether the UE supports the enhanced demodulation processing for HST-SFN joint transmission scheme with velocity up to 500km/h as specified in TS 38.101-4 [18]. This field applies to MN configured demodulation enhancement when MR-DC is not configured and SN configured demodulation enhancement when (NG)EN-DC is configured. | UE | TBD | No | FR1 only |

**Question 2: Do companies agree to capture the proposed clarification for NGED-DC in the descriptions of *ULTxSwitchingBandPair-r16*, *uplinkTxSwitching-OptionSupport-r16*, *handoverInterF*, *nr-HO-ToEN-DC-r16, measurementEnhancement-r16,* and *demodulationEnhancement-r16*?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments, if any** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.3 Rel-15 NR clarification on the support of NGEN-DC

In the 38.306 CR in R2-2008082 [5], it clarifies that two capabilities, *v2x-EUTRA* and *pdcp-DuplicationSR*,are also applicable for the case of NGEN-DC, see below:

**General parameters:**

| **Definitions for parameters** | **Per** | **M** | **FDD-TDD DIFF** | **FR1-FR2**  **DIFF** |
| --- | --- | --- | --- | --- |
| ***v2x-EUTRA***  Indicates whether the UE supports EUTRA V2X according to *UE-EUTRA-Capability* as defined in TS 36.331 [17], independent of the configured EN-DC band combination. This field is only applied to (NG)EN-DC. In UE-NR-Capability, this field is not used, and UE does not include the field. | UE | No | Yes | No |

**PDCP Parameters:**

| **Definitions for parameters** | **Per** | **M** | **FDD-TDD DIFF** |
| --- | --- | --- | --- |
| ***pdcp-DuplicationSRB***  Indicates whether the UE supports CA-based PDCP duplication over SRB1/2 and/or, if (NG)EN-DC is supported, SRB3 as specified in TS 38.323 [16]. | UE | No | No |

**Question 3: Do companies agree to capture the proposed clarification for NGED-DC in the descriptions of *v2x-EUTRA* and *pdcp-DuplicationSRB*?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments, if any** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 3 Conclusion

The proposals captured are the following:

# 4 References

[1] R2-111e Chair Notes 2020-08-17 1500 UTC.

[2] Draft\_RAN2\_110-e\_Meeting\_Report\_v2.

[3] R2-2008080 Clarification on the extended capability of NGEN-DC, vivo.

[4] R2-2008081 Clarification on the extended capability of NGEN-DC, vivo.

[5] R2-2008082 Clarification on the extended capability of NGEN-DC, vivo.