**3GPP TSG-RAN WG2 Meeting #111-eDRAFT R2-2008193**

**Online, 17–28 August 2020**

**Agenda item:** 8.12.3

**Source:** CATT

**Title: Draft** Summary of Offline 111 - DRX Aspects (CATT)‎

**Document for:** Discussion and Agreement

# 1 Introduction

This is to report the result of the following offline discusion as per the draft session report [1]

* [AT111e][111][REDCAP] DRX aspects (CATT)

Scope: Discuss the proposals in [R2-2007013](file:///C%3A%5CData%5C3GPP%5CRAN2%5CDocs%5CR2-2007013.zip), [R2-2007346](file:///C%3A%5CData%5C3GPP%5CRAN2%5CDocs%5CR2-2007346.zip), [R2-2007494](file:///C%3A%5CData%5C3GPP%5CRAN2%5CDocs%5CR2-2007494.zip) as well as proposals 1 to 4 in [R2-2006748](file:///C%3A%5CData%5C3GPP%5CRAN2%5CDocs%5CR2-2006748.zip). The intention is to identify design alternatives, collect company views and, whenever possible, also narrow down the proposals.

Initial intended outcome: summary of the offline discussion with e.g.:

* + - List of agreeable proposals (if any)
		- List of proposals that require online discussions

Initial deadline (for companies' feedback): Monday 2020-08-24 22:00 UTC

Initial deadline (for rapporteur's summary in R2-2008193): Tuesday 2020-08-25 02:00 UTC

The remainder of this document is organized as the following. In Section 2 we provide discussions based on company contribution [2-5]. In Section 3 the discussions are summarized with list of proposals.

# 2 Discussion

As per the scope, proposals from company contribution [2-5] are listed in the Appendix. In section 2.1-2.4, these proposals will be discussed in a few aspects.

All participants to this discussion are encouraged to leave their name/contact in section 5.

## 2.1 Support of eDRX in for RRC Inactive and/or Idle ‎

A first aspect in contribution [2-5] is on the support of eDRX in different NR RRC states, i.e., Inactive and/or Idle ‎state. In [2,3,5] there are explicit proposals/observations to study eDRX mechanims for both states, while in [4] evaluations show positive performance gain towards the same direction. Therefore, the following should be agreeable based on the summarized contributions.

**Proposal A RAN2 study eDRX mechanism for both RRC\_IDLE and RRC\_INACTIVE in this SI. ‎**

Please insert your views and comments to Proposal A in the table below.

Table 1

|  |  |  |
| --- | --- | --- |
| **Company name** | **Agree/Disagree** | **Comments if any** |
| Qualcomm | Agree |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.2 Baseline of NR eDRX mechanism

In [2-5] the discussions are on different detailed level regarding how eDRX should work for NR. There seems to be some commonality from the view point of high level principles.

* More specifically, [2] suggests to reuse LTE eDRX mechanism with possible consideration of NR system charicteristics, e.g., multiple beam.
* In [3] the procedures of eDRX mechanism for RRC\_IDLE UE and RRC\_INACTIVE in LTE are summarized and suggested to serve as baseline of NR eDRX mechanism‎.
* Similarly in [5] it is suggested that the feature (eDRX for NR) can follow similar approach as it was done for LTE I-eDRX.
* In [4]‎, it is suggested that eDRX mechanisms in LTE/NB-IoT such as PTW and HFN are used as the baseline for ‎introducing eDRX in RedCap‎.

All these seem along the line of using LTE as baseline. Therefore, it is possible to first agree on high level guidence for further eDRX mechianim studies as the following proposal. One motivation to first have such a guideline is to faciliate the discussions in the following sections, e.g., companies could then have a rough idea of the potential machanism on the table, as well as their complexities/impacts based on LTE work.

**Proposal B In further study of NR eDRX, the LTE ‎eDRX mechanism is used as baseline.**

Please insert your views and comments to proposal B in the table below.

Table 2

|  |  |  |
| --- | --- | --- |
| **Company name** | **Agree/Disagree** | **Comments if any** |
| Qualcomm | Agree | We can support using the eDRX signaling framework as baseline. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.3 eDRX cycle range

The group can further discuss to what extend/which components of the LTE eDRX mechanism will be studied/adopted for NR. It seems obvious such discussions depend on the eDRX cycle range. There seem to be different views from the company contributions on the possible eDRX cycle range.

For example, in [3] the following proposals were made

|  |
| --- |
| *Proposal 3: Consider the maximum value of 2621.44s (almost 44 min) eDRX period for RRC\_IDLE state as a starting point.**Proposal 4: Study the possibility of introducing longer eDRX period for RRC\_INACTIVE state (exceeding 10.24s****).*** |

In [5] the following were proposed

|  |
| --- |
| *Proposal 1.‎ NR paging cycle is extended up to 10.24 sec for UEs in RRC\_INACTIVE/RRC\_IDLE.‎**Proposal 3.‎ For UEs in RRC\_INACITVE, paging DRX cycle is not extended above 10.24 sec.‎**Proposal 4.‎ For UEs in RRC\_IDLE, to discuss whether to enable paging DRX cycles above 10.24 ‎sec similarly as it is done for LTE eDRX feature (including new Hyper-SFN, paging time window (PTW), ‎or paging hyper-frame (PH) concepts/mechanism).‎* |

In [4] there seems to be no explicit proposal regarding the value range.

There seems to be common understanding regarding the pros and cons of these possible ranges. A breif summary is as the following.

* It seems generally agreeable that longer eDRX cycle allows more power saving [3][4].
* For inactive case, an eDRX cycle range up to 10.24s has less impact to RAN, as otherwise RAN may need to discuss and introduce for inactive state some mechanims simliar as Hyper-SFN, paging time window (PTW), or paging hyper-frame (PH) that has been used for LTE. Besides, there is potential impact due to the NAS retransmission time limitation (For E-UTRA connected to 5GC, extending DRX cycle above 10.24 sec was not desirable for UEs in RRC\_INACTIVE ‎due to the foreseen CN impact. See some discussions in [5] which refers to CT1 situation).

Considering the potential performance gain vs compleixty (including RAN/CN impact), to extend the cycle range up to 10.24s seems to be a possible baseline for RRC\_INACTIVE. As there seems to be concern of going beyond this, it can be a point of further study. This is reflected in the following proposal.

**Proposal C For RRC\_INACTIVE, the DRX cycle is extended to 10.24s as baseline. FFS on the performance and complexity of further extension.**

Please insert your views and comments to Proposal C in the table below.

Table 3

|  |  |  |
| --- | --- | --- |
| **Company name** | **Agree/Disagree** | **Comments if any** |
| Qualcomm | Agree | In addition to concern on the possible impacts on RAN/CN by longer DRX cycles (>10.24s), we don’t see any of the three target RedCap use cases can have extra long eDRX cycles. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

For the case of idle, companies seem more willing to study even further extension of the cycle range (e.g., see P3 in [3], and P4 in [5], etc.). It seems possible to collect companies’ views on the following proposal.

**Proposal D For RRC\_IDLE, the DRX cycle is extended to 2621.44s as baseline.**

Please insert your views and comments to Proposal D in the table below.

Table 4

|  |  |  |
| --- | --- | --- |
| **Company name** | **Agree/Disagree** | **Comments if any** |
| Qualcomm | Disagree | We don’t see any of the three target RedCap use cases can have extra long eDRX cycles. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Whether the eDRX cycle needs to go even beyond ‎2621.44s ‎depends on the interested use case.

* In [3], it is observed to the requirement of the power saving and battery lifetime enhancement is from industrial ‎wireless sensors and wearables‎.
* In [5], the targeted use cases from the SID ‎[1]‎ RP-201386‎ are cited, and it is observed that WB-E-UTRAN connected to 5GC, extending DRX cycle feature is supported for UEs in RRC\_IDLE (with or ‎without suspend indication) up to 44 min, and for UEs in RRC\_INACTIVE up to 10.24 sec.‎
* In [4] there seems to be no explicit preference regarding the interested use cases.

In order to potentially narrow down the propoals, it seems useful to collect companies’ views regarding the following question.

**Question E Do you think DRX cycle range beyond 2621.44s should be considered in further studies of this SI?**

Please insert your views on Question E in the table below.

Table 5

|  |  |  |
| --- | --- | --- |
| **Company name** | **Yes/No** | **Comments if any** |
| Qualcomm | No | No use case for R17 RedCap would call for such a long cycle. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.4 Further discussions

Besides the previously mentioned aspects there are other proposals from the summarized contributions.

* In [2], there are proposals regarding the configuration of eDRX and the interaction between RAN and CN.
* In [3], further proposals were made regarding SI acquisition aspect, as well as the possible involvement of R4 for performance requirements during WI phase. ‎
* In [4], it is suggested to send an LS to SA2 to indicate our progress.

These proposals are either from only one company or more into later stage discussions. That being said, it seems the group can disucss on the need of sending an LS to SA2 or other potential WGs in SA or CT, to inform RAN2’s progress on the topic. This is reflected in the following.

**Question F Do you see a need that RAN2 inform its conclusions (all or some of them, if agreed) on the topic to SA2 or other SA/CT WGs?**

Please insert your views and comments to Question F in the table below.

Table 6

|  |  |  |
| --- | --- | --- |
| **Company name** | **Yes/No** | **Comments if any** |
| Qualcomm | Depends | It would depend on whether the agreements we make have any impact on SA2 or other WGs. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

And, companies can input if any on the following questsion.

**Question G Do you see any other issues (as per scope of this offline disc) that have not been covered by previous discussions?**

Please insert your views on Question G in the table below.

Table 7

|  |  |
| --- | --- |
| **Company name** | **Issues and comments if any** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# 3 Conclusion

This contribution is on the topic of eDRX in NR, under the R17 RedCap study item. For the topic, proposals from [2-5] were reviewed, and companies’ views have been collected. Based on the discussions the following set of proposals can be put to further checking in online session.

List of pontentially agreeable proposals

TBD

List of proposals for further discussions

TBD

# 4 References

[1] Draft report, RAN2-111e - R16 eMIMO-CLI-PRN-RACS - R17 NTN-REDCAP

[2] R2-2007013 eDRX for NR RRC Inactive and Idle States CATT

[3] R2-2007346 Discussion on eDRX for RRC\_INACTIVE and RRC\_IDLE‎ Huawei, HiSilicon

[4] R2-2007494 eDRX for reduced capability UEs MediaTek Inc.‎

[5] R2-2006748 Use cases target to extend paging DRX cycle and relax measurements for stationary devices Intel Corporation

# 5 Participants

|  |  |
| --- | --- |
| **Company Name** | **Participant name/contact** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# Appendix List of Company proposals

Proposals from [2]

|  |
| --- |
| Proposal 1: The LTE eDRX mechanism for idle mode should be reused for NR with the ‎consideration of multi-beam i.e. define eDRX cycle and paging time window.‎Proposal 2: The eDRX mechanism should apply for both NR RRC inactive and idle state.‎Proposal 3: Only one eDRX parameters can be configured for UE which apply for UE no matter ‎it is in RRC inactive or idle.‎Proposal 4: eDRX parameters should be exchanged between CN and RAN to support UE ‎monitor paging according to eDRX in RRC inactive if eDRX parameters are configured to the UE.‎Proposal 5: The eDRX parameters should be decided by CN. ‎Proposal 6: RAN 2 should discuss how to configure the eDRX parameters to UE:‎-‎Option 1: via NAS signaling by CN, and the CN send the eDRX parameters to RAN.‎‎-‎Option 2: via RRS signaling by RAN, the RAN acquires the eDRX parameters from CN. ‎ |

Proposals from [3]

|  |
| --- |
| Observation 1: the requirement of the power saving and battery lifetime enhancement is from industrial wireless sensors and wearables.Observation 2: the larger DRX period has large positive impact on UE power consumption in Non-RRC\_CONNECTED.Proposal 1: Study eDRX mechanism for both RRC\_IDLE and RRC\_INACTIVE. Proposal 2: the procedure of eDRX mechanism in LTE could be used as baseline of NR eDRX mechanism.* Idle mode eDRX parameter is negotiated by UE and AMF;
* gNB decides UE’s inactive eDRX parameters based on the negotiated eDRX parameters
* Include idle eDRX parameters and inactive eDRX parameters in CN PAGING MESSAGE and RNA PAGING MESSAGE respectively.

Proposal 3: Consider the maximum value of 2621.44s (almost 44 min) eDRX period for RRC\_IDLE state as a starting point.Proposal 4: Study the possibility of introducing longer eDRX period for RRC\_INACTIVE state (exceeding 10.24s).Proposal 5: Reuse existing DRX mechanism (based or PH and PTW) for RRC\_IDLE in NR if it is agreed to support eDRX cycle larger than 10.24. Proposal 6: Study whether to introduce PTW mechanism or not for RRC\_INACTIVE if it is agreed to introduce eDRX period exceeding 10.24s for RRC\_INACTIVE.Proposal 7: Study SI acquisition enhancement mechanism in NR after eDRX mechanism is introduced. Proposal 8: Involve RAN4 in the WID after REDCAP study item finishes and eDRX is agreed to be specified. |

Proposals from [4]

|  |
| --- |
| Observation 1: Introducing eDRX UEs can be beneficial for industrial wireless sensors and wearables use cases in RedCap.Proposal 1: eDRX mechanisms in LTE/NB-IoT such as PTW and HFN are used as the baseline for introducing eDRX in RedCap. The exact formulas and impact on other procedures can be discussed during the work item phase.Proposal 2: RAN2 to send an LS to SA2 with recommendation to introduce eDRX, to check if there are any potential issues for RedCap from 5GC perspective. |

Proposals from [5]

|  |
| --- |
| Observation 1.‎ Extending DRX cycle for NR UEs in RRC\_IDLE and RRC\_INACTIVE above 2.56sec ‎is needed in order to reach the battery lifetime of the target use cases (from years to days and weeks) ‎similarly as it was done in LTE Rel-13 extended DRX feature.‎Observation 2.‎ For WB-E-UTRAN connected to 5GC, extending DRX cycle feature is supported for ‎UEs in RRC\_IDLE (with or without suspend indication) up to 44 min. and for UEs in RRC\_INACTIVE up ‎to 10.24 sec.‎Observation 3.‎ During Rel-16 Power Saving SI phase, RAN2 captured in the conclusion of TR 38.840 ‎that it was desirable to define rules for UE specific DRX cycles extended up to 10.24 sec.‎Observation 4.‎ For E-UTRA connected to 5GC, extending DRX cycle above 10.24 sec was not ‎desirable for UEs in RRC\_INACTIVE due to the foreseen CN impact to the mobility management ‎procedures due to the smallest value of the NAS retransmission timer and the actual number of NAS ‎retransmission done).‎…(omitted)The proposals captured are the following:‎Proposal 1.‎ NR paging cycle is extended up to 10.24 sec for UEs in RRC\_INACTIVE/RRC\_IDLE.‎Proposal 2.‎ If Proposal 1 is agreed, this feature can follow similar approach as it was done for LTE ‎I-eDRX feature i.e. (1) upper layers configure eDRX, (2) when configured, eDRX value is used (instead of ‎the smallest), and (3) legacy NR PF/PO mechanism described in 38.304 applies.‎Proposal 3.‎ For UEs in RRC\_INACITVE, paging DRX cycle is not extended above 10.24 sec.‎Proposal 4.‎ For UEs in RRC\_IDLE, to discuss whether to enable paging DRX cycles above 10.24 ‎sec similarly as it is done for LTE eDRX feature (including new Hyper-SFN, paging time window (PTW), ‎or paging hyper-frame (PH) concepts/mechanism).‎…(omitted) |