**3GPP TSG-RAN WG2 #112-e *Draft\_R2-2009676***

**E-meeting, November 2020**

Agenda Item: 6.4.2

Source: OPPO

Title: Summary of [AT112-e][709][V2X]: Left issue on inter-frequency operation (OPPO)

Document for: Discussion, Decision

# Introduction


This is for the discussion below

* [AT112-e][709][V2X] Left issue on inter-frequency operation (OPPO)

Discuss proposals in R2-2009676 and prepare the agreeable CR in R2-2010939 (discussion summary in R2-2010938 if needed). CR will be agreed by email. Deadline is 12:00pm 11/12/2020 (UTC).

# Discussion

In last meeting, the following issue was discussed in “[Post111-e][701][V2X] 38.304 and 36.304 corrections”.



According to the email discussion of [Post111-e][701], there seem two interperatations of use case of the target section (section 8.2 of TS 38.304)

* One interpretation is the section is for inter-frequency cell reselection, i.e., UE was camping on Frequency-1, but later switches to Frequency-2;
* The other interpretation is the section is for a “virtual cell reselection”, i.e., UE keeps camping on Frequency-1, but also reading V2X SIB on Frequency-2;

Regardless which interpretation is correct, considering the former behavior of “*UE was camping on Frequency-1, but later switches to Frequency-2*” is allowed and already captured in TS 36.304/38.304, the uncertainty is whether the latter behaviour of “*UE keeps camping on Frequency-1, but also reading V2X SIB on Frequency-2*” is allowed, so it would be helpful to firstly check if RAN2 has common understanding on allowing the latter operation.

In details, according to [1]

*For NR-V2X:*

* *On the one hand, currently in TS 38.331, the UE behaviour for reading F2 while staying at F1 is not specified.*
* *On the other hand, there is a following agreement at least to address the dual-RAT transmission on PC5 interface (from RAN2#110), in the direction of allowing such operation but no specification needed.*

=> In the case UE supports both NR and LTE SL RAT, but UE’s camped cell can only provide one SL RAT configuration, then if the UE is also in coverage for the other RAT, then the UE may acquire the other SL RAT configuration by reading the broadcast V2X SIB on the concerned carrier. There will be no specification impact.

*Given the current text in TS 36.304 and TS 38.304 as follows, it is probably true that V2X SIB reading at F2 is allowed. But since there is no clear agreement or RRC specification, it will be beneficial for RAN2 to formally confirm for NR-V2X, whether the UE can stay at F1, but reading V2X SIB at F2.*

8.2 Cell selection and reselection for Sidelink

[…]

When UE is interested to perform NR sidelink communication on non-serving frequency, it may perform measurements on that frequency or the frequencies which can provide inter carrier NR sidelink configuration for that frequency for cell selection and intra-frequency reselection purpose in accordance with TS 38.133[8]. When UE is interested to perform V2X sidelink communication on non-serving frequency, it may perform measurements on that frequency or the frequencies which can provide inter carrier V2X sidelink configuration for that frequency for cell selection and intra-frequency reselection purpose in accordance with TS 38.133[8].

**Q1a: For NR-V2X, whether UE can keep camping on a carrier-1, and read V2X SIB on a carrier-2?**

* **Yes;**
* **No;**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Furthermore, if one answers Yes for Q1a, it needs to further clarify what is the applicable scenariofor this “read V2X SIB on a carrier-2” operation:

* Either limited to intra-frequency scenario, i.e., for PC5 activity can only happen at carrier-2;
* Or applicable to both inter-ferquency and intra-frequency scenario, i.e., PC5 activity can happen at not only carrier-2 but another carrier-3 (i.e., different from carrier-1 and carrier-2);

The latter one is probably true given the current specification,

8.2 Cell selection and reselection for Sidelink

[…]

When UE is interested to perform NR sidelink communication on non-serving frequency, it may perform measurements on that frequency or the frequencies which can provide inter carrier NR sidelink configuration for that frequency for cell selection and intra-frequency reselection purpose in accordance with TS 38.133[8]. When UE is interested to perform V2X sidelink communication on non-serving frequency, it may perform measurements on that frequency or the frequencies which can provide inter carrier V2X sidelink configuration for that frequency for cell selection and intra-frequency reselection purpose in accordance with TS 38.133[8].

**Q1b: If Yes to Q1a, for NR-V2X, for the “reading V2X SIB on a carrier-2”, whether it is applicable to both intra- and inter-carrier configuration scenario, i.e., PC5 activity can happen at not only carrier-2 but also another carrier-3 (i.e., different from carrier-1 and carrier-2)?**

* **Yes;**
* **No;**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

For TS 38.331, according to [1], if one answers Yes at least for Q1a, it is good to be clarified that the UE behaviour of “keep camping on a carrier-1, and read V2X SIB on a carrier-2” is allowed.

**Q2a: If Yes to Q1a (and Q1b), do you agree to clarify the UE operation (i.e., keep camping on a carrier-1, and read V2X SIB on a carrier-2) in TS 38.331?**

* **Yes;**
* **No;**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

In [1], it is proposed to add a NOTE to clarify that,

NOTE 5: A UE capable of NR sidelink communication and is configured by upper layers to perform NR sidelink communication on a frequency can acquire *SIB12* from a cell other than serving cell (for RRC\_INACTIVE or RRC\_IDLE) or primary cell (for RRC\_CONNECTED), if *SIB12* of serving cell (for RRC\_INACTIVE or RRC\_IDLE) or primary cell (for RRC\_CONNECTED) does not provide configuration for NR sidelink communication for the frequency, and if the cell providing configuration for NR sidelink communication for the frequency meets the S-criteria as defined in TS 38.304 [20].

**Q2b: If Yes to Q2a, do you agree with the change proposed in [1] above for TS 38.331?**

* **Yes;**
* **No;**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

For TS 36.304, currently there are two use cases captured

11.4 Cell selection and reselection for sidelink

The requirements defined in this clause for sidelink operation apply for UEs in RRC\_IDLE and in RRC\_CONNECTED.

When UE is interested to perform sidelink communication or sidelink discovery announcement on non-serving frequency, it shall perform measurements on that frequency for cell selection and intra-frequency reselection purpose in accordance with TS 36.133 [10]. When UE is interested to perform V2X sidelink communication on non-serving frequency, it may perform measurements on that frequency or the frequencies which can provide inter-carrier V2X sidelink configuration for that frequency for cell selection and intra-frequency reselection purpose in accordance with TS 36.133 [10]. When UE is interested to perform NR sidelink communication on non-serving frequency, it may perform measurements on that frequency or the frequencies which can provide inter-carrier NR sidelink configuration for that frequency for cell selection and intra-frequency reselection purpose in accordance with TS 36.133[10].

[…]

If the UE has selected a cell on a non-serving frequency for sidelink communication or V2X sidelink communication or NR sidelink communication or sidelink discovery announcement, it shall perform additional intra-frequency reselection process to select a better cell for sidelink operation on that frequency in accordance with clause 11.4.1.

Similarly, the two cases are included in TS 38.304

8.2 Cell selection and reselection for Sidelink

The requirements defined in this clause for sidelink operation apply for UEs in RRC\_IDLE, RRC\_INACTIVE and in RRC\_CONNECTED.

When UE is interested to perform NR sidelink communication on non-serving frequency, it may perform measurements on that frequency or the frequencies which can provide inter carrier NR sidelink configuration for that frequency for cell selection and intra-frequency reselection purpose in accordance with TS 38.133[8]. When UE is interested to perform V2X sidelink communication on non-serving frequency, it may perform measurements on that frequency or the frequencies which can provide inter carrier V2X sidelink configuration for that frequency for cell selection and intra-frequency reselection purpose in accordance with TS 38.133[8].

[…]

If the UE has selected a cell on a non-serving frequency for NR sidelink communication or V2X sidelink communication, it shall perform additional intra-frequency reselection process to select a better cell for sidelink operation on that frequency in accordance with clause 8.2.1.

Firstly, for cell selection, according to [1], it is used for PLMN selection as defined in TS 23.285

- If the UE finds such cell but not in the registered PLMN or a PLMN equivalent to the registered PLMN, and that cell belongs to a PLMN authorized for V2X communications over PC5 reference point and provides radio resources for V2X service then the UE shall perform PLMN selection triggered by V2X communications over PC5 reference point as defined in TS 23.122 [23]. If the UE has an ongoing emergency session, it shall not trigger any PLMN selection due to V2X communication over PC5 reference point.

So firstly, good to check whether cell selection is a valid use case.

**Q3a: Do you agree that cell selection is a valid use case of non-serving frequency measurement for NR-V2X?**

* **Yes;**
* **No;**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q3b: If No to Q3a, do you agree that “cell selection” is excluded for NR-V2X in TS 36.304 and TS 38.304?**

* **Yes;**
* **No;**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Secondly, for intra-frequency cell reselection, according to [1][2], it is used for vitual cell reselction, if the UE behaviour of “keep camping on a carrier-1, and read V2X SIB on a carrier-2” is allowed, as questioned in Q1a/b.

**Q4a: Do you agree that intra-frequency cell reselection is a valid use case of non-serving frequency measurement for NR-V2X?**

* **Yes (e.g., if one answer Yes to Q1a (and Q1b));**
* **No (e.g., if one answer No to Q1a);**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q4b: If No to Q4a, do you agree that “intra-frequency cell reselection” is excluded for NR-V2X in TS 36.304 and TS 38.304?**

* **Yes;**
* **No;**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Thirdly, according to [1][2], inter-frequency cell reselection should be included, rapporteur understands it could be

* Not only for the case of “*UE was camping on Frequency-1, but later switches to Frequency-2*”, where pre-measurement on F2 is needed;
* But also for the case of “*UE keeps camping on Frequency-1, but also reading V2X SIB on Frequency-2*”, where the reading on frequency-2 maybe later switch to another frequency-2’, since the inter-frequency configuration may come from any frequency, and thus pre-measurement on F2 is also needed.

**Q5a: Do you agree that inter-frequency cell reselection is a valid use case of non-serving frequency measurement for NR-V2X?**

* **Yes;**
* **No;**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q5b: If Yes to Q5a, do you agree that “inter-frequency cell reselection” is included for NR-V2X in TS 36.304 and TS 38.304?**

* **Yes;**
* **No;**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

1. xxx.

# Conclusion

We have the following proposals:

[Proposal 1 xxx.](#_Toc55254145)

# Reference

1. R2-2009676 Left issue on inter-frequency operation for NR-V2X OPPO discussion Rel-16 5G\_V2X\_NRSL-Core
2. R2-2008875 Discussion on left issue of 38.304 and 36.304 CATT discussion Rel-16 5G\_V2X\_NRSL-Core
3. R2-2008876 Correction to TS 38.304 CATT CR Rel-16 38.304 16.2.0 0188 - F 5G\_V2X\_NRSL-Core
4. R2-2008877 Correction to TS 36.304 CATT CR Rel-16 36.304 16.2.0 0813 - F 5G\_V2X\_NRSL-Core