3GPP TSG-RAN WG2 Meeting #113 Electronic R2-210xxxx

Elbonia, 25 January – 05 February 2021

**Agenda item: 5.4.2**

**Source: Nokia**

**Title: Summary of [AT113-e][008][NR15] LTE changes (Nokia)**

**WID/SID: NR\_newRAT-Core**

**Document for: Discussion and Decision**

# 1 Introduction

This document is the report of the following email discussion:

5.4.2 LTE changes related to NR

**[AT113-e][008][NR15] LTE changes (Nokia)**

Scope: Treat [R2-2100182](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113-e\Docs\R2-2100182.zip), [R2-2100946](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113-e\Docs\R2-2100946.zip), [R2-2101863](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113-e\Docs\R2-2101863.zip), [R2-2101864](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113-e\Docs\R2-2101864.zip), [R2-2101882](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113-e\Docs\R2-2101882.zip), [R2-2101881](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113-e\Docs\R2-2101881.zip)

Phase 1, determine agreeable parts, Phase 2, for agreeable parts Work on CRs.

Intended outcome: Report and Agreed CRs.

Deadline: Schedule A

[R2-2100182](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113-e\Docs\R2-2100182.zip) A remaining issue in SIB extension Samsung Electronics Co., Ltd discussion Rel-15 NR\_newRAT-Core

[R2-2100946](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113-e\Docs\R2-2100946.zip) Handling of 4-layer MIMO in EN-DC for Cat5 UEs Nokia, Nokia Shanghai Bell discussion Rel-15 NR\_newRAT-Core

[R2-2101863](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113-e\Docs\R2-2101863.zip) Reconfiguring RoHC and setting the drb-ContinueROHC simultaneously Qualcomm Incorporated CR Rel-15 36.331 15.12.0 4595 - F NR\_newRAT-Core

[R2-2101864](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113-e\Docs\R2-2101864.zip) Reconfiguring RoHC and setting the drb-ContinueROHC simultaneously Qualcomm Incorporated CR Rel-16 36.331 16.3.0 4596 - A NR\_newRAT-Core

[R2-2101882](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113-e\Docs\R2-2101882.zip) Correction on IDC indication Samsung CR Rel-15 36.331 15.12.0 4598 - F NR\_newRAT-Core

[R2-2101881](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113-e\Docs\R2-2101881.zip) Correction on IDC indication Samsung CR Rel-16 36.331 16.3.0 4597 - A NR\_newRAT-Core

# 2 **Discussion**

**Topic 1: SIB extension**

[R2-2100182](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113-e\Docs\R2-2100182.zip) A remaining issue in SIB extension Samsung Electronics Co., Ltd discussion Rel-15 NR\_newRAT-Core

As per the scenario in the paper to avoid potential IOT issue in the future, it is desirable to clarify the intended UE behavior upon receiving inconsistent SI.

|  |
| --- |
| **Proposal 1-1: Clarify the intended UE behaviour in the meeting minute that “upon receiving SI of which SIB type(s) is/are different from what was/were announced in the scheduling information in SIB1, UE decodes the SIB(s) of the SI as long as it can understand.”**  **Proposal 1-2: Clarify the intended UE behavior in 36.331 in the form of note that “upon receiving SI of which SIB type(s) is/are different from what was/were announced in the scheduling information in SIB1, UE decodes the SIB(s) of the SI as long as it can understand.”** |

**Question 1**: Do companies agree to the proposals made in [R2-2100182](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113-e\Docs\R2-2100182.zip)?

|  |  |  |
| --- | --- | --- |
| Answers to Question 1 | | |
| Company | Yes/No | Comments |
| Ericsson | Yes, P1-1 but… | PS: P1-1 and P1-2 are alternatives, not complementary in our understanding.  There can be a transitional period where the SIB1 scheduling, that the UE is using, does not match the actual SIB scheduling, for example when ETWS/CMAS is started, and the UE just acquired SIB1 scheduling, and is trying to acquire the SIBs.  In case the SIB1 scheduling does not match the content of the SI-message, the UE may still be able to decode the content of the SI-message, i.e. receive the actual SIB(s). However the UE should not be required to do so, i.e. SIB1 scheduling should match the SI-message content. In the example we provided the problem will eventually be resolved when the UE receives an SI modification indication in Paging message and receives the correct SIB1 scheduling.  We propose to capture the following wording in the chairman notes:  *In case the SIB1 scheduling does not match the SI-message content, the UE may be able to decode the SIB(s) in the SI-message, but the UE is not required to do so.* |
| Qcom | No | The proposals (1 & 2) are vague and restrict the UE ability to decode SIB(s) when possible. For instance is not clear what is meant by “**understand**” in  “**UE decodes the SIB(s) of the SI as long as it can understand”**   * Understand = expected order by the UE   Or   * Understand = best effort attempt to decode despite the fact the SI contents is not as scheduled by *schedulingInfoList* / *schedulingInfoListEx*   We believe these proposals restrict the UE ability to decode the SI when it can.  Ericson’s proposal seems acceptable. |
| T-Mobile USA | Yes P1-1 but… | The current language doesn’t require the UE to decode CMAS/EWTS SIB(s) when the scheduling info doesn’t match SIB1. Decoding CMAS/EWTS is mandatory in the case were the content of the SI-message doesn’t match SIB1, it is the remaining SIB’s that must be decoded by the end of the next SI-message where the misplaced SIB’s are located.  Suggest modifying the language to state:  “In the case when SIB1 scheduling does not match the SI-message content, the UE must decode the content of the inserted CMAS/ETWS message. Other SIB’s contained in the mismatched SI-message must be decoded the content of the displaced SIBs by the end of the next SI-message were the SIB’s in the mismatched SI-message are repeated.”  Putting a time limit of “by the next” allows the UE could decode the SIB’s in the mismatched SI-message or in the next SI-Message containing the same SIB’s that were in the mismatched SI-message. |
| Huawei, HiSilicon | No | We agree with Qualcomm that the proposals restrict the UE behaviour. It should be left to UE implementation, i.e. UE can decode, or delete, if the SIB1 scheduling does not match the SI-message content. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 1**: TBD.

**Proposal 1**: TBD.

**Topic 2: Cat5 MIMO issue**

[R2-2100946](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113-e\Docs\R2-2100946.zip) Handling of 4-layer MIMO in EN-DC for Cat5 UEs Nokia, Nokia Shanghai Bell discussion Rel-15 NR\_newRAT-Core

|  |
| --- |
| **Observation 1:** Cat5 UEs always support 4-layer MIMO in LTE-only mode, and always utilize 2-bit RI bit width.  **Observation 2:** Cat5 UEs need not support *maxLayersMIMO* signalling.  **Observation 3:** LTE Cat5 UE supporting EN-DC need not support 4-layer MIMO in EN-DC even though the UE does support 4-layer MIMO in LTE-only mode.  **Observation 4:** Cat5 UE RI bit width for TM3/4 is only determined according to the RRC signalling, PBCH antenna ports and UE category.  **Observation 5:** Any UE supporting EN-DC shall also support the configuration of *maxLayersMIMO* regardless of whether it supports 4-layer MIMO in EN-DC.  **Observation 6:** RAN2 discussion is needed on whether the signalling the value *twoLayers* via *maxLayersMIMO* for the case when UE only supports 2-layer MIMO is allowed or needed.  **Observation 7:** It is not clear what RI bit width Cat5 UE uses during EN-DC operation.  **Proposal 1:** RAN2 to clarify what is the correct interpretation on LTE RI bit width for Cat5 UEs in EN-DC: 1) The UE always used 2-bit RI bit width (even if it only supports 2-layer MIMO in EN-DC mode) or 2) The used RI bit width depend on the maximum support MIMO layers, i.e. if UE only supports 2 layers in EN-DC, it will use 1-bit RI bit width in EN-DC.  **Proposal 2:** Mandate Cat5 UEs to indicate *fourLayerTM3-TM4-r15* in all of the EN-DC FeatureSets.  **Proposal 3:** Allow signalling the value *twoLayers* for *maxLayersMIMO* for EN-DC case with TM3/4.  **Proposal 4:** Adopt the RI bit width solution for handling TM3/4 for Cat5 UEs also for the case of TM9/10 for Cat8 UEs . |

As proponent, we would first like companies to have a common understanding of the issue. The CR clarification part may come later but first the principles warrant a discussion.

**Question 2**: Do companies agree to the Observations and the issue based on Proposal 1 in [R2-2100946](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113-e\Docs\R2-2100946.zip)? If yes, then please continue with rest of the proposals and comment how we might end up clarifying this.

|  |  |  |
| --- | --- | --- |
| Answers to Question 2 | | |
| Company | Yes/No | Comments (e.g. changes required to be acceptable, why a CR is or is not needed) |
| Qcom | Check comments | Agree with the observations and the Proposal-1 to reach a common understanding on how to interpret the LTE RI bit width for CAT5 UE when UE is in EN-DC.  However we’re **objecting Proposal-2** that mandates on the CAT5 UE **to support 4 layers on all LTE CCs** while in EN-DC (although it supports 4 layers while in LTE), as this might not be possible once UE switch from LTE to EN-DC.  Further discussion is needed to reach a solution that satisfies all parties. |
| T-Mobile USA | Yes | We agree there is a mismatch, need to check on a solution. |
| Huawei, HiSilicon | - | For proposal1, we think Option 2) is more reasonable.  We also object Proposal 2. It can be relied on UE implementation to carry *fourLayerTM3-TM4-r15*.  We are open on Proposal 3/4 and further discussion is needed. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 2**: TBD.

**Proposal 2**: TBD.

**Topic 3: RoHC and setting the drb-ContinueROHC**

[R2-2101863](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113-e\Docs\R2-2101863.zip) Reconfiguring RoHC and setting the drb-ContinueROHC simultaneously Qualcomm Incorporated CR Rel-15 36.331 15.12.0 4595 - F NR\_newRAT-Core

[R2-2101864](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113-e\Docs\R2-2101864.zip) Reconfiguring RoHC and setting the drb-ContinueROHC simultaneously Qualcomm Incorporated CR Rel-16 36.331 16.3.0 4596 - A NR\_newRAT-Core

|  |
| --- |
| Current specification allows network to reconfigure the RoHC and set the drb-ContinueROHC to “*true*”, simultaneously in the same RRC Reconfiguration message. This would allow change in configuration parameters like maxCID and profiles. It is not clear how to handle the change of ROHC configuration parameters while continuing ROHC context.  The above of configuration defies the purpose of setting the drb-ContinueROHC where RoHC contexts won’t be sustained across mobility from source to target cell.  Therefore, we propose to add clarification to the spec that if network decides to reconfigure the RoHC, no need to set the drb-ContinueROHC to “*true*”.  **Similar CR was approved in NR spec (R2-2008038), the intention of this CR is to align both specs so that RoHC behavior is uniform across the RATs.** |

**Question 3**: Do companies agree to the intent in the CRs in [R2-2101863](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113-e\Docs\R2-2101863.zip) and [R2-2101864](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113-e\Docs\R2-2101863.zip)?

|  |  |  |
| --- | --- | --- |
| Answers to Question 3 | | |
| Company | Yes/No | Comments (e.g. changes required to be acceptable, why a CR is or is not needed) |
| Ericsson | No | We agree that there are certain RoHC configuration parameters which cannot be updated during a handover if the drb-ContinueRoHC flag is set. However, drb-ContinueRoHC was introduced in Rel-11 and if this is a problem then it must have existed since this release. If we want to correct the spec we need to go all the way back to Rel-11 which is a bit too much. |
| Qcom | Yes | **Proponent**  Similar change was adopted in NR, the intention is to unify RoHC across RATs (LTE and NR).  **Response to Ericsson comment**: agree, this go back to Rel.11 when drb-continueRoHC was introduced, however, **even if this CR is implemented from Rel-11 will not cause interoperability issue**, rather prevent suboptimal performance at UE, so it’s not too much to do. |
| Huawei, HiSilicon | No | The CR does not look essential. The issue can be avoided by smart network implementation. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 3**: TBD.

**Proposal 3**: TBD.

**Topic 4: IDC indication**

[R2-2101882](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113-e\Docs\R2-2101882.zip) Correction on IDC indication Samsung CR Rel-15 36.331 15.12.0 4598 - F NR\_newRAT-Core

[R2-2101881](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113-e\Docs\R2-2101881.zip) Correction on IDC indication Samsung CR Rel-16 36.331 16.3.0 4597 - A NR\_newRAT-Core

Companies are requested to check the CR cover page for the description but a short snapshot of why the

CR is required is listed below:

|  |
| --- |
| The reasons to have a CR is described as follows:  1. When victimSystemType or interferenceDirectionMRDC in AffectedCarrierFreqCombInfoMRDC changes from last transmitted InDeviceCoexIndication message, UE will not initiate a new transmission of InDeviceCoexIndication message.  2. Misalignment between text of UE procedure and ASN.1 format |

**Question 4**: Do companies agree to the CRs in [R2-2101881](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113-e\Docs\R2-2101881.zip) and [R2-2101882](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_113-e\Docs\R2-2101881.zip)?

|  |  |  |
| --- | --- | --- |
| Answers to Question 4 | | |
| Company | Yes/No | Comments |
| Ericsson | Yes |  |
| Qcom | Yes |  |
| Huawei, HiSilicon | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 4**: TBD.

**Proposal 4**: TBD.

# 4 Conclusion

Always echo the list of observations and proposals.

# Annex A – Contact Points

Respondents to the email discussion are kindly asked to fill in the following table.

|  |  |  |
| --- | --- | --- |
| Company | Name | Email Address |
| Nokia | Amaanat | amaanat.ali@nokia.com |
| Ericsson | Oscar | oscar.ohlsson@ericsson.com |
| Qualcomm | Mouaffac | mambriss@qti.qualcomm.com |
| T-Mobile USA | John Humbert | John.Humbert2@T-Mobile.com |
| Huawei, HiSilicon | Lili Zheng | zhenglili4@huawei.com |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |