**3GPP TSG-RAN WG2 Meeting #113 Electronic R2-210XXXX**

**25 January – 05 February 2021**

**Agenda item: 8.16.2**

**Source: Nokia**

**Title: Summary of [AT113-e][031][eNPN] SNPN with subscription or credentials by a separate entity**

**WID/SID: NG\_RAN\_PRN\_enh-Core - Release 17**

**Document for: Decision**

# 1 Introduction

This document is the summary of the following email discussion:

* [AT113-e][031][eNPN] SNPN with subscription or credentials by a separate entity (Nokia)

Scope: Take into account documents submitted to this section, 1st pass: identify what is required to be supported by AS and determine the RAN2 impact, if possible. Identify common views / potential initial agreements, Identify points that need further discussion. Can also gather comments on the need to ask questions to other group.

Intended outcome: Report with agreeable proposals and discussion points (not too many, preferably < 10) for treatment on-line

Deadline: 1st Deadline for Comments: Friday Jan 29 1000 UTC. Other deadline if needed by rapporteur. Report Ready for treatment on-line Feb 3.

## Contact person(s) for each participating company

|  |  |  |
| --- | --- | --- |
| Company | Name | Email address |
| Nokia | Gyorgy Wolfner | gyorgy.wolfner@nokia.com |
| ZTE | Wenting Li | li.wenting@zte.com.cn |
| OPPO | Jiangsheng Fan | fanjiangsheng@oppo.com |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 2 Discussion

Documents considered during this email discussion (papers submitted to agenda item 8.16.2):

[R2-2100543](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113-e/Docs/R2-2100543.zip) Overview of RAN2 impacts to support SNPN with 3rd party subscription Nokia, Nokia Shanghai Bell discussion Rel-17 NG\_RAN\_PRN\_enh

[R2-2101717](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113-e/Docs/R2-2101717.zip) Support SNPN along with credentials owned by an entity separate from the SNPN CMCC discussion Rel-17 NG\_RAN\_PRN\_enh-Core

[R2-2100241](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113-e/Docs/R2-2100241.zip) Initial Discussion on Credential by a Separate Entity OPPO discussion Rel-17 NG\_RAN\_PRN\_enh-Core

[R2-2100277](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113-e/Docs/R2-2100277.zip) Consideration on SNPN with Subscription or Credentials by a Separate Entity CATT discussion Rel-17 NG\_RAN\_PRN\_enh-Core

[R2-2100289](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113-e/Docs/R2-2100289.zip) Discussion of credentials by a separate entity in SNPN China Telecommunication discussion Rel-17

[R2-2100431](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113-e/Docs/R2-2100431.zip) Consideration on the Separate Entity Supporting ZTE Corporation, Sanechips discussion Rel-17 NG\_RAN\_PRN\_enh-Core

[R2-2100441](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113-e/Docs/R2-2100441.zip) Access to SNPN with credentials from a different entity Qualcomm Incorporated discussion

[R2-2100490](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113-e/Docs/R2-2100490.zip) SNPN and Service Provider (SP) separation Ericsson discussion Rel-17 NG\_RAN\_PRN\_enh-Core

[R2-2100634](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113-e/Docs/R2-2100634.zip) RAN2 impact on support SNPN along with subscription / credentials owned by an entity separate from the SNPN Intel Corporation discussion Rel-17 NG\_RAN\_PRN\_enh-Core

[R2-2100838](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113-e/Docs/R2-2100838.zip) Support SNPN with subscription or credentials by a separate entity vivo discussion

[R2-2100918](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113-e/Docs/R2-2100918.zip) SIB info for third party credentials and UE onboarding Sony discussion Rel-17 NG\_RAN\_PRN\_enh-Core

[R2-2101001](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113-e/Docs/R2-2101001.zip) Discussion on RAN2 impact of supporting SNPN with credentials owned by a separate entity Huawei, HiSilicon, China Telecom discussion Rel-17 NG\_RAN\_PRN\_enh-Core

[R2-2101515](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113-e/Docs/R2-2101515.zip) Support of SNPN with subscription or credentials by a separate entity LG Electronics discussion Rel-17

## 2.1 Broadcasting related issues

**Q1.1a: Do you agree that an indicator that "access using credentials from a separate entity is supported" should be broadcasted?**

**Q1.1b: Do you agree that the indicator should be broadcasted per SNPN in shared cells?**

**Q1.1c: Do you have a proposal in which SIB the indicator should be broadcasted?**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Company** | **Answer Q1.1a** | **Answer Q1.1b** | **Answer Q1.1c** | **Comments** |
| ZTE | Yes | Yes | Yes(SIB1) | As concluded in the SA2,   |  | | --- | | - For a UE configured to use SNPNs, automatic SNPN selection is performed in the following order:  - UE selects and attempts to register with the SNPN it was last registered with (if available).  - UE selects and attempts to register with the available SNPN identified by a PLMN ID and NID for which the UE has SUPI and credentials (i.e. as in Rel-16).  - UE selects an available and allowable SNPN, which broadcasts "access using credentials from a separate entity is supported" indication and an SNPN ID contained in the user-controlled list (if available)  - UE selects an available and allowable SNPN which broadcasts "access using credentials from a separate entity is supported" indication and a GID contained in the separate entity-controlled list (if available) |   Considering that this indication will affect the network/ cell selection,  we prefer to include it in the SIB1, FFS for the *NPN-IdentityInfo-r16* or add a new list to the *CellAccessRelatedInfo* |
| OPPO | Yes | Yes | Yes(SIB1) | The requirements from SA2 TR 23700-07-120 are quite clear, this indicator should be configured per SNPN. To speed up UE cell selection/reselection procedure, SIB1 is more suitable to include this indicator. Anyway, no much overhead will be introduced in SIB1, it’s still acceptable. |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

**Q1.2a: Do you agree that the Supported Group IDs (GIDs) should be broadcasted?**

**Q1.2b: Do you agree that the Supported Group IDs (GIDs) should be broadcasted per SNPN in shared cells?**

**Q1.2c: Do you have a proposal on the maximum number of Supported Group IDs (GIDs) to be broadcasted?**

**Q1.2d: Do you have a proposal in which SIB the Supported Group IDs (GIDs) should be broadcasted?**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Company** | **Answer Q1.2a** | **Answer Q1.2b** | **Answer Q1.2c** | **Answer Q1.2d** | **Comments** |
| ZTE | Yes | Yes | Yes(See comments) | Yes(See comments) | For the Q1.2c, we think the total number of the Group IDs can be counted independently from the legacy network IDs.E.g. the total number of the Group IDs of all of the SNPNs does not exceed 12 ( meanwhile, the total number of the legacy Network IDs including (PLMNs, PNI-NPNs, and SNPN) does not exceed 12)  For the Q1.2d, similar to question 1, considering that this indicate will affect the network/ cell selection, we prefer to include it in the SIB1, FFS for the *NPN-IdentityInfo-r16* or add a new list to the *CellAccessRelatedInfo.* |
| OPPO | Yes | Yes | Yes(See comments) | Yes(See comments) | For the Q1.2c, we have no strong view, fine with value 4, 8, 12, 16.  For the Q1.2d, if the overhead is not a big issue, SIB1 is more desirable for fast cell selection/reselection; otherwise, SIB10 is also acceptable. |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

**Q1.3a: Do you agree that an indicator whether "the SNPN allows registration attempts from UEs that are not explicitly configured to select the SNPN" should be broadcasted?**

**Q1.3b: Do you agree that the indicator should be broadcasted per SNPN in shared cells?**

**Q1.3c: Do you have a proposal in which SIB the indicator should be broadcasted?**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Company** | **Answer Q1.3a** | **Answer Q1.3b** | **Answer Q1.3c** | **Comments** |
| ZTE | Yes | Yes | Yes(See comments) | Similar to question 1, considering that this indicate will affect the network/ cell selection, we prefer to include it in the SIB1, FFS for the *NPN-IdentityInfo-r16* or add a new list to the *CellAccessRelatedInfo.* |
| OPPO | Yes | Yes | Yes(See comments) | Similar answer with Q1.1a~ Q1.1c. |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

**Q1.4: Other broadcasting related proposals (e.g. other parameters to be broadcasted) to support SNPN with subscription or credentials by a separate entity?**

|  |  |
| --- | --- |
| **Company** | **Proposal** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## 2.2 Impacts on cell selection and reselection

**Q2.1: Do you agree that the AS should report to the NAS about the broadcasted parameters listed in Q1.1, Q1.2 and Q1.3?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Answer** | **Comments** |
| ZTE | Yes | At least for the Q1.3, it shall be reported to the NAS, for that in the SA2’s interim conclusion, on the indication of Q1.3, it said “ - If the UE detects a plurality of such SNPNs, the order in which the UE selects and attempts a registration with an SNPN is implementation specific” we think the AS can send such kind of the SNPNs list and relaed indication in Q1.3 to the NAS and left the NAS to make the final decision.  For the Q1.1/1.2, it also depends on the interaction between NAS and AS, at least for the case that the NAS layer indicate a list of SNPNs in the user-controlled list, or a list of Group IDs, the UE AS should report to the NAS about the broadcasted parameters of the corresponding SNPNs /Group IDs explicitly. For the case that the NAS layer indicate only one SNPN or only one Group ID, the parameter in Q1.1, Q1.2 can be reported implicitly.  Anyway, the AS should report to the NAS about the broadcasted parameters listed in Q1.1, Q1.2 and Q1.3 explicitly or implicitly |
| OPPO | Yes | Based on these enhanced parameters reported by AS, i.e. parameters listed in Q1.1, Q1.2 and Q1.3, NAS will know which type of procedure will be triggered, but we still have some concern for GID, if only GID reported by AS matches with UE NAS configuration, whether the selected GID is visible to UE AS ? or only the selected SNPN ID associated to the GID will be visible to UE AS. We think NAS should clarify something on this as this issue has impact on AS behavior. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q2.2: Do you see any impacts on cell selection or cell reselection (e.g. a need to change suitable cell criteria) to support SNPN with subscription or credentials by a separate entity?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Answer** | **Comments (e.g. details on the impacts)** |
| ZTE | Yes | We think at least it will affect the suitable cell definition |
| OPPO | Maybe | Up to whether the selected GID is visible to UE AS. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.3 Other issues

**Q3.1: Do you see any impacts on connected mobility to support SNPN with subscription or credentials by a separate entity?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Answer** | **Comments (e.g. details on the impacts)** |
| ZTE | No | Up to now, we don’t see any impacts on the connected state mobility. |
| OPPO |  | Up to RAN3 to decide, RAN2 can just wait. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary:**

**Rapporteur's Proposal:**

**Q3.2: Other issues that are not covered by previous questions related to support SNPN with subscription or credentials by a separate entity to be discussed in RAN2**

|  |  |
| --- | --- |
| **Company** | **Issue** |
| ZTE | For the SNPN that only support group ID, whether the indication in the Q1.1 shall be set?  Though in the SA2 interim conclusion, it said that “- UE selects an available and allowable SNPN which broadcasts "access using credentials from a separate entity is supported" indication and a GID contained in the separate entity-controlled list (if available)” , we still have concern on the case that the SNPN only support Group ID. For example, for cell A, the SNPN 1 only support Group ID1, then the UE (with HSP 1) that include the SNPN1 in user-controlled list may try to access Cell A to access it’s corresponding HSP 1, but for the Cell A, it only support HSP with Group ID1, it doesn’t support HSP1. |
| OPPO | Suitable cell clarification:  Cell A: support SNPN1, SNPN2;  Cell B: support SNPN1 and GID1;  UE NAS: Home SNPN= SNPN2, but configured with GID1;  In the beginning, UE has done the registration in Cell B (GID1 match case), then UE moves to Cell A coverage, what’s the UE behavior:  UE behavior1: UE think Cell A is suitable as RSNPN, e.i. SNPN1 is broadcast by Cell A .  UE behavior2: UE think Cell A is not suitable and do registration again on SNPN2 as no GID1 is associated with SNPN1 in Cell A even if SNPN1 is broadcast by Cell A .  We believe NAS should clarify something |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

**Summary:**

**Rapporteur's Proposal:**

## 2.4 Proposed questions to other WGs

**Q4: Proposed questions to other WGs related to SNPN with subscription or credentials by a separate entity (please provide only a question if you think it is important to send an LS to other WGs from this RAN2 meeting)**

|  |  |  |
| --- | --- | --- |
| **Company** | **WG(s)** | **Question** |
| ZTE | RAN3/CT1/SA2 | **Whether the Ran node need the additional information for the AMF selection?** |
| OPPO | SA2 | **Question1 for clarification:**  Whether the GID configured in NAS will be given to AS after registration to assist UE subsequence cell reselection, just like the EPLMN list, which is given to UE AS after registration.  **Question2 for clarification:**  Cell A: support SNPN1, SNPN2;  Cell B: support SNPN1 and GID1;  UE NAS: Home SNPN= SNPN2, but configured with GID1;  In the beginning, UE has done the registration in Cell B (GID1 match case), then UE moves to Cell A coverage, what’s the UE behavior:  UE behavior1: UE think Cell A is suitable as RSNPN, e.i. SNPN1 is broadcast by Cell A .  UE behavior2: UE think Cell A is not suitable and do registration again on SNPN2 as no GID1 is associated with SNPN1 in Cell A even if SNPN1 is broadcast by Cell A .  Which UE behavior is desirable from NAS side? |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary:**

**Rapporteur's Proposal:**

# 3 Conclusions

## 3.1 Proposals that may be agreed

## 3.2 Proposals/Issues that requires further discussion

## 3.3 Potential questions to other WGs