**3GPP TSG-RAN WG2 Meeting #113 Electronic R2-210xxxx**

**25 January – 05 February 2021**

**Agenda item: 6.7.3 & 7.4.2**

**Source: Nokia**

**Title: Summary of [AT113-e][212][MOB] UE capability corrections for LTE and NR mobility (Nokia)**

**WID/SID: NR\_Mob\_enh-Core, LTE\_feMob-Core**

**Document for: Decision**

# 1 Introduction

This document is the summary of the following email discussion:

**Email discussions ([212])**

**[AT113-e][212][MOB] UE capability corrections for LTE and NR mobility (Nokia)**

Scope:

* + - Discuss which UE capability corrections (for LTE and NR) marked for this discussion are seen agreeable
    - Some (or even all) CRs may be merged together if seen needed

Intended outcome:

* + - Discussion summary in [R2-2101965](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2101965.zip) (by email rapporteur).
    - Agreeable CRs (if any)

Deadline for providing comments, for rapporteur inputs, conclusions and CR finalization:

* + - Initial deadline (for companies' feedback): 1st week Thu, UTC 0900
    - Initial deadline (for rapporteur's summary): 1st week Fri, UTC 0900
    - Deadline for CR finalization: 2nd week Thu, UTC 1000

**Web Conf 2nd week (summary of [212])**

[R2-2101965](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2101965.zip) Summary of [AT113-e][212][MOB] UE capability corrections for LTE and NR mobility (Nokia) Nokia discussion Rel-16 NR\_Mob\_enh-Core, LTE\_feMob-Core

By Email [212] (6)

UE capability aspects for DAPS:

[R2-2101025](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2101025.zip) Dummifying the field intraFreqMultiUL-TransmissionDAPS Nokia, Nokia Shanghai Bell, MediaTek, Intel Corporation CR Rel-16 38.331 16.3.1 2379 - F NR\_Mob\_enh-Core

[R2-2101026](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2101026.zip) Dummifying the field intraFreqMultiUL-TransmissionDAPS Nokia, Nokia Shanghai Bell, MediaTek, Intel Corporation CR Rel-16 38.306 16.3.0 0501 - F NR\_Mob\_enh-Core

[R2-2101027](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2101027.zip) Dummifying the field intraFreqMultiUL-TransmissionDAPS Nokia, Nokia Shanghai Bell, MediaTek, Intel Corporation CR Rel-16 36.331 16.3.0 4562 - F LTE\_feMob-Core

[R2-2101028](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2101028.zip) Dummifying the field intraFreqMultiUL-TransmissionDAPS Nokia, Nokia Shanghai Bell, MediaTek, Intel Corporation CR Rel-16 36.306 16.3.0 1803 - F LTE\_feMob-Core

[R2-2101360](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2101360.zip) Clarification on DAPS HO Capability Apple discussion Rel-16 NR\_Mob\_enh-Core

[R2-2101710](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2101710.zip) Understanding of DAPS in BWC-A band Huawei, HiSilicon discussion Rel-16 NR\_Mob\_enh-Core

By email [212] (3)

*Capability coordination for DAPS:*

[R2-2100618](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2100618.zip) DAPS capability coordination between source and target Intel Corporation discussion Rel-16 NR\_Mob\_enh-Core, LTE\_feMob-Core

[R2-2101712](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2101712.zip) Discussion on inter-node signalling for DAPS UE capability coordination Huawei, HiSilicon, MediaTek Inc., Qualcomm Incorporated, China Telecom, China Unicom discussion Rel-16 NR\_Mob\_enh-Core

[R2-2100486](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2100486.zip) Inter-node signalling for UE capability coordination in DAPS handover Ericsson discussion Rel-16 TEI16

*(moved from 6.7.3)*

## Contact person(s) for each participating company

|  |  |  |
| --- | --- | --- |
| Company | Name | Email address |
| Nokia | Amaanat | amaanat.ali@nokia.com |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 2 Discussion

## 2.1 Dummifying capabilities related to intra frequency multi UL transmission

[R2-2101025](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2101025.zip) Dummifying the field intraFreqMultiUL-TransmissionDAPS Nokia, Nokia Shanghai Bell, MediaTek, Intel Corporation CR Rel-16 38.331 16.3.1 2379 - F NR\_Mob\_enh-Core

[R2-2101026](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2101026.zip) Dummifying the field intraFreqMultiUL-TransmissionDAPS Nokia, Nokia Shanghai Bell, MediaTek, Intel Corporation CR Rel-16 38.306 16.3.0 0501 - F NR\_Mob\_enh-Core

[R2-2101027](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2101027.zip) Dummifying the field intraFreqMultiUL-TransmissionDAPS Nokia, Nokia Shanghai Bell, MediaTek, Intel Corporation CR Rel-16 36.331 16.3.0 4562 - F LTE\_feMob-Core

[R2-2101028](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2101028.zip) Dummifying the field intraFreqMultiUL-TransmissionDAPS Nokia, Nokia Shanghai Bell, MediaTek, Intel Corporation CR Rel-16 36.306 16.3.0 1803 - F LTE\_feMob-Core

[R2-2101360](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2101360.zip) Clarification on DAPS HO Capability Apple discussion Rel-16 NR\_Mob\_enh-Core

**Discussion:** It was probably clear from the RAN2#112-e meeting discussion that only the intraFreqMultiUL-TransmissionDAPS parameter was to be dummified but power sharing related ones would remain. Apple seems to have a bit different understanding of this. However, given that there may have been last minute rush due to limited time, something has been missed.

**Q1: What is the understanding from the companies about what was discussed related to the need and subsequent dummifying of *intraFreqMultiUL-TransmissionDAPS****?*

|  |  |
| --- | --- |
| **Company** | **View** |
| Nokia, Nokia Shanghai Bell | [Proponent] We think only the intraFreqMultiUL-TransmissionDAPS needs to be dummified but we are open to understand the technical background from the company that thinks otherwise. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

**Summary:**

**Rapporteur's Proposal:**

## 2.2 Understanding of DAPS in BWC-A band

The following CR was submitted:

[R2-2101710](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2101710.zip) Understanding of DAPS in BWC-A band Huawei, HiSilicon discussion Rel-16 NR\_Mob\_enh-Core

The contribution has observations but there are no concrete proposals. So we can discuss if companies can relate to the observations or have different view.

|  |
| --- |
| **Observation 1: UE can include two or more FSperCCs in BWC-A band to support DAPS handover.**  **Observation 2: it can be left for network implementation to configure DAPS in a BWC-A band, i.e. for intra-freq DAPS, network can configure source cell and target cell based on two FSperCCs within one BWC-A band; for inter-freq DAPS, network only configures source cell or target cell based on one FSperCC in one BWC-A band.**  **Observation 3: for BWC-A band, UE can indicate intra and inter freq DAPS UE capabilities in different BCs to enable different featuresets for these two cases, e.g. UE indicates intra-freq DAPS UE capability in a single-band BC, and indicates inter-freq DAPS UE capability in a multiple-band BC.** |

**Q2: Do companies support the observations in** [R2-2101710](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2101710.zip)?

|  |  |
| --- | --- |
| **Company** | **Agree/Disagree** |
| Nokia, Nokia Shanghai Bell | In our understanding, current specification restricts UE to report more than 1 CC FSPCC if it indicates BW class A. But we think we understand the intention of O1-O2 but think this is optimization over Rel-16 functionality and not so important.  About O3, we think there is a point we would like to clarify. It is our understanding from the network perspective that When this intra or inter frequency DAPS capability is included in a band combination with a single band entry and a single CC entry (i.e. non-CA band combination), the network may configure intra/inter-frequency DAPS to the UE as long as the UE supports CA in any single band or in any band combination. For this meeting we had prepared CR drafts but did not submit them as we thought this was general understanding of the companies. We are also fine to clarify this formally in TS 38.306. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

**Summary:**

**Rapporteur's Proposal:**

## 2.3 Capability coordination for DAPS

The following was submitted:

*Capability coordination for DAPS:*

[R2-2100618](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2100618.zip) DAPS capability coordination between source and target Intel Corporation discussion Rel-16 NR\_Mob\_enh-Core, LTE\_feMob-Core

[R2-2101712](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2101712.zip) Discussion on inter-node signalling for DAPS UE capability coordination Huawei, HiSilicon, MediaTek Inc., Qualcomm Incorporated, China Telecom, China Unicom discussion Rel-16 NR\_Mob\_enh-Core

[R2-2100486](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2100486.zip) Inter-node signalling for UE capability coordination in DAPS handover Ericsson discussion Rel-16 TEI16

*(moved from 6.7.3)*

**Discussion:**

**Option 1:** Support proposal in [R2-2100618](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2100618.zip) i.e. No changes are needed. The target can know what capability has been used in source based on source configuration and can use the rest of capability based on any of the UE supported DAPS combinations.

|  |
| --- |
| Observation 1: Based on the source configuration in indicated in handover preparation message the target knows which capability is used in source;  Observation 2: The target cannot know the exactly which bandcombination FeatureSetCombinationDAPS the source is using if the same source capability match multiple bandcombination FeatureSetCombinationDAPS.  Observation 3: The target needs to select the combination which not exceed the UE DAPS capability taking into the account the configuration used in the source.  Proposal: No changes are needed. The target can know what capability has been used in source based on source configuration and can use the rest of capability based on any of the UE supported DAPS combinations. |

**Option 2:** Support INM change based on [R2-2101712](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2101712.zip) & [R2-2100486](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2100486.zip).

|  |
| --- |
| Set of proposals from [R2-2101712](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2101712.zip)  Proposal 1: inter-node signalling is introduced for DAPS UE capability coordination.  Proposal 2: source gNB indicates the following elements to target gNB:   1. Allowed BC list; 2. Source band in every BC; 3. Allowed FS list in every BC; 4. Downlink FSperCC selected in source cell; 5. Uplink FSperCC selected in source cell.   Set of proposals from [R2-2100486](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_113-e/Docs/R2-2100486.zip)  Proposal 1 Adopt option B (inter-node signalling is added for UE capability coordination between source and target during DAPS handover).  Proposal 2 The source indicates the allowed BCs selected band entry and selected FSpCC to target.  Proposal 3 The inter-node signalling in proposal 2 is introduced for both NR and LTE. |

**Q3: Do companies agree with Option 1 or Option 2.**

|  |  |
| --- | --- |
| **Company** | **Views** |
| Nokia, Nokia Shanghai Bell | We think Option 1 would work i.e. target has the knowledge of the source configuration especially the PCell configuration and also has the corresponding UE capability.  One could think of Option 2 when the target would want to quickly know which FSPCC was used and what is the source band information so that the target can find a band combination that contains the {Source Band, Source FSPCC used for PCell}. It seems enough that the source mentions the band that it proposes the allocation of the single CC with the FeatureSetperCC property it wants to select. The target knows which band it wants to pick from and it can consult the BC list to see if there is at least one BC that has both these bands listed.  Furthermore, there seems to be a logical error in the CR proposed by Huawei.  FeatureSetPerCCEntryIndex ::= INTEGER (1.. maxNrofServingCells)  The index of per CC seems restricted from 1..32? whereas the list of CC's could have upto 1024 so ideally one should be able to indicate the correct index?  So, even if Option 1 would work Option 2 would be more efficient. Or do the proponent companies think Option 1 cannot work at all? |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

**Summary:**

**Rapporteur's Proposal:**

# 3 Conclusions

## 3.1 CRs that can be agreed as is

## 3.2 CRs that can be agreed with some changes / merges with other CRs

## 3.3 CRs that require online discussion

## 3.4 CRs that should not be pursued