3GPP TSG-RAN WG2 Meeting #113 Electronic R2-210XXXX

Elbonia, 25 January – 5 February 2020

**Agenda item: 6.8.2**

**Source: Rapporteur (Nokia)**

**Title: [AT113-e][220][DCCA] Stage-2, Fast Scell activation and early measurements (Nokia)**

**WID/SID: LTE\_NR\_DC\_CA\_enh-Core-**

**Release: Release 16**

**Document for: Discussion and Decision**

# 1 Introduction

This is discussion document for the email:

* [AT113-e][220][DCCA] Stage-2, Fast Scell activation and early measurements (Nokia)

Scope:

* + - Discuss corrections under 6.8.x marked for this discussion to see which CRs could be agreeable
		- Some (or even all) CRs may be merged together if seen needed

 Intended outcome:

* + - Discussion summary in R2-2101966 (by email rapporteur).
		- Agreeable CRs (if any)

 Deadline for providing comments, for rapporteur inputs, conclusions and CR finalization:

* + - Initial deadline (for companies' feedback): 1st week Thu, UTC 0900
		- Initial deadline (for rapporteur's summary in R2-2101966): 1st week Fri, UTC 09:00
		- Deadline for CR finalization: 2nd week Thu, UTC 1000

where following documents are to be treated:

### 6.8.1 General and Stage-2 Corrections

By Email [220] (1+2)

Stage-2 corrections:

[R2-2101400](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2101400.zip) CR on support of NR-DC within the same gNB-DU ZTE Corporation, Sanechips CR Rel-16 37.340 16.4.0 0246 - F LTE\_NR\_DC\_CA\_enh-Core

[R2-2101479](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2101479.zip) Corrections on UL power sharing Huawei, HiSilicon, ZTE Corporation (rapporteur) CR Rel-16 37.340 16.4.0 0248 - F NR\_newRAT-Core, LTE\_NR\_DC\_CA\_enh-Core

[R2-2101728](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2101728.zip) Corrections on UL power sharing vivo CR Rel-16 37.340 16.4.0 0250 - F LTE\_NR\_DC\_CA\_enh-Core

### 6.8.2 Fast Scell activation

By email [220] (1)

TCI state corrections:

[R2-2101747](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2101747.zip) Correction on tci-PresentInDCI ASUSTeK CR Rel-16 38.331 16.3.1 2436 - F LTE\_NR\_DC\_CA\_enh-Core

* Revised in [R2-2101942](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2101942.zip)

[R2-2101942](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2101942.zip) Correction on tci-PresentInDCI ASUSTeK CR Rel-16 38.331 16.3.1 2436 1 F LTE\_NR\_DC\_CA\_enh-Core [R2-2101747](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2101747.zip)

By Email [220] (3)

*Miscellaneous EMR corrections:*

[R2-2101570](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2101570.zip) Clarification on sCellState configuration upon SCell modification ZTE Corporation, Sanechips CR Rel-16 38.331 16.3.1 2422 - F LTE\_NR\_DC\_CA\_enh-Core

*(moved from 6.8.3)*

[R2-2100303](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2100303.zip) Corrections on condition of idle-inactive measurement configuration update OPPO CR Rel-16 38.331 16.3.1 2318 - F LTE\_NR\_DC\_CA\_enh-Core

[R2-2100304](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2100304.zip) Clarification on carrier frequency in MeasIdleConfigSIB OPPO CR Rel-16 38.331 16.3.1 2319 - F LTE\_NR\_DC\_CA\_enh-Core

By Email [220] (3)

*BWP-related corrections:*

[R2-2100305](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2100305.zip) Clarification on UE behaviour due to entering dormant BWP OPPO CR Rel-16 38.321 16.3.0 1011 - F LTE\_NR\_DC\_CA\_enh-Core

[R2-2101500](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2101500.zip) Correction on BWP operation Samsung CR Rel-16 38.321 16.3.0 1036 - F LTE\_NR\_DC\_CA\_enh-Core

[R2-2101017](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2101017.zip) Correction on first active uplink BWP vivo CR Rel-16 38.331 16.3.1 2375 - F LTE\_NR\_DC\_CA\_enh-Core

# 2 Discussion

## 2.1 UL power sharing stage-2 updates

By Email [220] (1+2)

Stage-2 corrections:

[R2-2101400](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2101400.zip) CR on support of NR-DC within the same gNB-DU ZTE Corporation, Sanechips CR Rel-16 37.340 16.4.0 0246 - F LTE\_NR\_DC\_CA\_enh-Core

In the above paper it is proposed to clarify in stage 2 spec, that NR-DC can also be supported between different cells within the same DU:

|  |  |  |
| --- | --- | --- |
| Company | Need for CR | Comments |
| Nokia | Neutral | Intention seems tob e good and we agree with the technical aspects. So we are fine to agree on the CR but as there is no interoperability problems foreseen is the category correct to be F? |
|  |  |  |
|  |  |  |

[R2-2101479](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2101479.zip) Corrections on UL power sharing Huawei, HiSilicon, ZTE Corporation (rapporteur) CR Rel-16 37.340 16.4.0 0248 - F NR\_newRAT-Core, LTE\_NR\_DC\_CA\_enh-Core

[R2-2101728](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2101728.zip) Corrections on UL power sharing vivo CR Rel-16 37.340 16.4.0 0250 - F LTE\_NR\_DC\_CA\_enh-Core

Two above papers Want to ensure that all MR-DC arcthitecture options are covered by stage-2 power sharing. :

|  |  |  |
| --- | --- | --- |
| Company | Need for CR | Comments |
| Nokia | Yes | We think it is good to ensure stage-2 is covering all architecture options. We have preference to Huawei style of capturing the changes as in our view it is easier to read and understand.  |
|  |  |  |
|  |  |  |

## 2.2 Fast SCell activation

### 2.2.1 TCI state corrections

By email [220] (1)

TCI state corrections:

[R2-2101747](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2101747.zip) Correction on tci-PresentInDCI ASUSTeK CR Rel-16 38.331 16.3.1 2436 - F LTE\_NR\_DC\_CA\_enh-Core

* Revised in [R2-2101942](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2101942.zip)

[R2-2101942](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2101942.zip) Correction on tci-PresentInDCI ASUSTeK CR Rel-16 38.331 16.3.1 2436 1 F LTE\_NR\_DC\_CA\_enh-Core [R2-2101747](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2101747.zip)

The paper indicates that According to TS 38.331, in case of cross carrier scheduling, the network sets tci-PresentInDCI field to enabled for the ControlResourceSet used for cross carrier scheduling in the scheduling cell, whose constraint was introduced in Rel-15.

But in Rel-16 MR-DC above constraint was removed with the introdcution of enableDefaultBeamForCSS and the network is allowed to set tci-PresentInDCI field to disabled in the concerned case if enableDefaultBeamForCSS is configured. Therefore it is proposed to remove the constraint in TS 38.331 to avoid contradiction or confusion.

|  |  |  |
| --- | --- | --- |
| Company | Need for CR | Comments |
| Nokia | Yes | This seems to be valid observations and good to correct to avoid IOT problems in future. |
|  |  |  |
|  |  |  |

### 2.2.1 Miscellaneous EMR corrections

By Email [220] (3)

*Miscellaneous EMR corrections:*

[R2-2101570](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2101570.zip) Clarification on sCellState configuration upon SCell modification ZTE Corporation, Sanechips CR Rel-16 38.331 16.3.1 2422 - F LTE\_NR\_DC\_CA\_enh-Core

*(moved from 6.8.3)*

The CR states: In Rel-16, SCell can be directly activated upon SCell configuration (i.e. including sCellState in RRCReconfiguration message) in case of SCell addition, reconfiguration with sync, and resuming an RRC connection. However, in the current procedure text in section 5.3.5.5.9, upon SCell modification, the UE shall check whether the sCellState is included only in case of configuration of SCG SCells in RRC resume, but not for other cases where sCellState may be included in the SCell configuration as well, e.g. MCG SCells in RRC resume and SCells in reconfiguration with sync

|  |  |  |
| --- | --- | --- |
| Company | Need for CR | Comments |
| Nokia | Yes | CR has valid observations and proposed corrrection seems tob e corrrct. Best to agree to avoid any debate in future which cases are supported for direct activation.. |
|  |  |  |
|  |  |  |

[R2-2100303](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2100303.zip) Corrections on condition of idle-inactive measurement configuration update OPPO CR Rel-16 38.331 16.3.1 2318 - F LTE\_NR\_DC\_CA\_enh-Core

CR states: If the RRCRelease message with/without suspendConfig was received in response to an RRCResumeRequest or an RRCResumeRequest1, the measIdleConfig IE can be also included in the RRCRelease message. In this case, the UE may also need to update the idle measurement configuration according to the SIB11/4 immediately. But idle measurement configuration update is missing for the case of “from RRC\_INACTIVE to RRC\_INACTIVE/RRC\_IDLE”.

|  |  |  |
| --- | --- | --- |
| Company | Need for CR | Comments |
| Nokia | Possibly | Intention seems to be OK but we are not sure if change would cover also RRC\_INACTIVE -> RRC\_INACTIVE case as that probably cannot be considered as “entering“ state when one is already in corresponding state. Secondly we wonder if there is need to change anything as UE will monitorin SIB changes during the access procedure and thus second bullet (one below the proposed change) would triggert he procedure as well. |
|  |  |  |
|  |  |  |

[R2-2100304](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2100304.zip) Clarification on carrier frequency in MeasIdleConfigSIB OPPO CR Rel-16 38.331 16.3.1 2319 - F LTE\_NR\_DC\_CA\_enh-Core

CR states: In RAN2#107 meeting, RAN2 make a agreement as below and common understanding is that only async SSB is configured in SIB11. But the spec is not clear.

 The legacy SSB measurement configurations in NR SIB2/4 and LTE SIB24 are reused for NR early measurements performed in frequencies which are candidates of cell selection/reselection, i.e. not introduce new measurement configurations in NR/LTE SIB for these SSBs.

|  |  |  |
| --- | --- | --- |
| Company | Need for CR | Comments |
| Nokia | No | This seems tob e purely editorial (thus category wrong) and thus we do not really see need fort he CR.. |
|  |  |  |
|  |  |  |

### 2.2.1 BWP related corrections

By Email [220] (3)

*BWP-related corrections:*

[R2-2100305](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2100305.zip) Clarification on UE behaviour due to entering dormant BWP OPPO CR Rel-16 38.321 16.3.0 1011 - F LTE\_NR\_DC\_CA\_enh-Core

CR states: When entering dormant BWP, the UE stay the current UL BWP, but stop some UL behaviour. But the current spec has misleading word. “a BWP” here only means DL dormant BWP, and “the BWP” is also mean “a BWP”. However, when entering dormant BWP, the UE stop UL behaviour one the current active UL BWP.

|  |  |  |
| --- | --- | --- |
| Company | Need for CR | Comments |
| Nokia | No | We do not identify ambiquity in the existing text and thus see no need fort he change.. |
|  |  |  |
|  |  |  |

[R2-2101500](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2101500.zip) Correction on BWP operation Samsung CR Rel-16 38.321 16.3.0 1036 - F LTE\_NR\_DC\_CA\_enh-Core

CR states: According to the current specification, UE does not monitor the PDCCH for the BWP if a BWP is activated and the active DL BWP for the Serving Cell is dormant BWP.

However, for dormant BWP, UE should monitor the PDCCH for the BWP to leave dormant BWP based on instruction from PDCCH as specified in TS 38.213.

Moreover, whether to monitor the PDCCH for the BWP would not be specified as shown in the procedural text for activated BWP or deactivated BWP.

|  |  |  |
| --- | --- | --- |
| Company | Need for CR | Comments |
| Nokia | Possibly | If we understand correctly Samsung is saying that the cross carrier scheduling for the dormant BWP should be allowed to activate another BWP through DCI. However, is the BWP switch is regarded as "PDCCH monitoring for the BWP"?Secondly , if the change would be agreed, what should the UE do if NW indicates a DL assignment for the dormant BWP through X-scheduling? |
|  |  |  |
|  |  |  |

[R2-2101017](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_113-e%5CR2-2101017.zip) Correction on first active uplink BWP vivo CR Rel-16 38.331 16.3.1 2375 - F LTE\_NR\_DC\_CA\_enh-Core

CR states: The field description of firstActiveUplinkBWP-Id states that “If configured for an SCell, this field contains the ID of the uplink bandwidth part to be used upon MAC-activation of an SCell.”.

However, according to the TS 38.321, if an SCell is configured with sCellState set to activated upon SCell configuration, the MAC entity shall activate the DL BWP and UL BWP indicated by firstActiveDownlinkBWP-Id and firstActiveUplinkBWP-Id respectively. It means firstActiveUplinkBWP-Id also indicate the UL BWP to be used upon activation of an SCell via RRC configuration.

Given above, the current description of firstActiveUplinkBWP-Id is not right..

|  |  |  |
| --- | --- | --- |
| Company | Need for CR | Comments |
| Nokia | Yes | It is also our understanding that *firstActivbeXXXBWP-Id* is supposed to be used for direct Scell activation |
|  |  |  |
|  |  |  |

# 3 Conclusion

* Initial deadline (for rapporteur's summary in R2-2101966): 1st week Fri, UTC 09:00

# 4 Contact Information

|  |  |
| --- | --- |
| Company | Email |
| Nokia | jarkko.t.koskela@nokia.com |
|  |  |
|  |  |
|  |  |
|  |  |