**3GPP TSG- Meeting # *R2-210xxxx***

**, 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.331** | **CR** | **2303** | **rev** | 1 | **Current version:** | **16.3.1** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Clarification on the inter-frequency operation | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | OPPO, Nokia, Nokia Shanghai Bell, Samsung Electronics, MediaTek Inc. | | | | | | | | | |
| ***Source to TSG:*** | RAN2 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** |  | | | | |  | ***Date:*** | | | 2021-01-04 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | In RAN2#112, it is agreed that  R2-2010938 Summary of [AT112-e][709][V2X]: Left issue on inter-frequency operation (OPPO) OPPO discussion Rel-16 5G\_V2X\_NRSL-Core  Proposal 1 For NR-V2X, UE can keep camping on a carrier-1 and read V2X SIB on a carrier-2.  Proposal 2 RAN2 confirm, for the behaviour of “keeping camping on a carrier-1 while reading V2X SIB on a carrier-2” in NR-V2X, the V2X SIB at carrier-2 is applicable to both intra- and inter-frequency carrier configuration scenario, i.e., NR PC5 activity can happen at not only carrier-2 but also another carrier-3 (i.e., different from carrier-1 and carrier-2).  Proposal 3 Cell selection, intra- and iner-frequency cell reselection are all valid use cases of non-serving frequency measurement for NR-V2X.   * All the proposals are agreed.   However, this conclusion is not visible from RRC specification. Considering this discussion / isssue is triggered mainly due to the lack of clarity, it would be necessary to reflect the agreement in RRC specification, to avoid misunderstanding in the future. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | A note is added in section 5.2.2.3.2 to clarify UE behavior as stated in the agreement is allowed.  **Impact analysis**  Impacted 5G architecture options:  NR SA  Impacted functionality:  Inter-frequency operation for NR SL  Inter-operability:   1. If UE implements according to the CR and the network does not, there is no inter-operability issue, since the SL activity at non-serving frequency does not relate to the network operation at serving frequency. 2. If the network implements according to the CR and the UE does not, there is no inter-operability issue, since i the SL activity at non-serving frequency does not relate to the network operation at serving frequency. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The UE behavior is still unclear in the RRC specification. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.2.2.3.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

*Start Change*

5.2.2.3.2 Acquisition of an SI message

For SI message acquisition PDCCH monitoring occasion(s) are determined according to *searchSpaceOtherSystemInformation*. If *searchSpaceOtherSystemInformation* is set to zero, PDCCH monitoring occasions for SI message reception in SI-window are same as PDCCH monitoring occasions for *SIB1* where the mapping between PDCCH monitoring occasions and SSBs is specified in TS 38.213[13]. If *searchSpaceOtherSystemInformation* is not set to zero, PDCCH monitoring occasions for SI message are determined based on search space indicated by *searchSpaceOtherSystemInformation*. PDCCH monitoring occasions for SI message which are not overlapping with UL symbols (determined according to *tdd-UL-DL-ConfigurationCommon*) are sequentially numbered from one in the SI window. The [x×N+K]th PDCCH monitoring occasion (s) for SI message in SI-window corresponds to the Kth transmitted SSB, where x = 0, 1, ...X-1, K = 1, 2, …N, N is the number of actual transmitted SSBs determined according to *ssb-PositionsInBurst* in *SIB1* and X is equal to CEIL(number of PDCCH monitoring occasions in SI-window/N). The actual transmitted SSBs are sequentially numbered from one in ascending order of their SSB indexes. The UE assumes that, in the SI window, PDCCH for an SI message is transmitted in at least one PDCCH monitoring occasion corresponding to each transmitted SSB and thus the selection of SSB for the reception SI messages is up to UE implementation.

When acquiring an SI message, the UE shall:

1> determine the start of the SI-window for the concerned SI message as follows:

2> if the concerned SI message is configured in the *schedulingInfoList*:

3> for the concerned SI message, determine the number *n* which corresponds to the order of entry in the list of SI messages configured by *schedulingInfoList* in *si-SchedulingInfo* in *SIB1*;

3> determine the integer value *x = (n – 1) × w*, where *w* is the *si-WindowLength*;

3> the SI-window starts at the slot #*a*, where *a* = *x* mod N, in the radio frame for which SFN mod *T* = FLOOR(*x*/N), where *T* is the *si-Periodicity* of the concerned SI message and N is the number of slots in a radio frame as specified in TS 38.213 [13];

2> else if the concerned SI message is configured in the *pos-SchedulingInfoList* and *offsetToSI-Used* is not configured:

3> create a concatented list of SI messages by appending the *pos-SchedulingInfoList* in *posSI-SchedulingInfo* in *SIB1 to schedulingInfoList* in *si-SchedulingInfo* in *SIB1*

3> for the concerned SI message, determine the number *n* which corresponds to the order of entry in the concatenated list;

3> determine the integer value *x = (n – 1) × w*, where *w* is the *si-WindowLength*;

3> the SI-window starts at the slot #*a*, where *a* = *x* mod N, in the radio frame for which SFN mod *T* = FLOOR(*x*/N), where *T* is the *posSI-Periodicity* of the concerned SI message and N is the number of slots in a radio frame as specified in TS 38.213 [13];

2> else if the concerned SI message is configured by the *pos-SchedulingInfoList* and *offsetToSI-Used* is configured:

3> determine the number *m* which corresponds to the number of SI messages with an associated *si-Periodicity* of 8 radio frames (80 ms), configured by *schedulingInfoList* in *SIB1*;

3> for the concerned SI message, determine the number *n* which corresponds to the order of entry in the list of SI messages configured by *pos-SchedulingInfoList* in *SIB1*;

3> determine the integer value *x* = *m* *× w +* (*n* – 1*)* *× w*, where *w* is the *si-WindowLength*

3> the SI-window starts at the slot #*a*, where *a* = *x* mod N, in the radio frame for which SFN mod *T* = FLOOR(*x*/N), where *T* is the posSI*-Periodicity* of the concerned SI message and N is the number of slots in a radio frame as specified in TS 38.213 [13];

1> receive the PDCCH containing the scheduling RNTI, i.e. SI-RNTI in the PDCCH monitoring occasion(s) for SI message acquisition, from the start of the SI-window and continue until the end of the SI-window whose absolute length in time is given by *si-WindowLength*, or until the SI message was received;

1> if the SI message was not received by the end of the SI-window, repeat reception at the next SI-window occasion for the concerned SI message in the current modification period;

NOTE 1: The UE is only required to acquire broadcasted SI message if the UE can acquire it without disrupting unicast data reception, i.e. the broadcast and unicast beams are quasi co-located.

NOTE 2: The UE is not required to monitor PDCCH monitoring occasion(s) corresponding to each transmitted SSB in SI-window.

NOTE 3: If the concerned SI message was not received in the current modification period, handling of SI message acquisition is left to UE implementation.

NOTE 4: A UE in RRC\_CONNECTED may stop the PDCCH monitoring during the SI window for the concerned SI message when the requested SIB(s) are acquired.

NOTE 5: A UE capable of NR sidelink communication and configured by upper layers to perform NR sidelink communication on a frequency, may acquire *SIB12* from a cell other than current serving cell (for RRC\_INACTIVE or RRC\_IDLE) or current PCell (for RRC\_CONNECTED), if *SIB12* of current serving cell (for RRC\_INACTIVE or RRC\_IDLE) or current PCell (for RRC\_CONNECTED) does not provide configuration for NR sidelink communication for the frequency, and if the other cell providing configuration for NR sidelink communication for the frequency meets the S-criteria as defined in TS 38.304 [20].

1> perform the actions for the acquired SI message as specified in sub-clause 5.2.2.4.

*End of Change*