**3GPP TSG-RAN WG2 Meeting #113-eR2-21xxxxx**

**Online, 25th Jan – 5th Feb 2021**

**Agenda item:** 8.13.2

**Source:** ZTE Corporation, Sanechips

**Title:** Report of[Offline-888][NRR17 SONMDT] Indication for 2-step RACH (ZTE)

**Document for:** Discussion and Agreement

# 1 Introduction

This is to report the result of the following email discussion at the RAN2#113-e meeting [1].

\* [AT113-e][888][NR/R17 SON/MDT]  Indication for 2-step RACH (ZTE)

* Working on the FFS part that “The RA report includes as indication of whether the DL beam quality, associated to the used 2 step RA resource, is above or below the msgA-RSRP-Threshold.”

    Intended outcome: Agreeable WF

Deadline: Thursday 04/02/2021

Based on email confirmation received from Chair, this email discussion also considers following proposals from paper R2-2102269 [2]:

* “Include the measured DL RSRP obtained just before performing RACH procedure in RA report, which can be used to optimize the RSRP threshold for RACH type selection.”

According to the chair’s guidance, this report is used to collect companies’ views on the need of inclusion of DL beam quality indication associated to the used 2 step RA resource [1], and to find an agreeable way forward. Companies are requested to provide their opinions before the deadline Thursday 04/02/2021, UTC 11:00.

# 2 Contact Information

To make it easier to find the correct contact delegate in each company for potential follow-up questions, the rapporteur encourages the delegates who provide input to provide their contact information in this table:

|  |  |
| --- | --- |
| Company | Contact: Name (E-mail) |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# 3 Discussion

During the RAN2#113-emeeting following agreements have been achieved for RA report[1]:

|  |
| --- |
| 2-step RA related SON:  1 The reporting granularity of whether the DL beam quality, associated to the used 2 step RA resource, is above or below the msgA-RSRP-ThresholdSSB is per-RA-attempt.  2 The RA report includes an indication that enables the network to know that the fallback from 2 step RA to 4 step RA was performed by the UE. FFS: Implicit vs explicit indication.  Choose ‘per RA procedure’ for the granularity of RA type (2 step RA vs 4 step RA) indication. FFS: Implicit vs explicit indication. |

The controversial issues are whether to include DL beam quality information associated to RA type selection in RA report. If does, how to address this information in RA report.

In order for companies to make informative decisions, some background knowledge regarding to *msgA-RSRP-Threshold* are given as follows:

*msgA-RSRP-Threshold* is an RSRP threshold for selection between 2-step RA type and 4-step RA type, which will only be used once during RA initialization procedure. According to the field description as specified in 38.331[3], this parameter is **mandatory present if both 2-step random access type and 4-step random access type are configured in the BWP, otherwise the field is not present.**

According to TS 38.321[4], in case both 2stepRA and 4step resource is configured for selected BWP, UE will first compare the **RSRP of downlink pathloss reference** with configured *msgA-RSRP-Threshold* to determine RA type. UE sets RA type to 2stepRA when the downlink pathloss reference is above *msgA-RSRP-Threshold*, otherwise UE sets RA type to 4stepRA. After determination of RA type, UE will for each RA attempt compares the **RSRP of beams** (SSBs/CSI-RSs) with *rsrp-ThresholdSSB*/*rsrp-ThresholdCSI-RS* (if RA type is 4stepRA) or *msgA-RSRP-ThresholdSSB* (if RA type is 2stepRA) to select suitable beam for RA attempt.

According to the summary in [5], companies in favor of the include the beam quality indication associated to *msgA-RSRP-Threshold* consider such information is helpful for NW to know whether the configured threshold for RA type selection is appropriate or not. While for opponent companies, they think UE will only use this threshold once during the whole RA procedure , and this information shall be able to deduce based on the RA type selected, there is no need to duplicate this information in RA report.

**Q1: Do companies agree to include the DL beam quality indication used to indicate whether used 2 step RA resource is above or below the *msgA-RSRP-Threshold* in RA report? If does, please also provide the preferred granularity (e.g., per RA procedure or per RA attempt) in the detailed comments.**

|  |  |  |
| --- | --- | --- |
| Company | Agree/Disagree | Detailed Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

It is proposed in [2] that comparing to the beam quality indication, the actual measured DL RSRP obtained just before performing RACH procedure is more useful for NW to optimize the 2step RACH configuration. Based on the detailed discussion, here the DL RSRP refers to the RSRP of DL pathloss reference, to avoid misunderstanding, the complete terminology“RSRP of DL pathloss reference” is used in the proposal instead of “DL RSRP”.

**Q2: Do companies agree to include the measured RSRP of DL pathloss reference** **obtained just before performing RACH procedure in RA report? If does, please also provide the preferred granularity (e.g., per RA procedure or per RA attempt) in the detailed comments.**

|  |  |  |
| --- | --- | --- |
| Company | Agree/Disagree | Detailed Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Conclusion:**

# 4 Conclusion

**TBD**

# 5 References

1. R2-113-e SONMDT HuNan 2021-01-29-0630 UTC
2. R2-2102269 Discussion on 2-step RACH reporting for SON OPPO discussion Rel-17 NR\_ENDC\_SON\_MDT\_enh-Core
3. 38.331 NR; Radio Resource Control (RRC) protocol specification (Release 16)
4. 38.321 NR; Medium Access Control (MAC) protocol specification (Release 16)
5. R2-2102265 Summary of AI 8.13.2 Ericsson discussion Rel-17 NR\_ENDC\_SON\_MDT\_enh-Core