**3GPP TSG-RAN WG2 #113bis-e *R2-210xxxx***

**E-meeting, April 2021**

Agenda Item: 6.2.2

Source: OPPO

Title: Summary of [704]

Document for: Discussion, Decision

# Introduction

This is to discuss the [704] as follows.

* [AT113bis-e][704][V2X/SL] PSFCH transmission (OPPO)

 **Scope:** Discuss what the current TX synchronization procedure is and what is limitation of PSFCH transmission, and what is RAN2 common understanding on PSFCH transmission (e.g. PSFCH is transmitted regardless of its own synchronization defined in the procedure or PSFCH may not be transmitted due to limitation of single synchronization defined in the procedure).

 **Intended outcome:** Discussion summary in R2-2104469.

 **Deadline:** 4/19, 14:00 (UTC).

# Discussion

According to sync procedure of R16 NR-V2X, specified in TS 38.331 section 5.8.6, for two UEs communicating via PC5



Figure 1 Sync procedure for UEs communication via PC5

Each UE (UE1 and UE2) based on the sync source in the proximity (gNB, GNSS and UE), and the sync configuration, to derive the sync reference, of which the sync is used as the reference of Tx sync of its own:

* UE1 to derive the sync for UE1 transmission, e.g., sync-1;
* UE2 to derive the sync for UE2 transmission, e.g., sync-2;

Since besides the GNSS, the gNB/UE sync reference may be different for different UE’s proximity, so the Tx-sync of each UE may be different.

Actually, the issue has previously already identified by RAN4, in LS of **R4-1912826**

*RAN4 is discussing the need of requirements for sidelink synchronization when multiple asynchronized sources are presented. RAN4 noticed that RAN1 agreed the following synchronization source priority.*

*[…]*

*With the above synchronization source priority, RAN4 identifies the following scenarios in which timing misalignment may exist between UEs communicating on SL*

* *UE1 and UE2 synced to two different gNBs, but the 2 gNBs are with different timing*
* *UE1 and UE2 synced to two different eNBs, but the 2 eNBs are with different timing*
* *UE1 synced to eNB, UE2 synced to gNB, eNB and gNB are with different timing*

*RAN4 would ask RAN2 to check if there is any signalling available for timing adjustment in the above scenarios where multiple gNB/eNB with different timing are presented.*

Where sync-1 and sync-2 are different, as shown below, symbol boundary is not aligned, which can be even larger than CP.



Figure 2 Un-sync-ed PSCCH/PSSCH Tx, and PSCCH/PSSCH Rx (when FB disabled)

According to the latest RAN1 discussion on UE feature, i.e., R1-2005111, RAN1 has evaluated the 3 alternatives below:

**Alt. 1: Delete FG 15-24 (i.e., UE supports sidelink reception using up to one synchronization reference in a band)**

**Alt. 2:**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 15-24 | Support of multiple synchronization references | 1) UE can support sidelink reception using up to A synchronization reference~~s~~ Rx timings in a ~~carrier/BWP~~ band | At least one of 15-1, 15-2, 15-3 | Yes | No | UE supports only a single synchronization reference in a ~~carrier/BWP~~ band. | Per band | N.A. | N.A. | N.A. | Component-1 candidate value set: {~~1,~~ 2, 3, 4}Note: A UE that does not support FG 15-24 supports sidelink reception using up to one synchronization reference RX timingin a band | Optional with capability signalling |

**Alt. 3:**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 15-24 | ~~Support of multiple synchronization references~~Number of tx and rx timings | 1. ~~UE can support sidelink reception using up to A synchronziaion references in a carrier/BWP~~
2. This parameter indicates the number of multiple reference TX/RX timings in a band for V2X sidelink communication
 | At least one of 15-1, 15-2, 15-3 | Yes | No | UE supports only a single synchronization reference in a ~~carrier/BWP~~ band. | Per band | N.A. | N.A. | N.A. | Component-1 candidate value set: {~~1,~~ 2, 3, 4}Note: A UE that does not support FG 15-24 supports sidelink reception using up to one synchronization reference TX/RX timing in a band | Optional with capability signalling |

And finally reached the following conclusion

**Conclusion:**

For Rel-16, UE supports sidelink transmission and reception using one reference timing.

1. RAN1 has concluded on single sync limitation for both Tx and Rx.

On the other hand, according to rapporteur understanding, in LTE (equivalent to NR when feedback is disabled), this problem can be solved in a way that the UE can perform

* Tx for PSCCH/PSSCH on sync-1;
* Rx for PSCCH/PSSCH on sync-2;

Please note that in this case, both UEs keep a single sync for Tx and for Rx. But when extending this scenario to 3 or more UEs, and when extending this to broadcast case, it is hard to secure single sync limitation for all the UEs as agreed by RAN1 for R16 NR-V2X.

1. In LTE, two UEs with different Tx-Sync can communicate with each other.

On the other hand, however, as copied from LTE, NR also include the Rx-sync configuration in pool configuration



This parameter is to help the UEs in cell-1, following sync-1, to get the sync-2 from cell-2, for reception of data of sync-2, i.e., it hints the scenario where R16 NR-V2X UEs bases on the Rx-sync configuration for each Rx pool, to perform reception on another sync.

1. ASN.1 in R16 NR-V2X includes the configuration for UEs in cell-1 following sync-1, to get the sync-2 from cell-2 for reception of data of sync-2.

So given all the colliding information above, we can start from checking the companies view. Maybe, we can start from no PSFCH case, i.e., exactly the same case as in LTE, where HARQ FB is disabled.

So Q1-1 is to ask for confirmation from companies whether this scenario can happen in R16 NR-V2X.

**Q1: In R16 NR V2X, for HARQ FB disabled case (i.e., same as LTE), is it possible that two UEs using different Tx-sync (larger than CP), can communicate with each other or not?**

**Interpretation-1 Yes, as in LTE, UE1 use its Tx-sync to transmit PSCCH/PSSCH to UE2, and UE1 receive PSCCH/PSSCH from UE2 based on UE2’s Tx-sync;**

**Interpretation-2: No, different from LTE, UE1 use its Tx-sync to transmit PSCCH/PSSCH to UE2, and also use the same sync to receive PSCCH/PSSCH from other nearby UEs**

* **2A: R16 NR-V2X only targets at the scenario where all UEs always have the same Tx-sync or at least Tx-sync with difference less than CP;**
* **2B: It may happen in R16 NR-V2X that neighbouring UE have different Tx-Sync (larger than CP), but if that happens, UEs cannot communicate with UEs who have Tx-sync with difference larger than CP**

|  |  |  |
| --- | --- | --- |
| Company | Interpretation | Comment |
| OPPO | 2B | Even though 1 is feasible for 2 UEs, it does not work for >= 3UEs and for G/B-cast case, considering the conclusion/limitation from R1 on the sync Tx/Rx sync.2A is not possible considering the existence of UE-based sync. |
|  |  |  |
|  |  |  |
|  |  |  |

The second step is what is the companies understanding of the current spec when HARQ FB is **enabled**, i.e., different from LTE, what the UE behaviour is.



Figure 3 Un-sync-ed PSCCH/PSSCH Tx + PSFCH Rx, and PSCCH/PSSCH Rx + PSFCH Tx (when FB enabled)

**Q2: In R16 NR V2X, is it possible that two UEs communicating via PC5 adopt different Tx-sync, for HARQ FB enabled case?**

**Interpretation-1: Yes**

* **1A: But PSFCH transmission cannot be performed on the different sync;**
* **1B: PSFCH transmission can be performed, but will be performed using the Tx-sync same as for PSCCH/PSSCH;**
* **1C: PSFCH transmission can be performed regardless of the sync used for PSCCH/PSSCH (i.e., the Tx-sync for PSFCH and for PSCCH/PSSCH can be different)**

**Interpretation-2: No, different from LTE, UE1 use its Tx-sync to transmit PSCCH/PSSCH to UE2, and also use the same sync to receive PSCCH/PSSCH from other nearby UEs**

* **2A: R16 NR-V2X only targets at the scenario where all UEs always have the same Tx-sync or at least Tx-sync with difference less than CP;**
* **2B: It may happen in R16 NR-V2X that neighbouring UE may have different Tx-Sync (larger than CP), and if that happens, UEs cannot communicate with UEs who have Tx-sync with difference larger than CP**

|  |  |  |
| --- | --- | --- |
| Company | Interpretation | Comment |
| OPPO | 2B | see response above. |
|  |  |  |
|  |  |  |
|  |  |  |

And for Q1/Q2, it is helpful to understand the consequence.

If one holds the view on 2A for Q1 and/or Q2, given the specified sync selection procedure

4> if *sl-SyncPriority* corresponding to the concerned frequency is set to *gnbEnb*:

5> UEs of which SLSSID is part of the set defined for in coverage, and *inCoverage*, included in the *MasterInformationBlockSidelink* message received from this UE, is set to *true*, starting with the UE with the highest PSBCH-RSRP result (priority group 1);

5> UE of which SLSSID is part of the set defined for in coverage, and *inCoverage*, included in the *MasterInformationBlockSidelink* message received from this UE, is set to *false*, starting with the UE with the highest PSBCH-RSRP result (priority group 2);

5> GNSS that is reliable in accordance with TS 38.101-1 [15] and TS 38.133 [14] (priority group 3);

5> UEs of which SLSSID is 0, and *inCoverage*, included in the *MasterInformationBlockSidelink* message received from this UE, is set to *true,* or of which SLSSID is 0 and SLSS is transmitted on slot(s) indicated by *sl-SSB-TimeAllocation3*, starting with the UE with the highest PSBCH-RSRP result (priority group 4);

5> UEs of which SLSSID is 0 and SLSS is not transmitted on slot(s) indicated by *sl-SSB-TimeAllocation3*, and *inCoverage*, included in the *MasterInformationBlockSidelink* message received from this UE, is set to *false*, starting with the UE with the highest PSBCH-RSRP result (priority group 5);

5> UEs of which SLSSID is 337 and *inCoverage*, included in the *MasterInformationBlockSidelink* message received from this UE, is set to *false*, starting with the UE with the highest PSBCH-RSRP result (priority group 5);

5> Other UEs, starting with the UE with the highest PSBCH-RSRP result (priority group 6);

4> if *sl-SyncPriority* corresponding to the concerned frequency is set to *gnss*, and *sl-NbAsSync* is set to *true:*

5> UEs of which SLSSID is 0, and *inCoverage*, included in the *MasterInformationBlockSidelink* message received from this UE, is set to *true*,or of which SLSSID is 0 and SLSS is transmitted on slot(s) indicated by *sl-SSB-TimeAllocation3*, starting with the UE with the highest PSBCH-RSRP result (priority group 1);

5> UEs of which SLSSID is 0 and SLSS is not transmitted on slot(s) indicated by *sl-SSB-TimeAllocation3*, and *inCoverage*, included in the *MasterInformationBlockSidelink* message received from this UE, is set to *false*, starting with the UE with the highest PSBCHS-RSRP result (priority group 2);

5> UEs of which SLSSID is 337 and *inCoverage*, included in the *MasterInformationBlockSidelink* message received from this UE, is set to *false*, starting with the UE with the highest PSBCH-RSRP result (priority group 2);

5> the cell detecteted by the UE as defined in 5.8.6.3 (priority group 3);

5> UEs of which SLSSID is part of the set defined for in coverage, and *inCoverage*, included in the *MasterInformationBlockSidelink* message received from this UE, is set to *true*, starting with the UE with the highest PSBCH-RSRP result (priority group 4);

5> UE of which SLSSID is part of the set defined for in coverage, and *inCoverage*, included in the *MasterInformationBlockSidelink* message received from this UE, is set to *false*, starting with the UE with the highest PSBCH-RSRP result (priority group 5);

5> Other UEs, starting with theUE with the highest S-RSRP result (priority group 6);

4> if *sl-SyncPriority* corresponding to the concerned frequency is set to *gnss*, and *sl-NbAsSync* is set to *false:*

5> UEs of which SLSSID is 0, and *inCoverage*, included in the *MasterInformationBlockSidelink* message received from this UE, is set to *true*, or of which SLSSID is 0 and SLSS is transmitted on slot(s) indicated by *sl-SSB-TimeAllocation3*, starting with the UE with the highest PSBCH-RSRP result (priority group 1);

5> UEs of which SLSSID is 0 and SLSS is not transmitted on slot(s) indicated by *sl-SSB-TimeAllocation3*, and *inCoverage*, included in the *MasterInformationBlockSidelink* message received from this UE, is set to *false*, starting with the UE with the highest PSBCHS-RSRP result (priority group 2);

5> UEs of which SLSSID is 337 and *inCoverage*, included in the *MasterInformationBlockSidelink* message received from this UE, is set to *false*, starting with the UE with the highest PSBCH-RSRP result (priority group 2);

5> Other UEs, starting with the UE with the highest PSBCH-RSRP result (priority group 3);

Rapporteur understand that even though network configuration can ensure sync between cells, and sync between gNB/GNSS, as long as UE-based sync reference is selected, there is no guarantee on the sync difference less than CP.

So good to check the view by companies

**Q2-1: If company holds the interpretation 2A to Q1 and/or Q2, what is your view to achieve that**

**Option-1: by network implementation (if this selected, please explain how)**

**Option-2: by UE implementation (if this selected, please explain how)**

**Option-3: other**

|  |  |  |
| --- | --- | --- |
| Company | Option | Comment |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Or if companies holds the interpretation of 2B:

Firstly, rapporteur understand it is against V2X design spirit that for safety reason, packet loss should be minimized as much as possible.

**Q2-2a: if company holds the interpretation 2B to Q1 and/or Q2, will it cause reception failure due to sync reference difference between nearby UEs in a V2X system?**

* **Yes**
* **No**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comment |
| OPPO | Yes | It is very unfortunate that R1 ends up with a solution different from LTE that may cause reception failure (to us, it can be easily solved by allowing more than 1 Rx sync), but that is the consequence. |
|  |  |  |
|  |  |  |
|  |  |  |

Secondly, it seems colliding with the ASN.1 configuration of Rx-sync in pool configuration, i.e. since the UE will always relies on the Tx-sync to perform reception, what is the point to include a Rx-sync configuration in Rx pool?

|  |
| --- |
| ***sl-SyncConfigIndex***Indicates the synchronisation configuration that is associated with a reception pool, by means of an index to the corresponding entry *SL-SyncConfigList* of in *SIB12* for NR sidelink communication. |

**Q2-2b: if company holds the interpretation 2B to Q1 and/or Q2, do you agree that the sl-SyncConfigIndex-r16 in SL-ResourcePool-r16 is useless, and thus can be dummified?**

* **Yes**
* **No**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comment |
| OPPO | Yes | Given the current R1 conclusion, we fail to understand how this parameter will work. |
|  |  |  |
|  |  |  |
|  |  |  |

1. xxx.

# Conclusion

We have the following proposal:

[Proposal 1 xxx.](#_Toc69160470)

# Reference

1. R2-2102881 Left issue on synchronization of PSSCH vs. PSFCH OPPO, Ericsson, Apple, Nokia, Nokia Shanghai Bell discussion Rel-16 5G\_V2X\_NRSL-Core
2. R1-2005111, Summary of email discussion/approval [101-e-Post-NR-UE-Features-05]