3GPP TSG-RAN WG2 #116e R2-21xxxxx

Electronic Meeting, 1 – 12 November 2021

Agenda Item: 5.3.2 / 6.1.3.3

Source: Samsung

Title: [AT116-e][007][NR1516] PDCP (Samsung)

Release: Rel-15/16

Document for: Discussion and Decision

# 1 Introduction

This document is to handle the following email discussion:

* [AT116-e][007][NR1516] PDCP (Samsung)

Scope: Determine agreeable parts in a first phase, for agreeable parts agree on CRs. Treat [R2-2111027](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2111027.zip) (AI 5.3.2), [R2-2109945](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2109945.zip), [R2-2109946](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2109946.zip), [R2-2109947](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2109947.zip), [R2-2110757](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2110757.zip), [R2-2110758](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2110758.zip)

Intended outcome: Report, Agreed CRs if applicable

Deadline: Schedule 1

The following documents are to be treated in this email discussion:

## 5.3.2 RLC PDCP SDAP

[R2-2111027](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2111027.zip) On association between RLC entities and PDCP entity Huawei, HiSilicon discussion Rel-15 NR\_newRAT-Core

## 6.1.3.3 PDCP

[R2-2109945](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2109945.zip) Clarification on the ciphering of LTE EHC header Samsung discussion Rel-16 NR\_IIOT-Core

[R2-2109946](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2109946.zip) CR for the ciphering of LTE EHC header (Rel-15) Samsung CR Rel-15 36.323 15.6.0 0297 - F NR\_IIOT-Core

[R2-2109947](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2109947.zip) CR for the ciphering of LTE EHC header (Rel-16) Samsung CR Rel-16 36.323 16.4.0 0298 - A NR\_IIOT-Core

[R2-2110757](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2110757.zip) Clarification on joint EHC and RoHC operation MediaTek Inc. CR Rel-16 38.323 16.5.0 0083 - F NR\_IIOT-Core

[R2-2110758](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2110758.zip) Clarification on joint EHC and RoHC operation MediaTek Inc. CR Rel-16 36.323 16.4.0 0299 - F NR\_IIOT-Core

2 Contact Information

The rapporteur encourages the delegates who provide input to provide their contact information in the below table:

|  |  |
| --- | --- |
| Company | Contact: Name (E-mail) |
| Samsung (Donggun Kim) | s\_dg.kim@samsung.com |
| Huawei, HiSilicon (Chong Lou) | louchong@huawei.com |
| LG Electronics (SeungJune Yi) | seungjune.yi@lge.com |
| ZTE Corporation | Dong.fei@zte.com.cn |
| Nokia | benoist.sebire@nokia.com |
| MediaTek | pradeep[dot]jose[at]mediatek[dot]com |
|  |  |
|  |  |
|  |  |
|  |  |

# 3 Discussion

## [R2-2111027](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2111027.zip) On association between RLC entities and PDCP entity Huawei, HiSilicon discussion Rel-15 NR\_newRAT-Core

**Proposal 1: RAN2 to discuss whether it is possible to lift the restriction about the symmetric association between RLC entities and PDCP entity in PDCP spec, to allow building asymmetric UM RLC entities for a radio bearer with marginal spec impact but offer much more flexibility.**

**Q1. Do you agree to lift the restriction about the symmetric association between RLC entities and PDCP entity specified in 38.323 to allow building asymmetric UM RLC entities for a radio bearer?**

|  |  |  |
| --- | --- | --- |
| Company | Agree/Disagree | Comments |
| Huawei, HiSilicon | Agree | Proponent, we don’t see much value to set this limitation in spec. |
| LGE | Comments | We have some sympathy for proposal. But, this change should not be considered for Rel-15/16. It could be discussed for TEI17. |
| ZTE | Not for R15 | It can only be discussed in TEI 17 |
| Nokia | Disagree | A more practical correction would be to not count RLC UM entities but regardless of the change, this should be TEI17. |
| MediaTek | Not for Rel15 | We do not see a reason to change Rel-15 specs for this. This can be discussed as part of TEI17 |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## [R2-2109945](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2109945.zip) Clarification on the ciphering of LTE EHC header Samsung discussion Rel-16 NR\_IIOT-Core

[R2-2109946](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2109946.zip) CR for the ciphering of LTE EHC header (Rel-15) Samsung CR Rel-15 36.323 15.6.0 0297 - F NR\_IIOT-Core

[R2-2109947](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2109947.zip) CR for the ciphering of LTE EHC header (Rel-16) Samsung CR Rel-16 36.323 16.4.0 0298 - A NR\_IIOT-Core

**Reason for change:**

In RAN2#107bis, RAN2 made the following agreements:

* The EHC function is in PDCP
* The EHC header is located after the SDAP header, and it is ciphered

However, it is not clear whether to cipher the EHC header in the current PDCP specification.

**Q2. Do you agree to clarify the ciphering of LTE EHC header in 36.323 given that RAN2 already clarified the ciphering of NR EHC header in 38.323 in the last meeting?**

|  |  |  |
| --- | --- | --- |
| Company | Agree/Disagree | Comments |
| Huawei, HiSilicon | Agree, but | We still don’t think it is essential. But we can follow the majority view. |
| LGE | Agree |  |
| ZTE | Follow the majorities | No strong view. |
| Nokia | agree |  |
| MediaTek | Agree |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q3. Which option do you prefer if you agree to clarify the ciphering of LTE EHC header in 36.323? or do you have any other suggestion?**

|  |
| --- |
| **Option 1 (LTE style)** 6.3.3 Data Length: Variable  The Data field may include either one of the following:  - Uncompressed PDCP SDU (user plane data, or control plane data); or  - Compressed PDCP SDU (user plane data only); or  - UDC header and UDC Data Block if UDC is configured.  - EHC header and compressed PDCP SDU if EHC is configured. |

If we go for Option 1, then one Rel-16 CR would be needed.

|  |
| --- |
| **Option 2 (NR style)** 6.3.3 Data Length: Variable  The Data field may include either one of the following:  - Uncompressed PDCP SDU (user plane data, or control plane data); or  - Compressed PDCP SDU (user plane data only); or  NOTE: All fields other than PDCP PDU header and MAC-I belong to Data field.‎ |

If we go for Option 2, then one Rel-15 CR and one Rel-16 CR would be needed.

|  |  |  |
| --- | --- | --- |
| Company | Preferred option | Comments |
| Huawei, HiSilicon | Option 2 with revisions | If we have to have a CR, we can compromise to Option 2 with revisions in order to align with NR spec, but we don’t think the last bullet of “UDC header and UDC Data Block if UDC is configured” should be removed. We see no issue with this bullet for the proposed NOTE. It is worthy noting that we should minimize the CR maintenance burden for developers especially it is just to beautify the LTE text. |
| LGE | Option 2 | We don’t understand Huawei’s concern. The NOTE covers UDC, and leaving the UDC bullet makes more confusion.  [LC]: Sorry I should be clearer when making the comment. Our concern is to remove the legacy text will cause more confusion for the developers to trace the CR history for internal implementation check. Given that Option 2 doesn’t affect the UDC bullet but to address EHC case, we don’t see a strong reason to remove LTE text and we can only compromise to add a generic NOTE. |
| Nokia | Option 2 with revisions | UDC header and UDC data block" line should not be removed since "UDC data block" is used instead of "Data" in PDU formats from section 6.2.14 till 6.2.16. |
| MediaTek | Option 2 with revisions | Agree with Nokia’s reasoning above |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q4. Do you agree to both** [**R2-2109946**](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2109946.zip) **(Rel-15 CR) and** [**R2-2109947**](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2109947.zip) **(Rel-16 CR) if you prefer Option 2?**

|  |  |  |
| --- | --- | --- |
| Company | Agree/Disagree | Comments |
| Huawei, HiSilicon | Agree with revisions | As above |
| LGE | Agree |  |
| Nokia | Agree with changes | See above |
| MediaTek | Agree with changes | See above |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## [R2-2110757](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2110757.zip) Clarification on joint EHC and RoHC operation MediaTek Inc. CR Rel-16 38.323 16.5.0 0083 - F NR\_IIOT-Core

[R2-2110758](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2110758.zip) Clarification on joint EHC and RoHC operation MediaTek Inc. CR Rel-16 36.323 16.4.0 0299 - F NR\_IIOT-Core

**Reason for change:**

When ROHC and EHC are jointly configured for a DRB, the current specifications require the EHC decompressor to bypass the ROHC decompressor for non-IP packets. When this operation was discussed in R2-109e, the understanding was that the EHC decompressor could detect the presence or absence of an IP header from the Ether type field in the Ethernet header (post decompression). Hence the following agreement was reached:

*When a DRB is configured with RoHC and EHC, the receiver/decompressor behaviour* ***for a packet that has non-IP Ethertype (after EHC decompression) is to bypass RoHC*** *and deliver the packet directly to higher layers.*

This agreement is currently captured in the PDCP specification as below:

*If a PDCP Data PDU including non-IP Ethernet packet is received from lower layers, the EHC decompressor shall bypass the ROHC decompressor and deliver the EHC decompressed non-IP Ethernet packet to upper layers*

However, the above requirement does not consider the case where the Ethernet header uses the Length field in place of the Ether type field. If the length field is used, there **is no way** for the EHC decompressor to know if the PDCP data PDU contains an IP packet or a non-IP packet, and the decompressor cannot meet the requirement above. Therefore, the specification needs to be updated to clarify that a mix of IP and non-IP packets can only be expected by the EHC decompressor, if the Ether type field is present in the Ethernet header.

|  |
| --- |
| **Proposed change**  5.12.7 Simultaneous configuration of ROHC and EHC  If both ROHC and EHC are configured for a DRB, the ROHC header shall be located after the EHC header. Figure 5.12.7-1 shows the location of the ROHC header and the EHC header in a PDCP Data PDU.      **Figure 5.12.7-1: Location of ROHC header and EHC header in a PDCP Data PDU**  If a PDCP SDU including non-IP Ethernet packet is received from upper layers, the EHC compressor shall bypass the ROHC compressor and submit the EHC compressed non-IP Ethernet packet to lower layers according to clause 5.2.1.  If a PDCP Data PDU including non-IP Ethernet packet is received from lower layers, the EHC decompressor shall bypass the ROHC decompressor and deliver the EHC decompressed non-IP Ethernet packet to upper layers according to clause 5.2.2.  If both ROHC and EHC are configured for a DRB, the DRB is only expected to have a mix of IP and non-IP packets if the Ethernet header contains the TYPE field. |

**Q5. Do you agree to** [**R2-2110757**](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2110757.zip) **(38.323) and** [**R2-2110758**](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116-e/Docs/R2-2110758.zip) **(36.323)?**

|  |  |  |
| --- | --- | --- |
| Company | Agree/Disagree | Comments |
| Huawei, HiSilicon |  | We think it is an internal UE implementation issue. Not sure if any spec update is needed on top of the previous agreement on “bypass ROHC/EHC for a non-IP packet”. Nevertheless, we understand the most critical issue is how to align the understanding on both transmitter and receiver. We need more time to check and tend to believe it is not a sensible/feasible approach to limit the network configuration.  *[MTK]: This isn’t a UE implementation issue. The same issue exists at the NW decompressor side when UL EHC is used. However, it’s a valid point that a better approach would be to align compressor and decompressor rather than limit NW configuration. A solution could be to specify that the RoHC compression is skipped if the Ethertype field is absent or if Ethertype field indicates that the packet is non-IP.* |
| LGE | Comments | We want to clarify first whether a mix of IP packet and non-IP packet is possible for one DRB. If mix is not allowed, the EHC decompressor can bypass the ROHC decompressor by configuration. Otherwise, internal check should be done by the EHC decompressor. But for internal check, we are wondering whether it is possible for the EHC decompressor to know whether the included field is LENGTH or TYPE field. We need more time to check whether the addressed problem is a real problem, and whether the proposed solution can solve the addressed problem.  *[MTK]: A mix of IP and non-IP packets are possible for an Ethernet PDU session as discussed in Rel-16. This is the reason why RoHC bypass behaviour was specified when EHC and RoHC are jointly configured. The EHC decompressor will know whether the included field is LENGTH or TYPE by the value indicated in the header.* |
| Nokia | Disagree | It is understood that EHC compressor and decompressor can identify if the PDCP SDU is an IP or non-IP Ethernet packet only if "Type" field is present in Ethernet header. If "Length" field is present in Ethernet header, EHC compressor cannot identify if it is an IP or non-IP Ethernet packet, hence EHC compressor should never bypass ROHC compressor. Similar logic applies for decompressor as well.  The proposed text should not be added in PDCP spec for the following reasons:  1) For the reason mentioned above  2) The text is not related to PDCP protocol and it is just additional information about the type of data expected for the DRB, hence not relevant to this spec.  *[MTK]: The logic stated above (EHC compressor bypasses RoHC if length field is present) isn’t present in the specification and therefore cannot be assumed to be always true. A solution for the issue raised could be to specify that the compressor follows the logic stated above.* |
| MediaTek | Agree; open to solutions (proponent) | The issue here is that when there’s a mix of IP and non-IP traffic along with an Ethernet header which uses the length field (instead of Ethertype), there is no way for the decompressor to know if an IP packet follows the Ethernet header or not. Therefore the decompressor does not know whether RoHC decompression should take place or not.  We are open to solutions for this issue. As indicated by Huawei and Nokia above, one option could be to specify the compressor behaviour so that it aligns with the decompressor. This would require compressor behaviour to be specified in PDCP as below:   1. Ethernet Frame with Ethertype indicating IP packet: perform RoHC compression. 2. Ethernet Frame with Ethertype indicating non-IP packet: bypass RoHC compression. 3. Ethernet Frame with Length: bypass RoHC compression.   Please see replies inline above as well. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Conclusion

**TBD**