3GPP TSG-RAN WG2 Meeting #116 Electronic R2-21xxxxx

**Online, November 1-12, 2021**

**Agenda item: 6.1.4.1.1**

**Source: vivo**

**Title: Draft-Summary of [AT116-e][010][NR16] Connection Control III (vivo)**

**Document for: Discussion and Decision**

# 1 Introduction

This document is a report on the following email discussion:

* [AT116-e][010][NR16] Connection Control III (vivo)

Scope: Determine agreeable parts in a first phase, for agreeable parts agree on CRs. Treat [R2-2110523](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_116-e\Docs\R2-2110523.zip), [R2-2110524](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_116-e\Docs\R2-2110524.zip), [R2-2110525](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_116-e\Docs\R2-2110525.zip), [R2-2110526](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_116-e\Docs\R2-2110526.zip), [R2-2109346](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_116-e\Docs\R2-2109346.zip), [R2-2110685](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_116-e\Docs\R2-2110685.zip), [R2-2110686](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_116-e\Docs\R2-2110686.zip), [R2-2111037](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_116-e\Docs\R2-2111037.zip), [R2-2111200](file:///D:\Documents\3GPP\tsg_ran\WG2\TSGR2_116-e\Docs\R2-2111200.zip)

Intended outcome: Report, Agreed CRs if applicable

Deadline: Schedule 1

The deadline Schedule 1 for this email discussion is copied from Chair notes:

* A first round with Deadline for comments Thursday W1 Nov 4 1200 UTC to settle scope what is agreeable etc
* A Final round with Final deadline Thursday W2 Nov 11 1200 UTC to settle details / agree CRs etc.
* Additional deadlines check points etc if needed are defined by the Rapporteur. In case some parts of an email discussion need more time, doesn’t converge, need on-line treatment etc Rapporteur please contact chair.

# 2 Contact Points

Respondents to the email discussion are kindly asked to fill in the following table.

|  |  |  |
| --- | --- | --- |
| Company | Name | Email Address |
| vivo(rapporteur) | Xiaodong Yang | yangxiaodong5g@vivo.com |
| Nokia |  | amaanat.ali@nokia.com |
| Huawei, HiSilicon | Lili Zheng | zhenglili4@huawei.com |
| Ericsson | Pradeepa Ramachandra | [pradeepa.ramachandra@ericsson.com](mailto:pradeepa.ramachandra@ericsson.com) |
| Qualcomm | Mouaffac | [mambriss@qti.qualcomm.com](mailto:mambriss@qti.qualcomm.com) |

# 3 Discussion

## 3.1 NR SA to ENDC Handover

This topic is from the following four contributions.

[1] R2-2110523 Discussion on the Timing Reference of PSCell SMTC Configuration vivo discussion Rel-16 NR\_newRAT-Core

[2] R2-2110524 Clarification on the Timing Reference of PSCell SMTC Configuration vivo CR Rel-16 38.331 16.6.0 2836 - F NR\_newRAT-Core

[3] R2-2110525 Define the UE capability for PSCell SMTC configuration vivo CR Rel-16 38.306 16.6.0 0652 - F NR\_newRAT-Core

[4] R2-2110526 Clarification on the Timing Reference of PSCell SMTC Configuration vivo CR Rel-16 36.331 16.6.0 4735 - F NR\_newRAT-Core

In [1], the company identifies that it’s unclear whether the UE applies the PSCell SMTC configuration based on the timing reference of NR PCell or target EUTRA PCell for the case of NR SA to EN-DC HO with PSCell addition. According to the proposal in [1], there are basically the following options to address such an ambiguous UE behavior:

* **Option 1**: The target NR PSCell SMTC configuration is provided through *MobilityFromNRCommand* based on the timing reference of source NR PCell;
* **Option 2**: The target NR PSCell SMTC configuration is provided through*targetRAT-MessageContainer* based on the timing reference of target EUTRA PCell.

**Question 1: For the Timing Reference of PSCell SMTC Configuration in NR SA to ENDC Handover, which option(s) do you prefer?**

* Option 1: based on the timing reference of source NR PCell;
* Option 2: based on the timing reference of target EUTRA PCell;
* Both Option 1 and Option 2;
* Other Option(s), please specify.

|  |  |  |
| --- | --- | --- |
| Company | Option(s) | Comments |
| Nokia | Option 2 | This is clearly more aligned with reference to existing specifications. |
| Huawei, HiSilicon | Option 2 | Option 1 requires the UE to keep the timing of the source NR PCell even after HO is finished. |
| Ericsson | Option-2 | As the target EUTRA cell is the one that decides on the SN addition, it is straight forward to configure the associated SMTC based on the timing of the target EUTRA PCell. |
| QCOM | Option-1 | Since it’s a one shot Handover, i.e. HO to PCell (LTE) and PSCell (NR) Target is expected to be executed simultenously, it makes sense to use the source Pcell timing.  Option-2 is mandating that only sequential HO can be executed for the one shot HO from NR SA to EN-DC, i.e. UE has to wait till Target PCell is acquired before initiating the PSCell addition, **which is a suboptimal behavior** and not acceptable. |
|  |  |  |

**Question 2-1: If Option 1 is preferred to Question 1, do companies agree with the intention of 38.331 CR in [2] i.e., clarify that the target NR PSCell SMTC configuration through *MobilityFromNRCommand* is based on the timing reference of source NR PCell?**

|  |  |  |
| --- | --- | --- |
| Company | Agree or not? | Comments |
| Nokia |  | See above |
| QCOM | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Question 2-2: If Option 1 is preferred to Question 1, do companies agree with the intention of 38.306 CR in [3] i.e., define a new UE capability for PSCell SMTC configuration?**

|  |  |  |
| --- | --- | --- |
| Company | Agree or not? | Comments |
| Nokia |  | See above |
| QCOM | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Question 3: If option 2 is preferred to Question 1, do companies agree with the intention of 36.331 CR in [4] i.e., clarify that the target NR PSCell SMTC configuration through *targetRAT-MessageContainer* is based on the timing reference of target EUTRA PCell?**

|  |  |  |
| --- | --- | --- |
| Company | Agree or not? | Comments |
| Nokia | We think no clarification is required for Option 2 being the correct understanding | Going with the description of smtc in TS 36.331. smtc. Entry into EN-DC and NR PSCell addition is clearly stated in this description.  The SSB periodicity/offset/duration configuration of target cell for NR PSCell addition and SN change. It is based on timing reference of EUTRA PCell.  NOTE 2.  If the field is absent, the UE uses the SMTC in the measObjectNR having the same SSB frequency and subcarrier spacing, as configured before the reception of the RRC message. |
| Huawei, HiSilicon | See comment | We think this scenario has not been specifically discussed in the past, but we tend to agree with Nokia that the current text in the spec can cover this scenario. So no additional modification is needed. |
| Ericsson | See comments | Currently, the specification does not mention anything regarding whether to use the source EUTRA cell or the target EUTRA cell as the timing reference for the NR PSCell at the time of E-UTRA PCell handover and PSCell/SN change. So, in such scenarios, the SMTC is not configured and the UE uses the SMTC configured in the measObjectNR having the same SSB frequency and subcarrier spacing, as configured before the reception of the RRC message.  We believe the same is applicable in this scenario also and we do not need to do anything unless we want to also clarify the UE behaviour (along the lines of option-2) for the case of EUTRA PCell change with simultaneous PSCell addition/change. |
|  |  |  |
|  |  |  |

## 3.2 UP security policy update

In the incoming LS from RAN3 [5], the following action is required:

**To RAN1 :** RAN3 kindly requests RAN2 to provide feedback whether the enabling/disabling of ciphering or integrity protection of one or multiple DRBs can be achieved by intra-cell handover within one RRC reconfiguration message.

There are several contributions related to this issue as follows.

[6] R2-2110685 Discussion on UP security policy updated by intra-cell handover Ericsson discussion Rel-16 TEI16

[7] R2-2110686 [Draft] Reply LS on UP security policy updated by intra-cell handover Ericsson LS out Rel-16 TEI16 To:RAN3 Cc:SA3

[8] R2-2111037 Discussion on Ls on UP security update vivo discussion Rel-16 TEI16

[9] R2-2111200 Discussion on UP security policy updated by intra-cell handover China Telecommunications discussion

Referring to contributions above, all companies express similar views, i.e., enabling/disabling of ciphering or integrity protection of one or multiple DRBs can be achieved by intra-cell handover within one RRC reconfiguration message. The rapporteur shares the same view with these companies, according to current TS 38.331, clause 5.3.1.2, integrity protection and ciphering for all DRBs related to the same PDU session are always activated together. A DRB can be reconfigured using *RRCReconfiguration* message according to the TS 38.331 clause 5.3.5.3.

In order to form a common view to reply to RAN3’s question, companies are encouraged to answer the following question.

**Question 4: Do companies agree that enabling/disabling of ciphering or integrity protection of one or multiple DRBs can be achieved by intra-cell handover within one RRC reconfiguration message？**

|  |  |  |
| --- | --- | --- |
| Company | Agree or not | Comments |
| Nokia | Yes | From NR perspective this implies reconfiguration and sync in single RRC message. We think also DRB release and add is another option and even that is possible with single reconfiguration message. |
| Huawei, HiSilicon | See comments | Whether/how the ciphering/integrity protecting can be enabled or disabled has been discussed in Rel-15, and RAN2 agreement is that it can only be done by DRB release and add. This was captured in RRC spec in section 5.3.5.6.5 as Note 5: Ciphering and integrity protection can be enabled or disabled for a DRB. The enabling/disabling of ciphering or integrity protection can be changed only by releasing and adding the DRB.”  Based on above, the key point to reply to RAN3 is that in RAN2 spec, enabling/disabling of ciphering or integrity protection of one or multiple DRBs can be achieved only by releasing and adding the DRB which can be configured in the same RRC reconfiguration message. In case of intra-cell handover, the target gNB can configure DRB release and add within the same target RRC reconfiguration message carrying reconfigurationWithSync. |
| Ericsson | Yes but | We agree in principle that enabling/disabling of ciphering and intergrity protection algorithms can do done via an intra-cell handover within one RRC reconfiguration message.  However, based on the text in the LS RAN3 understanding is the following:  However, according to TS38.331, ciphering and integrity protection can be changed only by releasing and adding the DRB.  This is not correct according to the current NR RRC when the changing on the security algorithm can only be done via a reconfiguration with sync. 5.3.1.2 AS Security The integrity protection and ciphering algorithms can only be changed with reconfiguration with sync. The AS keys (KgNB, KRRCint, KRRCenc, KUPint and KUPenc) change upon reconfiguration with sync (if *masterKeyUpdate* is included), and upon connection re-establishment and connection resume.  For us, this needs to be clarified in RAN3, otherwise they may get the wrong impression that DRB release and add is the only way to do it. |
|  |  |  |
|  |  |  |

# 4 Conclusion

TBD.

# 5 Reference

[1] R2-2110523 Discussion on the Timing Reference of PSCell SMTC Configuration vivo discussion Rel-16 NR\_newRAT-Core

[2] R2-2110524 Clarification on the Timing Reference of PSCell SMTC Configuration vivo CR Rel-16 38.331 16.6.0 2836 - F NR\_newRAT-Core

[3] R2-2110525 Define the UE capability for PSCell SMTC configuration vivo CR Rel-16 38.306 16.6.0 0652 - F NR\_newRAT-Core

[4] R2-2110526 Clarification on the Timing Reference of PSCell SMTC Configuration vivo CR Rel-16 36.331 16.6.0 4735 - F NR\_newRAT-Core

[5] R2-2109346 LS on UP security policy updated by intra-cell handover (R3-214464; contact: China Telecom) RAN3 LS in Rel-16 TEI16 To:RAN2 Cc:SA3

[6] R2-2110685 Discussion on UP security policy updated by intra-cell handover Ericsson discussion Rel-16 TEI16

[7] R2-2110686 [Draft] Reply LS on UP security policy updated by intra-cell handover Ericsson LS out Rel-16 TEI16 To:RAN3 Cc:SA3

[8] R2-2111037 Discussion on Ls on UP security update vivo discussion Rel-16 TEI16

[9] R2-2111200 Discussion on UP security policy updated by intra-cell handover China Telecommunications discussion