**3GPP TSG-RAN WG2 Meeting #116-e R2-210xxxx**

**Online, November 1 – 12, 2021**

**Source: Xiaomi**

**Title: Summary of [AT116-e][036][ePowSav] RLM/BFD relaxation (Xiaomi)**

**Agenda Item: 8.9.3**

**Document for: Discussion and Decision**

# Introduction

This contribution provides a summary of the following email discussion:

**RLM BFD relaxation**

* [AT116-e][036][ePowSav] RLM/BFD relaxation (XIaomi)

 Scope: Progress the topics of RLM/BFD relaxation based on contributions to this meeting. Identify agreements, and potential discussion points. Converge as much as possible offline. Cb Online if needed.

 Intended outcome: Report with Agreements

 Deadline: Wednesday W2 (Online CB if needed)

There could be online CB on Wednesday W2 if needed, therefore the deadline is: Monday W2 Nov 8 10:00 UTC

# Contact information

|  |  |  |
| --- | --- | --- |
| Company | Name  | Email address |
| Xiaomi | Rao Shi  | shirao@xiaomi.com |
| Samsung | Anil Agiwal | anilag@samsung.com |
| MediaTek | Li-Chuan TSENG | li-chuan.tseng@mediatek.com |
| OPPO | Haitao Li | lihaitao@oppo.com |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Discussion

In RAN4#100 meeting, an LS[1] on criteria for RLM/BFD relaxation has been sent to RAN2. And RAN4 respectfully ask RAN2 to take the conclusions made by RAN4 into considerations and start work in RAN2. RAN2 may work on as least following aspects:

 - Specify corresponding signaling for the relaxation criteria defined by RAN4.

Therefore, RAN2 should be responsible for starting to research RLM/BFD relaxation from RAN2 perspective.

## Signaling related for RLM/BFD relaxation criteria

### Provision for parameters of criteria

For the low mobility criteria, RAN4 have achieved agreements so far as follows:

* *Low mobility criterion (in RAN4#110e)*
	+ *Reuse Rel-16 low mobility criterion based on L3 RSRP measurement variation.*
		- *FFS the RSs for L3 RSRP measurement*

For the cell quality criterion, RAN4 have achieved agreements so far as follows:

* *Good serving cell quality criteria of RLM/BFD relaxation is defined as the radio link quality is better than a threshold. The radio link quality in good serving cell quality criteria for R17 RLM/BFD relaxation is based on SINR. (in RAN4 #98e-bis)*
* *UE reuse the SINR for RLM/BFD evaluation when determine whether the serving cell quality criteria is fulfilled or not (in RAN4 #99e)*
* *FFS: (in RAN4#110e)*
	+ *SINR definition for good serving cell quality criterion*
	+ *Predefined or configured threshold*

As we can see from RAN4 agreements, the low mobility criterion for RLM/BFD relaxation is reused based on Rel-16 RRM relaxation, which means there would be two parameters (i.e. SSearchDeltaP and TSearchDeltaP) configured by network. And for the cell quality criterion, some parameters may also require network configuration (e.g. threshold and offset). Therefore RAN2 should be responsible for providing parameters of criterion to UE if RAN4 decides to provide parameters instead of predefined or by implementation.

Some companies [3][4][5] mentioned that using dedicated RRC signalling to provide the RLM/NFD configuration is more reasonable. Here rapporteur think there could be two options (note that the pre-condition is that RAN4 decides to provide parameters instead of predefined or by implementation):

**Option 1:** Dedicated signalling (e.g. *RadioLinkMonitoringConfig*), which is applicable for the corresponding UE

**Option 2:** Broadcast signalling, which is applicable for all UEs in this cell

**Q1: Which option above do companies support if RAN4 decides to provide parameters instead of predefined or by implementation?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option 1/2** | **Comments** |
| Samsung | Option 1 | As the UE is in connected state, dedicated signaling can be used for the configuration.  |
| MediaTek | Option 1 |  |
| OPPO | Option 1 |   |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### Network enable and disable

In RAN4#98bis meeting, it was agreed that *network to enable and disable this feature*, which means the RLM/BFD relaxation should be configured and controlled by network. Some companies [4][5][6][7] mentioned this and considered that the network can enable/disable relaxed RLM/BFD via explicit or implicit way.

For this part, as RAN4 has not yet decided the final criteria, RAN2 is not sure whether there is configuration for corresponding criteria. For example, if the threshold of cell quality criterion is predefined or low mobility is evaluated by implementation, there would not be configuration for criteria. Therefore explicit indication (e.g. 1bit) should be introduced to enable/disable the RLM/BFD relaxation. On the contrary, if the parameters of criteria are configurable, then it is better to implicitly indicate to UE.

It is also noted that RAN4 has concluded that *whether relaxed RLM/BFD requirements can be applied depends on both the serving cell quality and UE mobility state*, it seems only both criteria are fulfilled that UE can perform RLM/BFD relaxation. Therefore, if one criterion is configurable and another is predefined or implementation, network still can implicitly indicate to UE based on that one configurable criterion.

Therefore, rapporteur suggests that:

**Proposal: The enable and disable for RLM/BFD relaxation should be controlled by network as follow:**

* **If the relaxation criteria is configurable, network implicitly indicates enable/disable by the presence/absent of configuration for RLM/BFD relaxation in signalling.**
* **If no any configuration is needed for RLM/BFD relaxation (e.g. based on predefined or implementation), explicit indication is introduced to enable/disable the RLM/BFD relaxation.**

**Q2: Do companies agree with the above proposal and if not, please provide your suggested change?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| Samsung | Yes |  |
| MediaTek | Yes |  |
| OPPO | Yes |   |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### UE capability

In last section, we talked about the network capability to enable/disable RLM/BFD relaxation. Here, rapporteur thinks from RAN2 perspective, we also need to consider the UE capability for RLM/BFD relaxation as this is an optional feature.

Referring to Rel-16 RRM relaxation, the UE capability of supporting RRM relaxation is optional features without UE radio access capability parameters. However, since UE performs RLM and BFD in RRC\_CONNECTED, it is straightforward to use AS capability procedure (i.e. *UECapabilityInformation*) to report UE capability. Therefore there could be some options to design UE capability:

**Option 1:** Using AS capability procedure to report UE capability

**Option 2:** Reusing Rel-16 RRM relaxation mechanism (i.e. optional features without UE radio access capability parameters)

**Option 3:** Other

**Q3: Which option above do companies support to design UE capability of supporting RLM/BFD relaxation?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option 1/2/3** | **Comments** |
| Samsung | Option 1 | *UECapabilityInformation*  can be used as UE is in connected state. |
| MediaTek | Option 1 |  |
| OPPO | Option 1 |   |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### The independence of RLM and BFD relaxation

Actually, RLM and BFD are two different mechanisms that RLM is monitored by UE for RLF in RRC layer and BFD is monitored by UE for BFR in MAC layer. Some companies [3][5][7] mentioned that whether RLM and BFD can be enabled/disabled separately can be further studied. For example, the network may consider RLM (applying on SpCell) is important and can not be relaxed while BFD can be relaxed with certain conditions (e.g. if only applied to SCells).

(BTW, Rapporteur reminds that DCCA scenario will be discussed in next question)

**Q4: Do companies agree that the network can enable/disable RLM and BFD relaxation separately (e.g. UE is configured relaxation for BFD but not for RLM)?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| Samsung | No | In our understanding, according to RAN4 LS criterion to perform RLM and BFD relaxation are same i.e. same thresholds etc. are applied. So it is not clear why RLM relaxation can be applied while the BFD relaxation is not applied or vice versa. |
| MediaTek | No |  |
| OPPO | See comments | Not sure about the intention of the question. BFD is applied for each serving cell, but RLM is only performed on SpCell. It depends on the granularity by which NW enable/disable RLM and BFD relaxation, e.g. per serving cell, or per cell group, or per UE? We think this issue should be first resolved.  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### RLM/BFD relaxation in DCCA scenario

RAN4 has confirmed that *Relaxed BFD/RLM requirements shall be supported for all deployment scenarios supported by current specification which includes: NR SA, EN-DC, NE-DC, NR intra-band CA, NR inter-band CA and NR-DC.* And some companies[2][3][4][7] mentioned that for RLM procedure, it is performed by UE in SpCell and BFD can be performed in PCell/PSCell/SCell. For example, considering DC may be deployed cross FR, MN is deployed on FR1 while SN is deployed on FR2. There would be different FR1 and FR2 requirements for RLM/BFD. Also different serving cell can have different requirement for BFD monitoring. Thus whether the configuration of RLM/BFD relaxation in different cell should be separate or not can be considered.

Therefore there are some considerations from RAN2 perspective for RLM/BFD relaxation in DCCA scenario:

**Q5.1: Do companies agree that RLM relaxation can be configured separately between MCG and SCG in DC case?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| Samsung | Yes |  |
| MediaTek | Yes |  |
| OPPO | See comments | This depends on the detailed relaxation criteria. If we reuse legacy low mobility and not-cell-edge criteria, then we don’t see the need for separate configuration between MCG and SCG. However, if we introduce beam-specific relaxation criteria, then I guess the configuration for MCG and SCG can be different. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q5.2: Do companies agree that BFD relaxation can be configured separately between PCell/PSCell and SCell?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| Samsung | Yes |  |
| MediaTek | Yes |  |
| OPPO |  | See comments for Q5.1. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### UE report of fulfilling and leaving criteria

Two companies[5][6] mentioned this, as UE shall monitor RLM/BFD in RRC\_CONNECTED which is important for the continuity of service. Any relaxation in RRC\_CONNECTED should be careful. Referring to Rel-17 RRM relaxation for redcap in RRC\_CONNECTED, when UE fulfills the criteria, the UE needs to inform network that the criterion is fulfilled, and the network indicate whether the UE can perform RRM measurement relaxation or not. Similarly, for RLM/BFD relaxation, such a mechanism could also be considered.

**Q6: Do companies agree that there should be a UE report mechanism when RLM/BFD relaxation is fulfilled and/or exit (but details can be further studied)?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| Samsung | Yes | Similar approach as redcap can be considered |
| MediaTek | Yes |  |
| OPPO | Yes |   |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## Issues related to RAN4

### The definition of low mobility criterion for BFD relaxation

RAN4 has concluded that *Reuse Rel-16 low mobility criterion based on L3 RSRP measurement variation*. According to companies contributions[2][4], some think Rel-16 low mobility criterion is designed to evaluate UE “L3 mobility” which is unaware of beam change. For example, UE circling around the cell is still considered as a low mobility UE, but BFR will happen therefore it is not suitable for BFD relaxation.

For this part, rapporteur think as least for this moment, RAN4 is still discussing what RS will be used for L3 RSRP in low mobility criterion. But anyway we can provide some information to RAN4 from RAN2 perspective since the corresponding criteria will be captured in RAN2 specification.

Therefore there are some suggestions for low mobility criteria for BFD relaxation:

**Option 1:** Using beam-level measurement

**Option 2:** Introducing beam-change related criterion

**Option 3:** Using the difference in SINR between the weakest BFD-RS and the strongest candidate beam which is not QCL with the weakest BFD RS is larger than a configured threshold.

**Option 4:** Waiting for RAN4 (maybe inform RAN4 of the concern about low mobility criterion for BFD from RAN2 perspective)

**Q7: Which option above do companies support to consider low mobility criterion for BFD relaxation?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option 1/2/3/4** | **Comments** |
| Samsung | See comments | Since the criterion is defined by RAN4, we can wait for RAN4 decision. |
| MediaTek | Option 4 | According to the WID, the criteria should be discussed in RAN4. We should avoid parallel discussions in two WGs.  |
| OPPO | Option 4 | Agree with Samsung and MediaTek. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### Responsibility between RAN2 and RAN4 for specification

Referring to Rel-16 RRM relaxation, there are some misunderstanding between RAN2 and RAN4 as some criteria and relaxed methods are put into both RAN2 and RAN4 specification. Therefore rapporteur thinks we can make the responsibility more clearly. Three companies[4][5][8] mentioned this part. With this relaxation procedure, one way is that RAN4 specification should capture the relaxed methods as well as the corresponding requirements for RLM/BFD relaxation, while RAN2 specification should capture the relaxation criteria as well as the RRC configurations. Rapporteur also wants to remind that RLM is handled by RRC layer while BFD is handle by MAC layer. So furthermore RAN2 can capture RLM relaxation criteria in RRC aspect (i.e. TS 38.331) and BFD relaxation criteria in MAC aspect (i.e. TS 38.321). However there is still argument[8] that the relaxed RLM/BFD criterion are discussed in RAN4 and captured in 38.133. Anyway rapporteur think we can proposal a suggestion as way forward.

**Proposal: The relaxation methods as well as the corresponding requirements for RLM/BFD relaxation should be captured in RAN4 specification, while the criteria as well as the configurations should be captured in RAN2 specification(e.g. RLM captured in TS 38.331 and BFD captured in TS 38.321).**

**Q8: Do companies agree with the above proposal and if not, please provide your suggested change?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| Samsung | No | Configuration aspects are captured in RRC. Detailed criterion is specified in 38.133 |
| MediaTek | No | The criteria are defined by RAN4, and should also be captured in RAN4 specifications (38.133) |
| OPPO | No | Same view as Samsung. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## LS information to RAN4

Once RAN2 has reached some agreements, rapporteur wonders whether to provide our suggestions to RAN4 as a reference for future work.

**Q9: Do companies agree to send an LS about our RAN2 suggestions to RAN4 as a reference for future work?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| Samsung | No strong view | We can follow majority view. |
| MediaTek | No | According to the WID, RAN2 should do RLM/BFD works based on RAN4 results. We can simply wait for RAN4. |
| OPPO | No | Agree with MediaTek. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## Other issues

If companies raise some issues which are not mentioned in this contribution, please provide your opinions here.

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |
|  |  |
|  |   |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

3. Conclusion

4. Reference

1. R2-2109362\_R4-2115349 LS on criteria for RLM/BFD relaxation
2. R2-2109454 Criteria and configuration for BFD relaxations Qualcomm Incorporated
3. R2-2109879 Signalling aspect on criteria of RLM/BFD relaxation Intel Corporation
4. R2-2109739 RAN2 impact on RLM/BFD relaxation for power saving vivo
5. R2-2110194 Discussion on RLM\_BFD measurement relaxation Xiaomi Communications
6. R2-2110541 Discussion on criteria for the RLM/BFD relaxation Huawei, HiSilicon
7. R2-2110404 Configurations for RLM/BFD Relaxation CATT
8. R2-2110414 Other aspects on UE power saving Ericsson