3GPP TSG-RAN WG2 Meeting #117-e R2-22XXXX

Electronic Meeting, 21 Feb – 3 January 2022

**Agenda item: 8.14.4**

**Source: CMCC**

**Title: Report for** **[AT117-e][047][QoE] UE capability (CMCC)**

**WID/SID: NR\_QoE**

**Document for: Discussion and Decision**

# Introduction

This document aims at initiating the discussion on UE capabilities for NR QoE.

* [AT117-e][047][QoE] UE capability (CMCC)

Scope: Treat R2-2202827, R2-2202988, R2-2203347, R2-2203404, R2-2203429, determine agreeable parts and discussion points. Determine need for LS outs if any.

Intended outcome: Report

Deadline: W1 Friday (for online CB W2 Monday).

**Contact List**

|  |  |  |
| --- | --- | --- |
| Company | Name | Email |
| Huawei, HiSilicon | Jun Chen | jun.chen@huawei.com |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Discussion

## Open issue 1: AS and APP layer interactions

In [1], it is suggested to discuss the open issue that whether and how AS layer obtains application capability. With the efforts from the companies participating, there are two options that rapporteur can humbly summarized:

**Option 1: How AS layer obtains application capability is based on UE implementation, which means there will be no spec impact.**

**Option 2: Introduce QoE capability interaction between AS layer and APP layer by e.g., AT-command.**

In the latest running CR of TS 38.306, *qoe-MeasReport-r15* and *qoe-MTSI-MeasReport-r15* relating both APP layer and AS layer capability are defined, which is similar to the existing UE capability IE in LTE QoE. And in LTE, there does not exist any interaction between AS layer and APP layer on QoE capability. Therefore, proposals in [2][3] suggest that NR QoE should be applied the same principle as well.

On the other hand, to ask SA4/CT1 on the AT-command that indicates APP layer capability on QoE to AS layer seems to be an alternative approach, as [4] propose.

And in [5], it is assumed that SA4 can address some mechanism on QoE capability interaction. It is the rapporteur’s understanding that no matter which option RAN2 agrees to accept, SA4/CT1 should be informed for such decision.

**Q1: Which option do you prefer on QoE capability integration between AS layer and APP Layer？**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option** | **Comments** |
| Huawei, HiSilicon | 1 | We think that the question should be: whether and how AS layer obtains application capability. For the question, we prefer option 1 because QoE feature is an E2E feature, and before UE setting the QoE UE capabilities in AS layer, it will anyway check with APP layer.  In other words, there will be co-ordinations between AS and APP layers, but we do not see a strong need to standardize them in 3GPP. If option 2 is selected, it means the co-ordinations is a must in the standard (e.g. RAN2, CT1, and maybe other WGs), and then every time RAN2 discusses QoE UE capabilties, there may be impacts to other WGs. In general, we think UE implementation can have the same effects as option 2 and option 2 may introduce extra work (for now and for the future). |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Summary:

Proposal:

## Open issue 2: App Layer requirement on QoE support

In both [4] and [6], there emerge the concerns about APP layer requirement on NR QoE.

And in [4], a case on multiple application for a same service type is presented as follows,

|  |
| --- |
| There can be several different applications for the same service type. UE capabilities for QoE are defined per service type. If the UE e.g., has three applications for streaming, but only one of the applications supports QoE, can the UE indicate support for QoE streaming or do all three applications need to support QoE? Or alternatively, the UE may not take the support in the application into account when reporting the AS UE capability for QoE. |

Therefore, the rapporteur would like to collect opinions on whether there exists a case that UE supports QMC for a certain service type, but not all related applications support QMC for further decision making.

**Q2.1: Do you think there exist the case illustrated above?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes or no** | **Comments** |
| Huawei, HiSilicon | Yes | In RAN2, we mainly discuss the service type for the QoE support. From SA4 point of view, they just specifiy the service type for QoE definitions, e.g. TS 26.247 is for Progressive Download and Dynamic Adaptive Streaming over HTTP (3GP-DASH). We think per service type definition for QoE is flexible, and any application supporting the TS 26.247 will have the same behaviours on QoE measurement collection behaviours.  In addition, the development of applications in the real world is changing quickly, so it is hard to define QoE per applications. So per service type QoE definitions are a good wayforward.  For the case showed above, we do not think there is a problem.  For example, operator A, network vendor B, UE vendor C and APP provider D can support QoE measurement collection for streaming, and then APP provider D is just one application for streaming (which means UE AS and UE APP only support QoE for application D for streaming). When the UE performs streaming services and QoE collection, it will only collect QoE from APP provider D, and operator A can collect the QoE and do the optimizations. In the future, if APP provider E can also support QoE measurement collection for streaming, operator A may differentiate the two applications by QoE reference ids.  In general, we think it is reasonable for the UE to only support one or more applications for the same service, and the current QoE design can work. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q2.2: If the answer to the above question is Yes, what and how the information should be** **interacted between AS layer and APP layer?**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| Huawei, HiSilicon | As we commented above, we do not see a need to define extra information. The current QoE design can work. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

Summary:

Proposal:

## Open issue 3: LS to CT1/SA4

Since the open issues on AS and APP layer interactions involve other WGs, also as proposed in [3], an LS on QoE UE capability should be sent to SA4 and CT1 after the meeting.

**Q3.1 Do you agree to send an LS on the** **QoE UE capability to related WGs (e.g., SA4, CT1)?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes or no** | **Comments** |
| Huawei, HiSilicon | FFS | It should be discussed case by case. For example, for UL segmentation capability, RAN2 has sent a LS to SA4 for double check; for “whether and how AS layer obtains application capability” in Q1, it is under discussions.  So we think Q3.1 can be more concrete so that companies can technically check it. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q3.2 If the answer to the above question is Yes, what should be captured in the LS?**

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# Summary

# References

1. R2-2202043 QoE related open issue list, China Unicom
2. R2-2203347 AS and application layer interactions for NR QoE UE capabilities, Huawei
3. R2-2202827 Discussion on UE Capability for QoE, ZTE
4. R2-2203429 UE capabilities for QoE measurements, Ericsson
5. R2-2202988 Capabilities of AS layer and application layer, Samsung
6. R2-2203404 UE Capabilities for QMC, Nokia