**3GPP TSG-RAN WG2 Meeting #117-e *R2-2202659***

**Electronic meeting, February 21 – March 3, 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.306** | **CR** | **-** | **rev** | **-** | **Current version:** | **16.7.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR to 38306 on UE capabilities for 71G |
|  |  |
| ***Source to WG:*** | Intel Corporation |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | NR\_ext\_to\_71GHz-Core |  | ***Date:*** | 2022-02-14 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* *Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Introduce UE Capabilities for NR operation up to 71GHz |
|  |  |
| ***Summary of change:*** | Introduce UE Capabilities for NR operation up to 71GHz:* Include the FR2-1 and FR2-2 differentiation to existing RAN2 determined UE capabilities
* Introduce new RLC RTT values for SCS 480kHz and 960kHz
* Including R1-24-1, 24-1a, 24-2
* Included new updates from RAN2#117 agreements below:
* 3-1: For existing UE capabilities that are with consistency check (’ UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands and all TDD-FR2 bands respectively.’) in the field description, update it to:

"UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively."* 3-3: Clarify in Annex B of TS 38.306 that for a UE capability which are not differentiated between FR2-1 and FR2-2, ‘FR2 TDD’ in Table B-1 includes both FR2-1 TDD and FR2-2 TDD.
* 3-4: Clarify in Annex B of TS 38.306 that for a UE capability which are differentiated between FR2-1 and FR2-2, ‘FR2 TDD’ in Table B-1 only means ‘FR2-1 TDD’.
 |
|  |  |
| ***Consequences if not approved:*** | UE capabilities for NR operation up to 71GHz is not introduced |
|  |  |
| ***Clauses affected:*** | 4.1.4, 4.2.1, 4.2.2, 4.2.6, 4.2.7, 4.2.9, 4.2.13 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS/TR 38.331 CR XXX |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

START OF 1st CHANGE

### 4.1.4 Total layer 2 buffer size for DL/UL

The total layer 2 buffer size is defined as the sum of the number of bytes that the UE is capable of storing in the RLC transmission windows and RLC reception and reassembly windows and also in PDCP reordering windows for all radio bearers.

The required total layer 2 buffer size in MR-DC and NR-DC is the maximum value of the calculated values based on the following equations:

- *MaxULDataRate\_MN* \* *RLCRTT\_MN* + *MaxULDataRate\_SN* \* *RLCRTT\_SN* + *MaxDLDataRate\_SN* \* *RLCRTT\_SN* + *MaxDLDataRate\_MN* *\** (*RLCRTT\_SN* + *X2/Xn delay* + *Queuing in SN*)

- *MaxULDataRate\_MN* \* *RLCRTT\_MN* + *MaxULDataRate\_SN* \* *RLCRTT\_SN* + *MaxDLDataRate\_MN* \* *RLCRTT\_MN* + *MaxDLDataRate\_SN* *\** (*RLCRTT\_MN* + *X2/Xn delay* + *Queuing in MN*)

Otherwise it is calculated by *MaxDLDataRate \* RLC RTT + MaxULDataRate \* RLC RTT*.

NOTE: Additional L2 buffer required for preprocessing of data is not taken into account in above formula.

The required total layer 2 buffer size is determined as the maximum total layer 2 buffer size of all the calculated ones for each band combination and the applicable Feature Set combination in the supported MR-DC or NR band combinations. The RLC RTT for NR cell group corresponds to the smallest SCS numerology supported in the band combination and the applicable Feature Set combination.

wherein

X2/Xn delay + Queuing in SN = 25ms if SCG is NR, and 55ms if SCG is EUTRA

X2/Xn delay + Queuing in MN = 25ms if MCG is NR, and 55ms if MCG is EUTRA

RLC RTT for EUTRA cell group = 75ms

RLC RTT for NR cell group is defined in Table 4.1.4-1

Table 4.1.4-1: RLC RTT for NR cell group per SCS

| SCS (kHz) | RLC RTT (ms) |
| --- | --- |
| 15KHz | 50 |
| 30KHz | 40 |
| 60KHz | 30 |
| 120KHz | 20 |
| 480KHz | 20 |
| 960KHz | 20 |

END OF 1st CHANGE

START OF 2nd CHANGE

### 4.2.1 Introduction

The following clauses define the UE radio access capability parameters. Only parameters for which there is the possibility for UEs to signal different values are considered as UE radio access capability parameters. Therefore, mandatory features without capability parameters that are the same for all UEs are not listed here.

The network needs to respect the signalled UE radio access capability parameters when configuring the UE and when scheduling the UE.

For capabilities that required to be set consistently for all FDD-FR1 bands (i.e. capabilities that are supposed to be per UE), the UE shall also set capability values for all SUL bands with same values for FDD-FR1 bands if SUL band is supported by the UE.

The UE may support different functionalities between FDD and TDD, and/or between FR1 and FR2. The UE shall indicate the UE capabilities as follows. In the table of UE capability parameter in subsequent clauses, "Yes" in the column by "FDD-TDD DIFF" and "FR1-FR2 DIFF" indicates the UE capability field can have a different value for between FDD and TDD or between FR1 and FR2 and "No" indicates if it cannot. “(Include FR2-2 diff)” in the column by "FR1-FR2 DIFF" indicates the UE capability field can have a different value for between FR2-1 and FR2-2. Regarding to the per UE capabilities that are FDD/TDD differentiated(i.e. capabilities indicated as "Yes" in the column by "FDD-TDD DIFF"), the corresponding capabilities indicated by the FDD capability is applied to SUL if SUL band is supported by the UE. "FD" in the column indicates to refer the associated field description. "FR1 only" or "FR2 only" in the column indicates the associated feature is only supported in FR1 or FR2 and "TDD only" indicates the associated feature is only supported in TDD and not applicable to SUL carriers. "N/A" in the column indicates it is not applicable to the feature (e,g. the signaling supports the UE to have different values between FDD and TDD or between FR1 and FR2).

1> set all fields of UE-NR/MRDC-Capability except fdd-Add-UE-NR/MRDC/Sidelink-Capabilities, tdd-Add-UE-NR/MRDC/Sidelink-Capabilities, fr1-Add-UE-NR/MRDC-Capabilities and fr2-Add-UE-NR/MRDC-Capabilities, to include the values applicable for all duplex mode(s) and frequency range(s) that the UE supports;

1> if UE supports both FDD (or SUL) and TDD and if (some of) the UE capability fields have a different value for FDD (or SUL) and TDD

2> if for FDD (and, if the UE supports SUL, for SUL), the UE supports additional functionality compared to what is indicated by the previous fields of UE-NR/MRDC-Capability/SidelinkParameters:

3> include field fdd-Add-UE-NR/MRDC/Sidelink-Capabilities and set it to include fields reflecting the additional functionality applicable for FDD;

2> if for TDD, the UE supports additional functionality compared to what is indicated by the previous fields of UE-NR/MRDC-Capability/SidelinkParameters:

3> include field tdd-Add-UE-NR/MRDC/Sidelink-Capabilities and set it to include fields reflecting the additional functionality applicable for TDD;

1> if UE supports both FR1 and FR2 and if (some of) the UE capability fields have a different value for FR1 and FR2:

2> if for FR1, the UE supports additional functionality compared to what is indicated by the previous fields of UE-NR/MRDC-Capability:

3> include field fr1-Add-UE-NR/MRDC-Capabilities and set it to include fields reflecting the additional functionality applicable for FR1;

2> if for FR2, the UE supports additional functionality compared to what is indicated by the previous fields of UE-NR/MRDC-Capability:

3> include field fr2-Add-UE-NR/MRDC-Capabilities and set it to include fields reflecting the additional functionality applicable for FR2;

NOTE 1: The fields which indicate "shall be set to 1" or "shall be set to *supported*" in the following tables means these features are purely mandatory and are assumed they are the same as mandatory without capability signaling.

NOTE 2: For the case where the UE is allowed to support different functionality between FDD and TDD and between FR1 and FR2 according to the specification, the UE capability indication is clarified in Annex B.

For optional features, the UE radio access capability parameter indicates whether the feature has been implemented and successfully tested. For mandatory features with the UE radio access capability parameter, the parameter indicates whether the feature has been successfully tested. In the table of UE capability parameter in subsequent clauses, "Yes" in the column by "M" indicates the associated feature is mandatory and "No" indicates the associated feature is optional. "CY" in the column indicates the associated feature is conditional mandatory and the condition is described in the field description and the associated feature is considered mandatory with capability parameter, when the described condition is satisfied. "FD" in the column indicates to refer the associated field description. Some parameters in subsequent clauses are not related to UE features and in the case, "N/A" is indicated in the column.

UE capability parameters have hierarchical structure. In the table of UE capability parameter in subsequent clauses, "Per" indicates the level the associated parameter is included. "UE" in the column indicates the associated parameter is signalled per UE, "Band" indicates it is signalled per band, "BC" indicates it is signalled per band combination, "FS" indicates it is signalled per feature set (per band per band combination), "FSPC" indicates it is signalled per feature set per component carrier (per CC per band per band combination), and "FD" in the column indicates to refer the associated field description.

END OF 2nd CHANGE

START OF 3rd CHANGE

### 4.2.2 General parameters

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Definitions for parameters | Per | M | FDD-TDD DIFF | **FR1-FR2**DIFF |
| ***accessStratumRelease***Indicates the access stratum release the UE supports as specified in TS 38.331 [9]. | UE | Yes | No | No |
| ***delayBudgetReporting***Indicates whether the UE supports delay budget reporting as specified in TS 38.331 [9]. | UE | No | No | No |
| ***dl-DedicatedMessageSegmentation-r16***Indicates whether the UE supports reception of segmented DL RRC messages. | UE | No | No | No |
| ***drx-Preference-r16***Indicates whether the UE supports providing its preference of a cell group on DRX parameters for power saving in RRC\_CONNECTED, as specified in TS 38.331 [9]. | UE | No | No | No |
| ***inactiveState***Indicates whether the UE supports RRC\_INACTIVE as specified in TS 38.331 [9]. | UE | Yes | No | No |
| ***inDeviceCoexInd-r16***Indicates whether the UE supports IDC (In-Device Coexistence) assistance information as specified in TS 38.331 [9]. | UE | No | No | No |
| ***maxBW-Preference-r16, maxBW-Preference-r17***Indicates whether the UE supports providing its preference of a cell group on the maximum aggregated bandwidth for power saving in RRC\_CONNECTED, as specified in TS 38.331 [9]. | UE | No | No | Yes(Include FR2-2 diff) |
| ***maxCC-Preference-r16***Indicates whether the UE supports providing its preference of a cell group on the maximum number of secondary component carriers for power saving in RRC\_CONNECTED, as specified in TS 38.331 [9]. | UE | No | No | No |
| ***maxMIMO-LayerPreference-r16, maxMIMO-LayerPreference-r17***Indicates whether the UE supports providing its preference of a cell group on the maximum number of MIMO layers for power saving in RRC\_CONNECTED, as specified in TS 38.331 [9]. | UE | No | No | Yes(Include FR2-2 diff) |
| ***mcgRLF-RecoveryViaSCG-r16***Indicates whether the UE supports recovery from MCG RLF via split SRB1 (if supported) and via SRB3 (if supported) as specified in TS 38.331[9]. | UE | No | No | No |
| ***minSchedulingOffsetPreference-r16***Indicates whether the UE supports providing its preference on the minimum scheduling offset for cross-slot scheduling of the cell group for power saving in RRC\_CONNECTED, as specified in TS 38.331 [9]. | UE | No | No | No |
| ***mpsPriorityIndication-r16***Indicates whether the UE supports *mpsPriorityIndication* on RRC release with redirect as defined in TS 38.331 [9]. | UE | No | No | No |
| ***onDemandSIB-Connected-r16***Indicates whether the UE supports the on-demand request procedure of SIB(s) or posSIB(s) while in RRC\_CONNECTED, as specified in TS 38.331 [9]. | UE | No | No | No |
| ***overheatingInd***Indicates whether the UE supports overheating assistance information. | UE | No | No | No |
| ***partialFR2-FallbackRX-Req***Indicates whether the UE meets only a partial set of the UE minimum receiver requirements for the eligible FR2 fallback band combinations as defined in Clause 4.2 of TS 38.101-2 [3] and Clause 4.2 of TS 38.101-3 [4]. If not indicated, the UE shall meet all the UE minimum receiver requirements for all the FR2 fallback combinations in TS 38.101-2 [3] and TS 38.101-3 [4]. The UE shall support configuration of any of the FR2 fallback band combinations regardless of the presence or the absence of this field. | UE | No | No | No |
| ***redirectAtResumeByNAS-r16***Indicates whether the UE supports reception of *redirectedCarrierInfo* in an *RRCRelease* message in response to an *RRCResumeRequest* or *RRCResumeRequest1* which is triggered by the NAS layer, as specified in TS 38.331 [9]. | UE | No | No | No |
| ***reducedCP-Latency***Indicates whether the UE supports reduced control plane latency as defined in TS 38.331 [9] | UE | No | No | No |
| ***referenceTimeProvision-r16***Indicates whether the UE supports provision of referenceTimeInfo in *DLInformationTransfer* message and in SIB9 and reference time information preference indication via assistance information, as specified in TS 38.331 [9]. | UE | No | No | No |
| ***releasePreference-r16***Indicates whether the UE supports providing its preference assistance information to transition out of RRC\_CONNECTED for power saving, as specified in TS 38.331 [9]. | UE | No | No | No |
| ***resumeWithStoredMCG-SCells-r16***Indicates whether the UE supports not deleting the stored MCG SCell configuration when initiating the resume procedure. | UE | No | No | No |
| ***resumeWithStoredSCG-r16***Indicates whether the UE supports not deleting the stored SCG configuration when initiating resume. The UE which indicates support for *resumeWithStoredSCG-r16* shall also indicate support for *resumeWithSCG-Config-r16*. | UE | No | No | No |
| ***resumeWithSCG-Config-r16***Indicates whether the UE supports (re-)configuration of an SCG during the resume procedure. | UE | No | No | No |
| ***splitSRB-WithOneUL-Path***Indicates whether the UE supports UL transmission via MCG path and DL reception via either MCG path or SCG path, as specified for the split SRB in TS 37.340 [7]. The UE shall not set the FDD/TDD specific fields for this capability (i.e. it shall not include this field in *UE-MRDC-CapabilityAddXDD-Mode*). | UE | No | No | No |
| ***splitDRB-withUL-Both-MCG-SCG***Indicates whether the UE supports UL transmission via both MCG path and SCG path for the split DRB as specified in TS 37.340 [7]. The UE shall not set the FDD/TDD specific fields for this capability (i.e. it shall not include this field in *UE-MRDC-CapabilityAddXDD-Mode*). | UE | Yes | No | No |
| ***srb3***Indicates whether the UE supports direct SRB between the SN and the UE as specified in TS 37.340 [7]. The UE shall not set the FDD/TDD specific fields for this capability (i.e. it shall not include this field in *UE-MRDC-CapabilityAddXDD-Mode*). This field is not applied to NE-DC. | UE | Yes | No | No |

**<<OMMITED>>**

### 4.2.6 MAC parameters

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Definitions for parameters | Per | M | FDD-TDD DIFF | FR1-FR2 DIFF |
| ***autonomousTransmission-r16***Indicates whether the UE supports autonomous transmission of the MAC PDU generated for a deprioritized configured uplink grant as specified in TS 38.321 [8]. A UE supporting this feature shall also support *lch-priorityBasedPrioritization-r16*. | UE | No | No | No |
| ***directMCG-SCellActivation-r16, directMCG-SCellActivation-r17***Indicates whether the UE supports direct NR MCG SCell activation, as specified in TS 38.321 [8], upon SCell addition, upon reconfiguration with sync of the MCG, as specified in TS 38.331 [9]. | UE | No | No | Yes (Include FR2-2 diff) |
| ***directMCG-SCellActivationResume-r16, directMCG-SCellActivationResume-r17***Indicates whether the UE supports direct NR MCG SCell activation, as specified in TS 38.321 [8], upon reception of an *RRCResume* message, as specified in TS 38.331 [9]. | UE | No | No | Yes(Include FR2-2 diff) |
| ***directSCG-SCellActivation-r16, directSCG-SCellActivation-r17***Indicates whether the UE supports direct NR SCG SCell activation, as specified in TS 38.321 [8], upon SCell addition and upon reconfiguration with sync of the SCG, both performed via an *RRCReconfiguration* message received via SRB3 or contained in an *RRC(Connection)Reconfiguration* message received via SRB1, as specified in TS 38.331 [9] and TS 36.331 [17].A UE indicating support of *directSCG-SCellActivation-r16* shall indicate support of EN-DC or support of NGEN-DC as specified in TS 36.331 [17] or support of NR-DC as specified in TS 38.331 [9]. | UE | No | No | Yes(Include FR2-2 diff) |
| ***directSCG-SCellActivationResume-r16, directSCG-SCellActivationResume-r17***Indicates whether the UE supports direct NR SCG SCell activation, as specified in TS 38.321 [8]:- upon reception of an *RRCReconfiguration* included in an *RRCConnectionResume* message, as specified in TS 38.331 [9] and TS 36.331 [17], if the UE indicates support of EN-DC or NGEN-DC, and support of *resumeWithSCG-Config-r16* as specified in TS 36.331 [17],- upon reception of an *RRCReconfiguration* included in an *RRCResume* message, as specified in TS 38.331 [9], if the UE indicates support of NR-DC and of *resumeWithSCG-Config-r16* as specified in TS 38.331 [9].A UE indicating support of *directSCG-SCellActivationResume-r16* shall indicate support of EN-DC or NGEN-DC and support of *resumeWithSCG-Config-r16* as specified in TS 36.331 [17] or indicate support of NR-DC and of *resumeWithSCG-Config-r16* as specified in TS 38.331 [9]. | UE | No | No | Yes(Include FR2-2 diff) |
| ***drx-Adaptation-r16***Indicates whether the UE supports DRX adaptation comprised of the following functional components:- Configured *ps-Offset* for the detection of DCI format 2\_6 with CRC scrambling by *ps*-RNTI and reported *MinTimeGap* before the start of *drx-onDurationTimer* of Long DRX- Indication of UE whether or not to start *drx-onDurationTimer* for the next Long DRX cycle by detection of DCI format 2\_6- Configured UE wakeup or not when DCI format 2\_6 is not detected at all monitoring occasions outside Active Time- Configured periodic CSI report apart from L1-RSRP (*ps-TransmitOtherPeriodicCSI*) when impacted by DCI format 2\_6 that *drx-onDurationTimer* does not start for the next Long DRX cycle- Configured periodic L1-RSRP report (*ps-TransmitPeriodicL1-RSRP*) when impacted by DCI format 2\_6 that *drx-onDurationTimer* does not start for the next Long DRX cycleThe capability signalling includes the minimum time gap between the end of the slot of last DCI format 2\_6 monitoring occasion and the beginning of the slot where the UE would start the *drx-onDurationTimer* of Long DRX for each SCS. The value *sl1* indicates 1 slot. The value *sl2* indicates 2 slots, and so on. Support of this feature is reported for licensed and unlicensed bands, respectively. When this field is reported, either of *sharedSpectrumChAccess-r16* or *non-SharedSpectrumChAccess-r16* shall be reported, at least. | UE | No | No | Yes |
| ***enhancedSkipUplinkTxConfigured-r16***Indicates whether the UE supports skipping UL transmission for a configured uplink grant only if no data is available for transmission and no UCI is multiplexed on the corresponding PUSCH of the uplink grant as specified in TS 38.321 [8]. | UE | No | Yes | No |
| ***enhancedSkipUplinkTxDynamic-r16***Indicates whether the UE supports skipping UL transmission for an uplink grant addressed to a C-RNTI only if no data is available for transmission and no UCI is multiplexed on the corresponding PUSCH of the uplink grant as specified in TS 38.321 [8]. | UE | No | Yes | No |
| ***lch-PriorityBasedPrioritization-r16***Indicates whether the UE supports prioritization between overlapping grants and between scheduling request and overlapping grants based on LCH priority as specified in TS 38.321 [8].  | UE | No | No | No |
| ***lch-ToConfiguredGrantMapping-r16***Indicates whether the UE supports restricting data transmission from a given LCH to a configured (sub-) set of configured grant configurations (see *allowedCG-List-r16* in *LogicalChannelConfig* in TS 38.331 [9]) as specified in TS 38.321 [8].  | UE | No | No | No |
| ***lch-ToGrantPriorityRestriction-r16***Indicates whether the UE supports restricting data transmission from a given LCH to a configured (sub-) set of dynamic grant priority levels (see *allowedPHY-PriorityIndex-r16* in *LogicalChannelConfig* in TS 38.331 [9]) as specified in TS 38.321 [8].  | UE | No | No | No |
| ***lch-ToSCellRestriction***Indicates whether the UE supports restricting data transmission from a given LCH to a configured (sub-) set of serving cells (see *allowedServingCells* in *LogicalChannelConfig*). A UE supporting *pdcp-DuplicationMCG-OrSCG-DRB* or *pdcp-DuplicationSRB* (see *PDCP-Config*) shall also support *lch-ToSCellRestriction*. | UE | No | No | No |
| ***lcp-Restriction***Indicates whether UE supports the selection of logical channels for each UL grant based on RRC configured restriction using RRC parameters *allowedSCS-List*, *maxPUSCH-Duration*, and *configuredGrantType1Allowed* as specified in TS 38.321 [8]. | UE | No | No | No |
| ***logicalChannelSR-DelayTimer***Indicates whether the UE supports the *logicalChannelSR-DelayTimer* as specified in TS 38.321 [8]. | UE | No | Yes | No |
| ***longDRX-Cycle***Indicates whether UE supports long DRX cycle as specified in TS 38.321 [8]. | UE | Yes | Yes | No |
| ***multipleConfiguredGrants***Indicates whether UE supports more than one configured grant configurations (including both Type 1 and Type 2) in a cell group. For each cell, the UE supports at most one configured grant per BWP and the maximum number of configured grant configurations per cell group is 2. If absent, for each configured cell group, the UE only supports one configured grant configuration on one serving cell. | UE | No | Yes | No |
| ***multipleSR-Configurations***Indicates whether the UE supports 8 SR configurations per PUCCH cell group as specified in TS 38.321 [8]. | UE | No | Yes | No |
| ***recommendedBitRate***Indicates whether the UE supports the bit rate recommendation message from the gNB to the UE as specified in TS 38.321 [8]. | UE | No | No | No |
| ***recommendedBitRateMultiplier-r16***Indicates whether the UE supports the bit rate multiplier for recommended bit rate MAC CE as specified in TS 38.321 [8], clause 6.1.3.20. This field is only applicable if the UE supports recommendedBitRate. | UE | No | No | No |
| ***recommendedBitRateQuery***Indicates whether the UE supports the bit rate recommendation query message from the UE to the gNB as specified in TS 38.321 [8]. This field is only applicable if the UE supports *recommendedBitRate*. | UE | No | No | No |
| ***secondaryDRX-Group-r16***Indicates whether UE supports secondary DRX group as specified in TS 38.321 [8]. | UE | No | Yes | No |
| ***shortDRX-Cycle***Indicates whether UE supports short DRX cycle as specified in TS 38.321 [8]. | UE | Yes | Yes | No |
| ***singlePHR-P-r16***Indicates whether UE supports the P bit in single PHR MAC CE as specified in TS 38.321 [8]. | UE | No | No | No |
| ***skipUplinkTxDynamic***Indicates whether the UE supports skipping of UL transmission for an uplink grant indicated on PDCCH if no data is available for transmission as specified in TS 38.321 [8]. | UE | No | Yes | No |
| ***spCell-BFR-CBRA-r16***Indicates whether the UE supports sending BFR MAC CE for SpCell BFR as specified in TS 38.321 [8]. | UE | No | No | No |
| ***srs-ResourceId-Ext-r16***Indicates whether the UE supports the extended 6-bit (Positioning) SRS resource ID in SP Positioning SRS Activation/Deactivation MAC CE, as specified in TS 38.321 [8]. | UE | No | No | No |
| ***tdd-MPE-P-MPR-Reporting-r16***Indicates whether the UE supports P-MPR reporting for Maximum Permissible Exposure, as specified in TS38.321 [8]. | UE | No | TDD only | FR2 only |
| *ul-LBT-FailureDetectionRecovery-r16*Indicates whether the UE supports consistent uplink LBT detection and recovery, as specified in TS 38.321 [8], for cells operating with shared spectrum channel access.This field applies to all serving cells with which the UE is configured with shared spectrum channel access. | UE | No | No | No |

END OF 3rd CHANGE

START OF 4th CHANGE

#### 4.2.7.2 *BandNR parameters*

| Definitions for parameters | Per | M | FDD-TDDDIFF | FR1-FR2DIFF |
| --- | --- | --- | --- | --- |
| ***activeConfiguredGrant-r16***Indicates whether the UE supports up to 12 configured/active configured grant configurations in a BWP of a serving cell. This field includes the following parameters:- *maxNumberConfigsPerBWP-r16* indicates the maximum number of configured/active configured grant configurations in a BWP of a serving cell.- *maxNumberConfigsAllCC-r16* indicates the maximum number of configured/active configured grant configurations across all serving cells in a MAC entity, and across MCG and SCG in case of NR-DC.The UE can include this feature only if the UE indicates supports of either *configuredUL-GrantType1* or *configuredUL-GrantType2*.NOTE:- For all the reported bands in FR1, a same X1 value is reported for *maxNumberConfigsAllCC-r16*. For all the reported bands in FR2, a same X2 value is reported for *maxNumberConfigsAllCC-r16*.- The total number of configured/active configured grant configurations across all serving cells in FR1 is no greater than X1.- The total number of configured/active configured grant configurations across all serving cells in FR2 is no greater than X2.- If the CA have some serving cell(s) in FR1 and some serving cell(s) in FR2, the total number of configured/active configured grant configurations across all serving cells is no greater than max(X1, X2). | Band | No | N/A | N/A |
| ***additionalActiveTCI-StatePDCCH***Indicates whether the UE supports one additional active TCI-State for control in addition to the supported number of active TCI-States for PDSCH. The UE can include this field only if *maxNumberActiveTCI-PerBWP* in *tci-StatePDSCH* is set to *n1*. Otherwise, the UE does not include this field. | Band | No | N/A | N/A |
| ***aperiodicBeamReport***Indicates whether the UE supports aperiodic 'CRI/RSRP' or 'SSBRI/RSRP' reporting on PUSCH. The UE provides the capability for the band number for which the report is provided (where the measurement is performed). | Band | Yes | N/A | N/A |
| ***aperiodicTRS***Indicates whether the UE supports DCI triggering aperiodic TRS associated with periodic TRS. | Band | No | N/A | Yes |
| ***asymmetricBandwidthCombinationSet***Defines the supported asymmetric channel bandwidth combination for the band as defined in the TS 38.101-1 [2]. Field encoded as a bit map, where bit N is set to "1" if UE support asymmetric channel bandwidth combination set N for this band as defined in the TS 38.101-1 [2]. The leading / leftmost bit (bit 0) corresponds to the asymmetric channel bandwidth combination set 1, the next bit corresponds to the asymmetric channel bandwidth combination set 2 and so on. UE shall support asymmetric channel bandwidth combination set 0. If the field is absent, the UE supports asymmetric channel bandwidth combination set 0. | Band | No | N/A | N/A |
| ***bandNR***Defines supported NR frequency band by NR frequency band number, as specified in TS 38.101-1 [2] and TS 38.101-2 [3]. | Band | Yes | N/A | N/A |
| ***beamCorrespondenceCSI-RS-based-r16***Indicates whether the UE support for beam correspondence based on CSI-RS has the ability to select its uplink beam based on measurement of CSI-RS. If a UE supports beam correspondence based on CSI-RS, then the network can expect the UE to also fulfil Rel-15 beam correspondence requirements.If UE supports neither *beamCorrespondenceSSB-based-r16*nor *beamCorrespondenceCSI-RS-based-r16*, gNB can expect the UE to fulfill beam correspondence based on Rel-15 beam correspondence requirements. | Band | No | TDD only | FR2 only |
| ***beamCorrespondenceSSB-based-r16***Indicates whether the UE support for beam correspondence based on SSB has the ability to select its uplink beam based on measurement of SSB. If a UE supports beam correspondence based on SSB, then the network can expect the UE to also fulfil Rel-15 beam correspondence requirements.If UE supports neither *beamCorrespondenceSSB-based-r16*nor *beamCorrespondenceCSI-RS-based-r16*, gNB can expect the UE to fulfil beam correspondence based on Rel-15 beam correspondence requirements. | Band | No | TDD only | FR2 only |
| ***beamCorrespondenceWithoutUL-BeamSweeping***Indicates how UE supports FR2 beam correspondence as specified in TS 38.101-2 [3], clause 6.6. The UE that fulfils the beam correspondence requirement without the uplink beam sweeping (as specified in TS 38.101-2 [3], clause 6.6) shall set the field to *supported*. The UE that fulfils the beam correspondence requirement with the uplink beam sweeping (as specified in TS 38.101-2 [3], clause 6.6) shall not report this field. | Band | Yes | N/A | FR2 only |
| ***beamManagementSSB-CSI-RS***Defines support of SS/PBCH and CSI-RS based RSRP measurements. The capability comprises signalling of- *maxNumberSSB-CSI-RS-ResourceOneTx* indicates maximum total number of configured one port NZP CSI-RS resources and SS/PBCH blocks that are supported by the UE to measure L1-RSRP as specified in TS 38.215 [13] within a slot and across all serving cells (see NOTE). On FR2, it is mandatory to report >=8; On FR1, it is mandatory with capability signalling to report >=8.- *maxNumberCSI-RS-Resource* indicates maximum total number of configured NZP-CSI-RS resources that are supported by the UE to measure L1-RSRP as specified in TS 38.215 [13] across all serving cells (see NOTE). It is mandated to report at least n8 for FR1.- *maxNumberCSI-RS-ResourceTwoTx* indicates maximum total number of two ports NZP CSI-RS resources that are supported by the UE to measure L1-RSRP as specified in TS 38.215 [13] within a slot and across all serving cells (see NOTE).- *supportedCSI-RS-Density* indicates density of one RE per PRB for one port NZP CSI-RS resource for RSRP reporting, if supported. On FR2, it is mandatory to report either "three" or "oneAndThree"; On FR1, it is mandatory with capability signalling to report either "three" or "oneAndThree".- *maxNumberAperiodicCSI-RS-Resource* indicates maximum number of configured aperiodic CSI-RS resources across all serving cells (see NOTE). For FR1 and FR2, the UE is mandated to report at least n4.NOTE: If the UE sets a value other than *n0* in an FR1 band, it shall set that same value in all FR1 bands. If the UE sets a value other than *n0* in an FR2 band, it shall set that same value in all FR2 bands. The UE supports a total number of resources equal to the maximum of the FR1 and FR2 value, but no more than the FR1 value across all FR1 serving cells and no more than the FR2 value across all FR2 serving cells. | Band | Yes | N/A | FD |
| ***beamReportTiming***Indicates the number of OFDM symbols between the end of the last symbol of SSB/CSI-RS and the start of the first symbol of the transmission channel containing beam report. The UE provides the capability for the band number for which the report is provided (where the measurement is performed). The UE includes this field for each supported sub-carrier spacing. | Band | Yes | N/A | N/A |
| ***beamSwitchTiming***Indicates the minimum number of OFDM symbols between the DCI triggering of aperiodic CSI-RS and aperiodic CSI-RS transmission. The number of OFDM symbols is measured from the end of the last symbol containing the indication to the start of the first symbol of CSI-RS. The UE includes this field for each supported sub-carrier spacing.NOTE: *beamSwitchTiming* of value (*sym224* or *sym336*) will be used to determine UE expectation/behaviour for aperiodic CSI-RS for tracking and latency requirements for L1-RSRP reporting as described in clause 5.1.6.1.1 of TS 38.214 [12], while UE behaviour/assumption regarding before or after beam switch timing is unspecified for measuring AP CSI-RS for CSI acquisition (without *trs-Info* and without repetition) and for beam management (with repetition 'off'). | Band | No | N/A | FR2 only |
| ***beamSwitchTiming-r16***Indicates the minimum number of required OFDM symbols (sym224, sym336) between the DCI triggering aperiodic CSI-RS and the corresponding aperiodic CSI-RS transmission in a CSI-RS resource set configured with repetition 'ON' if *enableBeamSwitchTiming-r16* is configured.For CSI-RS configured with repetition "*off*", the UE applies beam switch time of sym48 if *beamSwitchTiming-r16* is reported and *enableBeamSwitchTiming-r16* is configured. For CSI-RS configured without repetition and without *trs-info*, the UE applies beam switch time of sym48 if *beamSwitchTiming-r16* is reported and *enableBeamSwitchTiming-r16* is configured. | Band | No | N/A | FR2 only |
| ***bwp-DiffNumerology***Indicates whether the UE supports BWP adaptation up to 4 BWPs with the different numerologies, via DCI and timer. Except for SUL, the UE only supports the same numerology for the active UL and DL BWP. For the UE capable of this feature, the bandwidth of a UE-specific RRC configured DL BWP includes the bandwidth of the CORESET#0 (if CORESET#0 is present) and SSB for PCell and PSCell (if configured). For SCell(s), the bandwidth of the UE-specific RRC configured DL BWP includes SSB, if there is SSB on SCell(s). | Band | No | N/A | N/A |
| ***bwp-SameNumerology***Indicates whether UE supports BWP adaptation (up to 2/4 BWPs) with the same numerology, via DCI and timer. Except for SUL, the UE only supports the same numerology for the active UL and DL BWP. For the UE capable of this feature, the bandwidth of a UE-specific RRC configured DL BWP includes the bandwidth of the CORESET#0 (if CORESET#0 is present) and SSB for PCell and PSCell (if configured). For SCell(s), the bandwidth of the UE-specific RRC configured DL BWP includes SSB, if there is SSB on SCell(s). | Band | No | N/A | N/A |
| ***bwp-WithoutRestriction***Indicates support of BWP operation without bandwidth restriction. The Bandwidth restriction in terms of DL BWP for PCell and PSCell means that the bandwidth of a UE-specific RRC configured DL BWP may not include the bandwidth of CORESET #0 (if configured) and SSB. For SCell(s), it means that the bandwidth of DL BWP may not include SSB. | Band | No | N/A | N/A |
| ***cancelOverlappingPUSCH-r16***Indicates whether UE supports the cancellation of the (repetition of the) PUSCHs transmission on all other intra-band serving cell(s). The cancellation of the (repetition of the) PUSCH transmission on a the set of intra-band serving cell(s) includes all symbols from the earliest symbol that is overlapping with the first cancelled symbol of the PUSCH on the serving cell for which the DCI format 2\_4 is applicable to. If the UE supports this feature, the UE needs to report *pa-PhaseDiscontinuityImpacts* and *ul-CancellationSelfCarrier-r16*. | Band | No | N/A | N/A |
| ***channelBWs-DL***Indicates for each subcarrier spacing the UE supported channel bandwidths.Absence of the *channelBWs-DL* (without suffix) for a band or absence of specific scs-XXkHz entry for a supported subcarrier spacing means that the UE supports the channel bandwidths among [5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 100] and [50, 100, 200] that were defined in clause 5.3.5 of TS 38.101-1 version 15.7.0 [2] and TS 38.101-2 version 15.7.0 [3] for the given band or the specific SCS entry. For IAB-MT, to determine whether the IAB-MT supports a channel bandwidth of 100 MHz, the network checks c*hannelBW-DL-IAB-r16*.For FR1, the bits in *channelBWs-DL* (without suffix) starting from the leading / leftmost bit indicate 5, 10, 15, 20, 25, 30, 40, 50, 60 and 80MHz. For FR2, the bits in *channelBWs-DL* (without suffix) starting from the leading / leftmost bit indicate 50, 100 and 200MHz. The third / rightmost bit (for 200MHz) shall be set to 1. For IAB-MT the third / rightmost bit (for 200MHz) is ignored. To determine whether the IAB-MT supports a channel bandwidth of 200 MHz, the network checks *channelBW-DL-IAB-r16*.For FR1, the leading/leftmost bit in *channelBWs-DL-v1590* indicates 70MHz, the second leftmost bit indicates 45MHz, the third leftmost bit indicates 35MHz, the fourth leftmost bit indicates 100MHz and all the remaining bits in *channelBWs-DL-v1590* shall be set to 0. The fourth leftmost bit (for 100MHz) is not applicable for bands n41, n48, n77, n78, n79 and n90 as defined in TS 38.101-1 [2].NOTE: To determine whether the UE supports a specific SCS for a given band, the network validates the *supportedSubCarrierSpacingDL* and the *scs-60kHz*.To determine whether the UE supports a channel bandwidth of 90 MHz, the network may ignore this capability and validate instead the *channelBW-90mhz*, the *supportedBandwidthCombinationSet* and the *supportedBandwidthCombinationSetIntraENDC*. For serving cell(s) with other channel bandwidths the network validates the *channelBWs-DL*, the *supportedBandwidthCombinationSet*, the *supportedBandwidthCombinationSetIntraENDC*, the *asymmetricBandwidthCombinationSet* (for a band supporting asymmetric channel bandwidth as defined in clause 5.3.6 of TS 38.101-1 [2]) and *supportedBandwidthDL*. | Band | Yes | N/A | N/A |
| ***channelBWs-UL***Indicates for each subcarrier spacing the UE supported channel bandwidths.Absence of the *channelBWs-UL* (without suffix) for a band or absence of specific scs-XXkHz entry for a supported subcarrier spacing means that the UE supports the channel bandwidths among [5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 100] and [50, 100, 200] that were defined in clause 5.3.5 of TS 38.101-1 version 15.7.0 [2] and TS 38.101-2 version 15.7.0 [3] for the given band or the specific SCS entry. For IAB-MT, to determine whether the IAB-MT supports a channel bandwidth of 100 MHz, the network checks *channelBW-UL-IAB-r16*.For FR1, the bits in *channelBWs-UL* (without suffix) starting from the leading / leftmost bit indicate 5, 10, 15, 20, 25, 30, 40, 50, 60 and 80MHz. For FR2, the bits in *channelBWs-UL* (without suffix) starting from the leading / leftmost bit indicate 50, 100 and 200MHz. The third / rightmost bit (for 200MHz) shall be set to 1. For IAB-MT the third / rightmost bit (for 200MHz) is ignored. To determine whether the IAB-MT supports a channel bandwidth of 200 MHz, the network checks *channelBW-UL-IAB-r16*.For FR1, the leading/leftmost bit in *channelBWs-UL-v1590* indicates 70 MHz, the second leftmost bit indicates 45MHz, the third leftmost bit indicates 35MHz, the fourth leftmost bit indicates 100MHz and all the remaining bits in *channelBWs-UL-v1590* shall be set to 0. The fourth leftmost bit (for 100MHz) is not applicable for bands n41, n48, n77, n78, n79 and n90 as defined in TS 38.101-1 [2].NOTE: To determine whether the UE supports a specific SCS for a given band, the network validates the *supportedSubCarrierSpacingUL* and the *scs-60kHz*.To determine whether the UE supports a channel bandwidth of 90 MHz the network may ignore this capability and validate instead the *channelBW-90mhz*, the *supportedBandwidthCombinationSet* and the *supportedBandwidthCombinationSetIntraENDC*. For serving cell(s) with other channel bandwidths the network validates the *channelBWs-UL*, the *supportedBandwidthCombinationSet*, the *supportedBandwidthCombinationSetIntraENDC*, the *asymmetricBandwidthCombinationSet* (for a band supporting asymmetric channel bandwidth as defined in clause 5.3.6 of TS 38.101-1 [2]) and *supportedBandwidthUL*. | Band | Yes | N/A | N/A |
| ***channelBW-DL-IAB-r16***Indicates whether the IAB-MT supports channel bandwidth of 100 MHz for a given SCS in FR1 for DL or whether the IAB-MT supports channel bandwidth of 200 MHz for a given SCS in FR2 for DL. | Band | No | N/A | N/A |
| ***channelBW-UL-IAB-r16***Indicates whether the IAB-MT supports channel bandwidth of 100 MHz for a given SCS in FR1 for UL or whether the IAB-MT supports channel bandwidth of 200 MHz for a given SCS in FR2 for UL. | Band | No | N/A | N/A |
| ***codebookComboParametersAddition-r16***Indicates the UE supports of the mixed codebook combinations and the corresponding parameters supported by the UE.For mixed codebook types, UE reports support active CSI-RS resources and ports for up to 4 mixed codebook combinations in any slot. The following is the possible mixed codebook combinations:- {Type 1 Single Panel, Type 2, Null}- {Type 1 Single Panel, Type 2 with port selection, Null}- {Type 1 Single Panel, eType 2 with R=1, Null}- {Type 1 Single Panel, eType 2 with R=2, Null}- {Type 1 Single Panel, eType 2 with R=1 and port selection, Null}- {Type 1 Single Panel, eType 2 with R=2 and port selection, Null}- {Type 1 Single Panel, Type 2, Type 2 with port selection}- {Type 1 Multi Panel, Type 2, Null}- {Type 1 Multi Panel, Type 2 with port selection, Null}- {Type 1 Multi Panel, eType 2 with R=1, Null}- {Type 1 Multi anel, eType 2 with R=2, Null}- {Type 1 Multi Panel, eType 2 with R=1 with port selection, Null}- {Type 1 Multi Panel, eType 2 with R=2 with port selection, Null}- {Type 1 Multi Panel, Type 2, Type 2 with port selection}Parameters for each mixed codebook supported by the UE:- *supportedCSI-RS-ResourceListAdd-r16* indicates the list of supported CSI-RS resources in a band by referring to *codebookVariantsList*. The following parameters are included in *codebookVariantsList*:For *supportedCSI-RS-ResourceListAdd-r16* related to the additional codebooks:- The minimum of *maxNumberTxPortsPerResource* is '*p4*';- The minimum value of *totalNumberTxPortsPerBand* is 4.If a UE reports one or more mixed codebook combinations, then usage of active CSI-RS resources and ports for multiple codebooks in any slot is allowed only within those combinations. For coexisting of mixed codebooks in any slot, gNB needs to consider the mixed codebook combination capability as well as per codebook capability of each codebook type in the mixed codebook combination.UE indicates support of a codebook type in the mixed codebook combination shall indicates support of the individual codebook type in the per band capability. | Band | No | N/A | N/A |
| ***codebookParameters***Indicates the codebooks and the corresponding parameters supported by the UE.Parameters for type I single panel codebook (type1 singlePanel) supported by the UE, which are mandatory to report:- *supportedCSI-RS-ResourceList*;- a UE shall support a *maxNumberTxPortsPerResource* minimum value of 4 for codebook type I single panel in FR1 in the case of a single active CSI-resource across all bands in a band combination, regardless of what it reports in *supportedCSI-RS-ResourceList* with *maxNumberTxPortsPerResource*;- a UE shall support a *maxNumberTxPortsPerResource* minimum value of 8 when configured with wideband CSI report for codebook type I single panel in FR1 in the case of a single active CSI-resource across all bands in a band combination, regardless of what it reports in *supportedCSI-RS-ResourceList* with *maxNumberTxPortsPerResource*;- a UE shall support a *maxNumberTxPortsPerResource* minimum value of 2 for codebook type I single panel in FR2 in the case of a single active CSI-resource across all bands in a band combination, regardless of what it reports in *supportedCSI-RS-ResourceList* with *maxNumberTxPortsPerResource*.- *modes* indicates supported codebook modes (mode 1, both mode 1 and mode 2);- *maxNumberCSI-RS-PerResourceSet* indicates the maximum number of CSI-RS resource in a resource set.Parameters for type I multi-panel codebook (type1 multiPanel) supported by the UE, which are optional:- *supportedCSI-RS-ResourceList*;- *modes* indicates supported codebook modes (mode 1, mode 2, or both mode 1 and mode 2);- *maxNumberCSI-RS-PerResourceSet* indicates the maximum number of CSI-RS resource in a resource set;- *nrofPanels* indicates supported number of panels.Parameters for type II codebook (type2) supported by the UE, which are optional:- *supportedCSI-RS-ResourceList*;- *parameterLx* indicates the parameter "Lx" in codebook generation where x is an index of Tx ports indicated by *maxNumberTxPortsPerResource*;- *amplitudeScalingType* indicates the amplitude scaling type supported by the UE (wideband or both wideband and sub-band);- *amplitudeSubsetRestriction* indicates whether amplitude subset restriction is supported for the UE.Parameters for type II codebook with port selection (type2-PortSelection) supported by the UE, which are optional:- *supportedCSI-RS-ResourceList*;- *parameterLx* indicates the parameter "Lx" in codebook generation where x is an index of Tx ports indicated by *maxNumberTxPortsPerResource*;- *amplitudeScalingType* indicates the amplitude scaling type supported by the UE (wideband or both wideband and sub-band).*supportedCSI-RS-ResourceList* includes list of the following parameters:- *maxNumberTxPortsPerResource* indicates the maximum number of Tx ports in a resource;- *maxNumberResourcesPerBand* indicates the maximum number of resources across all CCs within a band simultaneously;- *totalNumberTxPortsPerBand* indicates the total number of Tx ports across all CCs within a band simultaneously.For each codebook type, the UE may report another list of supported CSI-RS resources via *supportedCSI-RS-ResourceListAlt* in *codebookParametersPerBand*. For type I single panel codebook (type1 singlePanel) supportedCSI-RS-ResourceListAlt,- a UE shall report at least one triplet in supportedCSI-RS-ResourceListAlt with maxNumberTxPortsPerResource greater than or equal to 8 for FR1;- a UE shall report at least one triplet in supportedCSI-RS-ResourceListAlt with maxNumberTxPortsPerResource greater than or equal to 2 for FR2. | Band | FD | N/A | N/A |
| ***codebookParametersAddition-r16***Indicates the UE support of additional codebooks and the corresponding parameters supported by the UE.Codebook etype 2 R=1 support parameter combination 1 to 6 and rank 1 to 2. Parameters for etype 2 R=1 (*etype2R1-r16*) supported by the UE, which are optional:- *supportedCSI-RS-ResourceListAdd-r16* indicates the list of supported CSI-RS resources in a band by referring to *codebookVariantsList*. The following parameters are included in *codebookVariantsList*:- *maxNumberTxPortsPerResource* indicates the maximum number of Tx ports in a resource of a band;- *maxNumberResourcesPerBand* indicates the maximum number of resources across all CCs in a band, simultaneously;- *totalNumberTxPortsPerBand* indicates the total number of Tx ports across all CCs in a band, simultaneously.- *paramComb7-8-r16* indicates the support of parameter combinations 7-8 for etype 2 R=1- *rank3-4-r16* indicates the support of rank 3,4.- *amplitudeSubsetRestriction-r16* indicates the support of amplitude subset restriction.Parameters for etype 2 R=2 (*etype2R2-r16*) supported by the UE, which are optional:- *supportedCSI-RS-ResourceListAdd-r16*;UE supporting *etype2R2-r16*supports also indicates support of *etype2R1-r16*.Codebook etype 2 R=1 with port selection supports 6 parameter combinations and rank 1,2. Parameters for etype 2 R=1 with port selection (*etype2R1-PortSelection-r16*) supported by the UE, which are optional:- *supportedCSI-RS-ResourceListAdd-r16*;- *rank3-4-r16* indicates the support of rank 3,4Parameters for etype 2 R=2 with port selection (*etype2R2-PortSelection-r16*) supported by the UE, which are optional:- *supportedCSI-RS-ResourceListAdd-r16*;UE supporting *etype2R2-PortSelection-r16* also indicates support of *etype2R1-PortSelection-r16*.For *supportedCSI-RS-ResourceListAdd-r16* related to the additional codebooks:- The minimum of *maxNumberTxPortsPerResource* is '*p4*';- The minimum value of *totalNumberTxPortsPerBand* is 4. | Band | No | N/A | N/A |
| ***condHandover-r16***Indicates whether the UE supports conditional handover including execution condition, candidate cell configuration and maximum 8 candidate cells. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively. | Band | No | N/A | N/A |
| ***condHandoverFailure-r16***Indicates whether the UE supports conditional handover during re-establishment procedure when the selected cell is configured as candidate cell for condition handover. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively. | Band | No | N/A | N/A |
| ***condHandoverTwoTriggerEvents-r16***Indicates whether the UE supports 2 trigger events for same execution condition. This feature is mandatory supported if the UE supports *condHandover-r16*. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively. | Band | CY | N/A | N/A |
| ***condPSCellChange-r16***Indicates whether the UE supports conditional PSCell change including execution condition, candidate cell configuration and maximum 8 candidate cells. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively. | Band | No | N/A | N/A |
| ***condPSCellChangeTwoTriggerEvents-r16***Indicates whether the UE supports 2 trigger events for same execution condition. This feature is mandatory supported if the UE supports *condPSCellChange-r16*. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively. | Band | CY | N/A | N/A |
| ***configuredUL-GrantType1-v1650***Indicates whether the UE supports Type 1 PUSCH transmissions with configured grant as specified in TS 38.214 [12] with UL-TWG-repK value of one. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *configuredUL-GrantType1-r16* applies. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively.The UE only includes *configuredUL-GrantType1-v1650* if *configuredUL-GrantType1* is absent. | Band | No | N/A | N/A |
| ***configuredUL-GrantType2-v1650***Indicates whether the UE supports Type 2 PUSCH transmissions with configured grant as specified in TS 38.214 [12] with UL-TWG-repK value of one. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *configuredUL-GrantType2-r16* applies. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively.The UE only includes *configuredUL-GrantType2*-v1650 if *configuredUL-GrantType2* is absent. | Band | No | N/A | N/A |
| ***crossCarrierScheduling-SameSCS***Indicates whether the UE supports cross carrier scheduling for the same numerology with carrier indicator field (CIF) in carrier aggregation where numerologies for the scheduling cell and scheduled cell are same. | Band | No | N/A | N/A |
| ***csi-ReportFramework***Indicates whether the UE supports CSI report framework. This capability signalling comprises the following parameters:- *maxNumberPeriodicCSI-PerBWP-ForCSI-Report* indicates the maximum number of periodic CSI report setting per BWP for CSI report;- *maxNumberPeriodicCSI-PerBWP-ForBeamReport* indicates the maximum number of periodic CSI report setting per BWP for beam report.- *maxNumberAperiodicCSI-PerBWP-ForCSI-Report* indicates the maximum number of aperiodic CSI report setting per BWP for CSI report;- *maxNumberAperiodicCSI-PerBWP-ForBeamReport* indicates the maximum number of aperiodic CSI report setting per BWP for beam report;- *maxNumberAperiodicCSI-triggeringStatePerCC* indicates the maximum number of aperiodic CSI triggering states in *CSI-AperiodicTriggerStateList* per CC;- *maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report* indicates the maximum number of semi-persistent CSI report setting per BWP for CSI report;- *maxNumberSemiPersistentCSI-PerBWP-ForBeamReport* indicates the maximum number of semi-persistent CSI report setting per BWP for beam report;- *simultaneousCSI-ReportsPerCC* indicates the number of CSI report(s) for which the UE can measure and process reference signals simultaneously in a CC of the band for which this capability is provided. The CSI report comprises periodic, semi-persistent and aperiodic CSI and any latency classes and codebook types. The CSI report in simultaneousCSI-ReportsPerCC includes the beam report and CSI report.The UE is mandated to report *csi-ReportFramework*. | Band | Yes | N/A | N/A |
| ***csi-ReportFrameworkExt-r16***Indicates whether the UE supports the extension of the maximum number of configured aperiodic CSI report settings for all codebook types. The capability signalling comprises the following:*maxNumberAperiodicCSI-PerBWP-ForCSI-ReportExt-r16* indicates the extended maximum number of aperiodic CSI report setting per BWP for CSI report. If present, the value of *maxNumberAperiodicCSI-PerBWP-ForCSI-Report-r16* shall replace the corresponding value in *csi-ReportFramework*. | Band | No | N/A | N/A |
| ***csi-RS-ForTracking***Indicates support of CSI-RS for tracking (i.e. TRS). This capability signalling comprises the following parameters:- *maxBurstLength* indicates the TRS burst length. Value 1 indicates 1 slot and value 2 indicates both of 1 slot and 2 slots. In this release UE is mandated to report value 2;- *maxSimultaneousResourceSetsPerCC* indicates the maximum number of TRS resource sets per CC which the UE can track simultaneously;- *maxConfiguredResourceSetsPerCC* indicates the maximum number of TRS resource sets configured to UE per CC. It is mandated to report at least 8 for FR1 and 16 for FR2;- *maxConfiguredResourceSetsAllCC* indicates the maximum number of TRS resource sets configured to UE across CCs. If the UE includes the field in an FR1 band, it shall set the same value in all FR1 bands. If the UE includes the field in an FR2 band, it shall set the same value in all FR2 bands. The UE supports a total number of resources equal to the maximum of the FR1 and FR2 value, but no more than the FR1 value across all FR1 serving cells and no more than the FR2 value across all FR2 serving cells. The UE is mandated to report at least 16 for FR1 and 32 for FR2.The UE is mandated to report *csi-RS-ForTracking*. | Band | Yes | N/A | N/A |
| ***csi-RS-IM-ReceptionForFeedback***Indicates support of CSI-RS and CSI-IM reception for CSI feedback. This capability signalling comprises the following parameters:- *maxConfigNumberNZP-CSI-RS-PerCC* indicates the maximum number of configured NZP-CSI-RS resources per CC;- *maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC* indicates the maximum number of ports across all configured NZP-CSI-RS resources per CC;- *maxConfigNumberCSI-IM-PerCC* indicates the maximum number of configured CSI-IM resources per CC;- *maxNumberSimultaneousNZP-CSI-RS-PerCC* indicates the maximum number of simultaneous CSI-RS-resources per CC;- *totalNumberPortsSimultaneousNZP-CSI-RS-PerCC* indicates the total number of CSI-RS ports in simultaneous CSI-RS resources per CC.The UE is mandated to report csi-RS-IM-ReceptionForFeedback. | Band | Yes | N/A | N/A |
| ***csi-RS-ProcFrameworkForSRS***Indicates support of CSI-RS processing framework for SRS. This capability signalling comprises the following parameters:- *maxNumberPeriodicSRS-AssocCSI-RS-PerBWP* indicates the maximum number of periodic SRS resources associated with CSI-RS per BWP;- *maxNumberAperiodicSRS-AssocCSI-RS-PerBWP* indicates the maximum number of aperiodic SRS resources associated with CSI-RS per BWP;- *maxNumberSP-SRS-AssocCSI-RS-PerBWP* indicates the maximum number of semi-persistent SRS resources associated with CSI-RS per BWP;- *simultaneousSRS-AssocCSI-RS-PerCC* indicates the number of SRS resources that the UE can process simultaneously in a CC, including periodic, aperiodic and semi-persistent SRS. | Band | No | N/A | N/A |
| ***defaultQCL-PerCORESETPoolIndex-r16***Indicates whether the UE supports default QCL assumption per CORESET pool index using multi-DCI based multi-TRP. The UE that indicates support of this feature shall support *multiDCI-MultiTRP-r16* and *simultaneousReceptionDiffTypeD-r16.* | Band | No | N/A | FR2 only |
| ***defaultQCL-TwoTCI-r16***Indicates whether the UE supports default QCL assumption with two TCI states using single-DCI based multi-TRP. The UE can include this field only if *simultaneousReceptionDiffTypeD-r16*is present. Otherwise, the UE does not include this field. | Band | No | N/A | FR2 only |
| ***enhancedSkipUplinkTxConfigured-v1660***Indicates whether the UE supports skipping UL transmission for a configured uplink grant only if no data is available for transmission and no UCI is multiplexed on the corresponding PUSCH of the uplink grant as specified in TS 38.321 [8]. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively.The UE only includes *enhancedSkipUplinkTxConfigured-v1660* if *enhancedSkipUplinkTxConfigured-r16* is absent. | Band | No | N/A | N/A |
| ***enhancedSkipUplinkTxDynamic-v1660***Indicates whether the UE supports skipping UL transmission for an uplink grant addressed to a C-RNTI only if no data is available for transmission and no UCI is multiplexed on the corresponding PUSCH of the uplink grant as specified in TS 38.321 [8]. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively.The UE only includes *enhancedSkipUplinkTxDynamic-v1660* if *enhancedSkipUplinkTxDynamic-r16* is absent. | Band | No | N/A | N/A |
| ***enhancedUL-TransientPeriod-r16***Indicates whether the UE supports enhanced UL performance for the transient period as specified in clause 6.3.3 of TS 38.101-1 [2]. If not reported, the UE supports transient period of 10us. | Band | No | N/A | FR1 only |
| ***extendedCP***Indicates whether the UE supports 60 kHz subcarrier spacing with extended CP length for reception of PDCCH, and PDSCH, and transmission of PUCCH, PUSCH, and SRS. | Band | No | N/A | N/A |
| ***groupBeamReporting***Indicates whether UE supports RSRP reporting for the group of two reference signals. | Band | No | N/A | N/A |
| ***groupSINR-reporting-r16***Indicates whether UE supports group based L1-SINR reporting. UE indicates support of this feature shall indicate support of *ssb-csirs-SINR-measurement-r16.* | Band | No | N/A | N/A |
| ***handoverUTRA-FDD-r16***Indicates whether the UE supports NR to UTRA-FDD CELL\_DCH CS handover for the PCell on the band. It is mandatory to support both UTRA-FDD measurement and event B triggered reporting, and periodic UTRA-FDD measurement and reporting if the UE supports HO to UTRA-FDD. If this field is included, then UE shall support IMS voice over NR. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively. | Band | No | N/A | N/A |
| ***maxMIMO-LayersForMulti-DCI-mTRP-r16***Indicates the interpretation of *maxNumberMIMO-LayersPDSCH* for multi-DCI based mTRP. If this field is included, *maxNumberMIMO-LayersPDSCH* is interpreted as the maximum number of layers per PDSCH for multi-DCI multi-TRP operation.If this field is not included, *maxNumberMIMO-LayersPDSCH* is interpreted as the maximum number of layers across two PDSCHs if having at least one RE overlapped, for multi-DCI multi-TRP operation. The UE that indicates support of this feature shall support *overlapPDSCHsFullyFreqTime-r16*.NOTE 1: For data rate calculation in clause 4.1.2, if this feature is indicated, each multi-DCI based multi-TRP CC is counted two times toward J. | Band | No | N/A | N/A |
| ***jointReleaseConfiguredGrantType2-r16***Indicates whether the UE supports joint release in a DCI for two or more configured grant Type 2 configurations for a given BWP of a serving cell. The UE can include this feature only if the UE indicates supports of *activeConfiguredGrant-r16*. | Band | No | N/A | N/A |
| ***jointReleaseSPS-r16***Indicates whether the UE supports joint release in a DCI for two or more SPS configurations for a given BWP of a serving cell. The UE can include this feature only if the UE indicates supports of *sps-r16*. | Band | No | N/A | N/A |
| ***lowPAPR-DMRS-PDSCH-r16***Indicates whether the UE supports low PAPR DMRS for PDSCH. | Band | No | N/A | N/A |
| ***lowPAPR-DMRS-PUCCH-r16***Indicates whether the UE supports low PAPR DMRS for PUCCH format 3 and format 4 with transform precoding and with pi/2 BPSK modulation. UE indicates support of this feature shall indicate support of *pucch-F3-4-HalfPi-BPSK* and any combination of support of *pucch-F3-WithFH*, *pucch-F4-WithFH* and *pucch-F1-3-4WithoutFH*. | Band | No | N/A | N/A |
| ***lowPAPR-DMRS-PUSCHwithoutPrecoding-r16***Indicates whether the UE supports low PAPR DMRS for PUSCH without transform precoding. | Band | No | N/A | N/A |
| ***lowPAPR-DMRS-PUSCHwithPrecoding-r16***Indicates whether the UE supports low PAPR DMRS for PUSCH with transform precoding and with pi/2 BPSK modulation. UE indicates support of this feature shall indicate support of *pusch-HalfPi-BPSK*. | Band | No | N/A | N/A |
| ***maxNumberActivatedTCI-States-r16***Indicates maximum number of activated TCI states. This capability signalling includes the following:- *maxNumberPerCORESET-Pool-r16* indicates maximal number of activated TCI states per *CORESETPoolIndex* per BWP per CC including data and control- *maxTotalNumberAcrossCORESET-Pool-r16* indicates maximal total number of activated TCI states across *CORESETPoolIndex* per BWP per CC including data and controlThe UE that indicates support of this feature shall support *multiDCI-MultiTRP-r16*. | Band | No | N/A | N/A |
| ***maxNumberCSI-RS-BFD***Indicates maximal number of CSI-RS resources across all CCs, and across MCG and SCG in case of NR-DC, for UE to monitor PDCCH quality. In this release, the maximum value that can be signalled is 16. If the UE includes the field in an FR1 band, it shall set the same value in all FR1 bands. If the UE includes the field in an FR2 band, it shall set the same value in all FR2 bands. The UE supports a total number of resources equal to the maximum of the FR1 and FR2 value, but no more than the FR1 value across all FR1 serving cells and no more than the FR2 value across all FR2 serving cells. It is mandatory with capability signalling for FR2 and optional for FR1. | Band | CY | N/A | N/A |
| ***maxNumberCSI-RS-SSB-CBD***Defines maximal number of different CSI-RS [and/or SSB] resources across all CCs, and across MCG and SCG in case of NR-DC, for new beam identifications. In this release, the maximum value that can be signalled is 128. If the UE includes the field in an FR1 band, it shall set the same value in all FR1 bands. If the UE includes the field in an FR2 band, it shall set the same value in all FR2 bands. The UE supports a total number of resources equal to the maximum of the FR1 and FR2 value, but no more than the FR1 value across all FR1 serving cells and no more than the FR2 value across all FR2 serving cells. It is mandatory with capability signalling for FR2 and optional for FR1. The UE is mandated to report at least 32 for FR2. | Band | CY | N/A | N/A |
| ***maxNumberNonGroupBeamReporting***Defines support of non-group based RSRP reporting using N\_max RSRP values reported. | Band | Yes | N/A | N/A |
| ***maxNumberRxBeam***Defines whether UE supports receive beamforming switching using NZP CSI-RS resource. UE shall indicate a single value for the preferred number of NZP CSI-RS resource repetitions per CSI-RS resource set. Support of Rx beam switching is mandatory for FR2. | Band | CY | N/A | N/A |
| ***maxNumberRxTxBeamSwitchDL***Defines the number of Tx and Rx beam changes UE can perform on this band within a slot. UE shall report one value per each subcarrier spacing supported by the UE. In this release, the number of Tx and Rx beam changes for scs-15kHz and scs-30kHz are not included. | Band | No | N/A | FR2 only |
| ***maxNumberSCellBFR-r16***Defines the maximum number of SCells configured for SCell beam failure recovery simultaneously. The UE indicating support of this also indicates the capabilities of *maxNumberCSI-RS-BFD, maxNumberSSB-BFD* and *maxNumberCSI-RS-SSB-CBD.* | Band | No | N/A | N/A |
| ***maxNumberSSB-BFD***Defines maximal number of different SSBs across all CCs, and across MCG and SCG in case of NR-DC, for UE to monitor PDCCH quality. In this release, the maximum value that can be signalled is 16. If the UE includes the field in an FR1 band, it shall set the same value in all FR1 bands. If the UE includes the field in an FR2 band, it shall set the same value in all FR2 bands. The UE supports a total number of resources equal to the maximum of the FR1 and FR2 value, but no more than the FR1 value across all FR1 serving cells and no more than the FR2 value across all FR2 serving cells. It is mandatory with capability signalling for FR2 and optional for FR1. | Band | CY | N/A | N/A |
| ***maxUplinkDutyCycle-PC2-FR1***Indicates the maximum percentage of symbols during a certain evaluation period that can be scheduled for uplink transmission so as to ensure compliance with applicable electromagnetic energy absorption requirements provided by regulatory bodies. This field is only applicable for FR1 power class 2 UE as specified in clause 6.2.1 of TS 38.101-1 [2]. If the field is absent, 50% shall be applied. Value n60 corresponds to 60%, value n70 corresponds to 70% and so on. This capability is not applicable to IAB-MT. | Band | No | N/A | FR1 only |
| ***maxUplinkDutyCycle-FR2***Indicates the maximum percentage of symbols during 1s that can be scheduled for uplink transmission at the UE maximum transmission power, so as to ensure compliance with applicable electromagnetic power density exposure requirements provided by regulatory bodies. This field is applicable for all power classes UE in FR2 as specified in TS 38.101-2 [3]. Value n15 corresponds to 15%, value n20 corresponds to 20% and so on. If the field is absent or the percentage of uplink symbols transmitted within any 1s evaluation period is larger than *maxUplinkDutyCycle-FR2*, the UE behaviour is specified in TS 38.101-2 [3]. This capability is not applicable to IAB-MT. | Band | No | N/A | FR2 only |
| ***maxUplinkDutyCycle-PC1dot5-MPE-FR1-r16***Indicates the maximum percentage of symbols during a certain evaluation period that can be scheduled for uplink transmission so as to ensure compliance with applicable electromagnetic energy absorption requirements provided by regulatory bodies. This field is only applicable for FR1 power class 1.5 UE as specified in clause 6.2.1 of TS 38.101-1 [2]. If the field is absent, UE shall mitigate MPE autonomously by P-MPR or by other means and no restriction on scheduled uplink duty cycle is needed. | Band | No | N/A | FR1 only |
| ***modifiedMPR-Behaviour***Indicates whether UE supports modified MPR behaviour defined in TS 38.101-1 [2] and TS 38.101-2 [3]. | Band | No | N/A | N/A |
| ***mpr-PowerBoost-FR2-r16***Indicates whether UE supports uplink transmission power boost by suspension of in-band emission (IBE) requirements as specified in TS 38.101-2 [3]. | Band | No | TDD only | FR2 only |
| ***multipleRateMatchingEUTRA-CRS-r16***Indicates whether the UE supports multiple E-UTRA CRS rate matching patterns, which is supported only for FR1. The capability signalling comprises the following parameters:- *maxNumberPatterns-r16* indicates the maximum number of LTE-CRS rate matching patterns in total within a NR carrier using 15 kHz SCS. The UE can report the value larger than 2 only if UE reports the value of *maxNumberNon-OverlapPatterns-r16* is larger than 1.- *maxNumberNon-OverlapPatterns-r16* indicates the maximum number of LTE-CRS non-overlapping rate matching patterns within a NR carrier using 15 kHz SCS.The UE can include this feature only if the UE indicates support of *rateMatchingLTE-CRS*. | Band | No | N/A | FR1 only |
| ***multipleTCI***Indicates whether UE supports more than one TCI state configurations per CORESET. UE is only required to track one active TCI state per CORESET. UE is required to support minimum between 64 and number of configured TCI states indicated by *tci-StatePDSCH*. This field shall be set to *supported*. | Band | Yes | N/A | N/A |
| ***nonGroupSINR-reporting-r16***Indicates N\_max L1-SINR values reported when UE supports non-group based L1-SINR reporting. UE indicates support of this feature shall indicate support of *ssb-csirs-SINR-measurement-r16.* | Band | No | N/A | N/A |
| ***olpc-SRS-Pos-r16***Indicates whether the UE supports OLPC for SRS for positioning. The capability signalling comprises the following parameters.- *olpc-SRS-PosBasedOnPRS-Serving-r16* indicates whether the UE supports OLPC for SRS for positioning based on PRS from the serving cell in the same band. The UE can include this field only if the UE supports *NR-DL-PRS-ProcessingCapability-r16* defined in TS 37.355 [22], and *srs-PosResources-r16*. Otherwise, the UE does not include this field;- *olpc-SRS-PosBasedOnSSB-Neigh-r16* indicates whether the UE supports OLPC for SRS for positioning based on SSB from the neighbouring cell in the same band. The UE can include this field only if the UE supports *srs-PosResources-r16*. Otherwise, the UE does not include this field;- *olpc-SRS-PosBasedOnPRS-Neigh-r16* indicates whether the UE supports OLPC for SRS for positioning based on PRS from the neighbouring cell in the same band. The UE can include this field only if the UE supports *olpc-SRS-PosBasedOnPRS-Serving-r16*. Otherwise, the UE does not include this field;NOTE: A PRS from a PRS-only TP is treated as PRS from a non-serving cell.- *maxNumberPathLossEstimatePerServing-r16* indicates the maximum number of pathloss estimates that the UE can simultaneously maintain for all the SRS resource sets for positioning per serving cell in addition to the up to four pathloss estimates that the UE maintains per serving cell for the PUSCH/PUCCH/SRS transmissios. The UE shall include this field if the UE supports any of *olpc-SRS-PosBasedOnPRS-Serving-r16, olpc-SRS-PosBasedOnSSB-Neigh-r16* and *olpc-SRS-PosBasedOnPRS-Neigh-r16.* Otherwise, the UE does not include this field. | Band | No | N/A | N/A |
| ***oneSlotPeriodicTRS-r16***Indicates whether the UE supports one-slot periodic TRS configuration only when no two consecutive slots are indicated as downlink slots by *tdd-UL-DL-ConfigurationCommon* or *tdd-UL-DL-ConfigDedicated*. If the UE supports this feature, the UE needs to report *csi-RS-ForTracking*. | Band | No | TDD only | FR1 only |
| ***outOfOrderOperationDL-r16***Indicates whether the UE supports out of order operation for DL. The UE that indicates support of this feature shall support *multiDCI-MultiTRP-r16*. The capability signalling comprises the following parameters:*- supportPDCCH-ToPDSCH-r16* indicates support out-of-order operation for PDCCH to PDSCH;*- supportPDSCH-ToHARQ-ACK-r16* indicates support out-of-order operation for PDSCH to HARQ-ACK. | Band | No | N/A | N/A |
| ***outOfOrderOperationUL-r16***Indicates whether the UE supports out of order operation for UL. The UE that indicates support of this feature shall support *multiDCI-MultiTRP-r16.*Note: Same closed loop index for power control across PUSCHs associated with different *CORESETPoolIndex* values is not supported by a UE indicating the support of this feature when TPC accumulation is enabled. | Band | No | N/A | N/A |
| ***overlapPDSCHsFullyFreqTime-r16***Indicates the maximal number of PDSCH scrambling sequences per serving cell when the UE supports PDSCHs with fully overlapping Resource Elements. The UE that indicates support of this feature shall support *multiDCI-MultiTRP-r16.*Note: A UE may assume that its maximum receive timing difference between the DL transmissions from two TRPs is within a Cyclic Prefix | Band | No | N/A | N/A |
| ***overlapPDSCHsInTimePartiallyFreq-r16***Indicates whether the UE support PDSCHs with partially overlapping Resource Elements. The UE that indicates support of this feature shall support *multiDCI-MultiTRP-r16.* | Band | No | N/A | N/A |
| ***overlapRateMatchingEUTRA-CRS-r16***Indicates whether the UE supports two LTE-CRS overlapping rate matching patterns within a part of NR carrier using 15 kHz SCS overlapping with a LTE carrier. If the UE supports this feature, the UE needs to report *multipleRateMatchingEUTRA-CRS-r16*. | Band | No | N/A | FR1 only |
| ***pdsch-256QAM-FR2***Indicates whether the UE supports 256QAM modulation scheme for PDSCH for FR2 as defined in 7.3.1.2 of TS 38.211 [6]. | Band | No | N/A | FR2 only |
| ***pdsch-MappingTypeB-Alt-r16***Indicates whether the UE supports PDSCH Type B scheduling of length 9 and 10 OFDM symbols, and DMRS shift for length-10 symbols. If the UE supports this feature, the UE needs to report *pdsch-MappingTypeB*. | Band | No | N/A | FR1 only |
| ***periodicBeamReport***Indicates whether UE supports periodic 'CRI/RSRP' or 'SSBRI/RSRP' reporting using PUCCH formats 2, 3 and 4 in one slot. | Band | Yes | N/A | N/A |
| ***powerBoosting-pi2BPSK***Indicates whether UE supports power boosting for pi/2 BPSK, when applicable as defined in 6.2 of TS 38.101-1 [2]. This capability is not applicable to IAB-MT. | Band | No | TDD only | FR1 only |
| ***ptrs-DensityRecommendationSetDL***For each supported sub-carrier spacing, indicates preferred threshold sets for determining DL PTRS density. It is mandated for FR2. For each supported sub-carrier spacing, this field comprises:- two values of *frequencyDensity*;- three values of *timeDensity*. | Band | CY | N/A | N/A |
| ***ptrs-DensityRecommendationSetUL***For each supported sub-carrier spacing, indicates preferred threshold sets for determining UL PTRS density. For each supported sub-carrier spacing, this field comprises:- two values of *frequencyDensity*;- three values of *timeDensity*;- five values of *sampleDensity*. | Band | No | N/A | N/A |
| ***pucch-SpatialRelInfoMAC-CE***Indicates whether the UE supports indication of *PUCCH-spatialrelationinfo* by a MAC CE per PUCCH resource. It is mandatory for FR2 and optional for FR1. | Band | CY | N/A | N/A |
| ***pusch-256QAM***Indicates whether the UE supports 256QAM modulation scheme for PUSCH as defined in 6.3.1.2 of TS 38.211 [6]. | Band | No | N/A | N/A |
| ***pusch-RepetitionMultiSlots-v1650***Indicates whether the UE supports transmitting PUSCH scheduled by DCI format 0\_1 when configured with higher layer parameter *pusch-AggregationFactor* > 1, as defined in clause 6.1.2.1 of TS 38.214 [12]. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *pusch-RepetitionMultiSlots-r16* applies. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively.The UE only includes *pusch-RepetitionMultiSlots-v1650* if *pusch-RepetitionMultiSlots* is absent. | Band | Yes | N/A | N/A |
| ***pusch-TransCoherence***Defines support of the uplink codebook subset by the UE for UL precoding for PUSCH transmission as described in clause 6.1.1.1 of TS 38.214 [12]. UE indicated support of partial coherent codebook subset shall also support non-coherent codebook subset. UE indicated support of full coherent codebook subset shall also support partial and non-coherent codebook subset. | Band | No | N/A | N/A |
| ***rateMatchingLTE-CRS***Indicates whether the UE supports receiving PDSCH with resource mapping that excludes the REs determined by the higher layer configuration LTE-carrier configuring common RS, as specified in TS 38.214 [12]. | Band | Yes | N/A | N/A |
| ***separateCRS-RateMatching-r16***Indicates whether the UE supports rate match around configured CRS patterns which is associated with *CORESETPoolIndex* (if configured) and are applied to the PDSCH scheduled with a DCI detected on a CORESET with the same value of *CORESETPoolIndex*. The UE that indicates support of this feature shall support *multiDCI-MultiTRP-r16* and *overlapRateMatchingEUTRA-CRS-r16.* This is only applicable for 15kHz SCS. | Band | No | N/A | FR1 only |
| ***semi-PersistentL1-SINR-Report-PUCCH-r16***Indicates whether the UE supports semi-persistent L1-SINR report on PUCCH. The UE indicating support of this feature shall include at least one of the following capabilities:- *supportReportFormat1-2OFDM-syms-r16* indicates support of report on PUCCH formats over 1 – 2 OFDM symbols once per slot (or piggybacked on a PUSCH)- *supportReportFormat4-14OFDM-syms-r16* indicates support of report on PUCCH formats over 4 – 14 OFDM symbols once per slot (or piggybacked on a PUSCH).The UE indicating support of this feature shall also indicate support of *ssb-csirs-SINR-measurement-r16.*  | Band | No | N/A | N/A |
| ***semi-PersistentL1-SINR-Report-PUSCH-r16***Indicates whether the UE supports semi-persistent L1-SINR report on PUSCH. The UE indicating support of this feature shall also indicate support of *ssb-csirs-SINR-measurement-r16.*  | Band | No | N/A | N/A |
| ***simul-SpatialRelationUpdatePUCCHResGroup-r16***Indicates whether the UE support PUCCH resource groups per BWP for simultaneous spatial relation update. The UE indicating support of this also indicates the capabilities of supported SRS resources and maximum supported spatial relations for the supported bands using *supportedSRS-Resources, maxNumberConfiguredSpatialRelations* and *pucch-SpatialRelInfoMAC-CE*. | Band | No | N/A | N/A |
| ***simulTX-SRS-AntSwitchingIntraBandUL-CA-r16***Indicates whether the UE support simultaneous transmission of SRS on different CCs for intra-band UL CA. The UE indicating support of this feature shall include at least one of the following capabilities:- *supportSRS-xTyR-xLessThanY-r16* indicates support transmission of SRS for xTyR (x<y) based antenna switching and SRS for CB/NCB/BM on different CCs in overlapped symbol(s) for intra-band UL CA.- *supportSRS-xTyR-xEqualToY-r16* indicates support transmission of SRS for xTyR (x=y) based antenna switching and SRS for CB/NCB/BM on different CCs in overlapped symbol(s) for intra-band UL CA.- *supportSRS-AntennaSwitching-r16* Indicates whether the UE support simultaneous transmission of SRS for antenna switching on different CCs in overlapped symbol(s) for intra-band UL CA.NOTE: For simultaneously antenna switching and antenna switching SRS in intra-band CAs with bands whose UL are switched together according to the reported *supportSRS-AntennaSwitching-r16*, the UE expects the same configuration of xTyR across the different CCs and the SRS resources overlapped in time domain from UE perspective are from the same UE antenna ports. | Band | No | N/A | N/A |
| ***simulSRS-MIMO-TransWithinBand-r16***Indicates the number of SRS resources for positioning and SRS resource for MIMO on a symbol within a band across multiple CCs. The UE can include this field only if the UE supports *srs-PosResources-r16*. Otherwise, the UE does not include this field. | Band | No | N/A | N/A |
| ***simulSRS-TransWithinBand-r16***Indicates the number of SRS resources for positioning on a symbol within a band across multiple CCs. The UE can include this field only if the UE supports *srs-PosResources-r16*. Otherwise, the UE does not include this field. | Band | No | N/A | N/A |
| ***simultaneousReceptionDiffTypeD-r16***Indicates whether the UE supports simultaneous reception with different QCL Type D reference signal as specified in TS38.213 [11]. | Band | No | N/A | FR2 only |
| ***spatialRelations, spatialRelations-v1640***Indicates whether the UE supports spatial relations. The capability signalling comprises the following parameters.- *maxNumberConfiguredSpatialRelations* indicates the maximum number of configured spatial relations per CC for PUCCH and SRS. It is not applicable to FR1 and applicable to FR2 only. The UE is mandated to report 16 or higher values. *maxNumberConfiguredSpatialRelations-v1640* indicates the maximum number of configured spatial relations per CC for PUCCH and SRS with UE supporting the configuration of maximum 64 PUCCH spatial relations per BWP per CC;- *maxNumberActiveSpatialRelations* indicates the maximum number of active spatial relations with regarding to PUCCH and SRS for PUSCH, per BWP per CC. It is not applicable to FR1 and applicable and mandatory to report one or higher value for FR2 only;- *additionalActiveSpatialRelationPUCCH* indicates support of one additional active spatial relation for PUCCH. It is mandatory with capability signalling if *maxNumberActiveSpatialRelations* is set to n1;- *maxNumberDL-RS-QCL-TypeD* indicates the maximum number of downlink RS resources used for QCL type D in the active TCI states and active spatial relation information, which is optional.The UE is mandated to report *spatialRelations* for FR2. if *maxNumberConfiguredSpatialRelations-v1640* is reported, UE shall report value *n96* in *maxNumberConfiguredSpatialRelations*. | Band | FD | N/A | FD |
| ***spatialRelationsSRS-Pos-r16***Indicates whether the UE supports spatial relations for SRS for positioning. The capability signalling comprises the following parameters.- *spatialRelation-SRS-PosBasedOnSSB-Serving-r16* indicates whether the UE supports spatial relation for SRS for positioning based on SSB from the serving cell in the same band. The UE can include this field only if the UE supports *srs-PosResources-r16*. Otherwise, the UE does not include this field;- *spatialRelation-SRS-PosBasedOnCSI-RS-Serving-r16* indicates whether the UE supports spatial relation for SRS for positioning based on CSI-RS from the serving cell in the same band. The UE can include this field only if the UE supports *spatialRelation-SRS-PosBasedOnSSB-Serving-r16*. Otherwise, the UE does not include this field;- *spatialRelation-SRS-PosBasedOnPRS-Serving-r16* indicates whether the UE supports spatial relation for SRS for positioning based on PRS from the serving cell in the same band. The UE can include this field only if the UE supports any of DL PRS Resources for DL AoD, DL PRS Resources for DL-TDOA or DL PRS Resources for Multi-RTT defined in TS37.355 [22], or *srs-PosResources-r16*. Otherwise, the UE does not include this field;- *spatialRelation-SRS-PosBasedOnSRS-r16* indicates whether the UE supports spatial relation for SRS for positioning based on SRS in the same band. The UE can include this field only if the UE supports *srs-PosResources-r16*. Otherwise, the UE does not include this field;- *spatialRelation-SRS-PosBasedOnSSB-Neigh-r16* indicates whether the UE supports spatial relation for SRS for positioning based on SSB from the neighbouring cell in the same band. The UE can include this field only if the UE supports *spatialRelation-SRS-PosBasedOnSSB-Serving-r16*. Otherwise, the UE does not include this field;- *spatialRelation-SRS-PosBasedOnPRS-Neigh-r16* indicates whether the UE supports spatial relation for SRS for positioning based on PRS from the neighbouring cell in the same band. The UE can include this field only if the UE supports *spatialRelation-SRS-PosBasedOnPRS-Serving-r16*. Otherwise, the UE does not include this field;NOTE: A PRS from a PRS-only TP is treated as PRS from a non-serving cell. | Band | No | N/A | FR2 only |
| ***sp-BeamReportPUCCH***Indicates support of semi-persistent 'CRI/RSRP' or 'SSBRI/RSRP' reporting using PUCCH formats 2, 3 and 4 in one slot. | Band | No | N/A | N/A |
| ***sp-BeamReportPUSCH***Indicates support of semi-persistent 'CRI/RSRP' or 'SSBRI/RSRP' reporting on PUSCH. | Band | No | N/A | N/A |
| ***sps-r16***Indicates whether the UE support of up to 8 configured SPS configurations in a BWP of a serving cell and up to 32 configured SPS configurations in a cell group. This field includes the following parameters:- *maxNumberConfigsPerBWP-r16* indicates the maximum number of active SPS configurations in a BWP of a serving cell.- *maxNumberConfigsAllCC-r16* indicates the maximum number of active SPS configurations across all serving cells in a MAC entity, and across MCG and SCG in case of NR-DC.The UE can include this feature only if the UE indicates supports of *downlinkSPS*.NOTE:- For all the reported bands in FR1, a same X1 value is reported for *maxNumberConfigsAllCC-r16*. For all the reported bands in FR2, a same X2 value is reported for *maxNumberConfigsAllCC-r16*.- The total number of active SPS configurations across all serving cells in FR1 is no greater than X1.- The total number of active SPS configurations across all serving cells in FR2 is no greater than X2.- If the CA have some serving cell(s) in FR1 and some serving cell(s) in FR2, the total number of active SPS configurations across all serving cells is no greater than max(X1, X2). | Band | No | N/A | N/A |
| ***srs-AssocCSI-RS***Parameters for the calculation of the precoder for SRS transmission based on channel measurements using associated NZP CSI-RS resource (srs-AssocCSI-RS) as described in clause 6.1.1.2 of TS 38.214 [12]. UE supporting this feature shall also indicate support of non-codebook based PUSCH transmission.This capability signalling includes list of the following parameters:- *maxNumberTxPortsPerResource* indicates the maximum number of Tx ports in a resource;- *maxNumberResourcesPerBand* indicates the maximum number of resources across all CCs within a band simultaneously;*-* *totalNumberTxPortsPerBand* indicates the total number of Tx ports across all CCs within a band simultaneously. | Band | No | N/A | N/A |
| ***ssb-csirs-SINR-measurement-r16***Indicates the limitations of the UE support of SSB/CSI-RS for L1-SINR measurement.This capability signalling includes list of the following parameters:Per slot limitations:- *maxNumberSSB-CSIRS-OneTx-CMR-r16* indicates the maximum number of SSB/CSI-RS (1TX) for Channel Measurement Report- *maxNumberCSI-IM-NZP-IMR-res-r16* indicates the maximum number of CSI-IM/NZP-IMR resources- maxNumberCSIRS-2Tx-res-r16 indicates the maximum number of CSI-RS (2TX) resources for Channel Measurement ReportMemory limitations:- *maxNumberSSB-CSIRS-res-r16* indicates the max number of SSB/CSI-RS resources as Channel Measurement Report- *maxNumberCSI-IM-NZP-IMR-res-mem-r16* indicates the maximum number of CSI-IM/NZP-IMR resourcesOther limitations:- *supportedCSI-RS-Density-CMR-r16* indicates supported density of CSI-RS for Channel Measurement Report.- *maxNumberAperiodicCSI-RS-Res-r16* indicates the maximum number of aperiodic CSI-RS resources across all CCs configured to measure L1-SINR (including CMR and IMR) shall not exceed MD\_1- *supportedSINR-meas* indicates the supported SINR measurements.- *supportedSINR-meas-r16* contains values {*ssbWithCSI-IM*, *ssbWithNZP-IMR*, *csirsWithNZP-IMR*, *csi-RSWithoutIMR*} representing {SSB as CMR with dedicated CSI-IM, SSB as CMR with dedicated NZP IMR, CSI-RS as CMR with dedicated NZP IMR configured, CSI-RS as CMR without dedicated IMR configured}. UE supporting this feature shall always support CSI-RS as CMR with dedicated IMR configured.- *supportedSINR-meas-v1670* indicates a 4-bit bitmap {ssbWithCSI-IM, ssbWithNZP-IMR, csirsWithNZP-IMR, csi-RSWithoutIMR}, where the leftmost bit corresponds to ssbWithCSI-IM, the next bit corresponds to ssbWithNZP-IMR and so on. UE indicating *supportedSINR-meas-v1670* shall always indicate *supportedSINR-meas-r16.*UE indicating support of this feature shall also support *periodicBeamReport* and *aperiodicBeamReport* or *sp-BeamReportPUCCH* and *sp-BeamReportPUSCH.* UE indicating support of *ssb-csirs-SINR-measurement-r16* shall support periodic and aperiodic L1-SINR report.NOTE 1: The reference slot duration is the shortest slot duration defined for the frequency range where the reported band belongs.NOTE 2: For *maxNumberSSB-CSIRS-res-r16* and *maxNumberCSI-IM-NZP-IMR-res-mem-r16* the configured CSI-RS resources for both active and inactive BWPs are counted.NOTE 3: For *maxNumberSSB-CSIRS-OneTx-CMR-r16, maxNumberCSI-IM-NZP-IMR-res-r16* and *maxNumberCSIRS-2Tx-res-r16*, CSI-RS resources configured as CMR without dedicated IMR are counted both as CMR and IMR.NOTE 4: For *maxNumberSSB-CSIRS-OneTx-CMR-r16*, *maxNumberCSI-IM-NZP-IMR-res-r16*, *maxNumberCSIRS-2Tx-res-r16*, *maxNumberAperiodicCSI-RS-Res-r16*, a SSB/CSI-RS resource is counted within the duration of a reference slot in which the corresponding reference signals are transmitted.NOTE 5: For *maxNumberSSB-CSIRS-OneTx-CMR-r16*, *maxNumberCSI-IM-NZP-IMR-res-r16*, *maxNumberCSIRS-2Tx-res-r16*, *maxNumberAperiodicCSI-RS-Res-r16*, if one resource used for L1-SINR measurement is referred N times by one or more CSI reporting settings with *reportQuantity-r16* = *ssb-Index-SINR-r16* or *cri-SINR-r16*, it is counted N times.NOTE 6: If more than one type of SINR measurement is indicated in *supportedSINR-meas-v1670*, it is left to UE implementation which SINR measurement to indicate in *supportedSINR-meas-r16*. | Band | No | N/A | N/A |
| ***support64CandidateBeamRS-BFR-r16***Indicates UE support of configuring maximum 64 candidate beam RSs per BWP per CC. UE indicating support of this feature shall also indicate support of *maxNumberCSI-RS-BFD, maxNumberSSB-BFD* and *maxNumberCSI-RS-SSB-CBD.* | Band | No | N/A | N/A |
| ***supportCodeWordSoftCombining-r16***Indicates whether UE supports codeword soft combining for FDMSchemeB. UE indicates support of this feature depends on whether the *supportFDM-SchemeB-r16* is also supported. | Band | No | N/A | N/A |
| ***supportFDM-SchemeA-r16***Indicates whether UE supports single DCI based FDMSchemeA. | Band | No | N/A | N/A |
| ***supportInter-slotTDM-r16***Indicates whether UE supports single-DCI based inter-slot TDM. This capability signalling includes the following:- *supportRepNumPDSCH-TDRA-r16* indicates support of RepNumR16 in PDSCH-TimeDomainResourceAllocation and the maximum value of RepNumR16- *maxTBS-Size-r16* indicates maximum TBS size.- *maxNumberTCI-states-r16* indicates the maximum number of TCI states. | Band | No | N/A | N/A |
| ***supportNewDMRS-Port-r16***Indicates whether UE supports of new DMRS port entry {0,2,3}. UE supports this feature should indicate support *singleDCI-SDM-scheme-r16* for the band. | Band | No | N/A | N/A |
| ***supportTDM-SchemeA-r16***Indicates whether UE supports single DCI based TDMSchemeA. The capability signalling includes the maximum TBS size. | Band | No | N/A | N/A |
| ***supportTwoPortDL-PTRS-r16***Indicates whether UE supports 2-port DL PT-RS. UE supports this feature should indicate support *singleDCI-SDM-scheme-r16* for the band. | Band | No | N/A | n/A |
| ***tci-StatePDSCH***Defines support of TCI-States for PDSCH. The capability signalling comprises the following parameters:- *maxNumberConfiguredTCIstatesPerCC* indicates the maximum number of configured TCI-states per CC for PDSCH. For FR2, the UE is mandated to set the value at least to 64 (i.e. value 128 is an optional value). For FR1, the UE is mandated to set these values at least to the maximum number of allowed SSBs in the supported band;- *maxNumberActiveTCI-PerBWP* indicates the maximum number of activated TCI-states per BWP per CC, including control and data. If a UE reports X active TCI state(s), it is not expected that more than X active QCL type D assumption(s) for any PDSCH and any CORESETs for a given BWP of a serving cell become active for the UE. The UE shall include this field.Note the UE is required to track only the active TCI states.The UE is mandated to report *tci-StatePDSCH*. | Band | Yes | N/A | N/A |
| ***trs-AdditionalBandwidth-r16***Indicates the UE supported TRS bandwidths, in addition to 52 RBs, for a 10MHz UE channel bandwidth. This field only applies for the BWPs configured with 52 RBs size and 15kHz SCS, in FDD bands.Value *trs-AddBW-Set1* indicates 28, 32, 36, 40, 44, 48 RBs.Value *trs-AddBW-Set2* indicates 32, 36, 40, 44, 48 RBs. | Band | No | FDD only | FR1 only |
| ***twoPortsPTRS-UL***Defines whether UE supports PT-RS with 2 antenna ports for UL transmission. | Band | No | N/A | N/A |
| ***type1-PUSCH-RepetitionMultiSlots-v1650***Indicates whether the UE supports Type 1 PUSCH transmissions with configured grant as specified in TS 38.214 [12] with UL-TWG-repK value equal to 2, 4, or 8 with a single repetition of the transport block within each slot, and redundancy version pattern as indicated by UL-TWG-RV-rep. A UE supporting this feature shall also support Type 1 PUSCH transmissions with configured grant as specified in TS 38.214 [12] with UL-TWG-repK value of one. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *type1-PUSCH-RepetitionMultiSlots-r16* applies. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively.The UE only includes *type1-PUSCH-RepetitionMultiSlots-v1650* if *type1-PUSCH-RepetitionMultiSlots* is absent | Band | No | N/A | N/A |
| ***type2-PUSCH-RepetitionMultiSlots-v1650***Indicates whether the UE supports Type 2 PUSCH transmissions with configured grant as specified in TS 38.214 [12] with UL-TWG-repK value equal to 2, 4, or 8 with a single repetition of the transport block within each slot, and redundancy version pattern as indicated by UL-TWG-RV-rep. A UE supporting this feature shall also support Type 2 PUSCH transmissions with configured grant as specified in TS 38.214 [12] with UL-TWG-repK value of one. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *type2-PUSCH-RepetitionMultiSlots-r16* applies. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively.The UE only includes *type2-PUSCH-RepetitionMultiSlots-v1650* if *type2-PUSCH-RepetitionMultiSlots* is absent | Band | No | N/A | N/A |
| ***txDiversity-r16***Indicates whether the UE supports transparent Tx diversity requirements as specified in the suffix G clauses of TS 38.101-1 [2] (see also clauses 4.2 and 4.3 of TS38.101-1 [2]). | Band | No | N/A | FR1 only |
| ***ue-PowerClass, ue-PowerClass-v1610***For FR1, if the UE supports the different UE power class than the default UE power class as defined in clause 6.2 of TS 38.101-1 [2], the UE shall report the supported UE power class in this field. For FR2, UE shall report the supported UE power class as defined in clause 6 and 7 of TS 38.101-2 [3] in this field. This capability is not applicable to IAB-MT. | Band | Yes | N/A | N/A |
| ***uplinkBeamManagement***Defines support of beam management for UL. This capability signalling comprises the following parameters:- *maxNumberSRS-ResourcePerSet-BM* indicates the maximum number of SRS resources per SRS resource set configurable for beam management, supported by the UE.- *maxNumberSRS-ResourceSet* indicates the maximum number of SRS resource sets configurable for beam management, supported by the UE.If the UE does not set *beamCorrespondenceWithoutUL-BeamSweeping* to *supported*, the UE shall report this capability. This feature is optional for the UE that supports beam correspondence without uplink beam sweeping as defined in clause 6.6, TS 38.101-2 [3].NOTE: The network uses *maxNumberSRS-ResourceSet* to determine the maximum number of SRS resource sets that can be configured to the UE for periodic/semi-persistent/aperiodic configurations as below:

|  |  |
| --- | --- |
| Maximum number of SRS resource sets across all time domain behaviour (periodic/semi-persistent/aperiodic) reported in *maxNumberSRS-ResourceSet* | Additional constraint on the maximum number of SRS resource sets configured to the UE for each supported time domain behaviour (periodic/semi-persistent/aperiodic) |
| 1 | 1 |
| 2 | 1 |
| 3 | 1 |
| 4 | 2 |
| 5 | 2 |
| 6 | 2 |
| 7 | 4 |
| 8 | 4 |

 | Band | No | N/A | FR2 only |

#### 4.2.7.2X *Ext71GAccessParamsPerBand*

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Definitions for parameters | Per | M | FDD-TDD DIFF | FR1-FR2 DIFF |
| ***dl-FR2-2-Support120KHzSCS-r17***Indicates whether the UE supports reception of 120kHz subcarrier spacing for DL data and control channels, SSB, and reference signals in FR2-2 for non-initial access.It is mandatory for UE supporting at least one FR2-2 frequency band.  | Band  | CY | N/A | N/A |
| ***ul-FR2-2-Support120KHzSCS-r17***Indicates whether the UE supports PRACH with 120KHz SCS and length 139 and transmission of 120kHz subcarrier spacing for UL data and control channels and reference signals in FR2-2UE indicating support of this feature shall also indicate support of *dl-FR2-2-Support120KHzSCS-r17.* | Band  | No | N/A | N/A |
| ***initialAccessSSB-120KHz-r17***Indicates whether the UE supports 120KHz SSB for initial access in FR2-2.UE indicating support of this feature shall also indicate support of *dl-FR2-2-Support120KHzSCS-r17* and *ul-FR2-2-Support120KHzSCS-r17.* | Band  | No | N/A | N/A |

END OF 4th CHANGE

START OF 5th CHANGE

### 4.2.9 *MeasAndMobParameters*

| Definitions for parameters | Per | M | FDD-TDD DIFF | FR1-FR2 DIFF |
| --- | --- | --- | --- | --- |
| ***cli-RSSI-Meas-r16***Indicates whether the UE can perform CLI RSSI measurements as specified in TS 38.215 [13] and supports periodical reporting and measurement event triggering as specified in TS 38.331 [9]. If the UE supports this feature, the UE needs to report *maxNumberCLI-RSSI-r16*. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measurement resources to be measured. | UE | No | TDD only | Yes |
| ***cli-SRS-RSRP-Meas-r16***Indicates whether the UE can perform SRS RSRP measurements as specified in TS 38.215 [13] and supports periodical reporting and measurement event triggering based on SRS-RSRP as specified in TS 38.331 [9]. If the UE supports this feature, the UE needs to report *maxNumberCLI-SRS-RSRP-r16* and *maxNumberPerSlotCLI-SRS-RSRP-r16*. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measurement resources to be measured. | UE | No | TDD only | Yes |
| ***condHandoverFDD-TDD-r16***Indicates whether the UE supports conditional handover between FDD and TDD cells. The parameter can only be set if *condHandover-r16* is set for at least one FDD band and one TDD band. The UE that indicates support of this feature shall also indicate support of *handoverFDD-TDD*. | UE | No | No | No |
| ***condHandoverFR1-FR2-r16***Indicates whether the UE supports conditional handover HO between FR1 and FR2. The parameter can only be set if *condHandover-r16* is set for at least one FR1 band and one FR2 band. The UE that indicates support of this feature shall also indicate support of *handoverFR1-FR2*. | UE | No | No | No |
| ***csi-RS-RLM***Indicates whether the UE can perform radio link monitoring procedure based on measurement of CSI-RS as specified in TS 38.213 [11] and TS 38.133 [5]. This parameter needs FR1 and FR2 differentiation. If the UE supports this feature, the UE needs to report *maxNumberResource-CSI-RS-RLM*. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *csi-RS-RLM-r16* applies. | UE | Yes | No | Yes |
| ***csi-RSRP-AndRSRQ-MeasWithSSB***Indicates whether the UE can perform CSI-RSRP and CSI-RSRQ measurement as specified in TS 38.215 [13], where CSI-RS resource is configured with an associated SS/PBCH. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. If the UE supports this feature, the UE needs to report *maxNumberCSI-RS-RRM-RS-SINR*. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *csi-RS-RLM-r16* applies. | UE | No | No | Yes |
| ***csi-RSRP-AndRSRQ-MeasWithoutSSB***Indicates whether the UE can perform CSI-RSRP and CSI-RSRQ measurement as specified in TS 38.215 [13], where CSI-RS resource is configured for a cell that transmits SS/PBCH block and without an associated SS/PBCH block. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. If the UE supports this feature, the UE needs to report *maxNumberCSI-RS-RRM-RS-SINR*. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *csi-RSRP-AndRSRQ-MeasWithoutSSB-r16* applies. | UE | No | No | Yes |
| ***csi-SINR-Meas***Indicates whether the UE can perform CSI-SINR measurements based on configured CSI-RS resources as specified in TS 38.215 [13]. If this parameter is indicated for FR1 and FR2 differently, each indication corresponding to the frequency range of measured target cell. If the UE supports this feature, the UE needs to report *maxNumberCSI-RS-RRM-RS-SINR*. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *csi-SINR-Meas-r16* applies. | UE | No | No | Yes |
| ***eutra-AutonomousGaps-r16***Defines whether the UE supports, upon configuration of *useAutonomousGaps* by the network, acquisition of relevant information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell using autonomous gap and reporting the acquired information to the network as specified in TS 38.331 [9] when MR-DC is not configured.  | UE | No | No | No |
| ***eutra-AutonomousGaps-NEDC-r16***Defines whether the UE supports, upon configuration of *useAutonomousGaps* by the network, acquisition of relevant information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell using autonomous gap and reporting the acquired information to the network as specified in TS 38.331 [9] when NE-DC is configured. | UE | No | No | No |
| ***eutra-AutonomousGaps-NRDC-r16***Defines whether the UE supports, upon configuration of *useAutonomousGaps* by the network, acquisition of relevant information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell using autonomous gap and reporting the acquired information to the network as specified in TS 38.331 [9] when NR-DC is configured. | UE | No | No | No |
| ***eutra-CGI-Reporting***Defines whether the UE supports acquisition of relevant CGI-information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when the (NG)EN-DC and NE-DC are not configured or, when consistent DRX is configured in NR-DC. The consistent DRX configuration implies that MN and SN have the same DRX cycle and on-duration configured by MN completely contains on-duration configured by SN. It is mandated if the UE supports EUTRA. | UE | CY | No | No |
| ***eutra-CGI-Reporting-NEDC***Defines whether the UE supports acquisition of relevant information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when theNE-DCis configured. | UE | No | No | No |
| ***eutra-CGI-Reporting-NRDC***Defines whether the UE supports acquisition of relevant information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when theNR-DC is configured wherein MN and SN have different DRX cycles, or on-duration configured by MN does not contain on-duration configured by SN if the DRX cycles are the same. | UE | No | No | No |
| ***eventA-MeasAndReport***Indicates whether the UE supports NR measurements and events A triggered reporting as specified in TS 38.331 [9]. This field only applies to SN configured measurement when (NG)EN-DC is configured. For NR SA, MN and SN configured measurement when NR-DC is configured, and MN configured measurement when NE-DC is configured, this feature is mandatory supported. | UE | Yes | Yes | No |
| ***eventB-MeasAndReport***Indicates whether the UE supports EUTRA measurement and event B triggered reporting as specified in TS 38.331 [9]. It is mandated if the UE supports EUTRA. | UE | CY | No | No |
| ***handoverLTE-5GC, handoverLTE-5GC-r17***Indicates whether the UE supports HO to EUTRA connected to 5GC. It is mandated if the UE supports EUTRA connected to 5GC. | UE | CY | Yes | Yes(Include FR2-2 diff) |
| ***handoverFDD-TDD***Indicates whether the UE supports HO between FDD and TDD. It is mandated if the UE supports both FDD and TDD. This field only applies to NR SA/NR-DC/NE-DC (e.g. PCell handover). For PSCell change when (NG)EN-DC/NR-DC is configured, this feature is mandatory supported. UEs supporting this shall indicate support of *handoverInterF* for both FDD and TDD. | UE | Yes | No | No |
| ***handoverFR1-FR2***Indicates whether the UE supports HO between FR1 and FR2. Support is mandatory for the UE supporting both FR1 and FR2. This field only applies to NR SA/NR-DC/NE-DC (e.g. PCell handover). For PSCell change when (NG)EN-DC/NR-DC is configured, this feature is mandatory supported. UEs supporting this shall indicate support of *handoverInterF* for both FR1 and FR2. | UE | Yes | No | No |
| ***handoverFR1-FR2-2***Indicates whether the UE supports HO between FR1 and FR2-2. This field only applies to NR SA/NR-DC/NE-DC (e.g. PCell handover) and PSCell change when (NG)EN-DC/NR-DC is configured. UEs supporting this shall indicate support of *handoverInterF* for both FR1 and FR2-2. | UE | No | No | No |
| ***handoverFR2-1-FR2-2***Indicates whether the UE supports HO between FR2-1 and FR2-2. This field only applies to NR SA/NR-DC/NE-DC (e.g. PCell handover) and PSCell change when (NG)EN-DC/NR-DC is configured. UEs supporting this shall indicate support of *handoverInterF* for both FR2-1 and FR2-2. | UE | No | No | No |
| ***handoverInterF, handoverInterF-r17***Indicates whether the UE supports inter-frequency HO. It indicates the support for inter-frequency HO from the corresponding duplex mode and from frequency range indicated to be supported as described in Annex B. This field only applies to NR SA/NR-DC/NE-DC (e.g. PCell handover). For PSCell change when (NG)EN-DC/NR-DC is configured, this feature is mandatory supported. | UE | Yes | Yes | Yes(Include FR2-2 diff) |
| ***handoverLTE-EPC, handoverLTE-EPC-r17***Indicates whether the UE supports HO to EUTRA connected to EPC. It is mandated if the UE supports EUTRA connected to EPC. | UE | CY | Yes | Yes(Include FR2-2 diff) |
| ***idleInactiveNR-MeasReport-r16, idleInactiveNR-MeasReport-r17***Indicates whether the UE supports configuration of NR SSB measurements in RRC\_IDLE/RRC\_INACTIVE and reporting of the corresponding results upon network request as specified in TS 38.331 [9]. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. | UE | No | No | Yes(Include FR2-2 diff) |
| ***idleInactiveNR-MeasBeamReport-r16***Indicates whether the UE supports beam level measurements in RRC\_IDLE/RRC\_INACTIVE and reporting of the corresponding beam measurement results upon network request as specified in TS 38.331 [9]. A UE supports this feature shall also support *idleInactiveNR-MeasReport-r16*. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. | UE | No | No | Yes |
| ***idleInactiveEUTRA-MeasReport-r16***Indicates whether the UE supports configuration of E-UTRA measurements in RRC\_IDLE/RRC\_INACTIVE and reporting of the corresponding results upon network request as specified in TS 38.331 [9]. | UE | No | No | No |
| ***idleInactive-ValidityArea-r16***Indicates whether the UE supports configuration of a validity area for NR measurements in RRC\_IDLE/RRC\_INACTIVE as specified in TS 38.331 [9]. | UE | No | No | No |
| ***independentGapConfig***This field indicates whether the UE supports two independent measurement gap configurations for FR1 and FR2 specified in clause 9.1.2 of TS 38.133 [5]. The field also indicates whether the UE supports the FR2 inter-RAT measurement without gaps when (NG)EN-DC is not configured. | UE | No | No | No |
| ***intraAndInterF-MeasAndReport***Indicates whether the UE supports NR intra-frequency and inter-frequency measurements and at least periodical reporting. This field only applies to SN configured measurement when (NG)EN-DC is configured. For NR SA, MN and SN configured measurement when NR-DC is configured, and MN configured measurement when NE-DC is configured, this feature is mandatory supported. | UE | Yes | Yes | No |
| ***interFrequencyMeas-NoGap-r16***Indicates whether the UE can perform inter-frequency SSB based measurements without measurement gaps if the SSB is completely contained in the active BWP of the UE as specified in TS 38.133 [5]. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of cells to be measured. | UE | No | No | Yes |
| ***periodicEUTRA-MeasAndReport***Indicates whether the UE supports periodic EUTRA measurement and reporting. It is mandated if the UE supports EUTRA. | UE | CY | No | No |
| ***maxNumberCLI-RSSI-r16***Defines the maximum number of CLI-RSSI measurement resources for CLI RSSI measurement. If the UE supports *cli-RSSI-Meas-r16*, the UE shall report this capability. | UE | CY | TDD only | No |
| ***maxNumberCLI-SRS-RSRP-r16***Defines the maximum number of SRS-RSRP measurement resources for SRS-RSRP measurement. If the UE supports *cli-SRS-RSRP-Meas-r16*, the UE shall report this capability.NOTE 1: A slot is based on minimum SCS among active BWPs across all CCs configured for SRS-RSRP measurement.NOTE 2: A SRS resource occasion that overlaps with the slot is counted as one measurement resource in the slot. | UE | CY | TDD only | No |
| ***increasedNumberofCSIRSPerMO-r16***Indicates support of up to 192 CSI-RS resource for L3 mobility configuration per measurement object configured with *associatedSSB*. | UE | No | No | Yes |
| ***maxNumberCSI-RS-RRM-RS-SINR***Defines the maximum number of CSI-RS resources for RRM and RS-SINR measurement across all measurement frequencies per slot. If UE supports any of *csi-RSRP-AndRSRQ-MeasWithSSB*, *csi-RSRP-AndRSRQ-MeasWithoutSSB*, and *csi-SINR-Meas*, UE shall report this capability. | UE | CY | No | No |
| ***maxNumberPerSlotCLI-SRS-RSRP-r16***Defines the maximum number of SRS-RSRP measurement resources per slot for SRS-RSRP measurement. If the UE supports *cli-SRS-RSRP-Meas-r16*, the UE shall report this capability. | UE | CY | TDD only | No |
| ***maxNumberResource-CSI-RS-RLM***Defines the maximum number of CSI-RS resources within a slot per spCell for CSI-RS based RLM. If UE supports any of *csi-RS-RLM* and *ssb-AndCSI-RS-RLM*, UE shall report this capability. | UE | CY | No | Yes |
| ***nr-AutonomousGaps-r16***Defines whether the UE supports, upon configuration of *useAutonomousGaps* by the network, acquisition of relevant information from a neighbouring NR cell by reading the SI of the neighbouring cell using autonomous gap and reporting the acquired information to the network as specified in TS 38.331 [9] when MR-DC is not configured. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. | UE | No | No | Yes |
| ***nr-AutonomousGaps-ENDC-r16***Defines whether the UE supports, upon configuration of *useAutonomousGaps* by the network, acquisition of relevant information from a neighbouring NR cell by reading the SI of the neighbouring cell using autonomous gap and reporting the acquired information to the network as specified in TS 38.331 [9] when (NG)EN-DC is configured. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. | UE | No | No | Yes |
| ***nr-AutonomousGaps-NEDC-r16***Defines whether the UE supports, upon configuration of *useAutonomousGaps* by the network, acquisition of relevant information from a neighbouring NR cell by reading the SI of the neighbouring cell using autonomous gap and reporting the acquired information to the network as specified in TS 38.331 [9] when NE-DC is configured. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. | UE | No | No | Yes |
| ***nr-AutonomousGaps-NRDC-r16***Defines whether the UE supports, upon configuration of *useAutonomousGaps* by the network, acquisition of relevant information from a neighbouring NR cell by reading the SI of the neighbouring cell using autonomous gap and reporting the acquired information to the network as specified in TS 38.331 [9] when NR-DC is configured. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. | UE | No | No | Yes |
| ***nr-CGI-Reporting***Defines whether the UE supports acquisition of relevant CGI-information from a neighbouring intra-frequency or inter-frequency NR cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when (NG)EN-DC and NE-DC are not configured or, when consistent DRX is configured in NR-DC. The consistent DRX configuration implies that MN and SN have the same DRX cycle and on-duration configured by MN completely contains on-duration configured by SN. | UE | Yes | No | No |
| ***nr-CGI-Reporting-ENDC***Defines whether the UE supports acquisition of relevant CGI-information from a neighbouring intra-frequency or inter-frequency NR cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when the (NG)EN-DC is configured. | UE | Yes | No | No |
| ***reportAddNeighMeasForPeriodic-r16***Defines whether the UE supports periodic reporting of best neighbour cells per serving frequency, as defined in TS 38.331 [9]. | UE | Yes | No | No |
| ***nr-CGI-Reporting-NEDC***Defines whether the UE supports acquisition of relevant information from a neighbouring intra-frequency or inter-frequency NR cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when the NE-DC is configured. | UE | Yes | No | No |
| ***nr-CGI-Reporting-NPN-r16***Defines whether the UE supports acquisition of NPN-relevant CGI-information from a neighbouring intra-frequency or inter-frequency NR NPN cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9]. If UE supports NPN, UE shall report this capability. | UE | CY | No | No |
| ***nr-CGI-Reporting-NRDC***Defines whether the UE supports acquisition of relevant information from a neighbouring intra-frequency or inter-frequency NR cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when the NR-DC is configured wherein MN and SN have different DRX cycles, or on-duration configured by MN does not contain on-duration configured by SN if the DRX cycles are the same. | UE | Yes | No | No |
| ***nr-NeedForGap-Reporting-r16***Indicates whether the UE supports reporting the measurement gap requirement information for NR target in the UE response to a network configuration RRC message. | UE | No | No | No |
| ***pcellT312-r16***Indicates whether the UE supports T312 based fast failure recovery for PCell. | UE | No | No | No |
| ***simultaneousRxDataSSB-DiffNumerology***Indicates whether the UE supports concurrent intra-frequency measurement on serving cell or neighbouring cell and PDCCH or PDSCH reception from the serving cell with a different numerology as defined in clause 8 and 9 of TS 38.133 [5]. | UE | No | No | Yes |
| ***simultaneousRxDataSSB-DiffNumerology-Inter-r16***Indicates whether the UE supports concurrent SSB based inter-frequency measurement without measurement gap on neighbouring cell and PDCCH or PDSCH reception from the serving cell with a different numerology as defined in clause 8 and 9 of TS 38.133 [5]. UE indicates support of this indicates support of *interFrequencyMeas-NoGap-r16*. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range where the SSB and PDCCH/PDSCH are received. | UE | No | No | Yes |
| ***sftd-MeasPSCell***Indicates whether the UE supports SFTD measurements between the PCell and a configured PSCell. If this capability is included in UE-MRDC-Capability, it indicates that the UE supports SFTD measurement between PCell and PSCell in (NG)EN-DC. If this capability is included in UE-NR-Capability, it indicates that the UE supports SFTD measurement between PCell and PSCell in NR-DC. | UE | No | Yes | No |
| ***sftd-MeasPSCell-NEDC***Indicates whether the UE supports SFTD measurement between the NR PCell and a configured E-UTRA PSCell in NE-DC. | UE | No | Yes | No |
| ***sftd-MeasNR-Cell***Indicates whether the SFTD measurement with and without measurement gaps between the EUTRA PCell and the NR cells is supported by the UE which is capable of EN-DC/NGEN-DC when EN-DC/NGEN-DC is not configured. The SFTD measurement without gaps can be used when the UE supports at least one EN-DC band combination consisting of the set of the current E-UTRA serving frequencies and the NR frequency where SFTD measurement is configured. In UE-NR-Capability, this field is not used, and UE does not include the field. | UE | No | Yes | No |
| ***sftd-MeasNR-Neigh***Indicates whether the inter-frequency SFTD measurement with and without measurement gaps between the NR PCell and inter-frequency NR neighbour cells is supported by the UE when MR-DC is not configured. The SFTD measurement without gaps can be used when the UE supports at least one DC or CA band combination consisting of the set of the current NR serving frequencies and the NR frequency where SFTD measurement is configured.  | UE | No | Yes | No |
| ***sftd-MeasNR-Neigh-DRX***Indicates whether the inter-frequency SFTD measurement using DRX off period between the NR PCell and the inter-frequency NR neighbour cells is supported by the UE when MR-DC is not configured. | UE | No | Yes | No |
| ***ssb-RLM***Indicates whether the UE can perform radio link monitoring procedure based on measurement of SS/PBCH block as specified in TS 38.213 [11] and TS 38.133 [5]. This field shall be set to *supported*. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *ssb-RLM-DynamicChAccess-r16* or *ssb-RLM-Semi-StaticChAccess-r16* applies. | UE | Yes | No | No |
| ***ssb-AndCSI-RS-RLM***Indicates whether the UE can perform radio link monitoring procedure based on measurement of SS/PBCH block and CSI-RS as specified in TS 38.213 [11] and TS 38.133 [5]. If the UE supports this feature, the UE needs to report *maxNumberResource-CSI-RS-RLM*. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *ssb-AndCSI-RS-RLM-r16* applies. | UE | No | No | No |
| ***ss-SINR-Meas***Indicates whether the UE can perform SS-SINR measurement as specified in TS 38.215 [13]. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *ss-SINR-Meas-r16* applies. | UE | No | No | Yes |
| ***supportedGapPattern***Indicates measurement gap pattern(s) optionally supported by the UE for NR SA, for NR-DC, for NE-DC and for independent measurement gap configuration on FR2 in (NG)EN-DC. The leading / leftmost bit (bit 0) corresponds to the gap pattern 2, the next bit corresponds to the gap pattern 3, as specified in TS 38.133 [5] and so on. The UE shall set the bits corresponding to the measurement gap pattern 13, 14, 17, 18 and 19 to 1 if the UE is an NR standalone capable UE that supports a band in FR2 or if the UE is an (NG)EN-DC capable UE that supports *independentGapConfig* and supports a band in FR2. | UE | CY | No | No |
| ***supportedGapPattern-r16***Indicates measurement gap pattern(s) optionally supported by the UE for NR SA, for NR-DC for PRS measurement and NR/E-UTRA RRM measurement. The leading / leftmost bit (bit 0) corresponds to the gap pattern 24, the next bit corresponds to the gap pattern 25, as specified in TS 38.133 [5]. The applicability of the gap patterns 24 and 25 is defined in clause 9.1.2 of TS 38.133 [5]. A UE that indicates support of this capability shall indicate support of *NR-DL-PRS-ProcessingCapability-r16* defined in TS 37.355 [22]. | UE | No | No | No |
| ***supportedGapPattern-NRonly-r16***Indicates measurement gap pattern(s) optionally supported by the UE for NR SA and NR-DC when the frequencies to be measured within this measurement gap are all NR frequencies. The leading / leftmost bit (bit 0) corresponds to the gap pattern 2, the next bit corresponds to the gap pattern 3 and so on. The UE shall set the bits corresponding to the measurement gap pattern 2, 3 and 11 to 1. | UE | FD | No | No |
| ***supportedGapPattern-NRonly-NEDC-r16***Indicates whether the UE supports gap patterns 2, 3 and 11 in NE-DC when the frequencies to be measured within this measurement gap are all NR frequencies. | UE | No | No | No |

END OF 5th CHANGE

START OF 6th CHANGE

### 4.2.13 IMS Parameters

| Definitions for parameters | Per | M | FDD-TDDDIFF | FR1-FR2DIFF |
| --- | --- | --- | --- | --- |
| ***voiceFallbackIndicationEPS-r16***Indicates whether the UE supports *voiceFallbackIndication* in *RRCRelease* and *MobilityFromNRCommand*. If this field is included, the UE shall support IMS voice over NR and IMS voice over E-UTRA via EPC. | UE | No | No | No |
| ***voiceOverEUTRA-5GC***Indicates whether the UE supports IMS voice over E-UTRA via 5GC. It is mandated to the UE if the UE is capable of IMS voice over E-UTRA via 5GC. Otherwise, the UE does not include this field. If this field is included and the UE is capable of E-UTRA with EPC, the UE shall support IMS voice over E-UTRA via EPC. | UE | No | No | No |
| ***voiceOverNR, voiceOverNR-r17***Indicates whether the UE supports IMS voice over NR. It is mandated to the UE if the UE is capable of IMS voice over NR. Otherwise, the UE does not include this field. If this field is included and the UE is capable of E-UTRA with EPC, the UE shall support IMS voice over E-UTRA via EPC. | UE | No | No | Yes(Include FR2-2 diff) |
| ***voiceOverSCG-BearerEUTRA-5GC***Indicates whether the UE supports IMS voice over SCG bearer of NE-DC. | UE | No | No | N/A |

NOTE: In this release of specification, IMS voice over split bearer is not supported for NR-DC and NE-DC.

END OF 6th CHANGE

START OF 7th CHANGE

Annex B (informative):
UE capability indication for UE capabilities with both FDD/TDD and FR1/FR2 differentiations

Annex B clarifies the UE capability indication for the case where the UE is allowed to support different functionality between FDD and TDD, and between FR1 and FR2. Table B-1 clarifies the setting of UE capability fields for cases where the UE supports the corresponding feature in different combinations of duplex mode and frequency range. There are two possible ways of UE capability indication in Case 3 and Case 8.

Table B-1: UE capability indication for UE capabilities with both FDD/TDD and FR1/FR2 differentiations

|  |  |
| --- | --- |
| Support for the feature | Setting of UE capability fields |
| Common UE capability (with suffix '-XDD-Diff') | Common UE capability (with suffix '-FRX-diff') | fdd-Add-UE-NR/MRDC-Capabilities | tdd-Add-UE-NR/MRDC-Capabilities | fr1-Add-UE-NR/MRDC-Capabilities | fr2-Add-UE-NR/MRDC-Capabilities |
| Case 1 | FR1 FDD: 'supported'FR1 TDD: 'supported'FR2 TDD: 'supported' | Included | Included | Not included | Not included | Not included | Not included |
| Case 2 | FR1 FDD: 'not supported'FR1 TDD: 'not supported'FR2 TDD: 'not supported' | Not included | Not included | Not included | Not included | Not included | Not included |
| Case 3 | FR1 FDD: 'not supported'FR1 TDD: 'supported'FR2 TDD: 'supported' | Not included | Included | Not included | Included | Not included | Not included |
| Not included | Not included | Not included | Included | Not included | Not included |
| Case 4 | FR1 FDD: 'not supported'FR1 TDD: 'not supported'FR2 TDD: 'supported' | Not included | Not included | Not included | Included | Not included | Included |
| Case 5 | FR1 FDD: 'not supported'FR1 TDD: 'supported'FR2 TDD: 'not supported' | Not included | Not included | Not included | Included | Included | Not included |
| Case 6 | FR1 FDD: 'supported'FR1 TDD: 'not supported'FR2 TDD: 'supported' | The current UE capability signalling does not support the UE capability indication for this case. |
| Case 7 | FR1 FDD: 'supported'FR1 TDD: 'not supported'FR2 TDD: 'not supported' | Not included | Not included | Included | Not included | Included | Not included |
| Case 8 | FR1 FDD: 'supported'FR1 TDD: 'supported'FR2 TDD: 'not supported' | Included | Not included | Not included | Not included | Included | Not included |
| Not included | Not included | Not included | Not included | Included | Not included |

NOTE 1: For a UE capability which cannot be differentiated between FR2-1 and FR2-2, ‘FR2 TDD’ in Table B-1 includes both ‘FR2-1 TDD’ and ‘FR2-2 TDD’.

NOTE 2: For a UE capability which can be differentiated between FR2-1 and FR2-2, ‘FR2 TDD’ in Table B-1 only means ‘FR2-1 TDD’.

END OF 7th CHANGE

# Annex A: RAN2 Agreements

## RAN2#117-e

* 2-1: To accommodate the UE total L2 buffer size requirement, it is left to the UE implementation to limit the maximum UL/DL data rate of the FR2-2 CC. No new UE capability is introduced for UE indicating L2 buffer size limitation for this release
* 3-0: All new Rel-17 UE capabilities that requires FRx differentiation, including between FR2-1 and FR2-2, will have to be per-band signalling (as already agreed in the main session)
* 3-1: For existing UE capabilities that are with consistency check (’ UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands and all TDD-FR2 bands respectively.’) in the field description, update it to:

"UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively."

* 3-2: [To agree] For new Rel-17 UE capabilities that are per UE capability signalling with FRx diff and/or xDD diff, include the following to the field description:
* UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively.
* 3-3: Clarify in Annex B of TS 38.306 that for a UE capability which are not differentiated between FR2-1 and FR2-2, ‘FR2 TDD’ in Table B-1 includes both FR2-1 TDD and FR2-2 TDD.
* 3-4: Clarify in Annex B of TS 38.306 that for a UE capability which are differentiated between FR2-1 and FR2-2, ‘FR2 TDD’ in Table B-1 only means ‘FR2-1 TDD’.
* 4.1-1: RAN2 to clarify the intra-NR handover capabilities in FR2-2 should be defined with separate IOT capability bit, even when the corresponding FR2-2 band is supported.
* 4.2-1: RAN2 to clarify that ‘eutra-5GC-HO-ToNR-TDD-FR2-r15’ and ‘eutra-EPC-HO-ToNR-TDD-FR2-r15’ in LTE indicates whether the UE supports handover from E-UTRA/5GC and E-UTRA/EPC to NR TDD FR2-1, respectively.
* 4.2-2: RAN2 to introduce new UE capabilities ‘eutra-5GC-HO-ToNR-TDD-FR2-r17’ and ‘eutra-EPC-HO-ToNR-TDD-FR2-r17’ in LTE to indicate whether the UE supports handover from E-UTRA/5GC and E-UTRA/EPC to NR TDD FR2-2, respectively.
* 4.2-3: RAN2 to clarify that ‘ims-VoiceOverNR-FR2-r15’ in LTE indicates whether the UE supports IMS voice over NR FR2-1, and RAN2 introduce a new UE capability ‘ims-VoiceOverNR-FR2-r17’ in LTE to indicate whether the UE supports IMS voice over NR FR2-2.
* 4.2-4: RAN2 to clarify ‘ce-EUTRA-5GC-HO-ToNR-TDD-FR2-r16’ in LTE indicates whether the UE supports handover from E-UTRA/5GC in coverage enhancement mode A or B to NR TDD FR2-1, and RAN2 add ‘ce-EUTRA-5GC-HO-ToNR-TDD-FR2-r17’ in LTE to indicate whether the UE supports handover from E-UTRA/5GC in coverage enhancement mode A or B to NR TDD FR2-2.
* Can discuss exact field names in CR discussion
* 4.3-1: From RAN2 point of view, FR2-2 are assumed to be also applicable to other Rel-17 features, unless otherwise specified (e.g. if the feature is only for FR1). No impact to the specification expected for cases where we don't specify otherwise.
* Companies can bring up cases (e.g. for some WIs where FR2-2 has not been discussed at all) where differentiation is needed by contributions to May meeting.
* 1: From the MAC layer perspective, there is no need for additional differentiation for licensed operation and “no-LBT” mode of shared spectrum.
* 1: RAN2 to reuse the existing prohibit timer (i.e., overheatingIndicationProhibitTimer) also for newly introduced OverheatingAssistance-r17.
* 2: RAN2 to reuse the existing prohibit timers (i.e., maxBW-PreferenceProhibitTimer-r16, maxMIMO-LayerPreferenceProhibitTimer-r16, minSchedulingOffsetPreferenceProhibitTimer-r16) for newly introduced power saving parameters (i.e., maxBW-PreferenceFR2-2-r17, maxMIMO-LayerPreferenceFR2-2-r17, minSchedulingOffsetPreferenceProhibitTimer-r16)
* 3: RAN2 to introduce new indicators (e.g., 1bit indicator for each new parameter in UAI) in OtherConfig IE as in the below TP. If it is agreed, the TP in Annex A.1 can be considered as baseline.

The related new parameters in UAI: maxBW-PreferenceFR2-2-r17, maxMIMO-LayerPreferenceFR2-2-r17, minSchedulingOffsetPreferenceFR2-2-r17

## RAN2#116bis-e

* 3: RAN2 confirm the baseline RLC RTT values for 480kHz and 960kHz to be 20ms. There is no need to further discuss this in RAN2.
* 1: Following two general options can be considered for LBT failure counting and indication (from PHY to MAC) for the case of independent per-beam LBT sensing.
* o Option 1: LBT failures are counted and indicated to MAC independently per beam
* o Option 2: LBT failures are counted and indicated to MAC per UL transmission, i.e. no beam indication included
* 2: For Option 2, i.e. LBT failures are counted and indicated to MAC per UL transmission, current Rel-16 LBT procedures can be baseline (i.e. no changes to the LBT failure detection and recovery procedure unless needed)
* 3: For Option 1, i.e. LBT failures are counted and indicated to MAC independently per beam, further changes/enhancements to the Rel-16 LBT procedures are required, i.e. LBT failure detection and recovery procedure.
* 6: “no-LBT mode” is already implicitly supported by Rel-16 specifications. FFS if additional differentiation from licensed operation in specification is required for some cases.
* 7: cg-RetransmissionTimer is optional for operation in the shared spectrum in FR2-2.
* 8: RAN2 assumes that no protocol changes are required in order to support LBT mode change.
* 4: From RAN2 point of view there is no need that PHY provides per-beam LBT failure indications to MAC in Rel-17. No need to send LS to RAN1 unless they request RAN2 view.
* A1: RAN2 does not agree to using the spare bit in MIB for the signaling of FR2-2 QCL assumptions for SSB. Respond to RAN1 LS accordingly.
* A2: The legacy MIB is used for FR2-2 (i.e. we do not define new MIB for FR2-2).
* A3: Up to RAN1 how to resolve QCL configuration (no suggestions from RAN2). This need not be included in LS to RAN1.
* A4: channelAccessMode2 is signaled as ENUMERATED {enabled}. This implies that the UE can not distinguish between licensed spectrum and shared spectrum without LBT. If RAN1 indicates there is need to distinguish these, we can revisit this agreement.
* B1: Add text with the new SCS values in the field description of the parameters listed in Table 1 in [R2-2201033](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_116bis-e/Docs/R2-2201033.zip)
* C1: The parameter enableTimeDomainHARQ-BundlingType1-r17 is introduced in ServingCellConfig with the value “ENUMERATED {enabled}”. FFS if the name can be shortened.
* C2: maxNrofMultiplePDSCHs-r17 is defined in pdsch-TimeDomainAllocationListForMultiPDSCH-r17 with the value 8.
* C3: No restrictions are captured in RRC for pdsch-TimeDomainAllocationListForMultiPDSCH.
* C4: The following are agreed for signaling of PDSCH TDRA:

• The new PDSCH-TimeDomainResourceAllocation-r17 IE can be configured with either PDSCH repetition or multiple PDSCH.

• Introduce the field pdsch-TimeDomainAllocationListDCI-1-2-r17 and the field pdsch-TimeDomainAllocationList-r17 so that PDSCH repetitions can be used with the new k0 value range.

* C5: Introduce the field pusch-TimeDomainAllocationListDCI-1-2-r17 and the field pusch-TimeDomainAllocationList-r17 so that PUSCH repetition can be used with the new k2 value range.
* C6: The IE pusch-TimeDomainAllocationListForMultiPUSCH-r17 is configured with up to 16 list elements.
* C8: New Rel-17 IEs for UL-AccessConfigListDCI-0-1 and UL-AccessConfigListDCI-1-1 are introduced. This does not follow the RAN1 agreement to re-use Rel-16 versions and thus may need to be confirmed by RAN1.
* C7: k2(n) should always be signaled by the network. If RAN1 indicates there is a reason to specify the absence case, we can revisit this.
* D1: A new parameter ra-ResponseWindow-r17 with the value ENUMERATED {sl240, sl320, sl640, sl960, sl1280, sl1920, sl2560} is introduced for 4-step RACH for operation in FR2-2 shared spectrum.
* D2: A new parameter msgB-ResponseWindow-r17 with the value ENUMERATED {sl640, sl960, sl1280, sl1920, sl2560} is introduced for 2-step RACH for operation in FR2-2.
* Proposal E1: New values, e.g. 0.0313ms, 0.0156ms, 0.01ms, are added to maxPUSCH-Duration for FR2-2.
* Proposal E2: New values are added to IEs in UAI power saving and overheating parameters to reflect the new SCS, K0/K2, and bandwidth sizes for FR2-2.
* Proposal E3: cg-RetransmissionTimer is optionally configured for operation in FR2-2 shared spectrum.
* Proposal E4: New periodicity and offset values corresponding to the existing absolute periodicity and offset are introduced for Configured Grant in FR2-2. FFS if we introduce new absolute values
* Proposal E5: New periodicity and offset values corresponding to the existing absolute periodicity and offset are introduced for Scheduling Request in FR2-2. FFS if we introduce new absolute values
* Proposal E6: New periodicity values corresponding to the existing absolute periodicities are introduced for SPS in FR2-2.
* E7: Secondary DRX group is supported for FR1/FR2-2 CA. FFS if any new texts in the specifications are necessary.
* FFS if we introduce any new DRX timer values. Can rediscuss this in February if there is sufficient support.

## RAN2#116-e

* #1: The below Rel-15 and Rel-16 UE capabilities will be differentiated for FR2-1 and FR2-2:

Rel-16 Power saving: maxBW-Preference-r16, maxMIMO-LayerPreference-r16

Rel-16 DCCA: directMCG-SCellActivation-r16, directMCG-SCellActivationResume-r16, directSCG-SCellActivation-r16, directSCG-SCellActivationResume-r16, idleInactiveNR-MeasReport-r16

Rel-15 IMS voice: voiceOverNR, handoverLTE-5GC, handoverInterF, handoverLTE-EPC

* FFS if any other UE capabilities will be needed
* #2: For an existing capability that required further FR2-1 and FR2-2 differentiation, a new IE specifically for FR2-2 (xxParametersFR2-2) is included in the existing per UE IE (XXParameters) as shown in [R2-2109883](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_116-e/Docs/R2-2109883.zip), where xx/XX can be mac-/MAC-, phy-/PHY-, measAndMob/MeasAndMob, ims-/IMS- and powSav-/PowSav- associated with per UE capabilities.
* For a new Rel-17 capability, align with the general decision for Rel-17 capabilities (see main session discussion, FFS whether we align new capabilities with above decision for existing capabilities or have per-band capabilities instead)
* #3: For inter-frequency handover between FR1 and FR2-2 and between FR2-1 and FR2-2, additional per UE capabilities (mandatory with UE capability) below may need to be introduced if handoverInterF requires further FR2-1 and FR2-2 differentiation: handoverFR1-FR2-2-r17, handoverFR2-1-FR2-2-r17
* #4: If a new UE capability introduced for FR2-2 is also applicable to FR2-1 and/or FR1 and the UE capability is per band, this can be expressed in the field description of the UE capability as “This capability is also applicable to FR1 and FR2-1”.
* #5: For UE capability that has to be per UE, “FR1-FR2 Diff” column can be used to express the need of the FR2-1 and FR2-2 differentiation by adding ‘(include FR2-2)’ on top of ‘Yes’ or ‘FR2 only’
* Can revisit these if practical problems are found

RLC impacts

*Proposal#1: Introduce the RLC RTT vales for SCS480kHz and 960kHz as 20ms and captured in the table:*

- Ericsson thinks this is not yet concluded in RAN1. Suggest to use "baseline". Lenovo supports.

- LGE thinks RAN1 thinks 120 kHz is the baseline and prefers Intel proposal. vivo thinks P1 but ould need RLC running CR.- Samsung and Huawei agree.

* #1: Introduce the RLC RTT vales for SCS480kHz and 960kHz as 20ms as baseline. This will be part of TS38.306. Can include this in the running CR for 38.306.

MAC impacts

* #4: RA-RNTI/MsgB-RNTI issue for 480kHz SCS and 960kHz SCS can wait further for RAN1 conclusion.
* 1: RAN2 to keep the current DRX timer values for now, but it can be revisited for performance optimization after high priority issues are resolved.

L2 buffer size

* #2: Keep the L2 buffer size definition as it reflects the upper bound of the L2 buffer size requirement.
* #3: FFS whether UE capability is needed to address concern on too high L2 buffer size requirement. Companies should bring analysis on this to next meeting.

PDCP impacts (Ericsson)

* 2 The existing PDCP SN space is sufficient to cope with the extreme cases in 71 GHz, therefore no spec changes are foreseen for the existing PDCP SN space.

## RAN2#115-e

* 1: Wait for RAN1 to progress on the calculation of RA-RNTI/MsgB-RNTI issue
* 6: Depending on whether RAN1 introduces new SCS for data channels, RAN2 will capture the RLC RTT vales for SCS480kHz and 960kHz in the TS38.306 table on RLC RTT for NR cell group per SCS. FFS on the values (wait for RAN1 progress on L1 processing latency)

No FRx diff

* 2: An existing UE capability applicable to FR2 is also applicable to FR2-2, unless otherwise stated (i.e. in the field description of the UE capability that it is not applicable to FR2-2) in TS38.306,
* 3: If a new UE capability introduced for FR2-2 is also applicable to FR2-1 and/or FR1 and the UE capability is per band, this can be expressed in the field description of the UE capability.

FRx diff

* 4: For an existing UE capability already requires FR1-FR2 Diff and further differentiation between FR2-1 and FR2-2 is needed, the existing UE capability is replicated for FR2-2.
* 5: For UE capability that has to be per UE, “FR1-FR2 Diff” column can be used to express the need of the FRx differentiation (via the ‘Yes/No’ and also whether it needs FR2-1 and FR2-2 differentiation).
* Both 4 and 5 are taken as working assumption (can be revisited once we see the capabilities from RAN1/4)
* As working assumption, RAN2 assumes no need to extend RLC timer values for NR operation with 480, 960 kHz SCS. Can be revisited when we get more information from RAN1/4.
* Wait for RAN1 before discussing L2 buffer size to see if we get prohibitively large buffer sizes.