**3GPP TSG-RAN WG2 Meeting #117-e *draft-R2-220XXXX***

**Electronic meeting, February 21 – March 3, 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **36.306** | **CR** | **-** | **rev** | **-** | **Current version:** | **16.7.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR to 36306 on UE capabilities for the support of NR 71GHz |
|  |  |
| ***Source to WG:*** | Apple Inc |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | NR\_ext\_to\_71GHz-Core |  | ***Date:*** | 2022-02-28 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* *Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Introduction of LTE UE Capabilities for NR operation up to 71G |
|  |  |
| ***Summary of change:*** | Introduce the following LTE UE Capabilities for NR operation up to 71G:* Clarify that the following existing RAN2 determined UE capabilities are applicable only to TDD-FR2.1:
	+ *eutra-5GC-HO-ToNR-TDD-FR2-r15*
	+ *eutra-EPC-HO-ToNR-TDD-FR2-r15*
	+ *ims-VoiceOverNR-FR2-r15*
	+ *ce-EUTRA-5GC-HO-ToNR-TDD-FR2-r16*
* Add the below new capabilities for Rel-17 TDD-FR2-2 operation:
	+ *eutra-5GC-HO-ToNR-TDD-FR2dot2-r17*
	+ *eutra-EPC-HO-ToNR-TDD-FR2dot2-r17*
	+ *ims-VoiceOverNR-FR2dot2-r17*
	+ *ce-EUTRA-5GC-HO-ToNR-TDD-FR2dot2-r17*
 |
|  |  |
| ***Consequences if not approved:*** | UE capabilities required by NR FR2-2 are not introduced in LTE |
|  |  |
| ***Clauses affected:*** | 4.3.34 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS/TR 36.331 CR XXX |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

START OF FIRST CHANGE

### 4.3.34 Inter-RAT Parameters NR

#### 4.3.34.1 *en-DC-r15*

This field indicates whether UE supports E-UTRA NR Dual Connectivity as specified in TS 37.340 [38].

#### 4.3.34.2 *supportedBandListEN-DC-r15*

Only applicable if the UE supports E-UTRA NR Dual Connectivity or NG-RAN E-UTRA-NR Dual Connectivity. This field includes the supported NR bands as defined in TS 38.101-1 [33] and TS 38.101-2 [34]. The presence of this field also indicates that the UE can perform both NR SS-RSRP and SS-RSRQ measurement in the included NR band(s) as specified in TS 38.215 [36].

#### 4.3.34.3 *supportedBandListNR-SA-r15*

This field indicates whether UE supports standalone NR, as specified in TS 38.331 [35], and includes the supported NR bands as defined in TS 38.101-1 [33] and TS 38.101-2 [34]. The presence of this field also indicates that the UE can perform both NR SS-RSRP and SS-RSRQ measurement in the included NR band(s) as specified in TS 38.215 [36].

#### 4.3.34.4 *eutra-5GC-HO-ToNR-FDD-FR1-r15*

This field indicates whether the UE supports handover from E-UTRA/5GC to NR FDD FR1. It is mandatory for UEs of this release of the specification if the UE supports the associated RATs and if the UE supports *eutra-5GC-r15*.

#### 4.3.34.5 *eutra-5GC-HO-ToNR-TDD-FR1-r15*

This field indicates whether the UE supports handover from E-UTRA/5GC to NR TDD FR1. It is mandatory for UEs of this release of the specification if the UE supports the associated RATs and if the UE supports *eutra-5GC-r15*.

#### 4.3.34.6 *eutra-5GC-HO-ToNR-FDD-FR2-r15*

This field indicates whether the UE supports handover from E-UTRA/5GC to NR FDD FR2. It is mandatory for UEs of this release of the specification if the UE supports the associated RATs and if the UE supports *eutra-5GC-r15*.

#### 4.3.34.7 *eutra-5GC-HO-ToNR-TDD-FR2-r15*

This field indicates whether the UE supports handover from E-UTRA/5GC to NR TDD FR2-1 as specified in TS 38.101-x[xx]. It is mandatory for UEs of this release of the specification if the UE supports the associated RATs and if the UE supports *eutra-5GC-r15*.

#### 4.3.34.8 *eutra-EPC-HO-ToNR-FDD-FR1-r15*

This field indicates whether the UE supports handover from E-UTRA/EPC to NR FDD FR1. It is mandatory for UEs of this release of the specification if the UE supports the associated RATs.

#### 4.3.34.9 *eutra-EPC-HO-ToNR-TDD-FR1-r15*

This field indicates whether the UE supports handover from E-UTRA/EPC to NR TDD FR1. It is mandatory for UEs of this release of the specification if the UE supports the associated RATs.

#### 4.3.34.10 *eutra-EPC-HO-ToNR-FDD-FR2-r15*

This field indicates whether the UE supports handover from E-UTRA/EPC to NR FDD FR2. It is mandatory for UEs of this release of the specification if the UE supports the associated RATs.

#### 4.3.34.11 *eutra-EPC-HO-ToNR-TDD-FR2-r15*

This field indicates whether the UE supports handover from E-UTRA/EPC to NR TDD FR2-1 as specified in TS 38.101-x[xx]. It is mandatory for UEs of this release of the specification if the UE supports the associated RATs.

#### 4.3.34.12 *sa-NR-r15*

This field indicates whether the UE supports standalone NR as specified in TS 38.331 [35].

#### 4.3.34.13 *ims-VoiceOverNR-FR1-r15*

This field indicates whether the UE supports IMS voice over NR FR1.

#### 4.3.34.14 *ims-VoiceOverNR-FR2-r15*

This field indicates whether the UE supports IMS voice over NR FR2-1 as specified in TS 38.101-x[xx].

#### 4.3.34.15 *eventB2-r15*

This field defines whether the UE supports event B2. In this release of specification, it is mandatory for a UE supporting NR SA operation to support *eventB2-r15*.

#### 4.3.34.16 *ss-SINR-Meas-NR-FR1-r15*

This field indicates whether the UE can perform NR FR1 SS-SINR measurement as specified in TS 38.215 [36].

#### 4.3.34.17 *ss-SINR-Meas-NR-FR2-r15*

This field indicates whether the UE can perform NR FR2 SS-SINR measurement as specified in TS 38.215 [36].

4.3.34.18 *ng-EN-DC-r15*

This field indicates whether UE supports NG-RAN E-UTRA-NR Dual Connectivity as specified in TS 37.340 [38].

#### 4.3.34.19 *nr-HO-ToEN-DC-r16*

This field indicates whether the UE supports inter-RAT handover from NR to EN-DC while NR-DC or NE-DC is not configured as defined in TS 37.340 [38]. It is mandatory to support inter-RAT handover from NR to EN-DC if the UE supports E-UTRA NR Dual Connectivity.

#### 4.3.34.20 *ce-EUTRA-5GC-HO-ToNR-FDD-FR1-r16*

This field indicates whether the UE supports handover from E-UTRA/5GC in coverage enhancement mode A or B to NR FDD FR1. A UE indicating support of *ce-EUTRA-5GC-HO-ToNR-FDD-FR1-r16* shall also indicate support of *ce-EUTRA-5GC-r16*. This feature is only applicable if the UE supports a UE Category other than Category M1 and M2.

#### 4.3.34.21 *ce-EUTRA-5GC-HO-ToNR-TDD-FR1-r16*

This field indicates whether the UE supports handover from E-UTRA/5GC in coverage enhancement mode A or B to NR TDD FR1. A UE indicating support of *ce-EUTRA-5GC-HO-ToNR-TDD-FR1-r16* shall also indicate support of *ce-EUTRA-5GC-r16*. This feature is only applicable if the UE supports a UE Category other than Category M1 and M2.

#### 4.3.34.22 *ce-EUTRA-5GC-HO-ToNR-FDD-FR2-r16*

This field indicates whether the UE supports handover from E-UTRA/5GC in coverage enhancement mode A or B to NR FDD FR2-1 as specified in TS 38.101-x[xx]. A UE indicating support of *ce-EUTRA-5GC-HO-ToNR-FDD-FR2-r16* shall also indicate support of *ce-EUTRA-5GC-r16*. This feature is only applicable if the UE supports a UE Category other than Category M1 and M2.

#### 4.3.34.23 *ce-EUTRA-5GC-HO-ToNR-TDD-FR2-r16*

This field indicates whether the UE supports handover from E-UTRA/5GC in coverage enhancement mode A or B to NR TDD FR2. A UE indicating support of *ce-EUTRA-5GC-HO-ToNR-TDD-FR2-r16* shall also indicate support of *ce-EUTRA-5GC-r16*. This feature is only applicable if the UE supports a UE Category other than Category M1 and M2.

#### 4.3.34.24 *extendedBand-n77-r16*

This field is only applicable for UEs that indicate support for band n77. If present, the UE supports the restriction to 3450 - 3550 MHz and 3700 - 3980 MHz ranges of band n77 in the USA as specified in Note 12 of Table 5.2-1 in TS 38.101-1 [33]. If absent, the UE supports only restriction to the 3700 - 3980 MHz range of band n77 in the USA. A UE that indicates this field shall also support NS value 55 as specified in TS 38.101-1 [33].

#### 4.3.34.25 *eutra-5GC-HO-ToNR-TDD-FR2dot2-r17*

This field indicates whether the UE supports handover from E-UTRA/5GC to NR TDD FR2-2 as specified in TS 38.101-x[xx]. A UE that indicates this field also supports *eutra-5GC-r15*.

#### 4.3.34.26 *eutra-EPC-HO-ToNR-TDD-FR2dot2-r17*

This field indicates whether the UE supports handover from E-UTRA/EPC to NR TDD FR2-2 as specified in TS 38.101-x[xx].

#### 4.3.34.27 *ims-VoiceOverNR-FR2dot2-r17*

This field indicates whether the UE supports IMS voice over NR FR2-2 as specified in TS 38.101-x[xx].

#### 4.3.34.28 *ce-EUTRA-5GC-HO-ToNR-FDD-FR2dot2-r17*

This field indicates whether the UE supports handover from E-UTRA/5GC in coverage enhancement mode A or B to NR FDD FR2-2 as specified in TS 38.101-x[xx]. A UE indicating support of *ce-EUTRA-5GC-HO-ToNR-FDD-FR2dot2-r17* shall also indicate support of *ce-EUTRA-5GC-r16*. This feature is only applicable if the UE supports a UE Category other than Category M1 and M2.

END OF THE CHANGE