3GPP TSG-RAN WG2 Meeting #118 Electronic R2-220xxxx

Online, May, 2022

**Agenda item: 5.1.4.1.2**

**Source: Apple**

**Title: DRAFT Summary of [AT118-e][018][NR1516] RRM and measurements (Apple)**

**WID/SID: NR\_newRAT-Core**

**Document for: Discussion and Decision**

# 1 Introduction

This document reflects the content and outcome of the following email discussion:

* [AT118-e][018][NR1516] RRM and measurements (Apple)

Scope: Treat R2-2204483, R2-2205678, R2-2206093, R2-2205294, R2-2205295, R2-2205296, R2-2205297, R2-2205213, R2-2205214, R2-2204611, R2-2204612, R2-2204613

Ph1 Determine agreeable parts, Ph2 for agreeable parts agree CRs (offline agreement, CB online only if necessary).

Intended outcome: Report, Agreed CRs

Deadline: Schedule 1

***NOTE: Discussions with Deadline Schedule 1:***

*A* ***first round*** *with* ***Deadline for comments W1 Thursd May 12th 1200 UTC*** *to settle scope what is agreeable etc*

*A Final round with* ***Final deadline W2 Wednesd May 18th 1200 UTC*** *to settle details / agree CRs etc.*

*Additional deadlines check points etc if needed are defined by the Rapporteur of each discussion respectively. In case some parts of an email discussion need more time, doesn’t converge, need on-line treatment, then please contact the chair.*

The discussion covers the following documents from AI 5.1.4.1.2 RRM and Measurements.

# 2 Contact Points

Respondents to the email discussion are kindly asked to fill in the following table.

|  |  |  |
| --- | --- | --- |
| Company | Name | Email Address |
| Huawei, HiSilicon | Lili Zheng | zhenglili4@huawei.com |
| Apple | Fangli XU | fangli\_xu@apple.com |
| Xiaomi | Xing Yang | Yangxing1@xiaomi.com |
| ZTE | LiuJing | liu.jing30@zte.com.cn |
| Nokia |  | amaanat.ali@nokia.com |
| Samsung | Sangyeob Jung | sy0123.jung@samsung.com |
| Qualcomm Inc. | Mouaffac | [mambriss@qti.qualcomm.com](mailto:mambriss@qti.qualcomm.com) |

# 3 Discussion

## 3.1 L3 Filter

|  |
| --- |
| **L3 filter**  R2-2204483 Reply LS to RAN2 on L3 filter configuration (R4-2207041; contact: Apple) RAN4 LS in Rel-15 NR\_newRAT-Core To:RAN2  R2-2205678 Clarification on L3 filtering configuration (filterCoefficient) Apple, Ericsson CR Rel-16 38.331 16.8.0 3111 - F NR\_newRAT-Core  R2-2205961 Clarification on L3 filtering configuration (filterCoefficient) Apple, Ericsson CR Rel-16 38.331 16.8.0 3139 - A NR\_newRAT-Core Late  => Revised in R2-2206093  R2-2206093 Clarification on L3 filtering configuration (filterCoefficient) Apple, Ericsson CR Rel-17 38.331 17.0.0 3139 1 A NR\_newRAT-Core  R2-2205294 Discussion on L3 filtering Huawei, HiSilicon discussion Rel-15 NR\_newRAT-Core  R2-2205295 Correction to L3 filtering (R15) Huawei, HiSilicon CR Rel-15 38.331 15.17.0 3063 - F NR\_newRAT-Core  R2-2205296 Correction to L3 filtering (R16) Huawei, HiSilicon CR Rel-16 38.331 16.8.0 3064 - A NR\_newRAT-Core  R2-2205297 Correction to L3 filtering (R17) Huawei, HiSilicon CR Rel-17 38.331 17.0.0 3065 - A NR\_newRAT-Core |

For the NR L3 filtering design is inherited from LTE. According to RRC spec description, for the filterCoefficient configuration, NW and UE operation should comply with the following principle:

1. UE’s L3 filter input rate is (from L1) is UE implementation dependent (as described in NOTE3);
2. NW provides the filterCoefficient configuration based on the assumed sample rate (according to the description marked in yellow as below);
3. UE adapts its Layer 3 filter implementation and scales the filter coefficient based on the UE’s actual L1 input rate; (according to the description marked in green as below).

|  |
| --- |
| Graphical user interface, text, application, email  Description automatically generated |

In RAN2#116e meeting, RAN2 discussed the sample rate X(ms) associated to the L3 filter configuration (i.e., *filterCoefficient k*) based on R2-2110022. And RAN2 reached the following common understandings during the offline discussion which were indicated in the LS to RAN4 (R2-2111590).

1. *The UE and gNB have the same understanding on the sample rate X.*
2. *The sample rate X is not changed due to L1/L2 operation, e.g. SCell activation/deactivation, BWP switching, etc.*

In RAN4 LS (R2-2204483/ R4-2207041), RAN4 provided the following feedback:

1. *According to current spec, the value of the sample rate X will be changed due to the L1/L2 operation, since the parameters which influence the value is changeable by the L1/L2 operation.*
2. *The lower bound(200ms, 400ms) of intra-frequency measurement period, which is only related to FR is unchangeable by the L1/L2 operation.*

Taking RAN4 feedback into account, in order to avoid the X value changeable due to L1/L2 operation, **R2-2205678 and R2-2206093** propose to clarify that the sample rate X is set to the fix value as RAN4 indicated, i.e. 200ms for FR1 and 400ms for FR2.

***Proposal: Change the value setting of the sample rate X for L3 filtering and set X value to 200ms for FR1 and 400ms for FR2.***

|  |
| --- |
| TP: |

But **R2-2205294 - R2-2205297** propose to make the sample rate X changeable and use the configured value of the ***filter coefficient k*** without adaptation.

***Proposal 1: When performing L3 filtering, the filter coefficient k uses the value received from the network, which is independent from the L1/L2 operation; the sample rate X follows the definition of 38.133, which is changeable by the L1/L2 operation.***

|  |
| --- |
| TP: |

#### **Question 1: Which option of the L3 filter clarification do you prefer?**

* Option 1: Set the sample rate X for L3 filtering as the fix value (R2-2205678 and R2-2206093)
* Option 2: The sample rate X is changeable due to L1/L2 operation, and UE uses the configured value of the ***filter coefficient k*** without adaptation. (R2-2205294 - R2-2205297)

|  |  |  |
| --- | --- | --- |
| Company | Preferred Option? | Comments |
| Huawei, HiSilicon | Option 2 | Proponent of Option2.  According to RAN4 LS, the value of the sample rate X will be changed due to the L1/L2 operation, so Option 1 is NBC and not aligned with RAN4 spec.  We would like to further clarify whether filterCoefficient k or sample rate X is changeable:  In LTE, the **sample rate is a fixed value**, but the **L1 measurement period is changeable**, so it is reasonable to adapt the filter coefficient k considering the relationship between sample rate and L1 measurement period, as captured in 36.331:   |  | | --- | | 2> adapt the filter such that the time characteristics of the filter are preserved at different input rates, observing that the *filterCoefficient* ***k*** assumes a sample rate equal to 200 ms; |   In NR, **the sample rate X equals to L1 measurement period** and both of them are changeable, which means **the sample rate has already been adapted to the L1 measurement period**. In this case, the UE should directly use the filter coefficient k configured by the network and no further adaptation is needed. If needed, it is unclear which principle should the adaptation follow.  Based on the above, the filter coefficient k is the value received from the network, which is independent from the L1/L2 operation; the sample rate X follows the definition of 38.133, which is changeable by the L1/L2 operation. |
| Apple | Option 1 | Option 1 is aligned with the RAN2 common understanding, i.e., UE and NW should hav ehte same understanding on the sample rate X for configuration.  But Option 2 is not aligned with it.  < from RAN2#115e meeting chairman notes>  Graphical user interface, text  Description automatically generated  <RAN2 common understanding in RAN2#116e is reflected in the LS to RAN4 - R2-2111590>  Text  Description automatically generated |
| Xiaomi | Option 2 | Option1 is not aligned with RAN4 LS. |
| ZTE | See comments | Option 1 allows the network to refine the K configuration if the network wants. But it may have NBC problem as HW pointed out.  Option 2 disallows the network to refine the K configuration because L1/L2 operation occurs more frequent than RRC reconfiguration.  However, due to lack of simulation results or test results, it is unclear about significance of refining the k value in real deployment, and how much difference in performance between Option 1 and Option 2?  We would like hear more views from companies, right now, either Option 1 or Option 2 is ok for us. |
| Nokia | See comments | In our view the current specification is correct and no changes are needed. In Nokia’s understanding the following text on adaptation of the filter needs to be kept in TS38.331: "adapt the filter such that the time characteristics of the filter are preserved at different input rates, observing that the filter Coefficient k assumes a sample rate equal to X ms; The value of X is equivalent to one intra-frequency L1 measurement period as defined in TS 38.133 [14] assuming non-DRX operation, and depends on frequency range."   * In order for the UE to meet all the UE RRM requirements in TS38.133 UE typically needs to have higher sampling rate than indicated by the L1 measurement period. * The filter parameter k is indicated for the L1 measurement period and when UE uses higher sampling rate, the UE needs to adjust the actual filter coefficient to match with the actual sampling rate while keeping the filter effect and length in time unchanged compared to the k valued signalled by the network assuming the L1 measurement period. * RAN4 has often assumed 50 ms sampling interval in its intra-frequency neighbour cell measurement related test cases when the intra-frequency L1 measurement period has been 200 ms in order to have enough oversampling for each measurement period and enable sliding window with much smaller step than 200 ms (i.e., 50 ms in this case).   If at all anything needs to be fixed or aligned to the RAN4 LS input we suggest to either introduce a NOTE or just extend the current  **Option 1: Add a note**    **Option 2: Extend current description** |
| Samsung | Option 2 | We understand that Option 1 is not entirely aligned with current RAN4 specification i.e. sample rate X can be changed due to the L1/L2 operation.  Simplest way seems to keep RAN4 specification reference as is in our specification and the UE just applies the configured filter coefficient without adaptation. |
| Qualcomm Inc | Option-2 | Option-2 is aligned with RAN4 requirement.  In addition, adjusting a parameter provided by the network (in this case it is the filter coefficient) doesn’t make sense as it makes the configuration of this parameter obsolete. |

#### **Question 2: Which release of the spec do you prefer the clarification to start with, i.e. Rel-15 or Rel-16?**

|  |  |  |
| --- | --- | --- |
| Company | Release? | Comments |
| Huawei, HiSilicon | R15 | Note that the changes in R2-2205295 (and accompanying shadow CRs) do not change the logic of current text, and bring no backward compatibility issues. |
| Apple | Rel-15 |  |
| Xiaomi | R15 |  |
| Nokia | Rel-15, but | We would request companies to accept our compromise text above which is fully backward compatible and does not remove any existing text from the specifications adversely impacting understanding. |
| Samsung | See comments | If we go for Option 1, we think it should be from Rel-16.  If we go for Option 2, we think that there seems no functional difference from both UE side and NW side. If it is the correct understanding, then it seems OK to have the clarification from Rel-15. |
| Qualcomm Inc | Rel-15 |  |

## 3.2 Correction on quantity configuration (R2-2205313/14)

|  |
| --- |
| R2-2205313 Correction on quantity configuration Xiaomi CR Rel-15 38.331 15.17.0 3067 - F NR\_newRAT-Core  R2-2205314 Correction on quantity configuration Xiaomi CR Rel-16 38.331 16.8.0 3068 - A NR\_newRAT-Core |

|  |  |
| --- | --- |
|  |  |

**Graphical user interface, text, application

Description automatically generated**

#### **Question 3: Do you agree with the CR?**

|  |  |  |
| --- | --- | --- |
| Company | Agree or not? | Comments |
| Huawei, HiSilicon | No | The logic inherits from LTE. The same proposal was discussed in R2-090471 and was rejected.  R2-090471: Correction on Quantity Configuration LG Electronics Inc. *~~CR 36.331 F~~ Disc*  Proposal 1:  - NTT DCM indicates that we agreed yesterday that the quanity config should always be present. This is covered in the NTT DCM CR so no need for this.  => Noted  Proposal 2:  => Noted (already covered by NTT DCM CR)  Proposal 3:  - Samsung indicates this was discussed when this was introduced. Network can configure all RAT’s initially and then there is no problem.  => Not needed  Proposal 4:  - Nokia thinks it is a bit more clearer.  => Proposal 4 will be included by ASN.1 rapporteur. |
| Apple | No | This is a change of UE behaviour. We dont see a strong reason for that. |
| Xiaomi | Yes | The change is more aligned with the logic of the delta configuration.  Thanks HW for the information. Seems the assumption is NW has to provide all RAT’s quantity configuration in LTE. We can check whether it’s still NW vendor’s common understanding in NR. |
| ZTE | No | This is optimization, not correction.  Since it is aligned with LTE and the change itself may cause NBC problem. We think the CR is not needed. |
| Nokia | No | Exactly this is not essential correction agree with the companies saying No. |
| Samsung | No | It has been from LTE so we do not see any necessity on this. |

## 3.3. Corrections on T321&T322 timer start (R2-2204611/12/13)

|  |
| --- |
| R2-2204611 38331CR Corrections on T321 and T322 timer start-R15 OPPO CR Rel-15 38.331 15.17.0 2981 - F NR\_newRAT-Core  R2-2204612 38331CR Corrections on T321 and T322 timer start-R16 OPPO CR Rel-16 38.331 16.8.0 2982 - A NR\_newRAT-Core  R2-2204613 38331CR Corrections on T321 and T322 timer start-R17 OPPO CR Rel-17 38.331 17.0.0 2983 - A NR\_newRAT-Core |

Text

Description automatically generated

#### **Question 4: Do you agree with the CR?**

|  |  |  |
| --- | --- | --- |
| Company | Agree or not? | Comments |
| Apple | No | The change looks like a cleanup. The purpose is already understandable from the original text, even though it is not optimum. |
| Xiaomi |  | Depends on whether NW would configure the measurement in such way, i.e. change report config without meas id change. Seems to be a corner case. We can check NW vendor’s understanding. |
| ZTE | No | The following sentence in the cover page is misleading. CGI reporting must have corresponding measId.  “The CGI reportConfig can be configured without corresponding measId”  If I understand correctly, this CR focus on the scenario e.g. a specific *reportConfig* is reconfigured from “event/periodical” to “reportCGI”, and the associated measObject and measID remain the same, so measObject and measID are not included in RRCReconfiguration message.  Actually, we don’t think this is a typical use case, and we don’t know if all existing UEs support such reconfiguration?  From network perspective, it is safer to remove the old reconfigConfig and add a new one for *reportCGI*.  If above operation is allowed, then it should also be allowed in LTE, which means LTE spec also needs update...  So we think the CR is not needed. Regarding the “conflict” between 7.1.1 and 5.5.2.3, we think there is no room for misunderstanding in real implementation. |
| Nokia | No | We am also not sure of the entire background of this. Anyway, to us this CR is doubtful, if we move procedure between the sections - this could be OK, but we have doubts if other changes are feasible – the proponents claim reportCGI does not require measID configuration and such test cases have been defined in 3GPP. However, in NR RRC framework reportCGI is a part of report configuration which is configured via measurement config. So can measConfig be provided without measID? In timer description (7.1) the wording is weird (If measConfig become available). What this availability suddenly means? |
| Samsung | No | We understand that NW reconfigures measId when reportConfig is changed. Also, current procedure text has been specified from LTE so we do not see any problem. |
| Qualcomm Inc. | Not | It’s a common understanding that the timers should start upon MeasID change/add … if there is a real need to do a change, it may be modifying the timer start time definition in the table in section 7.1.1 to reflect the common understanding. |

# 4 Conclusion

TBD.