**3GPP TSG-RAN WG2 Meeting #118 Electronic R2-220xxxx**

**Online Meeting, 9th – 20th May, 2022**

Agenda Item: 6.4.4.2

Source: Huawei, HiSilicon

**Title:** Report of [AT118-e][066][eIAB] BAP

Document for: Discussion and Decision

# Introduction

This paper aims at capturing the summary of offline discussion.

* [AT118-e][066][eIAB] BAP (Huawei)

Scope: 1. Address the remaining TS issues from tdocs submitted under AI 6.4 (and below), except those issues addressed in specific discussion. Review collect comments identify agreement points, points for online CB etc. 2. Progress the CR, merge all TS impacts into a single CR.

Intended outcome: Report, CR

Deadline: 1 for CB W2 Wed, 2 CR agreement is expected in Post meeting discussion

1. R2-2205253 Miscellaneous CR for TS 38.340 Huawei, HiSilicon
2. R2-2204793 Miscellaneous IAB Corrections on BAP in 38.340 ZTE, Sanechips
3. R2-2204912 Miscellaneous corrections to TS 38.340 Fujitsu
4. R2-2204881 Local congestion-based re-routing at divergence point of DL paths Nokia, Nokia Shanghai Bell
5. R2-2204913 SCG deactivation impact on NR eIAB Fujitsu discussion
6. R2-2205254 Corrections on the handling of unknown, unforeseen, and erroneous protocol data for header rewriting case in TS 38.340 Huawei, HiSilicon
7. R2-2204899 Corrections to 38340 vivo
8. R2-2206040 Miscellaneous corrections to 38.340 for eIAB Qualcomm Incorporated

# Discussion

**2.1 Miscellaneous/Editorial**

|  |  |  |
| --- | --- | --- |
| **Tdoc** | **Changes** | **Rapporteur’s suggestions** |
| R2-2205253 | All changes | **To be merged to Rapp CR and further reviewed in later phase.** |
| R2-2204793 | Changes in 5.2.1.3 | **Not pursued**  [Rapp]: The general note in the beginning already clarifies the applied topology of each routing entry.  “*In the BH Routing Configuration, the entry configured with Non-F1-terminating Topology Indicator IE applies to the BAP Data PDU considered as non-F1-terminating donor topology data, and the entry not configured with Non-F1-terminating Topology Indicator IE only applies to the BAP Data PDU not considered as non-F1-terminating donor topology data.*” |
| Changes in 5.2.1.4.1, 5.2.1.4.2 | **Not pursued**  [Rapp]: The “*, belonging to topology indicated by Ingress Non-F1-terminating Topology Indicator IE in F1AP,*” in the current spec already clarifies the topology of egress link. |
| Changes in 5.2.1.4.3 | **To be merged to Rapp CR and further reviewed in later phase.** |
| R2-2204912 | All changes | **To be merged to Rapp CR and further reviewed in later phase.** |
| R2-2204881 | Proposal 1 | **To be merged to Rapp CR and further reviewed in later phase.** |
| Proposal 2/3 | **See the discussion in below 2.2** |
| R2-2204913 |  | **See the discussion in below 2.3** |
| R2-2205254 |  | **See the discussion in below 2.4** |
| R2-2204899 | Changes in 5.2.1.3 on type indicator | **See the discussion in below 2.5** |
| Changes in 5.2.1.4.1 | **Not pursued**  [Rapp]: Similar to the comment on R2-2204793. |
| Changes in 5.3.1.2 | **Not pursued**  [Rapp]: current wording “per BAP routing ID” already covers that. |
| Others | **To be merged to Rapp CR and further reviewed in later phase.**  [Rapp]: there may be some minor update. |
| R2-2206040 | Changes in 3.1 | **See the discussion in below 2.5** |
| Changes on “*consider this BAP Data PDU to be routed in the non-F1-terminating IAB-donor’s topology*” | **Not pursued**  [Rapp]: The proposed wording does not change the meaning. |
| Change on F1AP IE naming of *Non-F1-terminating IAB-donor’s Topology Indicator* | Wait for RAN3 spec update first. |
| Changes in 5.4.1 | **Not pursued**  [Rapp]: Wording optimization. The proposed wording does not change the meaning. We should focus on essential/critical changes. |
| Other details | **To be merged to Rapp CR and further reviewed in later phase.**  [Rapp]: there may be some minor update/selection. |

**Q1: Do you agree with the rapporteur’s suggestion, and provide detailed comments otherwise.** (You can skip the changes if you agree with rapporteur’s suggestion)

|  |  |  |
| --- | --- | --- |
| **Companies** | **Tdoc/changed section** | **Comments** |
| Fujitsu |  | Agree with rapporteur’s suggestion. |
| ZTE | Changes in 5.2.1.3 and 5.2.1.4.1, 5.2.1.4.2 | It is suggested to have separate field description of *Non-F1-terminating Topology Indicator* IE for each entry of the BH Routing Configuration, *Ingress Non-F1-terminating Topology Indicator* IE and *Egress Non-F1-terminating Topology Indicator* IE for each entry of the BH RLC Channel Mapping Configuration, *Egress Non-F1-terminating Topology Indicator* IE for each entry of the Uplink Traffic to BH RLC Channel Mapping Configuration. In addition, the routing procedure and BH RLC channel mapping procedure should include the topology check, which follows legacy conventions and is helpful for the implementation. |
|  |  |  |
|  |  |  |
|  |  |  |

**2.2 DL re-routing in R2-2204881**

Following is proposed in R2-2204881

**Proposal 2**: An egress link may be determined as congested also locally by an IAB-DU or IAB-donor-DU.

**Proposal 3**: (To implement Proposal 2) amend the current BAP note to say “[…] if it is determined as congested based on the received flow control feedback, as defined in sub-clause 5.3.1, or locally by an IAB-DU or IAB-donor-DU.”

**Rapporteur’s view**: It seems purely IAB-node implementation that IAB node can consider the link not available/congestion in DL. Also, IAB-DU can also trigger the polling of flow control feedback, if it wants, where the received flow control feedback can also trigger the re-routing, if congested.

**Q2: Do you think the proposed change from P3 in R2-2204881 is needed?**

|  |  |  |
| --- | --- | --- |
| **Companies** | **Yes/No** | **Comments** |
| Fujitsu | Yes | Agree IAB node may decide a link is congested locally and re-route the traffic to another available link. It can also achieve load balance. It can decide congestion based on its own buffer without triggering a polling of a flow control feedback. |
| ZTE | Yes | We see the points of this proposal. If we allows the upstream node to perform re-routing, it is reasonable for the congested node to perform re-routing too. |
|  |  |  |
|  |  |  |
|  |  |  |

**2.3 SCG deactivation in R2-2204913**

Following is proposed in R2-2204913

Proposal 1: RAN2 to confirm that SCG deactivation is supported by IAB-MT.

Proposal 2: The egress link corresponding to IAB-MT’s SCG is not considered to be available if SCG is deactivated.

Proposal 3: When BH RLF occurs at MCG and SCG is deactivated at the IAB-MT, the IAB-DU may send a BH RLF detection indication to its child nodes.

Proposal 4: Adopt the TP for TS 38.340 in Annex.

**Rapporteur’s view**: It is good if companies can first confirm on whether SCG deactivation is supported by IAB-MT. Rapp understands that the SCG deactivation is somehow for the motivation of power saving, which is not needed for the IAB-node.

**Q3: Do you think SCG deactivation is supported by IAB-MT?**

|  |  |  |
| --- | --- | --- |
| **Companies** | **Yes/No** | **Comments** |
| Fujitsu | Yes | Normally, the NR DC framework (e.g., MCG/SCG-related procedures) is applicable to IAB-MT. It is reasonable and feasible that IAB-MT also supports SCG deactivation. Otherwise, we will have to state in spec that it is not applicable to IAB-MT. We don't see a strong reason that this DC/CA enhancement is excluded for IAB. |
| ZTE | See comment | It make sense that if the SCG of IAB MT could be be deactivated, the corresponding egress link should be regarded as unavailable. However, this is not R17 specific issue. R16 IAB also has this issue. |
|  |  |  |
|  |  |  |
|  |  |  |

As to the proposed changes, **rapporteur understanding**, even if the SCG deactivation is supported by IAB-MT:

Donor implementation should update the routing configuration together or even before deactivate SCG. If donor considers the SCG is not useful anymore, the all the routing entry via SCG should be released. So, with correct implementation, no BH link on the deactivated SCG will be used/considered by current BAP spec.

**Q4: Do you think the changes in R2-2204913 are needed?**

|  |  |  |
| --- | --- | --- |
| **Companies** | **Yes/No** | **Comments** |
| Fujitsu | Yes | The activation/deactivation mechanism of SCG is supported to have fast usage of SCG when MR-DC is configured. There is no need to create/release the routing entries in a fast way. With the changes in R2-2204913, the SCG deactivation and routing can work together properly. |
| ZTE | No | Agree with rapporteur’s comments. |
|  |  |  |
|  |  |  |
|  |  |  |

**2.4 Error handling in R2-2205254**

Following is proposed in R2-2205254

|  |
| --- |
| When a BAP Data PDU (after the BAP header rewriting operation in accordance with clause 5.2.1.5 or 5.2.1.3, if applied) that contains a BAP address which is not included in the configured BH Routing Configuration and is not the BAP address of this node is received; or when a BAP Control PDU that contains reserved or invalid values is received the BAP entity shall:  - discard the received BAP PDU. |

**The reason for change is copied:**

In R17, there may be some BAP data with the BAP address in header not included in the BH Routing Configuration, due to the header rewriting:

Case 1: At the boundary node, the non-F1-terminating topology data just received may contains BAP address not included in the routing configuration, but will contains the BAP address included in the routing configuration after header rewriting. So, we need to clarify that as long as the data after header rewriting contains the BAP address included in the routing configuration, it should not be discarded.

Case 2: At the IAB-node configured with inter-donor-DU re-routing, after the routing configuration is updated by F1AP after RLF recovery, there may be still some old data received from the descendant node, which contains the old BAP address not included in the new routing configuration. But, those data can be re-routed with header rewriting, which should not be discarded. So, we need to clarify that as long as the data after header rewriting contains the BAP address included in the routing configuration, it should not be discarded.

**Q5: Do you think the changes in R2-2205254 are needed?**

|  |  |  |
| --- | --- | --- |
| **Companies** | **Yes/No** | **Comments** |
| Fujitsu | See comment | Agree with the intention. Need to add more constraint like the following:  When a BAP Data PDU (after the BAP header rewriting operation in accordance with clause 5.2.1.5 or 5.2.1.3, if applied) that contains a BAP address which is not included in the configured BH Routing Configuration with the same topology indicator as this BAP Data PDU and is not the BAP address of this node is received; |
| ZTE | Yes, but... | We also think the topology should be considered when check the BH Routing configuration for the BAP address . |
|  |  |  |
|  |  |  |
|  |  |  |

**2.5 Terminology preference**

Following is proposed in R2-2204899

- an IAB Topology indicator, indicating whether the Egress Routing ID belongs to the non-F1-terminating donor topology, which is indicated by *Non-F1-terminating Topology Indicator* IE.

**Rapporteur’s view**: We use “Type indicator” to be a more general indicator for future proof. In R18 (or future release), we may also need some other indicator for the configured entry, e.g. the indicator of target logical DU of mobile IAB. Companies are welcome to comment if we need to change the current terminology.

**Q6: Do you think the change (Type indicator->Topology indicator) in R2-2204899 is needed?**

|  |  |  |
| --- | --- | --- |
| **Companies** | **Yes/No** | **Comments** |
| Fujitsu | Yes | This correction is reasonable.  It is expected that each parameter name being aligned with TS38.473. |
| ZTE | Yes | IAB topology is widely used in the R17 spec. It is more clear comapred with type indicator. |
|  |  |  |
|  |  |  |
|  |  |  |

Following is proposed in R2-2206040:

**BH RLC channel:** an RLC channel between two nodes, which is used to transport backhaul packets, as defined in TS 38.300 [2]**.**

**Boundary IAB-node**: as defined in TS 38.401 [6].

**Egress BH RLC channel:** a BH RLC channel on which a packet is transmitted by a node.

**Egress link**: a radio link on which a packet is transmitted by a node.

**F1-terminating IAB-donor**: as defined in TS 38.401 [2].

**IAB-donor**: as defined in TS 38.300 [2].

**IAB-donor-DU**: as defined in TS 38.401 [6].

**IAB-node**: as defined in TS 38.300 [2].

**Ingress BH RLC channel:** a BH RLC channel on which a packet is received by a node.

**Ingress link**: a radio link on which a packet is received by a node.

**Non-F1-terminating IAB-donor**: as defined in TS 38.401 [2].

**Rapporteur’s view**: It is fine to align the wording with RAN3 spec. But, those terms are frequently used in 38.340, it is preferred to also copy it in BAP spec.

**Q7: Do you agree to update the terms in sec. 3.1 as below (i.e. copy from the 38.401 spec and add reference)?**

|  |
| --- |
| **Boundary IAB-node**: an IAB-node with one RRC interface terminating at a different IAB-donor-CU than the F1 interface, as defined in TS 38.401 [6].  **F1-terminating donor**: refers to the IAB-donor that terminates F1 for the boundary IAB-node, as defined in TS 38.401 [6]  **Non-F1-terminating donor**: refers to the IAB-donor that has an RRC connection with the boundary node but does not terminate F1 with this boundary node, as defined in TS 38.401 [6] |

|  |  |  |
| --- | --- | --- |
| **Companies** | **Yes/No** | **Comments** |
| Fujitsu |  | Either way is fine, as long as they are aligned. |
| ZTE | See comment | We are fine to align the term with F1-terminating IAB-donor and non-F1-terminating IAB-donor as in TS38.401. However, we think the definition can be copied from 38.401 as rapporteur does. |
|  |  |  |
|  |  |  |
|  |  |  |

# Conclusion and proposals

Based on the above summary, following proposals are given

# Reference

1. R2-2205253 Miscellaneous CR for TS 38.340 Huawei, HiSilicon
2. R2-2204793 Miscellaneous IAB Corrections on BAP in 38.340 ZTE, Sanechips
3. R2-2204912 Miscellaneous corrections to TS 38.340 Fujitsu
4. R2-2204881 Local congestion-based re-routing at divergence point of DL paths Nokia, Nokia Shanghai Bell
5. R2-2204913 SCG deactivation impact on NR eIAB Fujitsu discussion
6. R2-2205254 Corrections on the handling of unknown, unforeseen, and erroneous protocol data for header rewriting case in TS 38.340 Huawei, HiSilicon
7. R2-2204899 Corrections to 38340 vivo
8. R2-2206040 Miscellaneous corrections to 38.340 for eIAB Qualcomm Incorporated