3GPP TSG-RAN WG2 Meeting #118-e R2- 220xxxx

Online, 9th May – 20th May, 2022

Source: CATT

Title: Report of [AT118-e][071][ePowSav] RRC (CATT) – Phase 2

Agenda Item: 6.9.1.3

Document for: Discussion and Decision

# Introduction

This contribution provides the report of the Phase 2 of the following email discussion:

* [AT118-e][071][ePowSav] RRC (CATT)

Scope: 1. For TRS/CSI-RS Address remaining issues, from tdocs under 6.9.3.3. not already addressed, Identify agreements, discussion points, etc. 2a. Allow further checking of the RRC Rapporteur resolutions in the RRC CR. 2b. Update the CR acc to meeting agreements

Intended outcome: 1. Report. 2 Agreed CR (in the end)

Deadline: CB W2 Tuesday, CR agreement expected by Post meeting discussion.

As background, the Chair’s notes for the related on-line discussion are copied below:

|  |
| --- |
| R2-2206493 Report of [AT118-e][071][ePowSav] RRC (CATT) CATT  DISCUSSION  P3   * CATT think this is for a stable configuration, for which there is no need to frequently re-activate. * Xiaomi prefer R1 decision, but no strong concerns. * QC want to add the comment that it doesn’t override the validity timer.   P1   * Xiaomi want to make further clarifications. * add the “infinity” value to the field *validityDuration (not intended to override the SIB validity timer).* * RAN2 understands there is no possible conflict or ambiguity between TRS/CSI-RS configuration broadcasted in SIB17 for idle/inactive UEs and TRS/CSI-RS configuration provided via dedicated signaling for connected UEs. No specification change is required.   Chair: P1 (or variant thereof) for email/offline agreement. |

And the related P1 was:

**Proposal 1 (17/17): UE considers the validity duration is ended at the boundary of the modification period during which UE receives the changed TRS/CSI-RS configuration or until the validity time duration expires, whichever is earlier.**

# Contact Information

|  |  |  |
| --- | --- | --- |
| **Company** | **Name** | **Email** |
| CATT | Pierre Bertrand | pierrebertrand@catt.cn |
| Ericsson | Martin van der Zee | martin.van.der.zee@ericsson.com |
| Xiaomi | Yanhua Li | Liyanhua1@xiaomi.com |
| Qualcomm | Linhai He | linhaihe@qti.qualcomm.com |
| Sequans | Noam Cayron | noam.cayron@sequans.com |
| Intel Corporation | Seau Sian Lim | seau.s.lim@intel.com |
| Samsung | Anil Agiwal | anilag@samsung.com |
| LGE | Soo Kim | soo.kim@lge.com |
| Sharp | LIU Lei | lei.liu@cn.sharp-world.com |
| Nokia | Jussi Koskinen | jussi-pekka.koskinen@nokia.com |
| Vivo | Chenli | Chenli5g@vivo.com |
| MediaTek | Li-Chuan TSENG | li-chuan.tseng@mediatek.com |
| Huawei, HiSilicon | Jagdeep Singh | [jagdeep.singh6@huawei.com](mailto:jagdeep.singh6@huawei.com) |
| Apple | Sethuraman Gurumoorthy | sethu@apple.com |
| CMCC | Xiaoxuan Tang | tangxiaoxuan@chinamobile.com |
| OPPO | Haitao Li | [lihaitao@oppo.com](mailto:lihaitao@oppo.com) |

# TRS/CSR-RS remaining issues

## TRS availability when SI change

In [1], it is discussed a potential issue when the TRS/CSI-RS configuration is changed during the validity duration, as illustrated in Figures 1 and 2:



**Figure 1: TRS configuration is changed during the idle/inactive TRS validity duration configured by RRC**



**Figure 2: UE receives the validity indication duration and the TRS/CSI-RS change indication at the same**

[1] questions whether the UE still follows the legacy validity duration configured by RRC in these cases, or if another behavior should be expected. Specifically, [1] suggests two options:

* Option 1: UE still considers the updated TRS/CSI-RS as available until the validity duration time duration expires (no specification change).
* Option 2: UE considers the validity duration is ended at the boundary of the modification period during which UE receives the changed TRS/CSI-RS configuration or until the validity time duration expires, whichever is earlier.

[1] argues Option 2 could allow a clean separation of the L1 based availability indications for the old and new configurations.

**Q1. Which option do you support from Option 1 and Option 2?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option1/2** | **Comment** |
| Ericsson | Option 2 | We think it needs to be clarified when L1 and L3 indicate something differently. In our understanding L3 should be leading here, e.g. the configuration might have changed or removed, in which case the L1 indication obviously is not valid anylonger. |
| Xiaomi | Option2 | I think we are meaning here is:  The TRS/CSI-RS availability is assumed to be ‘unavailable’ for all the TRS resource set group(s) upon getting the TRS/CSI-RS configuration modification.  Not only for the TRS resource set group whose configuration is changed, right? |
| Qualcomm | Option 2 | Agree with Ericsson |
| ZTE | Option 2 | From NW point of view, even though the scenario mentioned here we think it is not common since the intention of introduction of L1 indication is actually for not change the TRS Configuration during the validity period, we still think L3 signaling shall have a priority than L1 indication in case such an abnormal scenario really happen in the real deployment. |
| Sequans | Option 2 | Agree with Ericsson |
| Intel | Option 2 |  |
| Samsung | Option 2 | Once the configuration is changed, L1 indication for old configuration is not valid. New L1 indication is needed for availability indication of updated configuration. |
| LGE | Option 2 | Before UE starts SI update procedure, it may use TRS resources that was indicated before UE obtains the SIB for TRS configuration. Therefore, if an SI update procedure is performed(at the boundary of the modification period), the UE should consider the TRS as unavailable. |
| Sharp | Option 2 |  |
| Nokia | Option 2 | Agree with Ericsson |
| vivo | Option 2  (proponent) | As we have agreed, when UE acquires SIB-X with a TRS/CSI-RS configuration, it may receive the associated L1-based availability indication soon. Then if this SIB-X is changed within the previous valid duration time, UE may receive the changed TRS/CSI-RS configuration and new L1 based signaling within the valid duration time. And UE may be confused about how to deal with the new availability indication and the previous availability indication.  Besides, RAN1 has the following agreement in RAN1#107bis-e meeting:  *UE can receive L1 based signaling for TRS availability indication before the expiration/end of validity duration associated with previous L1 based signaling for TRS availability indication*   * *For each bit indicated as ‘1’ in the availability indication field of the current L1 based signaling ~~TRS availability indication~~, the UE assumes the corresponding TRS resource set(s) are available from the reference point until the end of the validity duration associated with the current L1 based signaling ~~indication~~.* * *For each bit indicated as ‘0’ in the availability indication field of the current L1 based signaling, the UE keeps the existing ~~current~~ assumption on the availability or unavailability of the corresponding TRS resource set(s).*   It can be observed that the indication of L1 based availability indication in and out of the validity duration is different. And in the above case, the new received L1 based signaling obviously should be considered as which is received out of the validity duration, which is not aligned with RAN1’s agreement.  Hence the case that TRS/CSI-RS configuration is changed within the validity time duration must be considered. And option2 is a straightforward method to resolve the issue. |
| CATT | Option 2 | Our understanding is that the L1 indication is associated with a TRS configuration (via the parameter *indBitID*), hence upon a new configuration it makes sense that the L1 indication associated with the old TRS configuration is no longer valid. |
| MediaTek | Option 2 | Agree with CATT |
| Huawei, HiSilicon | Option 2 | Agree with CATT |
| Apple | Option 2 | Agree with CATT |
| CMCC | Option 2 |  |
| OPPO | Option 2 |  |

Summary:

17 companies provided inputs to this question and all support Option 2.

**Proposal 1 (17/17): UE considers the validity duration is ended at the boundary of the modification period during which UE receives the changed TRS/CSI-RS configuration or until the validity time duration expires, whichever is earlier.**

## TRS availability when SI change – Phase 2

Although a majority of companies agreed the principle of Proposal 1 above, it seems some clarifications are needed on the exact related behavior. Specifically, during Phase 1 and online, Xiaomi had the following question:

|  |  |  |
| --- | --- | --- |
| Xiaomi | Option2 | I think we are meaning here is:  The TRS/CSI-RS availability is assumed to be ‘unavailable’ for all the TRS resource set group(s) upon getting the TRS/CSI-RS configuration modification.  Not only for the TRS resource set group whose configuration is changed, right? |

From rapporteur’s perspective, there could indeed be two understandings of Proposal 1.

Understanding 1: UE considers the validity duration is ended at the boundary of the modification period during which UE receives the ~~changed TRS/CSI-RS configuration~~  SI change notification or until the validity time duration expires, whichever is earlier.

In this case, Xiaomi is correct because, anyways, during this modification period, the UE does not know which TRS configuration *may* change, and actually it does not even know if SIB17 is impacted by the SI update. The drawback, of course, is that when the SI update is not for SIB17, then no TRS configuration is impacted although the network still needs to reactivate via L1 signaling all the TRS configurations.

Understanding 2: UE considers the validity duration is ended when ~~at the boundary of the modification period during which~~ UE receives the changed TRS/CSI-RS configuration in the modification period following a SI change notification or until the validity time duration expires, whichever is earlier.

In this case, the UE stops the validity duration timer of a TRS configuration at the time it receives the updated SIB17, if updated, and only for the TRS configuration that has changed. And the network only needs to reactivate the new TRS configuration via L1 signalling.

Rapporteur would like to check companies’ views on these two understandings.

**Q1a. Which understanding do you support?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Understanding 1/2** | **Comment** |
| CATT | Understanding 2 | This approach saves significant L1 signalling from network side. It is anyways assumed that, from the modification period boundary up to the time UE acquires the changed SIB(s), UE implementation will not assume any TRS available and will use SSB instead. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Summary:

# Conclusion

# Reference

1. R2-2204809 Discussion on TRS availability when SI change, vivo
2. R2-2204908 TRS/CSI-RS configuration in RRC\_CONNECTED, DENSO
3. R2-2206046 TRS and CSI-RS exposure, Ericsson