**3GPP TSG-RAN WG2 Meeting #118-e *R2-2206190***

**E-Meeting, 9 - 20 May, 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **36.331** | **CR** | **4794** | **rev** | **1** | **Current version:** | **17.0.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Corrections on the general ASN.1 issues | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Samsung | | | | | | | | | |
| ***Source to TSG:*** | R2 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | TEI17, NB\_IOTenh3-Core | | | | |  | ***Date:*** | | | 2022-04-28 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | F |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The changes included in this CR aim to correct general ASN.1 issues and minor/editorial changes. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | This CR includes the following change for RILs and minor/editorial changes:   1. H205: Clarify that *measUncomBarPre* in *LoggedMeasurementConfiguration* is for UE in RRC\_IDLE. 2. H202: Change “idle mode” to “*camped normally* state” in the field description of *loggedMeasIdleEventL1*. 3. H203: Change “idle mode” to “*any cell selection* state” in the field description of *loggedMeasIdleEventOutOfCoverage*. 4. H209: Add the reference to TS 36.304 in the field description of *inactiveStatePO-Determination*. 5. E806: Remove "sibType30-v1700, sibType31-v1700, sibType32-v1700" from SIB-Type (without suffix) and add a note in the ASN.1 code.   Note: This extention is not to be used any further for this release of the specification. If needed, use SIB-Type-v12j0 for new SIB(s).   1. Editorial changes (e.g. missing comma/space, style changes, etc.) and mirror changes in Rel-16 LTE RRC Rapporteur CR (CR4790r1) | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Miscellaneous errors will remain in the specification. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.3.3.4a, 5.3.5.3, 5.3.5.4, 5.5.2.13, 5.6.3.3, 5.6.8.2, 5.6.13a.1, 5.10.7.3, 5.10.8.2, 5.10.8a, 6.2.1, 6.2.2, 6.3.1, 6.3.6, 6.3.7, 6.7.3.6, 7.3.1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

#### 5.3.3.4a Reception of the *RRCConnectionResume* by the UE

The UE shall:

1> stop timer T300;

1> if T309 is running:

2> stop timer T309 for all access categories;

2> perform the actions as specified in 5.3.16.4.

1> stop T380 if running;

1> if the *RRCConnectionResume* is received in response to an *RRCConnectionResumeRequest* for EDT or for transmission using PUR:

2> discard the stored UE AS context and *resumeIdentity*;

2> if the *RRCConnectionResume* is received in response to an *RRCConnectionResumeRequest* for transmission using PUR:

3> instruct the associated MAC entity to start *timeAlignmentTimer*;

1> else:

2> if resuming an RRC connection from a suspended RRC connection in EPC; or

2> for NB-IoT, if resuming an RRC connection from a suspended RRC connection in 5GC and *fullConfig* is not present in the *RRCConnectionResume* message:

3> restore the PDCP state and re-establish PDCP entities for SRB2, if configured withE-UTRA PDCP, and for all DRBs that are configured with E-UTRA PDCP;

3> if *drb-ContinueROHC* is included:

4> indicate to lower layers that stored UE AS context is used and that *drb-ContinueROHC* is configured;

4> continue the header compression protocol context for the DRBs configured with the header compression protocol;

3> else:

4> indicate to lower layers that stored UE AS context is used;

4> reset the header compression protocol context for the DRBs configured with the header compression protocol;

3> if *restoreMCG-SCells* is included:

4> restore the MCG SCell(s) configuration, if stored;

3> else:

4> release the MCG SCell(s) from the UE AS context, if stored;

3> if *restoreSCG* is included:

4> restore *nr-SecondaryCellGroupConfig*, if stored;

3> else if the UE was configured with EN-DC:

4> perform MR-DC release, as specified in TS 38.331 [82], clause 5.3.5.10;

4> release *tdm-PatternConfig* or *tdm-PatternConfig2*, if configured;

3> discard the stored UE AS context and *resumeIdentity*;

3> configure lower layers to consider the restored MCG and SCG SCell(s) (if any) to be in deactivated state;

2> else if the *RRCConnectionResume* message includes the *fullConfig* (i.e., for resuming an RRC connection from RRC\_INACTIVE or for resuming a suspended RRC connection in 5GC):

3> perform the radio configuration procedure as specified in 5.3.5.8;

2> else if resuming an RRC connection from RRC\_INACTIVE:

3> restore the following from the stored UE Inactive AS context:

- MCG physical layer configuration,

- MCG MAC configuration,

- MCG RLC configuration,

- PDCP configuration;

3> if *restoreMCG-SCells* is included:

4> restore the MCG SCell(s) configuration, if stored;

3> else:

4> release the MCG SCell(s) from the UE Inactive AS context, if stored;

3> if *restoreSCG* is included:

4> restore *nr-SecondaryCellGroupConfig*, if stored;

3> else if the UE was configured with NGEN-DC:

4> perform MR-DC release, as specified in TS 38.331 [82], clause 5.3.5.10;

4> release *tdm-PatternConfig* or *tdm-PatternConfig2*, if configured;

3> discard the stored UE Inactive AS context;

3> configure lower layers to consider the restored MCG and SCG SCell(s) (if any) to be in deactivated state;

3> release the *rrc-InactiveConfig*, except *ran-NotificationAreaInfo*;

2> else (i.e., except for NB-IoT for resuming a suspended RRC connection in 5GC):

3> restore the physical layer configuration, the MAC configuration, the RLC configuration and the PDCP configuration from the stored UE AS context;

3> discard the stored UE AS context and *resumeIdentity*;

1> perform the radio resource configuration procedure in accordance with the received *radioResourceConfigDedicated* and as specified in 5.3.10.0;

NOTE 1: When performing the radio resource configuration procedure, for the physical layer configuration and the MAC Main configuration, the restored RRC configuration from the stored UE AS context is used as basis for the reconfiguration.

1> if the received *RRCConnectionResume* includes the *sCellToReleaseList*:

2> perform SCell release as specified in 5.3.10.3a;

1> if the received *RRCConnectionResume* includes the *sCellToAddModList*:

2> perform SCell addition or modification as specified in 5.3.10.3b;

1> if the received *RRCConnectionResume* includes the *sCellGroupToReleaseList*:

2> perform SCell group release as specified in 5.3.10.3d;

1> if the received *RRCConnectionResume* includes the *sCellGroupToAddModList*:

2> perform SCell group addition or modification as specified in 5.3.10.3e;

1> if the received *RRCConnectionResume* message includes the *nr-SecondaryCellGroupConfig*:

2> if the *RRCReconfiguration* includes the *scg-State*:

3> perform SCG deactivation as specified in TS 38.331 [82], clause 5.3.5.13b;

2> else:

3> perform SCG activation as specified in TS 38.331 [82], clause 5.3.5.13a;

2> perform NR RRC Reconfiguration as specified in TS 38.331 [82], clause 5.3.5.3;

1> if the received *RRCConnectionResume* message includes the *sk-Counter*:

2> perform key update procedure as specified in TS 38.331 [82], clause 5.3.5.8;

1> if the received *RRCConnectionResume* message includes the *nr-RadioBearerConfig1*:

2> perform radio bearer configuration as specified in TS 38.331 [82], clause 5.3.5.6;

1> if the received *RRCConnectionResume* message includes the *nr-RadioBearerConfig2*:

2> perform radio bearer configuration as specified in TS 38.331 [82], clause 5.3.5.6;

1> except if the *RRCConnectionResume* is received in response to an *RRCConnectionResumeRequest* for EDT or for transmission using PUR:

2> resume SRB2, SRB3 (if configured), and all DRBs, if any, including RBs configured with NR PDCP;

1> if stored, discard the cell reselection priority information provided by the *idleModeMobilityControlInfo* or inherited from another RAT;

1> if stored, discard the *altFreqPriorities* provided by the *RRCConnectionRelease*;

1> if stored, discard the dedicated offset provided by the *redirectedCarrierOffsetDedicated*;

1> if the *RRCConnectionResume* message includes the *measConfig*:

2> perform the measurement configuration procedure as specified in 5.5.2;

1> if T302 is running:

2> stop timer T302;

2> if the UE is connected to 5GC:

3> perform the actions as specified in 5.3.16.4;

1> stop timer T303, if running;

1> stop timer T305, if running;

1> stop timer T306, if running;

1> stop timer T308, if running;

1> perform the actions as specified in 5.3.3.7;

1> stop timer T320, if running;

1> stop timer T350, if running;

1> perform the actions as specified in 5.6.12.4;

1> stop timer T360, if running;

1> stop timer T322, if running;

1> stop timer T323, if running;

1> if timer T331 is running:

2> stop timer T331;

2> perform the actions as specified in 5.6.20.3;

1> if the UE is resuming an RRC connection after early security reactivation in accordance with conditions in 5.3.3.18 or *RRCConnectionResume* is received in response to an *RRCConnectionResumeRequest* from RRC\_INACTIVE:

2> ignore the *nextHopChainingCount* value indicated in the *RRCConnectionResume* message;

1> else:

2> if resuming an RRC connection from a suspended RRC connection in EPC:

3> update the KeNB key based on the KASME key to which the current KeNB is associated, using the *nextHopChainingCount* value indicated in the *RRCConnectionResume* message, as specified in TS 33.401 [32];

3> store the *nextHopChainingCount* value;

3> derive the KRRCint key associated with the previously configured integrity algorithm, as specified in TS 33.401 [32];

3> request lower layers to verify the integrity protection of the *RRCConnectionResume* message, using the previously configured algorithm and the KRRCint key;

3> if the integrity protection check of the *RRCConnectionResume* message fails:

4> perform the actions upon leaving RRC\_CONNECTED as specified in 5.3.12, with release cause 'other', upon which the procedure ends;

3> derive the KRRCenc key and the KUPenc key associated with the previously configured ciphering algorithm, as specified in TS 33.401 [32];

3> configure lower layers to resume integrity protection using the previously configured algorithm and the KRRCint key immediately, i.e., integrity protection shall be applied to all subsequent messages received and sent by the UE;

3> configure lower layers to resume ciphering and to apply the ciphering algorithm, the KRRCenc key and the KUPenc key, i.e. the ciphering configuration shall be applied to all subsequent messages received and sent by the UE;

1> enter RRC\_CONNECTED;

1> indicate to upper layers that the suspended RRC connection has been resumed;

1> stop the cell re-selection procedure;

1> consider the current cell to be the PCell;

1> set the content of *RRCConnectionResumeComplete* message as follows:

2> set the *selectedPLMN-Identity* to the PLMN selected by upper layers (see TS 23.122 [11], TS 24.301 [35] for E-UTRA/EPC and TS 24.501 [95] for E-UTRA/5GC) from the PLMN(s) included in the *plmn-IdentityList* in *SystemInformationBlockType1*;

2> set the *dedicatedInfoNAS* to include the information received from upper layers;

2> except for NB-IoT:

3> if resuming an RRC connection from a suspended RRC connection:

4> if the UE has radio link failure or handover failure information available in *VarRLF-Report* and if the RPLMN is included in *plmn-IdentityList* stored in *VarRLF-Report*:

5> include *rlf-InfoAvailable*;

4> if the UE has MBSFN logged measurements available for E-UTRA and if the RPLMN is included in *plmn-IdentityList* stored in *VarLogMeasReport*:

5> include *logMeasAvailableMBSFN*;

4> else if the UE has logged measurements available for E-UTRA and if the RPLMN is included in *plmn-IdentityList* stored in *VarLogMeasReport*:

5> include *logMeasAvailable*;

5> if Bluetooth measurement results are included in the logged measurements the UE has available:

6> include *logMeasAvailableBT*;

5> if WLAN measurement results are included in the logged measurements the UE has available:

6> include *logMeasAvailableWLAN*;

4> if the UE has connection establishment failure information available in *VarConnEstFailReport* and if the RPLMN is equal to *plmn-Identity* stored in *VarConnEstFailReport*:

5> include *connEstFailInfoAvailable*;

4> include the *mobilityState* and set it to the mobility state (as specified in TS 36.304 [4]) of the UE just prior to entering RRC\_CONNECTED state;

4> if the UE has flight path information available:

5> include *flightPathInfoAvailable*;

3> if the UE supports storage of mobility history information and the UE has mobility history information available in *VarMobilityHistoryReport*:

4> include *mobilityHistoryAvail*;

3> if the *idleModeMeasurementReq* is included in the *RRCConnectionResume* message:

4> if the UE has idle/inactive measurement information concerning cells other than the PCell available in *VarMeasIdleReport*:

5> set the *measResultListIdle-r16* in the *RRCConnectionResumeComplete* message to the value of *measReportIdle-r15* in the *VarMeasIdleReport*;

5> set the *measResultListExtIdle* in the *RRCConnectionResumeComplete* message to the value of *measReportIdle-r16* in the *VarMeasIdleReport*, if available;

5> set the *measResultListIdleNR* in the *RRCConnectionResumeComplete* message to the value of *measReportIdleNR* in the *VarMeasIdleReport*, if available;

5> discard the *VarMeasIdleReport* upon successful delivery of the *RRCConnectionResumeComplete* message is confirmed by lower layers;

3> else:

4> if the SIB2 contains *idleModeMeasurements* and the UE has E-UTRA idle/inactive measurement information concerning cells other than the PCell available in *VarMeasIdleReport*; or

4> if the SIB2 contains *idleModeMeasurementsNR* and the UE has NR idle/inactive measurement information available in *VarMeasIdleReport*:

5> include the *idleMeasAvailable*;

3> if the *RRCConnectionResume* message includes *nr-SecondaryCellGroupConfig*:

4> include *scg-ConfigResponseNR* in accordance with TS 38.331 [82], clause 5.3.5.3;

2> for NB-IoT:

3> if the UE supports serving cell idle mode measurements reporting and *servingCellMeasInfo* is present in *SystemInformationBlockType2-NB*:

4> set the *measResultServCell* to include the measurements of the serving cell;

NOTE 2: The UE includes the latest results of the serving cell measurements as used for cell selection/ reselection evaluation, which are performed in accordance with the performance requirements as specified in TS 36.133 [16].

3> if the UE is connected to EPC:

4> if the UE has radio link failure information available in *VarRLF-Report-NB* and if the RPLMN is included in *plmn-IdentityList* stored in *VarRLF-Report-NB*:

5> include *rlf-InfoAvailable*;

4> if the UE has ANR measurements information available in *VarANR-MeasReport-NB* and if the RPLMN is included in *plmn-IdentityList* stored in *VarANR-MeasReport-NB*:

5> include *anr-InfoAvailable*;

1> if the UE is configured to operate in EN-DC as result of this procedure, forward *upperLayerIndication* to upper layers as if the UE has received this field from SIB2, otherwise indicate to upper layers the absence of this field;

1> submit the *RRCConnectionResumeComplete* message to lower layers for transmission;

1> for NB-IoT:

2> if the UE supports connected mode measurements and *connMeasConfig* is present in *SystemInformationBlockType3-NB*:

3> perform measurements as specified in 5.5.8.

1> the procedure ends.

#### 5.3.5.3 Reception of an *RRCConnectionReconfiguration* not including the *mobilityControlInfo* by the UE

If the *RRCConnectionReconfiguration* message does not include the *mobilityControlInfo* and theUE is able to comply with the configuration included in this message, the UE shall:

1> if the *RRCConnectionReconfiguration* includes the *scg-State*:

2> perform SCG deactivation as specified in TS 38.331 [82], clause 5.3.5.13b;

1> else:

2> perform SCG activation as specified in TS 38.331 [82], clause 5.3.5.13a;

1> if the received *RRCConnectionReconfiguration* includes the *daps-SourceRelease*:

2> reset source MCG MAC and release the source MCG MAC configuration;

2> for each DAPS bearer:

3> re-establish the RLC entity or entities for the source PCell;

3> release the RLC entity or entities and the associated DTCH logical channel for the source PCell;

3> reconfigure the PDCP entity to release DAPS, as specified in TS 36.323 [8];

2> for each SRB:

3> release the PDCP entity for the source PCell;

3> release the RLC entity and the associated DCCH logical channel for the source PCell;

2> release the physical channel configuration for the source PCell;

1> if this is the first *RRCConnectionReconfiguration* message after successful completion of the RRC connection re-establishment procedure:

2> re-establish PDCP for SRB2 configured with E-UTRA PDCP entity and for all DRBs that are established and configured with E-UTRA PDCP, if any;

2> re-establish RLC for SRB2 and for all DRBs that are established and configured with E-UTRA RLC, if any;

2> if the *RRCConnectionReconfiguration* message includes the *fullConfig*:

3> perform the radio configuration procedure as specified in 5.3.5.8;

2> if the *RRCConnectionReconfiguration* message includes the *radioResourceConfigDedicated*:

3> perform the radio resource configuration procedure as specified in 5.3.10.0;

NOTE 1: Void

NOTE 2: Void

1> else:

2> if the *RRCConnectionReconfiguration* message includes the *radioResourceConfigDedicated*:

3> perform the radio resource configuration procedure as specified in 5.3.10.0;

NOTE 3: If the *RRCConnectionReconfiguration* message includes the establishment of radio bearers other than SRB1, the UE may start using these radio bearers immediately, i.e. there is no need to wait for an outstanding acknowledgment of the *SecurityModeComplete* message.

1> if the received *RRCConnectionReconfiguration* includes the *sCellToReleaseList*:

2> perform SCell release as specified in 5.3.10.3a;

1> if the received *RRCConnectionReconfiguration* includes the *sCellToAddModList*:

2> perform SCell addition or modification as specified in 5.3.10.3b;

1> if the received *RRCConnectionReconfiguration* includes the *sCellGroupToReleaseList*:

2> perform SCell group release as specified in 5.3.10.3d;

1> if the received *RRCConnectionReconfiguration* includes the *sCellGroupToAddModList*:

2> perform SCell group addition or modification as specified in 5.3.10.3e;

1> if the received *RRCConnectionReconfiguration* includes the *scg-Configuration*; or

1> if the current UE configuration includes one or more split DRBs configured with *pdcp-Config* and the received *RRCConnectionReconfiguration* includes *radioResourceConfigDedicated* including *drb-ToAddModList*:

2> perform SCG reconfiguration as specified in 5.3.10.10;

1> if the received *RRCConnectionReconfiguration* includes the *nr-Config* and it is set to *release*: or

1> if the received *RRCConnectionReconfiguration* includes *endc-ReleaseAndAdd* and it is set to *TRUE*:

2> perform MR-DC release as specified in TS 38.331 [82], clause 5.3.5.10;

1> if the received *RRCConnectionReconfiguration* includes the *sk-Counter*:

2> perform key update procedure as specified in TS 38.331 [82], clause 5.3.5.7;

1> if the received *RRCConnectionReconfiguration* includes the *nr-SecondaryCellGroupConfig*:

2> perform NR RRC Reconfiguration as specified in TS 38.331 [82], clause 5.3.5.3;

1> if the received *RRCConnectionReconfiguration* includes the *nr-RadioBearerConfig1*:

2> perform radio bearer configuration as specified in TS 38.331 [82], clause 5.3.5.6;

1> if the received *RRCConnectionReconfiguration* includes the *nr-RadioBearerConfig2*:

2> perform radio bearer configuration as specified in TS 38.331 [82], clause 5.3.5.6;

1> if this is the first *RRCConnectionReconfiguration* message after successful completion of the RRC connection re-establishment procedure:

2> resume SRB2 and all DRBs that are suspended, if any, including RBs configured with NR PDCP;

NOTE 4: The handling of the radio bearers after the successful completion of the PDCP re-establishment, e.g. the re-transmission of unacknowledged PDCP SDUs (as well as the associated status reporting), the handling of the SN and the HFN, is specified in TS 36.323 [8].

NOTE 5: The UE may discard SRB2 messages and data that it receives prior to completing the reconfiguration used to resume these bearers.

1> if the received *RRCConnectionReconfiguration* includes the *systemInformationBlockType1Dedicated*:

2> perfom the actions upon reception of the *SystemInformationBlockType1* message as specified in 5.2.2.7*;*

1> if the received *RRCConnectionReconfiguration* includes the *systemInformationBlockType2Dedicated*:

2> perfom the actions upon reception of the *SystemInformationBlockType2* message as specified in 5.2.2.9;

1> if the *RRCConnectionReconfiguration* message includes the *dedicatedInfoNASList*:

2> forward each element of the *dedicatedInfoNASList* to upper layers in the same order as listed;

1> if the *RRCConnectionReconfiguration* message includes the *measConfig*:

2> perform the measurement configuration procedure as specified in 5.5.2;

1> perform the measurement identity autonomous removal as specified in 5.5.2.2a;

1> if the *RRCConnectionReconfiguration* message includes the *otherConfig*:

2> perform the other configuration procedure as specified in 5.3.10.9;

1> if the *RRCConnectionReconfiguration* message includes the *sl-DiscConfig* or *sl-CommConfig*:

2> perform the sidelink dedicated configuration procedure as specified in 5.3.10.15;

1> if the *RRCConnectionReconfiguration* message includes the *sl-V2X-ConfigDedicated*:

2> perform the V2X sidelink communication dedicated configuration procedure as specified in 5.3.10.15a;

NOTE 5a: If the *sl-V2X-ConfigDedicated* was received embedded within an NR *RRCReconfiguration* message, the UE does not build an E-UTRA *RRCConnectionReconfigurationComplete* message for the received *sl-V2X-ConfigDedicated*.

1> if the *RRCConnectionReconfiguration* message includes the *sl-ConfigDedicatedForNR*:

2> perform the related procedures for NR sidelink communication in accordance with TS 38.331 [82], clause 5.3.5.14 and clause 5.5.2;

1> if the *RRCConnectionReconfiguration* message includes *wlan-OffloadInfo*:

2> perform the dedicated WLAN offload configuration procedure as specified in 5.6.12.2;

1> if the *RRCConnectionReconfiguration* message includes *rclwi-Configuration*:

2> perform the WLAN traffic steering command procedure as specified in 5.6.16.2;

1> if the *RRCConnectionReconfiguration* message includes *lwa-Configuration*:

2> perform the LWA configuration procedure as specified in 5.6.14.2;

1> if the *RRCConnectionReconfiguration* message includes *lwip-Configuration*:

2> perform the LWIP reconfiguration procedure as specified in 5.6.17.2;

1> upon RRC connection establishment, if UE does not need UL gaps during continuous uplink transmission:

2> configure lower layers to stop using UL gaps during continuous uplink transmission in FDD for *RRCConnectionReconfigurationComplete* message and subsequent uplink transmission in RRC\_CONNECTED except for UL transmissions as specified in TS36.211 [21];

1> if the *RRCConnectionReconfiguration* message includes the *conditionalReconfiguration*:

2> perform conditional reconfiguration as specified in 5.3.5.9;

NOTE 6: In case of conditional reconfiguration the text "if the received *RRCConnectionReconfiguration. . .*" corresponds to applying the stored *RRCConnectionReconfiguration* message (according to 5.3.5.9.5).

1> set the content of *RRCConnectionReconfigurationComplete* message as follows:

2> if the *RRCConnectionReconfiguration* message includes *perCC-GapIndicationRequest*:

3> include *perCC-GapIndicationList* and *numFreqEffective*;

2> if the frequencies are configured for reduced measurement performance:

3> include *numFreqEffectiveReduced*;

2> if the received *RRCConnectionReconfiguration* message included *nr-SecondaryCellGroupConfig*:

3> include *scg-ConfigResponseNR* in accordance with TS 38.331 [82], clause 5.3.5.3;

3> if the *RRCConnectionReconfiguration* message is applied due to a conditional reconfiguration execution:

4> include in *selectedCondReconfigurationToApply* the *condReconfigurationId* of the conditional reconfiguration which has been executed;

1> if the UE is configured to operate in EN-DC as result of this procedure, forward *upperLayerIndication*, as if the UE receives this field from SIB2, to upper layers, otherwise indicate upper layers absence of this field;

1> if the UE is configured with NE-DC:

2> if the received *RRCConnectionReconfiguration* message was included in an NR *RRCResume* message:

3> transfer the *RRCConnectionReconfigurationComplete* message via SRB1 embedded in NR RRC message *RRCResumeComplete* as specified in TS 38.331 [82], clause 5.3.13.4;

2> else:

3> transfer the *RRCConnectionReconfigurationComplete* message via SRB1 embedded in NR RRC message *RRCReconfigurationComplete* as specified in TS 38.331 [82], clause 5.3.5.3;

1> else:

2> submit the *RRCConnectionReconfigurationComplete* message to lower layers for transmission using the new configuration, upon which the procedure ends;

#### 5.3.5.4 Reception of an *RRCConnectionReconfiguration* including the *mobilityControlInfo* by the UE (handover)

If the *RRCConnectionReconfiguration* message includes the *mobilityControlInfo* and theUE is able to comply with the configuration included in this message, the UE shall:

1> if the *RRCConnectionReconfiguration* includes the *scg-State*:

2> perform SCG deactivation as specified in TS 38.331 [82], clause 5.3.5.13b;

1> else:

2> perform SCG activation as specified in TS 38.331 [82], clause 5.3.5.13a;

1> if *daps-HO* is not configured for any DRB:

2> stop timer T310, if running;

2> if timer T316 is running:

3> stop timer T316;

3> clear the information included in *VarRLF-Report*, if any;

2> resume MCG transmission, if suspended;

1> stop timer T312, if running;

1> start timer T304 with the timer value set to *t304,* as included in the *mobilityControlInfo*;

1> stop timer T370, if running;

1> if the *carrierFreq* is included:

2> consider the target PCell to be one on the frequency indicated by the *carrierFreq* with a physical cell identity indicated by the *targetPhysCellId*;

1> else:

2> consider the target PCell to be one on the frequency of the source PCell with a physical cell identity indicated by the *targetPhysCellId*;

1> if T309 is running:

2> stop timer T309 for all access categories;

2> perform the actions as specified in 5.3.16.4.

1> start synchronising to the DL of the target PCell;

NOTE 1: The UE should perform the handover as soon as possible following the reception of the RRC message triggering the handover, which could be before confirming successful reception (HARQ and ARQ) of this message.

1> if BL UE or UE in CE:

2> if *sameSFN-Indication* is not present in *mobilityControlInfo*:

3> acquire the *MasterInformationBlock* in the target PCell;

1> if *makeBeforeBreak* is configured:

2> perform the remainder of this procedure including and following resetting MAC after the UE has stopped the uplink transmission/downlink reception with the source PCell;

NOTE 1a: It is up to UE implementation when to stop the uplink transmission/ downlink reception with the source PCell to initiate re-tuning for connection to the target cell, as specified in TS 36.133 [16], if *makeBeforeBreak* is configured.

NOTE 1b: It is up to UE implementation when to stop the uplink transmission/ downlink reception with the source SCell(s) after receiving *RRCConnectionReconfiguration* message.

1> if *daps-HO* is configured for any DRB:

2> establish a MAC entity for the target PCell, with the same configuration as the MAC entity for the source PCell;

2> for each DRB configured with *daps-HO*:

3> establish the RLC entity or entities and the associated DTCH logical channel for the target PCell, with the same configurations as for the source PCell;

3> reconfigure the PDCP entity to configure DAPS as specified in TS36.323 [8].

2> for each DRB not configured with *daps-HO*:

3> re-establish PDCP;

3> re-establish the RLC entity and associate it, and the associated DTCH logical channel, to the target PCell;

2> for each SRB:

3> establish a PDCP entity for the target PCell, with the same configuration as the PDCP entity for the source PCell;

3> establish an RLC entity and an associated DCCH logical channel for the target PCell, with the same configuration as for the source PCell;

2> suspend the SRBs for the source PCell;

NOTE 1c: In order to understand if a *daps-HO* is configured, the UE needs to check the presence of the field *daps-HO* within the received *RadioResourceConfigDedicated* IE.

NOTE 1d: In DAPS handover, the UE may re-establish PDCP and RLC entity for a DRB not configured with *daps-HO* when MAC successfully completes the random access procedure. In this case, the UE suspends data transmission and reception for all DRBs not configured with *daps-HO* in the source PCell for the duration of the DAPS handover.

1> else (if *daps-HO* is not configured):

2> reset MCG MAC and SCG MAC, if configured;

2> release *uplinkDataCompression*, if configured;

2> re-establish PDCP for all RBs configured with *pdcp-config* that are established;

NOTE 2: The handling of the radio bearers after the successful completion of the PDCP re-establishment, e.g. the re-transmission of unacknowledged PDCP SDUs (as well as the associated status reporting), the handling of the SN and the HFN, is specified in TS 36.323 [8].

NOTE 2a: At handover the *reestablishPDCP* flag will be set for all RBs configured with NR PDCP in *nr-RadioBearerConfig1* or *nr-RadioBearerConfig2* TS 38.331 [82] which will cause the PDCP entity to be re-established also for these RBs.

2> re-establish MCG RLC and SCG RLC, if configured, for all RBs that are established;

1> for each SCell configured for the UE other than the PSCell:

2> if the received *RRCConnectionReconfiguration* message includes *sCellState* for the SCell and indicates *activated*:

3> configure lower layers to consider the SCell to be in activated state;

2> else if the received *RRCConnectionReconfiguration* message includes *sCellState* for the SCell and indicates *dormant*:

3> configure lower layers to consider the SCell to be in dormant state;

2> else:

3> configure lower layers to consider the SCell to be in deactivated state;

1> apply the value of the *newUE-Identity* as the C-RNTI in the target MCG;

1> if the *RRCConnectionReconfiguration* message includes the *fullConfig*:

2> perform the radio configuration procedure as specified in 5.3.5.8;

1> configure lower layers in accordance with the received *radioResourceConfigCommon*;

1> if the received *RRCConnectionReconfiguration* message includes the *rach-Skip*:

2> configure lower layers to apply the *rach-Skip* for the target MCG, as specified in TS 36.213 [23] and 36.321 [6];

1> configure lower layers in accordance with any additional fields, not covered in the previous, if included in the received mobilityControlInfo;

1> if the received *RRCConnectionReconfiguration* includes the *sCellToReleaseList*:

2> perform SCell release as specified in 5.3.10.3a;

1> if the received *RRCConnectionReconfiguration* includes the *sCellGroupToReleaseList*:

2> perform SCell group release as specified in 5.3.10.3d;

1> if the received *RRCConnectionReconfiguration* includes the *scg-Configuration*; or

1> if the current UE configuration includes one or more split DRBs and the received *RRCConnectionReconfiguration* includes *radioResourceConfigDedicated* including *drb-ToAddModList*:

2> perform SCG reconfiguration as specified in 5.3.10.10;

1> if the *RRCConnectionReconfiguration* message includes the *radioResourceConfigDedicated*:

2> perform the radio resource configuration procedure as specified in 5.3.10.0;

1> if the *securityConfigHO* (without suffix) is included in the *RRCConnectionReconfiguration*:

2> if the *keyChangeIndicator* received in the *securityConfigHO* is set to *TRUE*:

3> update the KeNB key based on the KASME key taken into use with the latest successful NAS SMC procedure, as specified in TS 33.401 [32];

2> else:

3> update the KeNB key based on the current KeNB or the NH, using the *nextHopChainingCount* value indicated in the *securityConfigHO*, as specified in TS 33.401 [32];

NOTE 2b: If the UE needs to update the S-KeNB key as specified in 5.3.10.10, the UE updates the S-KeNB after updating the KeNB key.

2> store the *nextHopChainingCount* value;

2> if the *securityAlgorithmConfig* is included in the *securityConfigHO*:

3> derive the KRRCint key associated with the *integrityProtAlgorithm*, as specified in TS 33.401 [32];

3> if connected as an RN; or

3> if capable of user plane integrity protection:

4> derive the KUPint key associated with the *integrityProtAlgorithm*, as specified in TS 33.401 [32];

3> derive the KRRCenc key and the KUPenc key associated with the *cipheringAlgorithm*, as specified in TS 33.401 [32];

2> else:

3> derive the KRRCint key associated with the current integrity algorithm, as specified in TS 33.401 [32];

3> if connected as an RN; or

3> if capable of user plane integrity protection:

4> derive the KUPint key associated with the current integrity algorithm, as specified in TS 33.401 [32];

3> derive the KRRCenc key and the KUPenc key associated with the current ciphering algorithm, as specified in TS 33.401 [32];

2> configure lower layers to apply the integrity protection algorithm and the KRRCint key, i.e. the integrity protection configuration shall be applied to all subsequent messages received and sent by the UE, including the message used to indicate the successful completion of the procedure;

2> configure lower layers to apply the ciphering algorithm, the KRRCenc key and the KUPenc key, i.e. the ciphering configuration shall be applied to all subsequent messages received and sent by the UE, including the message used to indicate the successful completion of the procedure;

NOTE 2c: For a DRB configured for DAPS HO, the new ciphering algorithm and the KUPenc key is applied for traffic exchange between the UE and the target MCG while the old ciphering algorithm and KUPenc key is applied for traffic exchange between the UE and the source MCG.

1> else if the *securityConfigHO-v1530* is included in the *RRCConnectionReconfiguration*:

2> if the *nas-Container* is received:

3> forward the *nas-Container* to upper layers;

2> if the *keyChangeIndicator-r15* is received and is set to *TRUE*:

3> update the KeNB key based on the KAMF key, as specified in TS 33.501 [86];

2> else:

3> update the KeNB key based on the current KeNB or the NH, using the received *nextHopChainingCount-r15*, as specified in TS 33.501 [86];

2> store the *nextHopChainingCount-r15* value;

2> if the security*AlgorithmConfig-r15* is received:

3> derive the KRRCint key associated with the *integrityProtAlgorithm*, as specified in TS 33.401 [32];

3> derive the KRRCenc key and the KUPenc key associated with the *cipheringAlgorithm*, as specified in TS 33.401 [32];

2> else:

3> derive the KRRCint key associated with the current integrity algorithm, as specified in TS 33.401 [32];

3> derive the KRRCenc key and the KUPenc key associated with the current ciphering algorithm, as specified in TS 33.401 [32];

1> if the received *RRCConnectionReconfiguration* includes the *nr-Config* and it is set to *release*; or

1> if the received *RRCConnectionReconfiguration* includes *endc-ReleaseAndAdd* and it is set to *TRUE*:

2> perform MR-DC release as specified in TS 38.331 [82], clause 5.3.5.10;

1> if the received *RRCConnectionReconfiguration* includes the *sk-Counter*:

2> perform key update procedure as specified in in TS 38.331 [82], clause 5.3.5.7;

1> if the received *RRCConnectionReconfiguration* includes the *nr-SecondaryCellGroupConfig*:

2> perform NR RRC Reconfiguration as specified in TS 38.331 [82], clause 5.3.5.3.

1> if the received *RRCConnectionReconfiguration* includes the *nr-RadioBearerConfig1*:

2> perform radio bearer configuration as specified in TS 38.331 [82], clause 5.3.5.6;

1> if the received *RRCConnectionReconfiguration* includes the *nr-RadioBearerConfig2*:

2> perform radio bearer configuration as specified in TS 38.331 [82], clause 5.3.5.6.

1> if connected as an RN:

2> configure lower layers to apply the integrity protection algorithm and the KUPint key, for current or subsequently established DRBs that are configured to apply integrity protection, if any;

1> if the received *RRCConnectionReconfiguration* includes the *sCellToAddModList*:

2> perform SCell addition or modification as specified in 5.3.10.3b;

1> if the received *RRCConnectionReconfiguration* includes the *sCellGroupToAddModList*:

2> perform SCell group addition or modification as specified in 5.3.10.3e;

1> if the received *RRCConnectionReconfiguration* includes the *systemInformationBlockType1Dedicated*:

2> perfom the actions upon reception of the *SystemInformationBlockType1* message as specified in 5.2.2.7;

1> perform the measurement related actions as specified in 5.5.6.1;

1> if the *RRCConnectionReconfiguration* message includes the *measConfig*:

2> perform the measurement configuration procedure as specified in 5.5.2;

1> perform the measurement identity autonomous removal as specified in 5.5.2.2a;

1> release *reportProximityConfig* and clear any associated proximity status reporting timer;

1> if the *RRCConnectionReconfiguration* message includes the *otherConfig*:

2> perform the other configuration procedure as specified in 5.3.10.9;

1> if the *RRCConnectionReconfiguration* message includes the *sl-DiscConfig* or *sl-CommConfig*:

2> perform the sidelink dedicated configuration procedure as specified in 5.3.10.15;

1> if the *RRCConnectionReconfiguration* message includes *wlan-OffloadInfo*:

2> perform the dedicated WLAN offload configuration procedure as specified in 5.6.12.2;

1> if *handoverWithoutWT-Change* is not configured:

2> release the LWA configuration, if configured, as described in 5.6.14.3;

1> release the LWIP configuration, if configured, as described in 5.6.17.3;

1> if the *RRCConnectionReconfiguration* message includes *rclwi-Configuration*:

2> perform the WLAN traffic steering command procedure as specified in 5.6.16.2;

1> if the *RRCConnectionReconfiguration* message includes *lwa-Configuration*:

2> perform the LWA configuration procedure as specified in 5.6.14.2;

1> if the *RRCConnectionReconfiguration* message includes *lwip-Configuration*:

2> perform the LWIP reconfiguration procedure as specified in 5.6.17.2;

1> if the *RRCConnectionReconfiguration* message includes the *sl-V2X-ConfigDedicated* or *mobilityControlInfoV2X*:

2> perform the V2X sidelink communication dedicated configuration procedure as specified in 5.3.10.15a;

NOTE 2d: In case of conditional reconfiguration the text "if the received *RRCConnectionReconfiguration. . .*" corresponds to applying the stored *RRCConnectionReconfiguration* message (according to 5.3.5.9.5).

1> if the UE is configured to operate in EN-DC as result of this procedure, forward *upperLayerIndication*, as if the UE receives this field from SIB2, to upper layers, otherwise indicate upper layers absence of this field;

1> set the content of *RRCConnectionReconfigurationComplete* message as follows:

2> if the UE has radio link failure or handover failure information available in *VarRLF-Report* and if the RPLMN is included in *plmn-IdentityList* stored in *VarRLF-Report*:

3> include *rlf-InfoAvailable*;

2> if the UE has MBSFN logged measurements available for E-UTRA and if the RPLMN is included in *plmn-IdentityList* stored in *VarLogMeasReport* and if T330 is not running:

3> include *logMeasAvailableMBSFN*;

2> else if the UE has logged measurements available for E-UTRA and if the RPLMN is included in *plmn-IdentityList* stored in *VarLogMeasReport*:

3> include the *logMeasAvailable*;

3> if Bluetooth measurement results are included in the logged measurements the UE has available:

4> include *logMeasAvailableBT*;

3> if WLAN measurement results are included in the logged measurements the UE has available:

4> include *logMeasAvailableWLAN*;

2> if the UE has connection establishment failure information available in *VarConnEstFailReport* and if the RPLMN is equal to *plmn-Identity* stored in *VarConnEstFailReport*:

3> include *connEstFailInfoAvailable*;

2> if the *RRCConnectionReconfiguration* message includes *perCC-GapIndicationRequest*:

3> include *perCC-GapIndicationList* and *numFreqEffective*;

2> if the frequencies are configured for reduced measurement performance:

3> include *numFreqEffectiveReduced*;

2> if the UE has flight path information available:

3> include *flightPathInfoAvailable*;

2> if the received *RRCConnectionReconfiguration* message included *nr-SecondaryCellGroupConfig*:

3> include *scg-ConfigResponseNR* in accordance with TS 38.331 [82], clause 5.3.5.3;

1> submit the *RRCConnectionReconfigurationComplete* message to lower layers for transmission;

1> if MAC successfully completes the random access procedure; or

1> if MAC indicates the successful reception of a PDCCH transmission addressed to C-RNTI and if *rach-Skip* is configured:

2> stop timer T304;

2> if *daps-HO* is configured for any DRB:

3> stop timer T310 for the source PCell, if running;

3> for each DAPS bearer trigger UL data switching, as specified in TS 36.323 [8];

2> release *rach-Skip*;

2> apply the parts of the CQI reporting configuration, the scheduling request configuration and the sounding RS configuration that do not require the UE to know the SFN of the target PCell, if any;

2> apply the parts of the measurement and the radio resource configuration that require the UE to know the SFN of the target PCell (e.g. measurement gaps, periodic CQI reporting, scheduling request configuration, sounding RS configuration), if any, upon acquiring the SFN of the target PCell;

NOTE 3: Whenever the UE shall setup or reconfigure a configuration in accordance with a field that is received it applies the new configuration, except for the cases addressed by the above statements.

2> if the UE is configured to provide IDC indications:

3> if the UE has initiated the transmission of an *InDeviceCoexIndication* message during the last 1 second preceding reception of the *RRCConnectionReconfiguration* message including *mobilityControlInfo*; or

3> if the *RRCConnectionReconfiguration* message is applied due to a conditional reconfiguration execution and the UE has initiated transmission of an *InDeviceCoexIndication* message since it was configured to do so in accordance with 5.6.9.2:

4> initiate transmission of the *InDeviceCoexIndication* message in accordance with 5.6.9.3;

2> if the UE is configured to provide power preference indications, overheating assistance information, SPS assistance information, delay budget report or maximum bandwidth preference indications:

3> if the UE has initiated the transmission of a *UEAssistanceInformation* message during the last 1 second preceding reception of the *RRCConnectionReconfiguration* message including *mobilityControlInfo*; or

3> if the *RRCConnectionReconfiguration* message is applied due to a conditional reconfiguration execution, and the UE has initiated transmission of a *UEAssistanceInformation* message for the corresponding cell group since it was configured to do so in accordance with 5.6.10.2:

4> initiate transmission of the *UEAssistanceInformation* message in accordance with 5.6.10.3;

2> if *SystemInformationBlockType15* is broadcast by the PCell:

3> if the UE has initiated the transmission of a *MBMSInterestIndication* message during the last 1 second preceding reception of the *RRCConnectionReconfiguration* message including *mobilityControlInfo*; or

3> if the *RRCConnectionReconfiguration* message is applied due to a conditional reconfiguration execution and the UE supports MBMS reception and the UE has initiated transmission of an *MBMSInterestIndication* message since it was configured to do so in accordance with 5.8.5.2:

4> ensure having a valid version of *SystemInformationBlockType15* for the PCell;

4> determine the set of MBMS frequencies of interest in accordance with 5.8.5.3;

4> determine the set of MBMS services of interest in accordance with 5.8.5.3a;

4> initiate transmission of the *MBMSInterestIndication* message in accordance with 5.8.5.4;

2> if *SystemInformationBlockType18* is broadcast by the target PCell; and the UE initiated the transmission of a *SidelinkUEInformation* message indicating a change of sidelink communication related parameters relevant in target PCell (i.e. change of *commRxInterestedFreq* or *commTxResourceReq*, *commTxResourceReqUC* if *SystemInformationBlockType18* includes *commTxResourceUC-ReqAllowed* or *commTxResourceInfoReqRelay* if PCell broadcasts *SystemInformationBlockType19* including *discConfigRelay*) during the last 1 second preceding reception of the *RRCConnectionReconfiguration* message including *mobilityControlInfo*; or

2> if *SystemInformationBlockType19* is broadcast by the target PCell; and the UE initiated the transmission of a *SidelinkUEInformation* message indicating a change of sidelink discovery related parameters relevant in target PCell (i.e. change of *discRxInterest* or *discTxResourceReq*, *discTxResourceReqPS* if *SystemInformationBlockType19* includes *discConfigPS* or *discRxGapReq* or *discTxGapReq* if the UE is configured with *gapRequestsAllowedDedicated* set to *true* or if the UE is not configured with *gapRequestsAllowedDedicated* and *SystemInformationBlockType19* includes *gapRequestsAllowedCommon*) during the last 1 second preceding reception of the *RRCConnectionReconfiguration* message including *mobilityControlInfo*; or

2> if *SystemInformationBlockType21* is broadcast by the target PCell; and the UE initiated the transmission of a *SidelinkUEInformation* message indicating a change of V2X sidelink communication related parameters relevant in target PCell (i.e. change of *v2x-CommRxInterestedFreqList* or *v2x-CommTxResourceReq*) during the last 1 second preceding reception of the *RRCConnectionReconfiguration* message including *mobilityControlInfo*; or

2> if the *RRCConnectionReconfiguration* message is applied due to a conditional reconfiguration execution, and at least one of *SystemInformationBlockType18*, *SystemInformationBlockType19*, and *SystemInformationBlockType21* is broadcast by the target PCell, and the UE has initiated transmission of a *SidelinkUEInformation* message since it was configured to do so in accordance with 5.10.2.2:

3> initiate transmission of the *SidelinkUEInformation* message in accordance with 5.10.2.3;

2> remove all the entries within *VarConditionalReconfiguration*, if any;

2> for each *measId* of the source SpCell configuration, if the associated *reportConfig* is *condReconfigurationTriggerEUTRA*:

3> remove the entry with the matching *measId* from the *measIdList* within the *VarMeasConfig*;

3> remove the entry with the matching *reportConfigId* from the *reportConfigList* within the *VarMeasConfig*;

3> if the *measObjectId* is only included in a *MeasIdToAddMod*:

4> remove the entry with the matching *measObjectId* from the *measObjectList* within the *VarMeasConfig*;

2> the procedure ends;

NOTE 4: The UE is not required to determine the SFN of the target PCell by acquiring system information from that cell before performing RACH access in the target PCell,

#### 5.5.2.13 NR measurement timing configuration

The UE shall setup the first SS/PBCH block measurement timing configuration (SMTC) in accordance with the received *periodicityAndOffset* (providing *Periodicity* and *Offset* value for the following condition) in the *MTC-SSB-NR* configuration i.e., the first subframe of each SMTC occasion occurs at an SFN and subframe of the PCell meeting the following condition:

SFN mod *T* = FLOOR(*Offset*/10);

if the *Periodicity* is larger than *sf5*:

subframe = *Offset* mod 10;

else:

subframe = *Offset* or (*Offset* +5);

with *T* = CEIL(*Periodicity*/10).

On the concerned frequency, the UE shall not consider SS/PBCH block transmission in subframes outside the SMTC occasion which lasts for *ssb-Duration* for measurements including RRM measurements except for SFTD measurement (see TS 36.133 [16], clause 8.1.2.4.25.2 and 8.1.2.4.26.1).

If *smtc2-LP* is present, for cells indicated in the *pci-List* parameter in *smtc2-LP* for inter-RAT cell reselection, the UE shall setup an additional SS/PBCH block measurement timing configuration (SMTC) in accordance with the received *periodicity* parameter in the *smtc2-LP* configuration and use the *Offset* (derived from parameter *periodicityAndOffset*) and *ssb-Duration* parameter from the *measTimingConfig* configuration for that frequency. The first subframe of each SMTC occasion occurs at an SFN and subframe of the NR SpCell or serving cell (for cell reselection) meeting the above condition.

#### 5.6.2.3 Actions related to transmission of *ULInformationTransfer* message

The UE shall set the contents of the *ULInformationTransfer* message as follows:

1> if there is a need to transfer NAS information:

2> if the UE is a NB-IoT UE:

3> set the *dedicatedInfoNAS* to include the information received from upper layers;

2> else:

3> set the *dedicatedInfoType* to include the *dedicatedInfoNAS*;

1> if there is a need to transfer CDMA2000 1XRTT information:

2> set the *dedicatedInfoType* to include the *dedicatedInfoCDMA2000-1XRTT*;

1> if there is a need to transfer CDMA2000 HRPD information:

2> set the *dedicatedInfoType* to include the *dedicatedInfoCDMA2000-HRPD*;

1> upon RRC connection establishment, if UE supports the Control Plane CIoT EPS/5GS optimisation and UE does not need UL gaps during continuous uplink transmission:

2> configure lower layers to stop using UL gaps during continuous uplink transmission in FDD for *ULInformationTransfer* message and subsequent uplink transmission in RRC\_CONNECTED except for UL transmissions as specified in TS 36.211 [21];

1> if there is a need to transfer F1-C related information (applies only to IAB-MT):

2> include the *dedicatedInfoF1c*;

1> submit the *ULInformationTransfer* message to lower layers for transmission, upon which the procedure ends;

#### 5.6.3.3 Reception of the *UECapabilityEnquiry* by the UE

The UE shall:

1> for NB-IoT, set the contents of *UECapabilityInformation* message as follows:

2> include the UE Radio Access Capability Parameters within the *ue-Capability*;

2> include *ue-RadioPagingInfo*;

2> submit the *UECapabilityInformation* message to lower layers for transmission, upon which the procedure ends;

1> else, set the contents of *UECapabilityInformation* message as follows:

2> if the *ue-CapabilityRequest* includes *eutra*:

3> include the *UE-EUTRA-Capability* within a *ue-CapabilityRAT-Container* and with the *rat-Type* set to *eutra*;

3> if the UE supports FDD and TDD:

4> set all fields of *UECapabilityInformation*, except field *fdd-Add-UE-EUTRA-Capabilities* and *tdd-Add-UE-EUTRA-Capabilities* (including their sub-fields), to include the values applicable for both FDD and TDD (i.e. functionality supported by both modes);

4> if (some of) the UE capability fields have a different value for FDD and TDD:

5> if for FDD, the UE supports additional functionality compared to what is indicated by the previous fields of *UECapabilityInformation*:

6> include field *fdd-Add-UE-EUTRA-Capabilities* and set it to include fields reflecting the additional functionality applicable for FDD;

5> if for TDD, the UE supports additional functionality compared to what is indicated by the previous fields of *UECapabilityInformation*:

6> include field *tdd-Add-UE-EUTRA-Capabilities* and set it to include fields reflecting the additional functionality applicable for TDD;

NOTE 1: The UE includes fields of *XDD-Add-UE-EUTRA-Capabilities* in accordance with the following:

- The field is included only if one or more of its sub-fields (or bits in the feature group indicators string) has a value that is different compared to the value signalled elsewhere within *UE-EUTRA-Capability*;

(this value signalled elsewhere is also referred to as the *Common value*, that is supported for both XDD modes)

- For the fields that are included in *XDD-Add-UE-EUTRA-Capabilities*, the UE sets:

- the sub-fields (or bits in the feature group indicators string) that are not allowed to be different to the same value as the *Common value*;

- the sub-fields (or bits in the feature group indicators string) that are allowed to be different to a value indicating at least the same functionality as indicated by the *Common value*;

3> else (UE supports single xDD mode):

4> set all fields of *UECapabilityInformation*, except field *fdd-Add-UE-EUTRA-Capabilities* and *tdd-Add-UE-EUTRA-Capabilities* (including their sub-fields), to include the values applicable for the xDD mode supported by the UE;

3> compile a list of band combinations, candidate for inclusion in the *UECapabilityInformation* message, comprising of band combinations supported by the UE according to the following priority order (i.e. listed in order of decreasing priority):

4> include all non-CA bands, regardless of whether UE supports carrier aggregation, only:

- if the UE includes *ue-Category-v1020* (i.e. indicating category 6 to 8); or

- if for at least one of the non-CA bands, the UE supports more MIMO layers with TM9 and TM10 than implied by the UE category; or

- if the UE supports TM10 with one or more CSI processes; or

- if the UE supports 1024QAM in DL;

4> if the *UECapabilityEnquiry* message includes *requestedFrequencyBands* and UE supports *requestedFrequencyBands*:

5> include all 2DL+1UL CA band combinations, only consisting of bands included in *requestedFrequencyBands*;

5> include all other CA band combinations, only consisting of bands included in *requestedFrequencyBands*, and prioritized in the order of *requestedFrequencyBands*, (i.e. first include remaining band combinations containing the first-listed band, then include remaining band combinations containing the second-listed band, and so on);

4> else (no requested frequency bands):

5> include all 2DL+1UL CA band combinations;

5> include all other CA band combinations;

4> if UE supports *maximumCCsRetrieval* and if the *UECapabilityEnquiry* message includes the *requestedMaxCCsDL* and the *requestedMaxCCsUL* (i.e. both UL and DL maximums are given):

5> remove from the list of candidates the band combinations for which the number of CCs in DL exceeds the value indicated in the *requestedMaxCCsDL* or for which the number of CCs in UL exceeds the value indicated in the *requestedMaxCCsUL*;

5> indicate in *requestedCCsUL* the same value as received in *requestedMaxCCsUL*;

5> indicate in *requestedCCsDL* the same value as received in *requestedMaxCCsDL*;

4> else if UE supports *maximumCCsRetrieval* and if the *UECapabilityEnquiry* message includes the *requestedMaxCCsDL* (i.e. only DL maximum limit is given):

5> remove from the list of candidates the band combinations for which the number of CCs in DL exceeds the value indicated in the *requestedMaxCCsDL*;

5> indicate value in *requestedCCsDL* the same value as received in *requestedMaxCCsDL*;

4> else if UE supports *maximumCCsRetrieval* and if the *UECapabilityEnquiry* message includes the *requestedMaxCCsUL* (i.e. only UL maximum limit is given):

5> remove from the list of candidates the band combinations for which the number of CCs in UL exceeds the value indicated in the *requestedMaxCCsUL*;

5> indicate in *requestedCCsUL* the same value as received in *requestedMaxCCsUL;*

4> if the UE supports *reducedIntNonContComb* and the *UECapabilityEnquiry* message includes *requestReducedIntNonContComb*:

5> set *reducedIntNonContCombRequested* to true;

5> remove from the list of candidates the intra-band non-contiguous CA band combinations which support is implied by another intra-band non-contiguous CA band combination included in the list of candidates as specified in TS 36.306 [5], clause 4.3.5.21:

4> if the UE supports *requestReducedFormat* and UE supports *skipFallbackCombinations* and *UECapabilityEnquiry* message includes *requestSkipFallbackComb*:

5> set *skipFallbackCombRequested* to true;

5> for each band combination included in the list of candidates (including 2DL+1UL CA band combinations), starting with the ones with the lowest number of DL and UL carriers, that concerns a fallback band combination of another band combination included in the list of candidates as specified in TS 36.306 [5]:

6> remove the band combination from the list of candidates;

6> include *differentFallbackSupported* in the band combination included in the list of candidates whose fallback concerns the removed band combination, if its capabilities differ from the removed band combination;

4> if the UE supports *requestReducedFormat* and *diffFallbackCombReport*, and *UECapabilityEnquiry* message includes *requestDiffFallbackCombList*:

5> if the UE does not support *skipFallbackCombinations* or *UECapabilityEnquiry* message does not include *requestSkipFallbackComb*:

6> remove all band combination from the list of candidates;

5> for each CA band combination indicated in *requestDiffFallbackCombList*:

6> include the CA band combination, if not already in the list of candidates;

6> include the fallback combinations for which the supported UE capabilities are different from the capability of the CA band combination;

5> include CA band combinations indicated in *requestDiffFallbackCombList* into *requestedDiffFallbackCombList*;

3> if the *UECapabilityEnquiry* message includes *requestReducedFormat* and UE supports *requestReducedFormat*:

4> include in *supportedBandCombinationReduced* as many as possible of the band combinations included in the list of candidates, including the non-CA combinations, determined according to the rules and priority order defined above;

3> else:

4> if the *UECapabilityEnquiry* message includes *requestedFrequencyBands* and UE supports *requestedFrequencyBands*:

5> include in *supportedBandCombination* as many as possible of the band combinations included in the list of candidates, including the non-CA combinations and up to 5DL+5UL CA band combinations, determined according to the rules and priority order defined above;

5> include in *supportedBandCombinationAdd* as many as possible of the remaining band combinations included in the list of candidates, (i.e. the candidates not included in *supportedBandCombination)*, up to 5DL+5UL CA band combinations, determined according to the rules and priority order defined above;

4> else:

5> include in *supportedBandCombination* as many as possible of the band combinations included in the list of candidates, including the non-CA combinations and up to 5DL+5UL CA band combinations, determined according to the rules defined above;

5> if it is not possible to include in *supportedBandCombination* all the band combinations to be included according to the above, selection of the subset of band combinations to be included is left up to UE implementation;

3> indicate in *requestedBands* the same bands and in the same order as included in *requestedFrequencyBands*, if received;

3> if the UE is a category 0, M1 or M2 UE, or supports any UE capability information in *ue-RadioPagingInfo,* according to TS 36.306 [5]:

4> include *ue-RadioPagingInfo* and set the fields according to TS 36.306 [5];

3> if the UE supports (NG)EN-DC or NE-DC and if *requestedFreqBandsNR-MRDC* is included in the request:

4> include into *featureSetsEUTRA* the feature sets that are applicable for the received *requestedFreqBandsNR-MRDC* and *requestedCapabilityCommon* as specified in TS 38.331 [82], clause 5.6.1.4.

NOTE 2: The network must include the *requestedFreqBandsNR-MRDC* in order to obtain feature sets for E-UTRA and MR-DC.

NOTE 3: Even if the network requests (only) capabilities for *eutra*, it may include NR band numbers in the *requestedFreqBandsNR-MRDC* in order to ensure that the UE includes all necessary feature sets (i.e. E-UTRA and NR) needed for subsequently requested *eutra-nr* capabilities.

3> if the *UECapabilityEnquiry* message includes *requestSTTI-SPT-Capability* and if the UE supports short TTI and/or SPT (i.e., *sTTI-SPT-Supported*):

4> for each band combination the UE included in a field of the *UECapabilityInformation* message in accordance with the previous:

5> if the UE supports short TTI, include the short TTI capabilities for each of the band combinations using the *stti-SPT-BandParameters*;

5> if the UE supports SPT, include the SPT capabilities for each of the band combinations using the *stti-SPT-BandParameters*;

NOTE 4: The UE may have to add/repeat the band combinations to the list of band combinations included earlier, to include short TTI capabilities and/or SPT capabilities.

2> if the *ue-CapabilityRequest* includes *geran-cs* and if the UE supports GERAN CS domain:

3> include the UE radio access capabilities for GERAN CS within a *ue-CapabilityRAT-Container* and with the *rat-Type* set to *geran-cs*;

2> if the *ue-CapabilityRequest* includes *geran-ps* and if the UE supports GERAN PS domain:

3> include the UE radio access capabilities for GERAN PS within a *ue-CapabilityRAT-Container* and with the *rat-Type* set to *geran-ps*;

2> if the *ue-CapabilityRequest* includes *utra* and if the UE supports UTRA:

3> include the UE radio access capabilities for UTRA within a *ue-CapabilityRAT-Container* and with the *rat-Type* set to *utra*;

2> if the *ue-CapabilityRequest* includes *cdma2000-1XRTT* and if the UE supports CDMA2000 1xRTT:

3> include the UE radio access capabilities for CDMA2000 within a *ue-Capability**RAT-Container* and with the *rat-Type* set to *cdma2000-1XRTT*;

2> if the *ue-CapabilityRequest* includes *nr* and if the UE supports NR:

3> include the UE radio access capabilities for NR within a *ue-CapabilityRAT-Container*, with the *rat-Type* set to *nr*;

3> include band combinations and feature sets as specified in TS 38.331 [82], clause 5.6.1.4, considering the included *requestedFreqBandsNR-MRDC*, *requestedCapabilityNR*, the *eutra-nr-only* flag and *requestedCapabilityCommon* (if present);

2> if the *ue-CapabilityRequest* includes *eutra-nr* and if the UE supports (NG)EN-DC or NE-DC:

3> include the UE radio access capabilities for EUTRA-NR within a *ue-CapabilityRAT-Container*, with the *rat-Type* set to *eutra-nr*;

3> include band combinations as specified in TS 38.331 [82], clause 5.6.1.4, considering the included *requestedFreqBandsNR-MRDC*, *requestedCapabilityNR* (if present) and *requestedCapabilityCommon* (if included)*;*

1> if the RRC message segmentation is enabled based on the field *rrc-SegAllowed* received, and the encoded RRC message is larger than the maximum supported size of a PDCP SDU specified in TS 36.323 [8]:

2> initiate the UL message segment transfer procedure as specified in clause 5.6.22;

1> else:

2> submit the *UECapabilityInformation* message to lower layers for transmission, upon which the procedure ends;

#### 5.6.8.2 Initiation

While T330 is running, the UE shall:

1> if measurement logging is suspended:

2> if during the last logging interval the IDC problems detected by the UE is resolved, resume measurement logging;

1> if not suspended, perform the logging in accordance with the following:

2> if *targetMBSFN-AreaList* is included in *VarLogMeasConfig*:

3> if the UE is camping normally on an E-UTRA cell or is connected to E-UTRA; and

3> if the RPLMN is included in *plmn-IdentityList* stored in *VarLogMeasReport*;and

3> if the PCell (in RRC\_CONNECTED) or cell where the UE is camping (in RRC\_IDLE) is part of the area indicated by *areaConfiguration* if configured in *VarLogMeasConfig*:

4> for MBSFN areas, indicated in *targetMBSFN-AreaList,* from which the UE is receiving MBMS service:

5> perform MBSFN measurements in accordance with the performance requirements as specified in TS 36.133 [16];

NOTE 1: When configured to perform MBSFN measurement logging by *targetMBSFN-AreaList*, the UE is not required to receive additional MBSFN subframes, i.e. logging is based on the subframes corresponding to the MBMS services the UE is receiving.

5> perform logging at regular time intervals as defined by the *loggingInterval* in *VarLogMeasConfig,* but only for those intervals for which MBSFN measurement results are available as specified in TS 36.133 [16];

2> else:

3> if the *loggedEventTriggerConfig* is configured in *VarLogMeasConfig*, and *eventType* is set to *outOfCoverage*:

4> perform the logging at regular time intervals as defined by the *loggingInterval* in *VarLogMeasConfig* only when the UE is in *any cell selection* state;

4> upon transition from *any cell selection* state to *camped normally* state in E-UTRA:

5> if the RPLMN is included in *plmn-IdentityList* stored in *VarLogMeasReport*; and

5> if *areaConfiguration* is not included in *VarLogMeasConfig* or if the current camping cell is part of the area indicated by *areaConfiguration* in *VarLogMeasConfig*:

6> perform the logging;

3> else if the *loggedEventTriggerConfig* is configured in *VarLogMeasConfig* and *eventType* is set to *eventL1*:

4> if the UE is in *camped normally* state on an E-UTRA cell and if the RPLMN is included in *plmn-IdentityList* stored in *VarLogMeasReport*:

5> if *areaConfiguration* is not included in *VarLogMeasConfig*; or

5> if the serving cell is part of the area indicated by *areaConfiguration* in *VarLogMeasConfig*:

6> perform the logging at regular time intervals as defined by the *loggingInterval* in *VarLogMeasConfig* only when the conditions indicated by the *eventL1* are met;

3> else if the UE is in *any cell selection* state (as specified in TS 36.304 [4]):

4> perform the logging at regular time intervals, as defined by the *loggingInterval* in *VarLogMeasConfig*;

3> else if the UE is camping normally on an E-UTRA cell and if the RPLMN is included in *plmn-IdentityList* stored in *VarLogMeasReport* and, if the cell is part of the area indicated by *areaConfiguration* if configured in *VarLogMeasConfig*:

4> perform the logging at regular time intervals, as defined by the *loggingInterval* in *VarLogMeasConfig*;

2> when adding a logged measurement entry in *VarLogMeasReport*, include the fields in accordance with the following:

3> if the UE detected IDC problems during the last logging interval:

4> if *measResultServCell* in *VarLogMeasReport* is not empty:

5> include *inDeviceCoexDetected*;

5> suspend measurement logging from the next logging interval;

4> else:

5> suspend measurement logging;

NOTE 1A: The UE may detect the start of IDC problems as early as Phase 1 as described in clause 23.4 of TS 36.300 [9].

3> set the *relativeTimeStamp* to indicate the elapsed time since the moment at which the logged measurement configuration was received;

3> if detailed location information became available during the last logging interval, set the content of the *locationInfo* as follows:

4> include the *locationCoordinates*;

3> if *wlan-NameList* is included in *VarLogMeasConfig*:

4> if detailed WLAN measurements are available:

5> include *logMeasResultListWLAN*, in order of decreasing RSSI for WLAN APs;

3> if *bt-NameList* is included in *VarLogMeasConfig*:

4> if detailed Bluetooth measurements are available:

5> include *logMeasResultListBT*, in order of decreasing RSSI for Bluetooth beacons;

3> if *measUncomBarPre* is included in *VarLogMeasConfig*:

4> if available, include the *uncomBarPreMeasResult*;

3> if *targetMBSFN-AreaList* is included in *VarLogMeasConfig*:

4> for each MBSFN area, for which the mandatory measurements result fields became available during the last logging interval:

5> set the *rsrpResultMBSFN*, *rsrqResultMBSFN* to include measurement results that became available during the last logging interval;

5> include the fields *signallingBLER-Result* or *dataBLER-MCH-ResultList* if the concerned BLER results are availble,

5> set the *mbsfn-AreaId* and *carrierFreq* to indicate the MBSFN area in which the UE is receiving MBSFN transmission;

4> if in RRC\_CONNECTED:

5> set the *servCellIdentity* to indicate global cell identity of the PCell;

5> set the *measResultServCell* to include the layer 3 filtered measured results of the PCell;

5> if available, set the *measResultNeighCells* to include the layer 3 filtered measured results of SCell(s) and neighbouring cell(s) measurements that became available during the last logging interval, in order of decreasing RSRP, for at most the following number of cells: 6 intra-frequency and 3 inter-frequency cells per frequency and according to the following:

6> for each cell included, include the optional fields that are available;

5> if available, optionally set the *measResultNeighCells* to include the layer 3 filtered measured results of neighbouring cell(s) measurements that became available during the last logging interval, in order of decreasing RSCP(UTRA)/RSSI(GERAN)/PilotStrength(cdma2000), for at most the following number of cells: 3 inter-RAT cells per frequency/set of frequencies (GERAN), and according to the following:

6> for each cell included, include the optional fields that are available;

4> if in RRC\_IDLE:

5> set the *servCellIdentity* to indicate global cell identity of the serving cell;

5> set the *measResultServCell* to include the quantities of the serving cell;

5> if available, set the *measResultNeighCells*, in order of decreasing ranking-criterion as used for cell re-selection, to include neighbouring cell measurements that became available during the last logging interval for at most the following number of neighbouring cells: 6 intra-frequency and 3 inter-frequency neighbours per frequency and according to the following:

6> for each neighbour cell included, include the optional fields that are available;

5> if available, optionally set the *measResultNeighCells,* in order of decreasing ranking-criterion as used for cell re-selection, to include neighbouring cell measurements that became available during the last logging interval, for at most the following number of cells: 3 inter-RAT cells per frequency/set of frequencies (GERAN), and according to the following:

6> for each cell included, include the optional fields that are available;

4> for the cells included according to the previous (i.e. covering previous and current serving cells as well as neighbouring EUTRA cells) include results according to the extended RSRQ if corresponding results are available according to the associated performance requirements defined in TS 36.133 [16];

4> for the cells included according to the previous (i.e. covering previous and current serving cells as well as neighbouring EUTRA cells) include RSRQ type if the result was based on measurements using a wider band or using all OFDM symbols;

NOTE 2: The UE includes the latest results in accordance with the performance requirements as specified in TS 36.133 [16]. E.g. RSRP and RSRQ results are available only if the UE has a sufficient number of results/ receives a sufficient number of subframes during the logging interval.

3> else:

4> if the UE is in *any cell selection* state (as specified in TS 36.304 [4]):

5> set *anyCellSelectionDetected* to indicate the detection of no suitable or no acceptable cell found;

5> if the *loggedEventTriggerConfig* is not configured in the *VarLogMeasConfig*;

6> set the *servCellIdentity* to indicate global cell identity of the last logged cell that the UE was camping on;

6> set the *measResultServCell* to include the quantities of the last logged cell the UE was camping on;

5> else if the RPLMN at the time of entering the *any cell selection* state is included in *plmn-IdentityList* stored in *VarLogMeasReport*; and

5> if *areaConfiguration* is not included in *VarLogMeasConfig* or if the last suitable cell that the UE was camping on is part of the area indicated by *areaConfiguration* in *VarLogMeasConfig*:

6> set the *servCellIdentity* to indicate global cell identity of the last suitable cell that the UE was camping on;

6> set the *measResultServingCell* to include the quantities of the last suitable cell the UE was camping on;

5> else:

6> set the fields within the *servCellIdentity* and *measResultServingCell* to all zeros to indicate unavailability of the *servCellIdentity* and *measResultServCell*.

4> else:

5> set the *servCellIdentity* to indicate global cell identity of the cell the UE is camping on;

5> set the *measResultServCell* to include the quantities of the cell the UE is camping on;

4> if available, set the *measResultNeighCells*, in order of decreasing ranking-criterion as used for cell re-selection, to include neighbouring cell measurements that became available during the last logging interval for at most the following number of neighbouring cells: 6 intra-frequency and 3 inter-frequency neighbours per frequency as well as 3 inter-RAT neighbours, per frequency/ set of frequencies (GERAN) per RAT and according to the following:

5> for each neighbour cell included, include the optional fields that are available;

4> for the cells included according to the previous (i.e. covering previous and current serving cells as well as neighbouring EUTRA cells) include results according to the extended RSRQ if corresponding results are available according to the associated performance requirements defined in TS 36.133 [16];

4> for the cells included according to the previous (i.e. covering previous and current serving cells as well as neighbouring EUTRA cells) include RSRQ type if the result was based on measurements using a wider band or using all OFDM symbols;

NOTE 3: The UE includes the latest results of the available measurements as used for cell reselection evaluation in RRC\_IDLE or as used for evaluation of reporting criteria or for measurement reporting according to 5.5.3 in RRC\_CONNECTED, which are performed in accordance with the performance requirements as specified in TS 36.133 [16].

2> when the memory reserved for the logged measurement information becomes full, stop timer T330 and perform the same actions as performed upon expiry of T330, as specified in 5.6.6.4;

### 5.6.13a NR SCG failure information

#### 5.6.13a.1 General



Figure 5.6.13a.1-1: NR SCG failure information

The purpose of this procedure is to inform E-UTRAN about an SCG failure the UE has experienced (e.g. SCG radio link failure, failure to successfully complete an SCG reconfiguration with sync), as specified in TS 38.331 [82], clause 5.7.3.2.

#### 5.10.7.3 Transmission of SLSS

The UE shall select the SLSSID and the subframe in which to transmit SLSS as follows:

1> if triggered by sidelink discovery announcement and in coverage on the frequency used for sidelink discovery, as defined in TS 36.304 [4], clause 11.4:

2> select the SLSSID included in the entry of *discSyncConfig* included in the received *SystemInformationBlockType19*, that includes *txParameters*;

2> use *syncOffsetIndicator* corresponding to the selected SLSSID;

2> for each pool used for the transmission of discovery announcements (each corresponding to the selected SLSSID):

3> if a subframe indicated by *syncOffsetIndicator* corresponds to the first subframe of the discovery transmission pool;

4> if *discTxGapConfig* is configured and includes the concerned subframe; or the subframe is not used for regular uplink transmission:

5> select the concerned subframe;

3> else:

4> if *discTxGapConfig* is configured and includes the concerned subframe; or the subframe is not used for regular uplink transmission:

5> select the subframe indicated by *syncOffsetIndicator* that precedes and which, in time domain, is nearest to the first subframe of the discovery transmission pool;

3> if the sidelink discovery announcements concern PS; and if *syncTxPeriodic* is included:

4> additionally select each subframe that periodically occurs 40 subframes after the selected subframe;

1> if triggered by sidelink communication and in coverage on the frequency used for sidelink communication, as defined in TS 36.304 [4], clause 11.4:

2> select the SLSSID included in the entry of *commSyncConfig* that is included in the received *SystemInformationBlockType18* and includes *txParameters*;

2> use *syncOffsetIndicator* corresponding to the selected SLSSID;

2> if in RRC\_CONNECTED; and if *networkControlledSyncTx* is configured and set to *on*:

3> select the subframe(s) indicated by *syncOffsetIndicator*;

2> else (when transmitting communication):

3> select the subframe(s) indicated by *syncOffsetIndicator* within the SC period in which the UE intends to transmit sidelink control information or data;

1> if triggered by V2X sidelink communication and in coverage on the frequency used for V2X sidelink communication, as defined in TS 36.304 [4], clause 11.4; or

1> if triggered by V2X sidelink communication, and out of coverage on the frequency used for V2X sidelink communication, and the concerned frequency is included in *v2x-InterFreqInfoList* in *RRCConnectionReconfiguration* or in *v2x-InterFreqInfoList* within *SystemInformationBlockType21* of the serving cell/ PCell;

2> if the UE has selected GNSS as synchronization reference in accordance with 5.10.8.2:

3> select SLSSID 0;

3> use *syncOffsetIndicator* included in the entry of *v2x-SyncConfig* corresponding to the concerned frequency in *v2x-InterFreqInfoList* or within *SystemInformationBlockType21*, that includes *txParameters* and *gnss-Sync*;

3> select the subframe(s) indicated by *syncOffsetIndicator*;

2> if the UE has selected a cell as synchronization reference in accordance with 5.10.8.2:

3> select the SLSSID included in the entry of *v2x-SyncConfig* configured for the concerned frequency in *v2x-InterFreqInfoList* or within *SystemInformationBlockType21*, that includes *txParameters* and does not include *gnss-Sync*;

3> use *syncOffsetIndicator* corresponding to the selected SLSSID;

3> select the subframe(s) indicated by *syncOffsetIndicator*;

1> else if triggered by V2X sidelink communication and the UE has GNSS as the synchronization reference:

2> select SLSSID 0;

2> if *syncOffsetIndicator3* is configured for the frequency used for V2X sidelink communication in *SL-V2X-Preconfiguration*:

3> select the subframe(s) indicated by *syncOffsetIndicator3*;

2> else:

3> select the subframe(s) indicated by *syncOffsetIndicator1*;

1> else:

2> select the synchronisation reference UE (i.e. SyncRef UE) as defined in 5.10.8;

2> if the UE has a selected SyncRef UE and *inCoverage* in the *MasterInformationBlock-SL* or *MasterInformationBlock-SL-V2X* message received from this UE is set to *TRUE*; or

2> if the UE has a selected SyncRef UE and *inCoverage* in the *MasterInformationBlock-SL* or *MasterInformationBlock-SL-V2X* message received from this UE is set to *FALSE* while the SLSS from this UE is part of the set defined for out of coverage, see TS 36.211 [21]:

3> select the same SLSSID as the SLSSID of the selected SyncRef UE;

3> select the subframe in which to transmit the SLSS according to the *syncOffsetIndicator1* or *syncOffsetIndicator2* included in the preconfigured sidelink parameters (i.e. *preconfigSync* in *SL-Preconfiguration* or *v2x-CommPreconfigSync* in *SL-V2X-Preconfiguration* defined in 9.3) corresponding to the concerned frequency, such that the subframe timing is different from the SLSS of the selected SyncRef UE;

2> else if the UE has a selected SyncRef UE and the SLSS from this UE was transmitted on the subframe indicated by *syncOffsetIndicator3* that is included in the *syncOffsetIndicators* in *SL-V2X-Preconfiguration*, and is corresponding to the frequency used for V2X sidelink communication:

3> select SLSSID 169;

3> select the subframe(s) indicated by *syncOffsetIndicator2*;

2> else if the UE has a selected SyncRef UE:

3> select the SLSSID from the set defined for out of coverage having an index that is 168 more than the index of the SLSSID of the selected SyncRef UE, see TS 36.211 [21];

3> select the subframe in which to transmit the SLSS according to *syncOffsetIndicator1* or *syncOffsetIndicator2* included in the preconfigured sidelink parameters (i.e. *preconfigSync* in *SL-Preconfiguration* or *v2x-CommPreconfigSync* in *SL-V2X-Preconfiguration* defined in 9.3), such that the subframe timing is different from the SLSS of the selected SyncRef UE;

2> else (i.e. no SyncRef UE selected):

3> if the UE has not randomly selected an SLSSID:

4> if triggered by V2X sidelink communication, randomly select, using a uniform distribution, an SLSSID from the set of sequences defined for out of coverage except SLSSID 168 and 169, see TS 36.211 [21];

4> else, randomly select, using a uniform distribution, an SLSSID from the set of sequences defined for out of coverage, see TS 36.211 [21];

4> select the subframe in which to transmit the SLSS according to the *syncOffsetIndicator1* or *syncOffsetIndicator2* (arbitrary selection between these) included in the preconfigured sidelink parameters (i.e. *preconfigSync* in *SL-Preconfiguration* or *v2x-CommPreconfigSync* in *SL-V2X-Preconfiguration* defined in 9.3);

#### 5.10.8.2 Selection and reselection of synchronisation reference

The UE shall:

1> if triggered by V2X sidelink communication, and in coverage on the frequency for V2X sidelink communication; or

1> if triggered by V2X sidelink communication, and out of coverage on the frequency for V2X sidelink communication, and the frequency used to transmit V2X sidelink communication is included in *v2x-InterFreqInfoList* in *RRCConnectionReconfiguration* or in *v2x-InterFreqInfoList* within *SystemInformationBlockType21* or *SystemInformationBlockType26* of the serving cell/ PCell:

2> if *syncFreqList* is not included in *RRCConnectionReconfiguration* nor in *SystemInformationBlockType26*; or

2> if *syncFreqList* is included in *RRCConnectionReconfiguration* or in *SystemInformationBlockType26*, and none of the frequency(ies) selected as specified in TS 36.321 [6] is included in the *syncFreqList*; or

2> if *syncFreqList* is included in *RRCConnectionReconfiguration* or in *SystemInformationBlockType26*, and no synchronisation carrier frequency is selected as specified in 5.10.8a:

3> if *typeTxSync* is configured for the concerned frequency and set to *enb*:

4> select a cell as the synchronization reference source as defined in 5.10.13.3;

3> else if *typeTxSync* for the concerned frequency is not configured or is set to *gnss*, and GNSS is reliable in accordance with TS 36.101 [42] and TS 36.133 [16]:

4> select GNSS as the synchronization reference source;

3> else (i.e., there is no GNSS which is reliable in accordance with TS 36.101 [42] and TS 36.133 [16]):

4> search SLSSID=0 on the concerned frequency to detect candidate SLSS, in accordance with TS 36.133 [16];

4> when evaluating the detected SLSS, apply layer 3 filtering as specified in 5.5.3.2 using the preconfigured *filterCoefficient* as defined in 9.3, before using the S-RSRP measurement results;

4> if the S-RSRP of the SyncRef UE identified by the detected SLSS exceeds the minimum requirement defined in TS 36.133 [16]:

5> select the SyncRef UE;

4> else (i.e., no SLSSID=0 detected):

5> select a cell as the synchronization reference source as defined in 5.10.13.3;

2> if *syncFreqList* is included in *RRCConnectionReconfiguration* or in *SystemInformationBlockType26*, and the UE has selected a synchronisation carrier frequency as specified in 5.10.8a:

3> consider the synchornisation reference source (i.e. eNB, GNSS or SyncRef UE) that is selected on the synchronisation carrier frequency as the synchronization reference;

1> else, if triggered by V2X sidelink communication, and out of coverage on the frequency for V2X sidelink communication, and for the frequency used for V2X sidelink communication, if *syncPriority* in *SL-V2X-Preconfiguration* is set to *gnss* and GNSS is reliable in accordance with TS 36.101 [42] and TS 36.133 [16]:

2> select GNSS as the synchronization reference source;

1> else, for the frequency used for sidelink communication, V2X sidelink communication or sidelink discovery, if out of coverage on that frequency as defined in TS 36.304 [4], clause 11.4:

2> if triggered by sidelink communication or sidelink discovery; or

2> if triggered by V2X sidelink communication, and *syncFreqList* is not included in *SL-V2X-Preconfiguration*; or

2> if triggered by V2X sidelink communication, and *syncFreqList* is included in *SL-V2X-Preconfiguration*, and none of the frequency(ies) selected as specified in TS 36.321 [6] is included in the *syncFreqList*; or

2> if triggered by V2X sidelink communication, and *syncFreqList* is included in *SL-V2X-Preconfiguration*, and no synchronisation carrier frequency is selected as specified in 5.10.8a:

3> perform a full search (i.e. covering all subframes and all possible SLSSIDs) to detect candidate SLSS, in accordance with TS 36.133 [16]

3> when evaluating the one or more detected SLSSIDs, apply layer 3 filtering as specified in 5.5.3.2 using the preconfigured *filterCoefficient* as defined in 9.3, before using the S-RSRP measurement results;

3> if the UE has selected a SyncRef UE:

4> if the S-RSRP of the strongest candidate SyncRef UE exceeds the minimum requirement TS 36.133 [16] by *syncRefMinHyst* and the strongest candidate SyncRef UE belongs to the same priority group as the current SyncRef UE and the S-RSRP of the strongest candidate SyncRef UE exceeds the S-RSRP of the current SyncRef UE by *syncRefDiffHyst*; or

4> if the S-RSRP of the candidate SyncRef UE exceeds the minimum requirement TS 36.133 [16] by *syncRefMinHyst* and the candidate SyncRef UE belongs to a higher priority group than the current SyncRef UE; or

4> if GNSS becomes reliable in accordance with TS 36.101 [42] and TS 36.133 [16], and GNSS belongs to a higher priority group than the current SyncRef UE; or

4> if the S-RSRP of the current SyncRef UE is less than the minimum requirement defined in TS 36.133 [16]:

5> consider no SyncRef UE to be selected;

3> if the UE has selected GNSS as the synchronization reference for V2X sidelink communication:

4> if the S-RSRP of the candidate SyncRef UE exceeds the minimum requirement defined in TS 36.133 [16] by *syncRefMinHyst* and the candidate SyncRef UE belongs to a higher priority group than GNSS; or

4> if GNSS becomes not reliable in accordance with TS 36.101 [42] and TS 36.133 [16]:

5> consider GNSS not to be selected;

3> if the UE has not selected a SyncRef UE and has not selected GNSS as synchronization reference source:

4> if not concerning V2X sidelink communication, and if the UE detects one or more SLSSIDs for which the S-RSRP exceeds the minimum requirement defined in TS 36.133 [16] by *syncRefMinHyst* and for which the UE received the corresponding *MasterInformationBlock-SL* message (candidate SyncRef UEs), select a SyncRef UE according to the following priority group order:

5> UEs of which *inCoverage*, included in the *MasterInformationBlock-SL* message received from this UE, is set to *TRUE*, starting with the UE with the highest S-RSRP result (priority group 1);

5> UEs of which SLSSID is part of the set defined for in coverage, starting with the UE with the highest S-RSRP result (priority group 2);

5> Other UEs, starting with the UE with the highest S-RSRP result (priority group 3);

4> for V2X sidelink communication, if the UE detects one or more SLSSIDs for which the S-RSRP exceeds the minimum requirement defined in TS 36.133 [16] by *syncRefMinHyst* and for which the UE received the corresponding *MasterInformationBlock-SL-V2X* message (candidate SyncRef UEs), or if the UE detects GNSS that is reliable in accordance with TS 36.101 [42] and TS 36.133 [16], select a synchronization reference according to the following priority group order:

5> if *syncPriority* corresponding to the concerned frequency in *SL-V2X-Preconfiguration* is set to *enb*:

6> UEs of which SLSSID is part of the set defined for in coverage, and *inCoverage*, included in the *MasterInformationBlock-SL-V2X* message received from this UE, is set to *TRUE*, starting with the UE with the highest S-RSRP result (priority group 1);

6> UE of which SLSSID is part of the set defined for in coverage, and *inCoverage*, included in the *MasterInformationBlock-SL-V2X* message received from this UE, is set to *FALSE*, starting with the UE with the highest S-RSRP result (priority group 2);

6> GNSS that is reliable in accordance with TS 36.101 [42] and TS 36.133 [16] (priority group 3);

6> UEs of which SLSSID is 0, and *inCoverage*, included in the *MasterInformationBlock-SL-V2X* message received from this UE, is set to *TRUE*, or of which SLSSID is 0 and SLSS is transmitted on subframes indicated by *syncOffsetIndicator3,* starting with the UE with the highest S-RSRP result (priority group 4);

6> UEs of which SLSSID is 0 and is not transmitted on subframes indicated by *syncOffsetIndicator3*, and *inCoverage*, included in the *MasterInformationBlock-SL-V2X* message received from this UE, is set to *FALSE*, starting with the UE with the highest S-RSRP result (priority group 5);

6> UEs of which SLSSID is 169, and *inCoverage*, included in the *MasterInformationBlock-SL-V2X* message received from this UE, is set to *FALSE*, starting with the UE with the highest S-RSRP result (priority group 5);

6> Other UEs, starting with the UE with the highest S-RSRP result (priority group 6);

5> if *syncPriority* corresponding to the concerned frequency in *SL-V2X-Preconfiguration* is set to *gnss:*

6> GNSS that is reliable in accordance with TS 36.101 [42] and TS 36.133 [16] (priority group 1);

6> UEs of which SLSSID is part of the set defined for in coverage, and *inCoverage*, included in the *MasterInformationBlock-SL-V2X* message received from this UE, is set to *TRUE*, starting with the UE with the highest S-RSRP result (priority group 2);

6> UEs of which SLSSID is 0, and *inCoverage*, included in the *MasterInformationBlock-SL-V2X* message received from this UE, is set to *TRUE*, or of which SLSSID is 0 and SLSS is transmitted on subframes indicated by *syncOffsetIndicator3,* starting with the UE with the highest S-RSRP result (priority group 2);

6> UE of which SLSSID is part of the set defined for in coverage, and *inCoverage*, included in the *MasterInformationBlock-SL-V2X* message received from this UE, is set to *FALSE*, starting with the UE with the highest S-RSRP result (priority group 3);

6> UEs of which SLSSID is 0 and is not transmitted on subframes indicated by *syncOffsetIndicator3*, and *inCoverage*, included in the *MasterInformationBlock-SL-V2X* message received from this UE, is set to *FALSE*, starting with the UE with the highest S-RSRP result (priority group 3);

6> UEs of which SLSSID is 169, and *inCoverage*, included in the *MasterInformationBlock-SL-V2X* message received from this UE, is set to *FALSE*, starting with the UE with the highest S-RSRP result (priority group 3);

6> Other UEs, starting with the UE with the highest S-RSRP result (priority group 4);

2> if triggered by V2X sidelink communication, and *syncFreqList* is included in *SL-V2X-Preconfiguration*, and the UE has selected a synchronisation carrier frequency as specified in 5.10.8a;

3> consider the synchornization reference source (i.e. eNB, GNSS or SyncRef UE) that selected on the synchronisation carrier frequency as the synchronization reference;

### 5.10.8a Selection and reselection of synchronisation carrier frequency

For the frequency(ies) which are in coverage for the UE as defined in TS 36.304 [4], clause 11.4 and which have been selected for V2X sidelink communication as specified in TS 36.321 [6], and/or for the frequency(ies) which are out of coverage for the UE and included in *v2x-InterFreqInfoList* within *RRCConnectionReconfiguration* or *SystemInformationBlockType21* or *SystemInformationBlockType26* of the serving cell/ PCell and which have been selected for V2X sidelink communication as specified in TS 36.321 [6], the UE capable of V2X sidelink communication and synchronisation carrier frequency selection shall:

1> if *syncFreqList* is included in *RRCConnectionReconfiguration* or in *SystemInformationBlockType26*, and includes at least one of the concerned frequency(ies):

2> if no synchronisation carrier frequency is selected:

3> if *typeTxSync* is configured for the concerned frequency(ies) and set to *enb*; or

3> if *typeTxSync* for the concerned frequency(ies) is not configured or is set to *gnss*, and GNSS is reliable in accordance with TS 36.101 [42] and TS 36.133 [16]:

4> select one frequency from the concerned frequency(ies) which are included in *syncFreqList* as the synchronisation carrier frequency.

3> else (i.e., there is no GNSS which is reliable in accordance with TS 36.101 [42] and TS 36.133 [16]):

4> select the synchronisation reference source(s) on the concerned frequency(ies) which are included in *syncFreqList* according to 5.10.8.2:

4> if SyncRef UE(s) with SLSSID=0 is detected on at least one frequency from the concerned frequency(ies):

5> select one frequency from the concerned frequency(ies) with the SyncRef UE(s) with SLSSID=0 detected as the synchronisation carrier frequency;

4> else (i.e., no SLSSID=0 detected and UE selects a cell as the synchronisation reference source):

5> select one frequency from the concerned frequencies which are included in *syncFreqList* as the synchronisation carrier frequency;

2> else (i.e. the synchronisation carrier frequency is selected):

3> if the UE selects GNSS as the synchronisation reference source, and GNSS is unreliable in accordance with TS 36.101 [42] and TS 36.133 [16]; or

3> if the UE selects a cell as the synchronisation reference source, and the cell cannot fulfil the S criterion in accordance with TS 36.304 [4]; or

3> if the UE selects a SyncRef UE and the S-RSRP of the current SyncRef UE is less than the minimum requirement defined in TS 36.133 [16]; or

3> if the synchronisation carrier frequency is not selected for V2X sidelink communication as specified in TS 36.321 [6]:

4> consider no synchronisation carrier frequency is selected;

For the frequency(ies) which are out of coverage for the UE and not included in *v2x-InterFreqInfoList* within *RRCConnectionReconfiguration* nor *SystemInformationBlockType21* nor *SystemInformationBlockType26* of the serving cell/ PCell and which have been selected for V2X sidelink carrier communication as specified in TS 36.321 [6], the UE capable of V2X sidelink communication and selection of synchronisation carrier frequency selection shall:

1> if *syncFreqList* is included in *SL-V2X-Preconfiguration*, and at least one of the concerned frequency(ies) is included in *syncFreqList*:

2> if no synchronisation carrier frequency is selected:

3> if *syncPriority* in *SL-V2X-Preconfiguration* is set to gnss and GNSS is reliable in accordance with TS 36.101 [42] and TS 36.133 [16]:

4> select one frequency from the concerned frequency(ies) which are included in *syncFreqList* as the synchronisation carrier frequency.

3> else:

4> select the synchronisation reference source(s) on the concerned frequency(ies) which are included in *SyncFreqList* according to 5.10.8.2;

4> select the frequency with the highest synchronisation reference source priority as the synchronisation carrier frequency, according to the following priority gourp order:

5> if *syncPriority* corresponding to the concerned frequency(ies) in *SL-V2X-Preconfiguration* is set to *enb*:

6> the frequency(ies) with SyncRef UE of which SLSSID is part of the set defined for in coverage, and *inCoverage*, included in the *MasterInformationBlock-SL-V2X* message received from this UE, is set to *TRUE* (priority group 1);

6> the frequency(ies) with SyncRef UE of which SLSSID is part of the set defined for in coverage, and *inCoverage*, included in the *MasterInformationBlock-SL-V2X* message received from this UE, is set to *FALSE* (priority group 2);

6> the frequency(ies) using GNSS as synchronisation reference source (priority group 3);

6> the frequency(ies) with SyncRef UE of which SLSSID is 0, and *inCoverage*, included in the *MasterInformationBlock-SL-V2X* message received from this UE, is set to *TRUE*, or of which SLSSID is 0 and SLSS is transmitted on subframes indicated by *syncOffsetIndicator3* (priority group 4);

6> the frequency(ies) with SyncRef UE of which SLSSID is 0 and is not transmitted on subframes indicated by *syncOffsetIndicator3*, and *inCoverage*, included in the *MasterInformationBlock-SL-V2X* message received from this UE, is set to *FALSE* (priority group 5);

6> the frequency(ies) with SyncRef UE of which SLSSID is 169, and *inCoverage*, included in the *MasterInformationBlock-SL-V2X* message received from this UE, is set to *FALSE* (priority group 5);

6> the frequency(ies) with other SyncRef UE (priority group 6);

5> if *syncPriority* corresponding to the concerned frequency(ies) in *SL-V2X-Preconfiguration* is set to *gnss*:

6> the frequency(ies) with SyncRef UE of which SLSSID is part of the set defined for in coverage, and *inCoverage*, included in the *MasterInformationBlock-SL-V2X* message received from this UE, is set to *TRUE* (priority group 1);

6> the frequency(ies) with SyncRef UE of which SLSSID is 0, and *inCoverage*, included in the *MasterInformationBlock-SL-V2X* message received from this UE, is set to *TRUE*, or of which SLSSID is 0 and SLSS is transmitted on subframes indicated by *syncOffsetIndicator3* (priority group 1);

6> the frequency(ies) with SyncRef UE of which SLSSID is part of the set defined for in coverage, and *inCoverage*, included in the *MasterInformationBlock-SL-V2X* message received from this UE, is set to *FALSE* (priority group 2);

6> the frequency(ies) with SyncRef UE of which SLSSID is 0 and is not transmitted on subframes indicated by *syncOffsetIndicator3*, and *inCoverage*, included in the *MasterInformationBlock-SL-V2X* message received from this UE, is set to *FALSE* (priority group 2);

6> the frequency(ies) with SyncRef UE of which SLSSID is 169, and *inCoverage*, included in the *MasterInformationBlock-SL-V2X* message received from this UE, is set to *FALSE* (priority group 2);

6> the frequency(ies) with other SyncRef UE (priority group 3);

2> else (i.e. the synchronisation carrier frequency is selected):

3> if the UE selects GNSS as the synchronisation reference source, and GNSS is unreliable in accordance with TS 36.101 [42] and TS 36.133 [16]; or

3> if the UE selects a SyncRef UE and the S-RSRP of the current SyncRef UE is less than the minimum requirement defined in TS 36.133 [16]; or

3> if the synchronisation carrier frequency is not selected for V2X sidelink communication as specified in TS 36.321 [6]:

4> consider no synchronisation carrier frequency is selected;

NOTE 1: If more than one selected carrier frequencies satisfy the condition as the synchronisation carrier frequency for V2X sidelink communication, how to select one synchronisation carrier frequency is up to UE implementation.

NOTE 2: All concerned carrier frequency(ies) have the same *typeTxSync* and *syncPriority* configured.

### 6.2.1 General message structure

#### – *LoggedMeasurementConfiguration*

The *LoggedMeasurementConfiguration* message is used by E-UTRAN to configure the UE to perform logging of measurement results while in RRC\_IDLE or to perform logging of measurement results for MBSFN while in both RRC\_IDLE and RRC\_CONNECTED. It is used to transfer the logged measurement configuration for network performance optimisation, see TS 37.320 [60].

Signalling radio bearer: SRB1

RLC-SAP: AM

Logical channel: DCCH

Direction: E-UTRAN to UE

*LoggedMeasurementConfiguration message*

-- ASN1START

LoggedMeasurementConfiguration-r10 ::= SEQUENCE {

criticalExtensions CHOICE {

c1 CHOICE {

loggedMeasurementConfiguration-r10 LoggedMeasurementConfiguration-r10-IEs,

spare3 NULL, spare2 NULL, spare1 NULL

},

criticalExtensionsFuture SEQUENCE {}

}

}

LoggedMeasurementConfiguration-r10-IEs ::= SEQUENCE {

traceReference-r10 TraceReference-r10,

traceRecordingSessionRef-r10 OCTET STRING (SIZE (2)),

tce-Id-r10 OCTET STRING (SIZE (1)),

absoluteTimeInfo-r10 AbsoluteTimeInfo-r10,

areaConfiguration-r10 AreaConfiguration-r10 OPTIONAL, -- Need OR

loggingDuration-r10 LoggingDuration-r10,

loggingInterval-r10 LoggingInterval-r10,

nonCriticalExtension LoggedMeasurementConfiguration-v1080-IEs OPTIONAL

}

LoggedMeasurementConfiguration-v1080-IEs ::= SEQUENCE {

lateNonCriticalExtension-r10 OCTET STRING OPTIONAL,

nonCriticalExtension LoggedMeasurementConfiguration-v1130-IEs OPTIONAL

}

LoggedMeasurementConfiguration-v1130-IEs ::= SEQUENCE {

plmn-IdentityList-r11 PLMN-IdentityList3-r11 OPTIONAL, -- Need OR

areaConfiguration-v1130 AreaConfiguration-v1130 OPTIONAL, -- Need OR

nonCriticalExtension LoggedMeasurementConfiguration-v1250-IEs OPTIONAL

}

LoggedMeasurementConfiguration-v1250-IEs ::= SEQUENCE {

targetMBSFN-AreaList-r12 TargetMBSFN-AreaList-r12 OPTIONAL, -- Need OP

nonCriticalExtension LoggedMeasurementConfiguration-v1530-IEs OPTIONAL

}

LoggedMeasurementConfiguration-v1530-IEs ::= SEQUENCE {

bt-NameList-r15 BT-NameList-r15 OPTIONAL, --Need OR

wlan-NameList-r15 WLAN-NameList-r15 OPTIONAL, --Need OR

nonCriticalExtension LoggedMeasurementConfiguration-v1700-IEs OPTIONAL

}

LoggedMeasurementConfiguration-v1700-IEs ::= SEQUENCE {

loggedEventTriggerConfig-r17 LoggedEventTriggerConfig-r17 OPTIONAL, --Need OR

measUncomBarPre-r17 ENUMERATED {true} OPTIONAL, --Need OR

nonCriticalExtension SEQUENCE {} OPTIONAL

}

TargetMBSFN-AreaList-r12 ::= SEQUENCE (SIZE (0..maxMBSFN-Area)) OF TargetMBSFN-Area-r12

TargetMBSFN-Area-r12 ::= SEQUENCE {

mbsfn-AreaId-r12 MBSFN-AreaId-r12 OPTIONAL, -- Need OR

carrierFreq-r12 ARFCN-ValueEUTRA-r9,

...

}

LoggedEventTriggerConfig-r17 ::= SEQUENCE {

eventType-r17 EventType-r17

}

EventType-r17 ::= CHOICE {

outOfCoverage NULL,

eventL1 SEQUENCE {

l1-Threshold-r17 ThresholdEUTRA,

hysteresis-r17 Hysteresis,

timeToTrigger-r17 TimeToTrigger

},

...

}

-- ASN1STOP

| *LoggedMeasurementConfiguration* field descriptions |
| --- |
| ***absoluteTimeInfo***  Indicates the absolute time in the current cell. |
| ***areaConfiguration***  Used to restrict the area in which the UE performs measurement logging to cells broadcasting either one of the included cell identities or one of the included tracking area codes/ identities. |
| ***eventType***  The value *outOfCoverage* indicates the UE to perform logging of measurements when the UE enters *any cell selection* state, and the value *eventL1* indicates the UE to perform logging of measurements when the triggering condition (similar as event A2 as specified in 5.5.4.3) as configured in the event is met for the camping cell in *camped normally* state. |
| ***measUncomBarPre***  If configured, the UE attempts to perform the uncompensated Barometeric pressure measurement in RRC\_IDLE as defined in TS 37.355 [109]. |
| ***plmn-IdentityList***  Indicates a set of PLMNs defining when the UE performs measurement logging as well as the associated status indication and information retrieval i.e. the UE performs these actions when the RPLMN is part of this set of PLMNs. |
| ***targetMBSFN-AreaList***  Used to indicate logging of MBSFN measurements and further restrict the area and frequencies for which the UE performs measurement logging for MBSFN. If both MBSFN area id and carrier frequency are present, a specific MBSFN area is indicated. If only carrier frequency is present, all MBSFN areas on that carrier frequency are indicated. If there is no entry in the list, any MBSFN area is indicated. |
| ***tce-Id***  Parameter Trace Collection Entity Id: See TS 32.422 [58]. |
| ***traceRecordingSessionRef***  Parameter Trace Recording Session Reference: See TS 32.422 [58] |

### 6.2.2 Message definitions

#### – *FailureInformation*

The *FailureInformation* message is used to provide information regarding failures detected by the UE, e.g. radio link failure for one of the RLC entities configured with PDCP duplication or failure of a DAPS HO.

Signalling radio bearer: SRB1

RLC-SAP: AM

Logical channel: DCCH

Direction: UE to E‑UTRAN

*FailureInformation message*

-- ASN1START

FailureInformation-r15 ::= SEQUENCE {

failedLogicalChannelInfo-r15 FailedLogicalChannelInfo-r15 OPTIONAL

-- nonCriticalExtension is removed in this version as OPTIONAL was missing

}

FailureInformation-r16 ::= SEQUENCE {

criticalExtensions CHOICE {

failureInformation FailureInformation-r16-IEs,

criticalExtensionsFuture SEQUENCE {}

}

}

FailedLogicalChannelInfo-r15 ::= SEQUENCE {

failedLogicalChannelIdentity-r15 SEQUENCE {

cellGroupIndication-r15 ENUMERATED {mn, sn},

logicalChannelIdentity-r15 INTEGER (1..10) OPTIONAL,

logicalChannelIdentityExt-r15 INTEGER (32..38) OPTIONAL

},

failureType ENUMERATED {duplication, spare3, spare2, spare1}

}

FailureInformation-r16-IEs ::= SEQUENCE {

failedLogicalChannelIdentity-r16 FailedLogicalChannelIdentity-r16 OPTIONAL,

failureType-r16 ENUMERATED {duplication, dapsHO-failure,

spare2, spare1} OPTIONAL,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

FailedLogicalChannelIdentity-r16 ::= SEQUENCE {

cellGroupIndication-r16 ENUMERATED {mn, sn},

logicalChannelIdentity-r16 INTEGER (1..10) OPTIONAL,

logicalChannelIdentityExt-r16 INTEGER (32..38) OPTIONAL

}

-- ASN1STOP

| *FailureInformation* field descriptions |
| --- |
| ***cellGroupIndication***  This field indicates the cell group (MCG, SCG) of the RLC entity for which the PDCP duplication failure occurred. |
| ***failureType***  This field indicates the type of failure reported. Value *duplication* indicates that a radio link failure for one of the RLC entities configured with PDCP duplication has been detected. Value *dapsHO-failure* indicates that timer T304 expired during a DAPS HO. |
| ***logicalChannelIdentity, logicalChannelIdentityExt***  This field indicates the logical channel identity of the RLC entity for which the PDCP duplication failure occurred. |

NOTE: The UE may apply the *FailureInformation-r16* message to report a failure defined in REL-15, but only if it is configured with a feature incorporating a failure that can only be reported by the *FailureInformation-r16* message.

#### – *RRCConnectionResume*

The *RRCConnectionResume* message is used to resume the suspended RRC connection.

Signalling radio bearer: SRB1

RLC-SAP: AM

Logical channel: DCCH

Direction: E‑UTRAN to UE

*RRCConnectionResume* message

-- ASN1START

RRCConnectionResume-r13 ::= SEQUENCE {

rrc-TransactionIdentifier RRC-TransactionIdentifier,

criticalExtensions CHOICE {

c1 CHOICE {

rrcConnectionResume-r13 RRCConnectionResume-r13-IEs,

spare3 NULL,

spare2 NULL,

spare1 NULL

},

criticalExtensionsFuture SEQUENCE {}

}

}

RRCConnectionResume-r13-IEs ::= SEQUENCE {

radioResourceConfigDedicated-r13 RadioResourceConfigDedicated OPTIONAL, -- Need ON

nextHopChainingCount-r13 NextHopChainingCount,

measConfig-r13 MeasConfig OPTIONAL, -- Need ON

antennaInfoDedicatedPCell-r13 AntennaInfoDedicated-v10i0 OPTIONAL, -- Need ON

drb-ContinueROHC-r13 ENUMERATED {true} OPTIONAL, -- Need OP

lateNonCriticalExtension OCTET STRING OPTIONAL,

rrcConnectionResume-v1430-IEs RRCConnectionResume-v1430-IEs OPTIONAL

}

RRCConnectionResume-v1430-IEs ::= SEQUENCE {

otherConfig-r14 OtherConfig-r9 OPTIONAL, -- Need ON

rrcConnectionResume-v1510-IEs RRCConnectionResume-v1510-IEs OPTIONAL

}

RRCConnectionResume-v1510-IEs ::= SEQUENCE {

sk-Counter-r15 INTEGER (0.. 65535) OPTIONAL, -- Need ON

nr-RadioBearerConfig1-r15 OCTET STRING OPTIONAL, -- Need ON

nr-RadioBearerConfig2-r15 OCTET STRING OPTIONAL, -- Need ON

nonCriticalExtension RRCConnectionResume-v1530-IEs OPTIONAL

}

RRCConnectionResume-v1530-IEs ::= SEQUENCE {

fullConfig-r15 ENUMERATED {true} OPTIONAL, -- Need ON

nonCriticalExtension RRCConnectionResume-v1610-IEs OPTIONAL

}

RRCConnectionResume-v1610-IEs ::= SEQUENCE {

idleModeMeasurementReq-r16 ENUMERATED {true} OPTIONAL, -- Need ON

restoreMCG-SCells-r16 ENUMERATED {true} OPTIONAL, -- Need ON

restoreSCG-r16 ENUMERATED {true} OPTIONAL, -- Cond EarlySec

sCellToAddModList-r16 SCellToAddModList-r16 OPTIONAL, -- Cond EarlySec

sCellToReleaseList-r16 SCellToReleaseListExt-r13 OPTIONAL, -- Need ON

sCellGroupToReleaseList-r16 SCellGroupToReleaseList-r15 OPTIONAL, -- Need ON

sCellGroupToAddModList-r16 SCellGroupToAddModList-r15 OPTIONAL, -- Cond EarlySec

nr-SecondaryCellGroupConfig-r16 OCTET STRING OPTIONAL, -- Cond RestoreSCG

p-MaxEUTRA-r16 P-Max OPTIONAL, -- Cond SCG

p-MaxUE-FR1-r16 P-Max OPTIONAL, -- Cond SCG

tdm-PatternConfig-r16 TDM-PatternConfig-r15 OPTIONAL, -- Cond FDD-PCell

tdm-PatternConfig2-r16 TDM-PatternConfig-r15 OPTIONAL, -- Need OR

nonCriticalExtension RRCConnectionResume-v1700-IEs OPTIONAL

}

RRCConnectionResume-v1700-IEs ::= SEQUENCE {

scg-State-r17 ENUMERATED {deactivated} OPTIONAL, -- Need OP

nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- ASN1STOP

| *RRCConnectionResume* field descriptions |
| --- |
| ***drb-ContinueROHC***  This field indicates whether to continue or reset the header compression protocol context for the DRBs configured with EUTRA PDCP and the header compression protocol. Presence of the field indicates that the header compression protocol context continues while absence indicates that the header compression protocol context is reset. |
| ***fullConfig***  Indicates that the full configuration option is applicable for the *RRCConnectionResume* message. |
| ***idleModeMeasurementReq***  This field indicates that the UE shall report the idle/inactive measurements to the network in the *RRCConnectionResumeComplete* message |
| ***p-MaxEUTRA***  Indicates the maximum power available for E-UTRA. |
| ***p-MaxUE-FR1***  The maximum total transmit power to be used by the UE across all serving cells in frequency range 1 (FR1) across all cell groups. The maximum transmit power that the UE may use may be additionally limited on cell- or cell-group level. |
| ***nr-RadioBearerConfig1, nr-RadioBearerConfig2***  Includes the NR *RadioBearerConfig* IE as specified in TS 38.331 [82]. The field includes the configuration of RBs configured with NR PDCP. |
| ***nr-SecondaryCellGroupConfig***  Includes the NR *RRCReconfiguration* message as specified in TS 38.331 [82]. In this version of the specification, the NR RRC message only includes fields *secondaryCellGroup*, with at least *reconfigurationWithSync, otherConfig* and/ or *measConfig*. |
| ***restoreMCG-Scells***  Indicates that the UE shall restore the MCG Scell configurations from the UE AS Context or UE Inactive AS Context, if configured. |
| ***restoreSCG***  If included, the UE shall restore the SCG configurations from the UE AS Context or UE Inactive AS Context. |
| ***sCellGroupToAddModList***  Indicates the SCell group to be added or modified. |
| ***sCellGroupToReleaseList***  Indicates the SCell group to be released. |
| ***sCellToAddModList***  List of SCells to be added or modified. |
| ***sCellToReleaseList***  List of SCells to be released. |
| ***scg-State***  Indicates that the SCG is deactivated. |
| ***sk-Counter***  A one-shot counter used upon initial configuration of S-KgNB as well as upon refresh of S-KgNB. E-UTRAN provides this field when the UE is configured with an (SN-terminated) RB using S-KgNB or NR SCG is configured. |
| ***tdm-PatternConfig***  This field is used when power control or IMD issues require single UL transmission in (NG)EN-DC as specified in TS 38.101-3 [101] and TS 38.213 [88]. |
| ***tdm-PatternConfig2***  This field is used for dual UL transmission in EN-DC with LTE FDD PCell and for single UL transmission in EN-DC with LTE FDD/TDD PCell, as specified in TS 38.101-3 [101] and TS 38.213 [88].  The network sets at most one of *tdm-PatternConfig* and *tdm-PatternConfig2* to setup.  When this field is configured in EN-DC with LTE TDD PCell, it is not applicable if TDD configuration is sa0 or sa6 in SIB1. |

| Conditional presence | Explanation |
| --- | --- |
| *EarlySec* | For EPC, the field is optionally present, Need ON, if the UE supports early security reactivation; otherwise the field is not present.  For 5GC, the field is optionally present, Need ON. |
| *RestoreSCG* | The field is mandatory present if *restoreSCG* is configured. It is optionally present, Need ON, otherwise.  For EPC, this field can be present only if the UE supports early security reactivation. |
| *FDD-PCell* | This field is optionally present, need ON, for an FDD PCell if there is no SCell with configured uplink. Otherwise, the field is not present, need OR. |
| *SCG* | This field is optionally present, need OR, if *nr-SecondaryCellGroupConfig* is present, otherwise it is absent, need OR. |

#### – *SystemInformationBlockType1*

*SystemInformationBlockType1* contains information relevant when evaluating if a UE is allowed to access a cell and defines the scheduling of other system information. *SystemInformationBlockType1-BR* uses the same structure as *SystemInformationBlockType1*.

Signalling radio bearer: N/A

RLC-SAP: TM

Logical channels: BCCH and BR-BCCH

Direction: E‑UTRAN to UE

*SystemInformationBlockType1 message*

-- ASN1START

SystemInformationBlockType1-BR-r13 ::= SystemInformationBlockType1

SystemInformationBlockType1 ::= SEQUENCE {

cellAccessRelatedInfo SEQUENCE {

plmn-IdentityList PLMN-IdentityList,

trackingAreaCode TrackingAreaCode,

cellIdentity CellIdentity,

cellBarred ENUMERATED {barred, notBarred},

intraFreqReselection ENUMERATED {allowed, notAllowed},

csg-Indication BOOLEAN,

csg-Identity CSG-Identity OPTIONAL -- Need OR

},

cellSelectionInfo SEQUENCE {

q-RxLevMin Q-RxLevMin,

q-RxLevMinOffset INTEGER (1..8) OPTIONAL -- Need OP

},

p-Max P-Max OPTIONAL, -- Need OP

freqBandIndicator FreqBandIndicator,

schedulingInfoList SchedulingInfoList,

tdd-Config TDD-Config OPTIONAL, -- Cond TDD

si-WindowLength ENUMERATED {

ms1, ms2, ms5, ms10, ms15, ms20,

ms40},

systemInfoValueTag INTEGER (0..31),

nonCriticalExtension SystemInformationBlockType1-v890-IEs OPTIONAL

}

SystemInformationBlockType1-v890-IEs::= SEQUENCE {

lateNonCriticalExtension OCTET STRING (CONTAINING SystemInformationBlockType1-v8h0-IEs) OPTIONAL,

nonCriticalExtension SystemInformationBlockType1-v920-IEs OPTIONAL

}

-- Late non critical extensions

SystemInformationBlockType1-v8h0-IEs ::= SEQUENCE {

multiBandInfoList MultiBandInfoList OPTIONAL, -- Need OR

nonCriticalExtension SystemInformationBlockType1-v9e0-IEs OPTIONAL

}

SystemInformationBlockType1-v9e0-IEs ::= SEQUENCE {

freqBandIndicator-v9e0 FreqBandIndicator-v9e0 OPTIONAL, -- Cond FBI-max

multiBandInfoList-v9e0 MultiBandInfoList-v9e0 OPTIONAL, -- Cond mFBI-max

nonCriticalExtension SystemInformationBlockType1-v10j0-IEs OPTIONAL

}

SystemInformationBlockType1-v10j0-IEs ::= SEQUENCE {

freqBandInfo-r10 NS-PmaxList-r10 OPTIONAL, -- Need OR

multiBandInfoList-v10j0 MultiBandInfoList-v10j0 OPTIONAL, -- Need OR

nonCriticalExtension SystemInformationBlockType1-v10l0-IEs OPTIONAL

}

SystemInformationBlockType1-v10l0-IEs ::= SEQUENCE {

freqBandInfo-v10l0 NS-PmaxList-v10l0 OPTIONAL, -- Need OR

multiBandInfoList-v10l0 MultiBandInfoList-v10l0 OPTIONAL, -- Need OR

nonCriticalExtension SystemInformationBlockType1-v10x0-IEs OPTIONAL

}

SystemInformationBlockType1-v10x0-IEs ::= SEQUENCE {

-- This field is only for late non-critical extensions from Rel-10 or Rel-11 onwards

lateNonCriticalExtension OCTET STRING OPTIONAL,

nonCriticalExtension SystemInformationBlockType1-v12j0-IEs OPTIONAL

}

SystemInformationBlockType1-v12j0-IEs ::= SEQUENCE {

schedulingInfoList-v12j0 SchedulingInfoList-v12j0 OPTIONAL, -- Need OR

schedulingInfoListExt-r12 SchedulingInfoListExt-r12 OPTIONAL, -- Need OR

nonCriticalExtension SystemInformationBlockType1-v15g0-IEs OPTIONAL

}

SystemInformationBlockType1-v15g0-IEs ::= SEQUENCE {

bandwidthReducedAccessRelatedInfo-v15g0 SEQUENCE {

posSchedulingInfoList-BR-r15 SchedulingInfoList-BR-r13

} OPTIONAL, -- Need OR

nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- Regular non critical extensions

SystemInformationBlockType1-v920-IEs ::= SEQUENCE {

ims-EmergencySupport-r9 ENUMERATED {true} OPTIONAL, -- Need OR

cellSelectionInfo-v920 CellSelectionInfo-v920 OPTIONAL, -- Cond RSRQ

nonCriticalExtension SystemInformationBlockType1-v1130-IEs OPTIONAL

}

SystemInformationBlockType1-v1130-IEs ::= SEQUENCE {

tdd-Config-v1130 TDD-Config-v1130 OPTIONAL, -- Cond TDD-OR

cellSelectionInfo-v1130 CellSelectionInfo-v1130 OPTIONAL, -- Cond WB-RSRQ

nonCriticalExtension SystemInformationBlockType1-v1250-IEs OPTIONAL

}

SystemInformationBlockType1-v1250-IEs ::= SEQUENCE {

cellAccessRelatedInfo-v1250 SEQUENCE {

category0Allowed-r12 ENUMERATED {true} OPTIONAL -- Need OP

},

cellSelectionInfo-v1250 CellSelectionInfo-v1250 OPTIONAL, -- Cond RSRQ2

freqBandIndicatorPriority-r12 ENUMERATED {true} OPTIONAL, -- Cond mFBI

nonCriticalExtension SystemInformationBlockType1-v1310-IEs OPTIONAL

}

SystemInformationBlockType1-v1310-IEs ::= SEQUENCE {

hyperSFN-r13 BIT STRING (SIZE (10)) OPTIONAL, -- Need OR

eDRX-Allowed-r13 ENUMERATED {true} OPTIONAL, -- Need OR

cellSelectionInfoCE-r13 CellSelectionInfoCE-r13 OPTIONAL, -- Need OP

bandwidthReducedAccessRelatedInfo-r13 SEQUENCE {

si-WindowLength-BR-r13 ENUMERATED {

ms20, ms40, ms60, ms80, ms120,

ms160, ms200, spare},

si-RepetitionPattern-r13 ENUMERATED {everyRF, every2ndRF, every4thRF,

every8thRF},

schedulingInfoList-BR-r13 SchedulingInfoList-BR-r13 OPTIONAL, -- Cond SI-BR

fdd-DownlinkOrTddSubframeBitmapBR-r13 CHOICE {

subframePattern10-r13 BIT STRING (SIZE (10)),

subframePattern40-r13 BIT STRING (SIZE (40))

} OPTIONAL, -- Need OP

fdd-UplinkSubframeBitmapBR-r13 BIT STRING (SIZE (10)) OPTIONAL, -- Need OP

startSymbolBR-r13 INTEGER (1..4),

si-HoppingConfigCommon-r13 ENUMERATED {on,off},

si-ValidityTime-r13 ENUMERATED {true} OPTIONAL, -- Need OP

systemInfoValueTagList-r13 SystemInfoValueTagList-r13 OPTIONAL -- Need OR

} OPTIONAL, -- Cond BW-reduced

nonCriticalExtension SystemInformationBlockType1-v1320-IEs OPTIONAL

}

SystemInformationBlockType1-v1320-IEs ::= SEQUENCE {

freqHoppingParametersDL-r13 SEQUENCE {

mpdcch-pdsch-HoppingNB-r13 ENUMERATED {nb2, nb4} OPTIONAL, -- Need OR

interval-DLHoppingConfigCommonModeA-r13 CHOICE {

interval-FDD-r13 ENUMERATED {int1, int2, int4, int8},

interval-TDD-r13 ENUMERATED {int1, int5, int10, int20}

} OPTIONAL, -- Need OR

interval-DLHoppingConfigCommonModeB-r13 CHOICE {

interval-FDD-r13 ENUMERATED {int2, int4, int8, int16},

interval-TDD-r13 ENUMERATED { int5, int10, int20, int40}

} OPTIONAL, -- Need OR

mpdcch-pdsch-HoppingOffset-r13 INTEGER (1..maxAvailNarrowBands-r13) OPTIONAL -- Need OR

} OPTIONAL, -- Cond Hopping

nonCriticalExtension SystemInformationBlockType1-v1350-IEs OPTIONAL

}

SystemInformationBlockType1-v1350-IEs ::= SEQUENCE {

cellSelectionInfoCE1-r13 CellSelectionInfoCE1-r13 OPTIONAL, -- Need OP

nonCriticalExtension SystemInformationBlockType1-v1360-IEs OPTIONAL

}

SystemInformationBlockType1-v1360-IEs ::= SEQUENCE {

cellSelectionInfoCE1-v1360 CellSelectionInfoCE1-v1360 OPTIONAL, -- Cond QrxlevminCE1

nonCriticalExtension SystemInformationBlockType1-v1430-IEs OPTIONAL

}

SystemInformationBlockType1-v1430-IEs ::= SEQUENCE {

eCallOverIMS-Support-r14 ENUMERATED {true} OPTIONAL, -- Need OR

tdd-Config-v1430 TDD-Config-v1430 OPTIONAL, -- Cond TDD-OR

cellAccessRelatedInfoList-r14 SEQUENCE (SIZE (1..maxPLMN-1-r14)) OF

CellAccessRelatedInfo-r14 OPTIONAL, -- Need OR

nonCriticalExtension SystemInformationBlockType1-v1450-IEs OPTIONAL

}

SystemInformationBlockType1-v1450-IEs ::= SEQUENCE {

tdd-Config-v1450 TDD-Config-v1450 OPTIONAL, -- Cond TDD-OR

nonCriticalExtension SystemInformationBlockType1-v1530-IEs OPTIONAL

}

SystemInformationBlockType1-v1530-IEs ::= SEQUENCE {

hsdn-Cell-r15 ENUMERATED {true} OPTIONAL, -- Need OR

cellSelectionInfoCE-v1530 CellSelectionInfoCE-v1530 OPTIONAL, -- Need OP

crs-IntfMitigConfig-r15 CHOICE {

crs-IntfMitigEnabled NULL,

crs-IntfMitigNumPRBs ENUMERATED {n6, n24}

} OPTIONAL, -- Need OR

cellBarred-CRS-r15 ENUMERATED {barred, notBarred},

plmn-IdentityList-v1530 PLMN-IdentityList-v1530 OPTIONAL, -- Need OR

posSchedulingInfoList-r15 PosSchedulingInfoList-r15 OPTIONAL, -- Need OR

cellAccessRelatedInfo-5GC-r15 SEQUENCE {

cellBarred-5GC-r15 ENUMERATED {barred, notBarred},

cellBarred-5GC-CRS-r15 ENUMERATED {barred, notBarred},

cellAccessRelatedInfoList-5GC-r15 SEQUENCE (SIZE (1..maxPLMN-r11)) OF

CellAccessRelatedInfo-5GC-r15

} OPTIONAL, -- Need OP

ims-EmergencySupport5GC-r15 ENUMERATED {true} OPTIONAL, -- Need OR

eCallOverIMS-Support5GC-r15 ENUMERATED {true} OPTIONAL, -- Need OR

nonCriticalExtension SystemInformationBlockType1-v1540-IEs OPTIONAL

}

SystemInformationBlockType1-v1540-IEs ::= SEQUENCE {

si-posOffset-r15 ENUMERATED {true} OPTIONAL, -- Need ON

nonCriticalExtension SystemInformationBlockType1-v1610-IEs OPTIONAL

}

SystemInformationBlockType1-v1610-IEs ::= SEQUENCE {

eDRX-Allowed-5GC-r16 ENUMERATED {true} OPTIONAL, -- Need OR

transmissionInControlChRegion-r16 ENUMERATED {true} OPTIONAL, -- Cond BW-reduced

campingAllowedInCE-r16 ENUMERATED {true} OPTIONAL, -- Need OR

plmn-IdentityList-v1610 PLMN-IdentityList-v1610 OPTIONAL, -- Need OR

nonCriticalExtension SystemInformationBlockType1-v1700-IEs OPTIONAL

}

SystemInformationBlockType1-v1700-IEs ::= SEQUENCE {

cellAccessRelatedInfo-v1700 SEQUENCE {

cellBarred-NTN-r17 ENUMERATED {barred, notBarred},

plmn-IdentityList-v1700 PLMN-IdentityList-v1700 OPTIONAL -- Need OR

} OPTIONAL, -- Need OR

nonCriticalExtension SEQUENCE {} OPTIONAL

}

PLMN-IdentityList ::= SEQUENCE (SIZE (1..maxPLMN-r11)) OF PLMN-IdentityInfo

PLMN-IdentityInfo ::= SEQUENCE {

plmn-Identity PLMN-Identity,

cellReservedForOperatorUse ENUMERATED {reserved, notReserved}

}

PLMN-IdentityList-v1530 ::= SEQUENCE (SIZE (1..maxPLMN-r11)) OF PLMN-IdentityInfo-v1530

PLMN-IdentityInfo-v1530 ::= SEQUENCE {

cellReservedForOperatorUse-CRS-r15 ENUMERATED {reserved, notReserved}

}

PLMN-IdentityList-r15::= SEQUENCE (SIZE (1..maxPLMN-r11)) OF PLMN-IdentityInfo-r15

PLMN-IdentityList-v1610::= SEQUENCE (SIZE (1..maxPLMN-r11)) OF PLMN-IdentityInfo-v1610

PLMN-IdentityList-v1700::= SEQUENCE (SIZE (1..maxPLMN-r11)) OF PLMN-IdentityInfo-v1700

PLMN-IdentityInfo-r15 ::= SEQUENCE {

plmn-Identity-5GC-r15 CHOICE{

plmn-Identity-r15 PLMN-Identity,

plmn-Index-r15 INTEGER (1..maxPLMN-r11)

},

cellReservedForOperatorUse-r15 ENUMERATED {reserved, notReserved},

cellReservedForOperatorUse-CRS-r15 ENUMERATED {reserved, notReserved}

}

PLMN-IdentityInfo-v1610 ::= SEQUENCE {

cp-CIoT-5GS-Optimisation-r16 ENUMERATED {true} OPTIONAL, -- Need OR

up-CIoT-5GS-Optimisation-r16 ENUMERATED {true} OPTIONAL, -- Need OR

iab-Support-r16 ENUMERATED {true} OPTIONAL -- Need OR

}

PLMN-IdentityInfo-v1700 ::= SEQUENCE {

trackingAreaList-r17 TrackingAreaList-r17 OPTIONAL -- Need OP

}

SchedulingInfoList ::= SEQUENCE (SIZE (1..maxSI-Message)) OF SchedulingInfo

SchedulingInfoList-v12j0 ::= SEQUENCE (SIZE (1..maxSI-Message)) OF SchedulingInfo-v12j0

SchedulingInfoListExt-r12 ::= SEQUENCE (SIZE (1..maxSI-Message)) OF SchedulingInfoExt-r12

SchedulingInfo ::= SEQUENCE {

si-Periodicity SI-Periodicity-r12,

sib-MappingInfo SIB-MappingInfo

}

SchedulingInfo-v12j0 ::= SEQUENCE {

sib-MappingInfo-v12j0 SIB-MappingInfo-v12j0 OPTIONAL -- Need OR

}

SchedulingInfoExt-r12 ::= SEQUENCE {

si-Periodicity-r12 SI-Periodicity-r12,

sib-MappingInfo-r12 SIB-MappingInfo-v12j0

}

SchedulingInfoList-BR-r13 ::= SEQUENCE (SIZE (1..maxSI-Message)) OF SchedulingInfo-BR-r13

SchedulingInfo-BR-r13 ::= SEQUENCE {

si-Narrowband-r13 INTEGER (1..maxAvailNarrowBands-r13),

si-TBS-r13 ENUMERATED {b152, b208, b256, b328, b408, b504, b600, b712, b808, b936}

}

SIB-MappingInfo ::= SEQUENCE (SIZE (0..maxSIB-1)) OF SIB-Type

SIB-MappingInfo-v12j0 ::= SEQUENCE (SIZE (1..maxSIB-1)) OF SIB-Type-v12j0

SIB-Type ::= ENUMERATED {

sibType3, sibType4, sibType5, sibType6,

sibType7, sibType8, sibType9, sibType10,

sibType11, sibType12-v920, sibType13-v920,

sibType14-v1130, sibType15-v1130,

sibType16-v1130, sibType17-v1250, sibType18-v1250,

..., sibType19-v1250, sibType20-v1310, sibType21-v1430,

sibType24-v1530, sibType25-v1530, sibType26-v1530,

sibType26a-v1610, sibType27-v1610, sibType28-v1610,

sibType29-v1610

-- Note: This extention is not to be used any further for this release of the specification. If needed, use SIB-Type-v12j0 for new SIB(s).

}

SIB-Type-v12j0 ::= ENUMERATED {

sibType19-v1250, sibType20-v1310, sibType21-v1430,

sibType24-v1530, sibType25-v1530, sibType26-v1530,

sibType26a-v1610, sibType27-v1610, sibType28-v1610,

sibType29-v1610, sibType30-v1700, sibType31-v1700, sibType32-v1700,

spare3, spare2, spare1, ...}

SI-Periodicity-r12 ::= ENUMERATED {rf8, rf16, rf32, rf64, rf128, rf256, rf512}

SystemInfoValueTagList-r13 ::= SEQUENCE (SIZE (1..maxSI-Message)) OF SystemInfoValueTagSI-r13

SystemInfoValueTagSI-r13 ::= INTEGER (0..3)

CellSelectionInfo-v920 ::= SEQUENCE {

q-QualMin-r9 Q-QualMin-r9,

q-QualMinOffset-r9 INTEGER (1..8) OPTIONAL -- Need OP

}

CellSelectionInfo-v1130 ::= SEQUENCE {

q-QualMinWB-r11 Q-QualMin-r9

}

CellSelectionInfo-v1250 ::= SEQUENCE {

q-QualMinRSRQ-OnAllSymbols-r12 Q-QualMin-r9

}

CellAccessRelatedInfo-r14 ::= SEQUENCE {

plmn-IdentityList-r14 PLMN-IdentityList,

trackingAreaCode-r14 TrackingAreaCode,

cellIdentity-r14 CellIdentity

}

CellAccessRelatedInfo-5GC-r15 ::= SEQUENCE {

plmn-IdentityList-r15 PLMN-IdentityList-r15,

ran-AreaCode-r15 RAN-AreaCode-r15 OPTIONAL, -- Need OR

trackingAreaCode-5GC-r15 TrackingAreaCode-5GC-r15,

cellIdentity-5GC-r15 CellIdentity-5GC-r15

}

CellIdentity-5GC-r15 ::= CHOICE{

cellIdentity-r15 CellIdentity,

cellId-Index-r15 INTEGER (1..maxPLMN-r11)

}

TrackingAreaList-r17 ::= SEQUENCE (SIZE (1..maxTAC-r17)) OF TrackingAreaCode

PosSchedulingInfoList-r15 ::= SEQUENCE (SIZE (1..maxSI-Message)) OF PosSchedulingInfo-r15

PosSchedulingInfo-r15 ::= SEQUENCE {

posSI-Periodicity-r15 ENUMERATED {rf8, rf16, rf32, rf64, rf128, rf256, rf512},

posSIB-MappingInfo-r15 PosSIB-MappingInfo-r15

}

PosSIB-MappingInfo-r15 ::= SEQUENCE (SIZE (1..maxSIB)) OF PosSIB-Type-r15

PosSIB-Type-r15 ::= SEQUENCE {

encrypted-r15 ENUMERATED { true } OPTIONAL, -- Need OP

gnss-id-r15 GNSS-ID-r15 OPTIONAL, -- Need OP

sbas-id-r15 SBAS-ID-r15 OPTIONAL, -- Need OP

posSibType-r15 ENUMERATED { posSibType1-1,

posSibType1-2,

posSibType1-3,

posSibType1-4,

posSibType1-5,

posSibType1-6,

posSibType1-7,

posSibType2-1,

posSibType2-2,

posSibType2-3,

posSibType2-4,

posSibType2-5,

posSibType2-6,

posSibType2-7,

posSibType2-8,

posSibType2-9,

posSibType2-10,

posSibType2-11,

posSibType2-12,

posSibType2-13,

posSibType2-14,

posSibType2-15,

posSibType2-16,

posSibType2-17,

posSibType2-18,

posSibType2-19,

posSibType3-1,

...,

posSibType1-8-v1610,

posSibType2-20-v1610,

posSibType2-21-v1610,

posSibType2-22-v1610,

posSibType2-23-v1610,

posSibType2-24-v1610,

posSibType2-25-v1610,

posSibType4-1-v1610,

posSibType5-1-v1610,

posSibType1-9-v1700,

posSibType1-10-v1700

},

...

}

-- ASN1STOP

| *SystemInformationBlockType1* field descriptions |
| --- |
| ***bandwithReducedAccessRelatedInfo***  Access related information for BL UEs and UEs in CE. NOTE 3. |
| ***campingAllowedInCE***  Indicates whether non-BL UE is allowed to camp in the non-standalone BL cell in enhanced coverage mode when S-criterion for normal coverage is fulfilled. The field is not applicable for standalone BL cell. |
| ***category0Allowed***  The presence of this field indicates category 0 UEs are allowed to access the cell. |
| ***cellAccessRelatedInfoList***  This field contains a list allowing signalling of access related information per PLMN. One PLMN can be included in only one entry of this list. NOTE 4. |
| ***cellAccessRelatedInfoList-5GC***  This field contains a PLMN list and a list allowing signalling of access related information per PLMN for PLMNs that provides connectivity to 5GC. One PLMN can be included in only one entry of this list. NOTE4 |
| ***cellBarred, cellBarred-CRS***  barred means the cell is barred, as defined in TS 36.304 [4]. |
| ***cellBarred-5GC, cellBarred-5GC-CRS***  barred means the cell is barred for connectivity to 5GC, as defined in TS 36.304 [4]. |
| ***cellBarred-NTN***  barred means the cell is barred for connectivity to NTN, as defined in TS 36.304 [4]. | |
| ***cellIdentity***  Indicates the cell identity. NOTE 2. |
| ***cellId-Index***  The index of the cell ID in the PLMN lists for EPC, indicates UE the corresponding cell ID is used for 5GC. Value 1 indicates the cell ID of the 1st PLMN list for EPC in the SIB1. Value 2 indicates the cell ID of the 2nd PLMN list for EPC, and so on. |
| ***cellReservedForOperatorUse, cellReservedForOperatorUse-CRS***  As defined in TS 36.304 [4]. |
| ***cellSelectionInfoCE***  Cell selection information for BL UEs and UEs in CE. If absent, coverage enhancement S criteria is not applicable. NOTE 3. |
| ***cellSelectionInfoCE1***  Cell selection information for BL UEs and UEs in CE supporting CE Mode B. E-UTRAN includes this IE only if *cellSelectionInfoCE* is present in *SystemInformationBlockType1-BR*. NOTE 3. | |
| ***cp-CIoT-5GS-Optimisation***  Indicates whether the UE is allowed to establish the connection with Control plane CIoT 5GS optimisation, see TS 24.501 [95]. |
| ***crs-IntfMitigConfig***  *crs-IntfMitigEnabled* indicates CRS interference mitigation is enabled for the cell, as specified in TS 36.133 [16], clause 3.6.1.1. For BL UEs supporting *ce-CRS-IntfMitig,* presence of *crs-IntfMitigNumPRBs* indicates CRS interference mitigation is enabled in the cell, as specified in TS 36.133 [16], clauses 3.6.1.2 and 3.6.1.3, and the value of *crs-IntfMitigNumPRBs* indicates number of PRBs, i.e. 6 or 24 PRBs, for CRS transmission in the central cell BW when CRS interference mitigation is enabled. For UEs not supporting this feature, the behaviour is undefined if this field is configured and the field *cellBarred* in *SystemInformationBlockType1* (*SystemInformationBlockType1-BR* for BL UEs or UEs in CE) is set to *notbarred*. | |
| ***csg-Identity***  Identity of the Closed Subscriber Group the cell belongs to. |
| ***csg-Indication***  If set to TRUE the UE is only allowed to access the cell if it is a CSG member cell, if selected during manual CSG selection or to obtain limited service, see TS 36.304 [4]. |
| ***eCallOverIMS-Support***  Indicates whether the cell supports eCall over IMS services via EPC for UEs as defined in TS 23.401 [41]. If absent, eCall over IMS via EPC is not supported by the network in the cell.NOTE 2. |
| ***eCallOverIMS-Support5GC***  Indicates whether the cell supports eCall over IMS services via 5GC as defined in TS 23.401 [41]. If absent, eCall over IMS via 5GC is not supported by the network in the cell.NOTE 2. |
| ***eDRX-Allowed***  The presence of this field indicates if idle mode extended DRX is allowed in the cell for the UE connected to EPC. The UE shall stop using extended DRX in idle mode if *eDRX-Allowed* is not present when connected to EPC. |
| ***eDRX-Allowed-5GC***  The presence of this field indicates if idle mode extended DRX is allowed in the cell for the UE connected to 5GC. The UE shall stop using extended DRX in idle mode if *eDRX-Allowed-5GC* is not present when connected to 5GC. |
| ***encrypted***  The presence of this field indicates that the posSibType is encrypted as specified in TS 36.355 [54]. |
| ***fdd-DownlinkOrTddSubframeBitmapBR***  The set of valid subframes for FDD downlink or TDD transmissions, see TS 36.213 [23].  If this field is present, *SystemInformationBlockType1-BR-r13* is transmitted in *RRCConnectionReconfiguration*, and if *RRCConnectionReconfiguration* does not include *systemInformationBlockType2Dedicated*, UE may assume the valid subframes in fdd-*DownlinkOrTddSubframeBitmapBR* are not indicated as MBSFN subframes. If this field is not present, the set of valid subframes is the set of non-MBSFN subframes as indicated by *mbsfn-SubframeConfigList*. If neither this field nor *mbsfn-SubframeConfigList* is present, all subframes are considered as valid subframes for FDD downlink transmission, all DL subframes according to the uplink-downlink configuration (see TS 36.211 [21]) are considered as valid subframes for TDD DL transmission, and all UL subframes according to the uplink-downlink configuration (see TS 36.211 [21]) are considered as valid subframes for TDD UL transmission.  The first/leftmost bit corresponds to the subframe #0 of the radio frame satisfying SFN mod x = 0, where x is the size of the bit string divided by 10. Value 0 in the bitmap indicates that the corresponding subframe is invalid for transmission. Value 1 in the bitmap indicates that the corresponding subframe is valid for transmission. |
| ***fdd-UplinkSubframeBitmapBR***  The set of valid subframes for FDD uplink transmissions for BL UEs, see TS 36.213 [23].  If the field is not present, then UE considers all uplink subframes as valid subframes for FDD uplink transmissions.  The first/leftmost bit corresponds to the subframe #0 of the radio frame satisfying SFN mod x = 0, where x is the size of the bit string divided by 10. Value 0 in the bitmap indicates that the corresponding subframe is invalid for transmission. Value 1 in the bitmap indicates that the corresponding subframe is valid for transmission. |
| ***freqBandIndicatorPriority***  If the field is present and supported by the UE, the UE shall prioritize the frequency bands in the *multiBandInfoList* field in decreasing priority order. Only if the UE does not support any of the frequency band in *multiBandInfoList,* the UE shall use the value in *freqBandIndicator* field. Otherwise, the UE applies frequency band according to the rules defined in *multiBandInfoList.* NOTE 2. |
| ***freqBandInfo***  A list of *additionalPmax* and *additionalSpectrumEmission* values, as defined in TS 36.101 [42], table 6.2.4-1, for UEs neither in CE nor BL UEs and TS 36.101 [42], table 6.2.4E-1, for UEs in CE or BL UEs, for the frequency band in *freqBandIndicator*. If E-UTRAN includes *freqBandInfo-v10l0* it includes the same number of entries, and listed in the same order, as in *freqBandInfo-r10*. |
| ***freqHoppingParametersDL***  Downlink frequency hopping parameters for BR versions of SI messages, MPDCCH/PDSCH of paging, MPDCCH/PDSCH of RAR/Msg4 and unicast MPDCCH/PDSCH. If not present, the UE is not configured downlink frequency hopping. |
| ***gnss-ID***  The presence of this field indicates that the *posSibType* is for a specific GNSS. |
| ***hsdn-Cell***  This field indicates this is a HSDN cell as specified in TS 36.304 [4]. |
| ***hyperSFN***  Indicates hyper SFN which increments by one when the SFN wraps around. |
| ***iab-Support***  This field combines both the support of IAB-node and the cell status for IAB-node. If the field is present, the cell supports IAB-nodes and the cell is also considered as a candidate for cell (re)selection for IAB-nodes; if the field is absent, the cell does not support IAB and/or the cell is barred for IAB-node. | |
| ***ims-EmergencySupport***  Indicates whether the cell supports IMS emergency bearer services via EPC for UEs in limited service mode. If absent, IMS emergency call via EPC is not supported by the network in the cell for UEs in limited service mode.NOTE 2. |
| ***ims-EmergencySupport5GC***  Indicates whether the cell supports IMS emergency bearer services for UEs in limited service mode via 5GC. If absent, IMS emergency call via 5GC is not supported by the network in the cell for UEs in limited service mode. NOTE 2. |
| ***intraFreqReselection***  Used to control cell reselection to intra-frequency cells when the highest ranked cell is barred, or treated as barred by the UE, as specified in TS 36.304 [4].NOTE 2. |
| ***multiBandInfoList***  A list of additional frequency band indicators, as defined in TS 36.101 [42], table 5.5-1, that the cell belongs to. If the UE supports the frequency band in the *freqBandIndicator* field it shall apply that frequency band. Otherwise, the UE shall apply the first listed band which it supports in the *multiBandInfoList* field. If E-UTRAN includes *multiBandInfoList-v9e0* it includes the same number of entries, and listed in the same order, as in *multiBandInfoList* (i.e. without suffix). See Annex D for more descriptions. The UE shall ignore the rule defined in this field description if *freqBandIndicatorPriority*is present and supported by the UE. |
| ***multiBandInfoList-v10j0***  A list of *additionalPmax* and *additionalSpectrumEmission* values, as defined in TS 36.101 [42], table 6.2.4-1, for UEs neither in CE nor BL UEs and TS 36.101 [42], table 6.2.4E-1, for UEs in CE or BL UEs, for the frequency bands in *multiBandInfoList* (i.e. without suffix) and *multiBandInfoList-v9e0*. If E-UTRAN includes *multiBandInfoList-v10j0*, it includes the same number of entries, and listed in the same order, as in *multiBandInfoList* (i.e. without suffix). If E-UTRAN includes *multiBandInfoList-v10l0* it includes the same number of entries, and listed in the same order, as in *multiBandInfoList-v10j0*. |
| ***plmn-IdentityList***  List of PLMN identities. The first listed *PLMN-Identity* is the primary PLMN.If *plmn-IdentityList-v1530* is included, E-UTRAN includes the same number of entries, and listed in the same order, as in *plmn-IdentityList* (without suffix). If *plmn-IdentityList-v1610* is included, E-UTRAN includes the same number of entries, and listed in the same order, as in *plmn-IdentityList-r15*. If *plmn-IdentityList-v1700* is included, E-UTRAN includes the same number of entries, and listed in the same order, as in *plmn-IdentityList* (without suffix). NOTE 2. |
| ***plmn-Index***  Index of the PLMN in the *plmn-IdentityList* fields included in SIB1 for EPC, indicating the same PLMN ID is connected to 5GC. Value 1 indicates the 1st PLMN in the 1st *plmn-IdentityList* included in SIB1, value 2 indicates the 2nd PLMN in the same *plmn-IdentityList*, or when no more PLMNs are present within the same *plmn-IdentityList*, then the PLMN listed 1st in the subsequent *plmn-IdentityList* within the same SIB1 and so on. NOTE 6. |
| ***p-Max***  Value applicable for the cell. If absent the UE applies the maximum power according to its capability as specified in TS 36.101 [42], clause 6.2.2.NOTE 2. This field is ignored by IAB-MT. The IAB-MT applies output power and emissions requirements, as specified in TS 38.174 [107]. |
| ***posSchedulingInfoList-BR***  Indicates additional scheduling information of positioning SI messages for BL UEs and UEs in CE. E-UTRAN always includes this field if *posSchedulingInfoList-r15* is included in *SystemInformationBlockType1-BR*, and includes the same number of entries, and listed in the same order, as in *posSchedulingInfoList-r15*. |
| ***posSIB-MappingInfo***  List of the posSIBs mapped to this *SystemInformation* message. |
| ***posSibType***  The positioning SIB type is defined in TS 36.355 [54]. |
| ***q-QualMin***  Parameter "Qqualmin" in TS 36.304 [4]. If *cellSelectionInfo-v920* is not present, the UE applies the (default) value of negative infinity for Qqualmin. NOTE 1. |
| ***q-QualMinRSRQ-OnAllSymbols***  If this field is present and supported by the UE, the UE shall, when performing RSRQ measurements, perform RSRQ measurement on all OFDM symbols in accordance with TS 36.214 [48]. NOTE 1. |
| ***q-QualMinOffset***  Parameter "Qqualminoffset" in TS 36.304 [4]. Actual value Qqualminoffset = field value [dB]. If *cellSelectionInfo-v920* is not present or the field is not present, the UE applies the (default) value of 0 dB for Qqualminoffset.Affects the minimum required quality level in the cell. |
| ***q-QualMinWB***  If this field is present and supported by the UE, the UE shall, when performing RSRQ measurements, use a wider bandwidth in accordance with TS 36.133 [16]. NOTE 1. |
| ***q-RxLevMinOffset***  Parameter Qrxlevminoffset in TS 36.304 [4]. Actual value Qrxlevminoffset = field value \* 2 [dB]. If absent, the UE applies the (default) value of 0 dB for Qrxlevminoffset*.* Affects the minimum required Rx level in the cell. |
| ***sbas-ID***  The presence of this field indicates that the *posSibType* is for a specific SBAS. |
| ***schedulingInfoList***  Indicates scheduling information of SI messages. The *schedulingInfoList-v12j0* (if present) provides additional SIBs mapped into the SI message scheduled via *schedulingInfoList* (without suffix). If E-UTRAN includes *schedulingInfoList-v12j0*, it includes the same number of entries, and listed in the same order, as in *schedulingInfoList* (without suffix). |
| ***schedulingInfoListExt***  Indicates scheduling information of additional SI messages. The UE concatenates the entries of *schedulingInfoListExt* to the entries in *schedulingInfoList*, according to the general concatenation principles for list extension as defined in 5.1.2. If the *schedulingInfoListExt* is present, E-UTRAN ensures that the total number of entries of this field plus *schedulingInfoList* (without suffix) shall not exceed the value of *maxSI-Message*. |
| ***sib-MappingInfo***  List of the SIBs mapped to this *SystemInformation* message. There is no mapping information of SIB2; it is always present in the first *SystemInformation* message listed in the *schedulingInfoList* (without suffix) list. If present, *sib-MappingInfo-v12j0* indicates one or more additional SIBs mapped to the concerned SI message listed in the *schedulingInfoList* (without suffix) list. If *schedulingInfoList-v12j0* or *schedulingInfoListExt-r12* is present, E-UTRAN does not include any value indicating SIB of type 19 or higher in *sib-MappingInfo* (without suffix). No new SIBs should be added to the IE SIB-Type (without suffix). If *schedulingInfoList-v12j0* is present, E-UTRAN ensures that the total number of entries of this field plus *sib-MappingInfo* (without suffix) shall not exceed the value of *maxSIB-1*. |
| ***si-HoppingConfigCommon***  Frequency hopping activation/deactivation for BR versions of SI messages and MPDCCH/PDSCH of paging. |
| ***si-Narrowband***  This field indicates the index of a narrowband used to broadcast the SI message towards BL UEs and UEs in CE, see TS 36.211 [21], clause 6.4.1 and TS 36.213 [23], clause 7.1.6. Field values (1..*maxAvailNarrowBands-r13*) correspond to narrowband indices (0..*maxAvailNarrowBands-r13*-1) as specified in TS 36.211 [21]. |
| ***si-RepetitionPattern***  Indicates the radio frames within the SI window used for SI message transmission. Value everyRF corresponds to every radio frame, value every2ndRF corresponds to every 2 radio frames, and so on. The first transmission of the SI message is transmitted from the first radio frame of the SI window. |
| ***si-Periodicity, posSI-Periodicity***  Periodicity of the SI-message in radio frames, such that rf8 denotes 8 radio frames, rf16 denotes 16 radio frames, and so on. If the *si-posOffset* is configured, the *posSI-Periodicity* of rf8 cannot be used. |
| ***si-posOffset***  This field, if present and set to *true* indicates that the SI messages in *PosSchedulingInfoList* are scheduled with an offset of 8 radio frames compared to SI messages in *SchedulingInfoList*. *si-posOffset* may be present only if the shortest configured SI message periodicity for SI messages in *SchedulingInfoList* is 80ms. |
| ***si-TBS***  This field indicates the transport block size information used to broadcast the SI message towards BL UEs and UEs in CE, see TS 36.213 [23], Table 7.1.7.2.1-1, for a 6 PRB bandwidth and a QPSK modulation. |
| ***schedulingInfoList-BR***  Indicates additional scheduling information of SI messages for BL UEs and UEs in CE. It includes the same number of entries, and listed in the same order, as in *schedulingInfoList* (without suffix). |
| ***si-ValidityTime***  Indicates system information validity timer. If set to TRUE, the timer is set to 3h, otherwise the timer is set to 24h. |
| ***si-WindowLength, si-WindowLength-BR***  Common SI scheduling window for all SIs. Unit in milliseconds, where ms1 denotes 1 millisecond, ms2 denotes 2 milliseconds and so on. In case s*i-WindowLength-BR-r13* is present and the UE is a BL UE or a UE in CE, the UE shall use s*i-WindowLength-BR-r13* and ignore the original field *si-WindowLength* (without suffix). UEs other than BL UEs or UEs in CE shall ignore the extension field s*i-WindowLength-BR-r13.* |
| ***startSymbolBR***  For BL UEs and UEs in CE, indicates the OFDM starting symbol for any MPDCCH, PDSCH scheduled on the same cell except the PDSCH carrying *SystemInformationBlockType1-BR*, see TS 36.213 [23]. Values 1, 2, and 3 are applicable for *dl-Bandwidth* greater than 10 resource blocks. Values 2, 3, and 4 are applicable otherwise. |
| ***systemInfoValueTagList***  Indicates SI message specific value tags for BL UEs and UEs in CE. It includes the same number of entries, and listed in the same order, as in *schedulingInfoList* (without suffix). |
| ***systemInfoValueTagSI***  SI message specific value tag as specified in clause 5.2.1.3. Common for all SIBs within the SI message other than MIB, SIB1, SIB10, SIB11, SIB12, SIB14 and SIB31. |
| ***systemInfoValueTag***  Common for all SIBs other than MIB, MIB-MBMS, SIB1, SIB1-MBMS, SIB10, SIB11, SIB12, SIB14 and SIB31. Change of MIB, MIB-MBMS, SIB1 and SIB1-MBMS is detected by acquisition of the corresponding message. |
| ***tdd-Config***  Specifies the TDD specific physical channel configurations. NOTE 2. |
| ***trackingAreaCode/trackingAreaCode-5GC***  A *trackingAreaCode* that is common for all the PLMNs listed. NOTE2. NOTE 5. |
| ***trackingAreaList***  A list of tracking area codes for the PLMN listed.  For the first entry in *plmn-IdentityList-v1700*: If this field is present,thelist oftracking area codes include the tracking area code in *trackingAreaCode*andthe tracking area codesin *trackingAreaList*. If this field is absent, *trackingAreaCode* applies.  For other entries in *plmn-IdentityList-v1700*: If this field is present,thelist oftracking area codes include the tracking area codesin *trackingAreaList*. If this field is absent, the list of tracking area codes of the preceding entry in *plmn-IdentityList-v1700* applies.  The total number of signalled tracking area codes across all PLMNs cannot be more than *maxTAC-r17*. | |
| ***transmissionInControlChRegion***  Indicates, for BL UEs and UEs in CE, LTE control channel region may be used for DL broadcast transmission. NOTE 3. |
| ***up-CIoT-5GS-Optimisation***  Indicates whether the UE is allowed to resume the connection with User plane CIoT 5GS optimisation, see TS 24.501 [95]. |

NOTE 1: The value the UE applies for parameter "Qqualmin" in TS 36.304 [4] depends on the *q-QualMin* fields signalled by E-UTRAN and supported by the UE. In case multiple candidate options are available, the UE shall select the highest priority candidate option according to the priority order indicated by the following table (top row is highest priority).

|  |  |  |
| --- | --- | --- |
| q-QualMinRSRQ-OnAllSymbols | q-QualMinWB | Value of parameter "Qqualmin" in TS 36.304 [4] |
| Included | Included | *q-QualMinRSRQ-OnAllSymbols* – (*q-QualMin* – *q-QualMinWB*) |
| Included | Not included | *q-QualMinRSRQ-OnAllSymbols* |
| Not included | Included | *q-QualMinWB* |
| Not included | Not included | *q-QualMin* |

NOTE 2: E-UTRAN sets this field to the same value for all instances of SIB1 message that are broadcasted within the same cell.

NOTE 3: E-UTRAN configures this field only in the BR version of SIB1 message.

NOTE 4: E-UTRAN configures at most 6 EPC PLMNs in total (i.e. across all the PLMN lists except for PLMN lists in *cellAccessRelatedInfoList-5GC* in SIB1). E-UTRAN configures at most 6 5GC PLMNs in total (i.e. across all the PLMN lists in *cellAccessRelatedInfoList-5GC* in SIB1).

NOTE 5: E-UTRAN configures only one value for this parameter per PLMN.

NOTE 6: E-UTRAN configures *plmn-Index* only if the *cellBarred* is set to *notBarred.*

| Conditional presence | Explanation |
| --- | --- |
| *BW-reduced* | The field is optional present, Need OR, if *schedulingInfoSIB1-BR* in MIB is set to a value greater than 0. Otherwise the field is not present. |
| *FBI-max* | The field is mandatory present if *freqBandIndicator* (i.e. without suffix) is set to *maxFBI*. Otherwise the field is not present. |
| *mFBI* | The field is optional present, Need OR, if *multiBandInfoList* is present. Otherwise the field is not present. |
| *mFBI-max* | The field is mandatory present if one or more entries in *multiBandInfoList* (i.e. without suffix, introduced in -v8h0) is set to *maxFBI*. Otherwise the field is not present. |
| *RSRQ* | The field is mandatory present if SIB3 is being broadcast and *threshServingLowQ* is present in SIB3; otherwise optionally present, Need OP. |
| *RSRQ2* | The field is mandatory present if *q-QualMinRSRQ-OnAllSymbols* is present in SIB3; otherwise it is not present and the UE shall delete any existing value for this field. |
| *Hopping* | The field is mandatory present if *si-HoppingConfigCommon* field is broadcasted and set to *on*. Otherwise the field is optionally present, need OP. |
| *QrxlevminCE1* | The field is optionally present, Need OR, if *q-RxLevMinCE1-r13* is set below -140 dBm. Otherwise the field is not present. |
| *TDD* | This field is mandatory present for TDD; it is not present for FDD and the UE shall delete any existing value for this field. |
| *TDD-OR* | The field is optional present for TDD, need OR; it is not present for FDD. |
| *WB-RSRQ* | The field is optionally present, need OP if the measurement bandwidth indicated by *allowedMeasBandwidth* in *systemInformationBlockType3* is 50 resource blocks or larger; otherwise it is not present. |
| *SI-BR* | The field is mandatory present if *schedulingInfoSIB1-BR* is included in MIB with a value greater than 0. Otherwise the field is not present. |

#### – *UEInformationResponse*

The *UEInformationResponse* message is used by the UE to transfer the information requested by the E-UTRAN.

Signalling radio bearer: SRB1 or SRB2 (when logged measurement information is included)

RLC-SAP: AM

Logical channel: DCCH

Direction: UE to E-UTRAN

*UEInformationResponse message*

-- ASN1START

UEInformationResponse-r9 ::= SEQUENCE {

rrc-TransactionIdentifier RRC-TransactionIdentifier,

criticalExtensions CHOICE {

c1 CHOICE {

ueInformationResponse-r9 UEInformationResponse-r9-IEs,

spare3 NULL, spare2 NULL, spare1 NULL

},

criticalExtensionsFuture SEQUENCE {}

}

}

UEInformationResponse-r9-IEs ::= SEQUENCE {

rach-Report-r9 RACH-Report-r16 OPTIONAL,

rlf-Report-r9 RLF-Report-r9 OPTIONAL,

nonCriticalExtension UEInformationResponse-v930-IEs OPTIONAL

}

-- Late non critical extensions

UEInformationResponse-v9e0-IEs ::= SEQUENCE {

rlf-Report-v9e0 RLF-Report-v9e0 OPTIONAL,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- Regular non critical extensions

UEInformationResponse-v930-IEs ::= SEQUENCE {

lateNonCriticalExtension OCTET STRING (CONTAINING UEInformationResponse-v9e0-IEs) OPTIONAL,

nonCriticalExtension UEInformationResponse-v1020-IEs OPTIONAL

}

UEInformationResponse-v1020-IEs ::= SEQUENCE {

logMeasReport-r10 LogMeasReport-r10 OPTIONAL,

nonCriticalExtension UEInformationResponse-v1130-IEs OPTIONAL

}

UEInformationResponse-v1130-IEs ::= SEQUENCE {

connEstFailReport-r11 ConnEstFailReport-r11 OPTIONAL,

nonCriticalExtension UEInformationResponse-v1250-IEs OPTIONAL

}

UEInformationResponse-v1250-IEs ::= SEQUENCE {

mobilityHistoryReport-r12 MobilityHistoryReport-r12 OPTIONAL,

nonCriticalExtension UEInformationResponse-v1530-IEs OPTIONAL

}

UEInformationResponse-v1530-IEs ::= SEQUENCE {

measResultListIdle-r15 MeasResultListIdle-r15 OPTIONAL,

flightPathInfoReport-r15 FlightPathInfoReport-r15 OPTIONAL,

nonCriticalExtension UEInformationResponse-v1610-IEs OPTIONAL

}

UEInformationResponse-v1610-IEs ::= SEQUENCE {

rach-Report-v1610 RACH-Report-v1610 OPTIONAL,

measResultListExtIdle-r16 MeasResultListExtIdle-r16 OPTIONAL,

measResultListIdleNR-r16 MeasResultListIdleNR-r16 OPTIONAL,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

RACH-Report-r16 ::= SEQUENCE {

numberOfPreamblesSent-r16 NumberOfPreamblesSent-r11,

contentionDetected-r16 BOOLEAN

}

RACH-Report-v1610 ::= SEQUENCE {

initialCEL-r16 INTEGER (0..3),

edt-Fallback-r16 BOOLEAN

}

RLF-Report-r9 ::= SEQUENCE {

measResultLastServCell-r9 SEQUENCE {

rsrpResult-r9 RSRP-Range,

rsrqResult-r9 RSRQ-Range OPTIONAL

},

measResultNeighCells-r9 SEQUENCE {

measResultListEUTRA-r9 MeasResultList2EUTRA-r9 OPTIONAL,

measResultListUTRA-r9 MeasResultList2UTRA-r9 OPTIONAL,

measResultListGERAN-r9 MeasResultListGERAN OPTIONAL,

measResultsCDMA2000-r9 MeasResultList2CDMA2000-r9 OPTIONAL

} OPTIONAL,

...,

[[ locationInfo-r10 LocationInfo-r10 OPTIONAL,

failedPCellId-r10 CHOICE {

cellGlobalId-r10 CellGlobalIdEUTRA,

pci-arfcn-r10 SEQUENCE {

physCellId-r10 PhysCellId,

carrierFreq-r10 ARFCN-ValueEUTRA

}

} OPTIONAL,

reestablishmentCellId-r10 CellGlobalIdEUTRA OPTIONAL,

timeConnFailure-r10 INTEGER (0..1023) OPTIONAL,

connectionFailureType-r10 ENUMERATED {rlf, hof} OPTIONAL,

previousPCellId-r10 CellGlobalIdEUTRA OPTIONAL

]],

[[ failedPCellId-v1090 SEQUENCE {

carrierFreq-v1090 ARFCN-ValueEUTRA-v9e0

} OPTIONAL

]],

[[ basicFields-r11 SEQUENCE {

c-RNTI-r11 C-RNTI,

rlf-Cause-r11 ENUMERATED {

t310-Expiry, randomAccessProblem,

rlc-MaxNumRetx, t312-Expiry-r12},

timeSinceFailure-r11 TimeSinceFailure-r11

} OPTIONAL,

previousUTRA-CellId-r11 SEQUENCE {

carrierFreq-r11 ARFCN-ValueUTRA,

physCellId-r11 CHOICE {

fdd-r11 PhysCellIdUTRA-FDD,

tdd-r11 PhysCellIdUTRA-TDD

},

cellGlobalId-r11 CellGlobalIdUTRA OPTIONAL

} OPTIONAL,

selectedUTRA-CellId-r11 SEQUENCE {

carrierFreq-r11 ARFCN-ValueUTRA,

physCellId-r11 CHOICE {

fdd-r11 PhysCellIdUTRA-FDD,

tdd-r11 PhysCellIdUTRA-TDD

}

} OPTIONAL

]],

[[ failedPCellId-v1250 SEQUENCE {

tac-FailedPCell-r12 TrackingAreaCode

} OPTIONAL,

measResultLastServCell-v1250 RSRQ-Range-v1250 OPTIONAL,

lastServCellRSRQ-Type-r12 RSRQ-Type-r12 OPTIONAL,

measResultListEUTRA-v1250 MeasResultList2EUTRA-v1250 OPTIONAL

]],

[[ drb-EstablishedWithQCI-1-r13 ENUMERATED {qci1} OPTIONAL

]],

[[ measResultLastServCell-v1360 RSRP-Range-v1360 OPTIONAL

]],

[[ logMeasResultListBT-r15 LogMeasResultListBT-r15 OPTIONAL,

logMeasResultListWLAN-r15 LogMeasResultListWLAN-r15 OPTIONAL

]],

[[ measResultListNR-r16 MeasResultCellListNR-r15 OPTIONAL,

previousNR-PCellId-r16 CellGlobalIdNR-r16 OPTIONAL,

failedNR-PCellId-r16 CHOICE {

cellGlobalId CellGlobalIdNR-r16,

pci-arfcn SEQUENCE {

physCellId-r16 PhysCellIdNR-r15,

carrierFreq-r16 ARFCN-ValueNR-r15

}

} OPTIONAL,

reconnectCellId-r16 CHOICE {

nrReconnectCellId CellGlobalIdNR-r16,

eutraReconnectCellId SEQUENCE {

cellGlobalId-r16 CellGlobalIdEUTRA,

trackingAreaCode-EPC-r16 TrackingAreaCode OPTIONAL,

trackingAreaCode-5GC-r16 TrackingAreaCode-5GC-r15 OPTIONAL

}

} OPTIONAL,

timeUntilReconnection-r16 TimeUntilReconnection-r16 OPTIONAL

]],

[[ measResultListNR-v1640 SEQUENCE {

carrierFreqNR-r16 ARFCN-ValueNR-r15

} OPTIONAL,

measResultListExtNR-r16 MeasResultFreqListNR-r16 OPTIONAL

]]

}

RLF-Report-v9e0 ::= SEQUENCE {

measResultListEUTRA-v9e0 MeasResultList2EUTRA-v9e0

}

MeasResultList2EUTRA-r9 ::= SEQUENCE (SIZE (1..maxFreq)) OF MeasResult2EUTRA-r9

MeasResultList2EUTRA-v9e0 ::= SEQUENCE (SIZE (1..maxFreq)) OF MeasResult2EUTRA-v9e0

MeasResultList2EUTRA-v1250 ::= SEQUENCE (SIZE (1..maxFreq)) OF MeasResult2EUTRA-v1250

MeasResult2EUTRA-r9 ::= SEQUENCE {

carrierFreq-r9 ARFCN-ValueEUTRA,

measResultList-r9 MeasResultListEUTRA

}

MeasResult2EUTRA-v9e0 ::= SEQUENCE {

carrierFreq-v9e0 ARFCN-ValueEUTRA-v9e0 OPTIONAL

}

MeasResult2EUTRA-v1250 ::= SEQUENCE {

rsrq-Type-r12 RSRQ-Type-r12 OPTIONAL

}

MeasResultList2UTRA-r9 ::= SEQUENCE (SIZE (1..maxFreq)) OF MeasResult2UTRA-r9

MeasResult2UTRA-r9 ::= SEQUENCE {

carrierFreq-r9 ARFCN-ValueUTRA,

measResultList-r9 MeasResultListUTRA

}

MeasResultList2CDMA2000-r9 ::= SEQUENCE (SIZE (1..maxFreq)) OF MeasResult2CDMA2000-r9

MeasResult2CDMA2000-r9 ::= SEQUENCE {

carrierFreq-r9 CarrierFreqCDMA2000,

measResultList-r9 MeasResultsCDMA2000

}

LogMeasReport-r10 ::= SEQUENCE {

absoluteTimeStamp-r10 AbsoluteTimeInfo-r10,

traceReference-r10 TraceReference-r10,

traceRecordingSessionRef-r10 OCTET STRING (SIZE (2)),

tce-Id-r10 OCTET STRING (SIZE (1)),

logMeasInfoList-r10 LogMeasInfoList-r10,

logMeasAvailable-r10 ENUMERATED {true} OPTIONAL,

...,

[[ logMeasAvailableBT-r15 ENUMERATED {true} OPTIONAL,

logMeasAvailableWLAN-r15 ENUMERATED {true} OPTIONAL

]]

}

LogMeasInfoList-r10 ::= SEQUENCE (SIZE (1..maxLogMeasReport-r10)) OF LogMeasInfo-r10

LogMeasInfo-r10 ::= SEQUENCE {

locationInfo-r10 LocationInfo-r10 OPTIONAL,

relativeTimeStamp-r10 INTEGER (0..7200),

servCellIdentity-r10 CellGlobalIdEUTRA,

measResultServCell-r10 SEQUENCE {

rsrpResult-r10 RSRP-Range,

rsrqResult-r10 RSRQ-Range

},

measResultNeighCells-r10 SEQUENCE {

measResultListEUTRA-r10 MeasResultList2EUTRA-r9 OPTIONAL,

measResultListUTRA-r10 MeasResultList2UTRA-r9 OPTIONAL,

measResultListGERAN-r10 MeasResultList2GERAN-r10 OPTIONAL,

measResultListCDMA2000-r10 MeasResultList2CDMA2000-r9 OPTIONAL

} OPTIONAL,

...,

[[ measResultListEUTRA-v1090 MeasResultList2EUTRA-v9e0 OPTIONAL

]],

[[ measResultListMBSFN-r12 MeasResultListMBSFN-r12 OPTIONAL,

measResultServCell-v1250 RSRQ-Range-v1250 OPTIONAL,

servCellRSRQ-Type-r12 RSRQ-Type-r12 OPTIONAL,

measResultListEUTRA-v1250 MeasResultList2EUTRA-v1250 OPTIONAL

]],

[[ inDeviceCoexDetected-r13 ENUMERATED {true} OPTIONAL

]],

[[ measResultServCell-v1360 RSRP-Range-v1360 OPTIONAL

]],

[[ logMeasResultListBT-r15 LogMeasResultListBT-r15 OPTIONAL,

logMeasResultListWLAN-r15 LogMeasResultListWLAN-r15 OPTIONAL

]],

[[ anyCellSelectionDetected-r15 ENUMERATED {true} OPTIONAL

]],

[[ measResultListNR-r16 MeasResultCellListNR-r15 OPTIONAL

]],

[[ measResultListNR-v1640 SEQUENCE {

carrierFreqNR-r16 ARFCN-ValueNR-r15

} OPTIONAL,

measResultListExtNR-r16 MeasResultFreqListNR-r16 OPTIONAL

]],

[[ uncomBarPreMeasResult-r17 OCTET STRING OPTIONAL

]]

}

MeasResultListMBSFN-r12 ::= SEQUENCE (SIZE (1..maxMBSFN-Area)) OF MeasResultMBSFN-r12

MeasResultMBSFN-r12 ::= SEQUENCE {

mbsfn-Area-r12 SEQUENCE {

mbsfn-AreaId-r12 MBSFN-AreaId-r12,

carrierFreq-r12 ARFCN-ValueEUTRA-r9

},

rsrpResultMBSFN-r12 RSRP-Range,

rsrqResultMBSFN-r12 MBSFN-RSRQ-Range-r12,

signallingBLER-Result-r12 BLER-Result-r12 OPTIONAL,

dataBLER-MCH-ResultList-r12 DataBLER-MCH-ResultList-r12 OPTIONAL,

...

}

DataBLER-MCH-ResultList-r12 ::= SEQUENCE (SIZE (1.. maxPMCH-PerMBSFN)) OF DataBLER-MCH-Result-r12

DataBLER-MCH-Result-r12 ::= SEQUENCE {

mch-Index-r12 INTEGER (1..maxPMCH-PerMBSFN),

dataBLER-Result-r12 BLER-Result-r12

}

BLER-Result-r12 ::= SEQUENCE {

bler-r12 BLER-Range-r12,

blocksReceived-r12 SEQUENCE {

n-r12 BIT STRING (SIZE (3)),

m-r12 BIT STRING (SIZE (8))

}

}

BLER-Range-r12 ::= INTEGER(0..31)

MeasResultList2GERAN-r10 ::= SEQUENCE (SIZE (1..maxCellListGERAN)) OF MeasResultListGERAN

MeasResultFreqListNR-r16::= SEQUENCE (SIZE (1..maxFreq-1-r16)) OF MeasResultFreqFailNR-r15

ConnEstFailReport-r11 ::= SEQUENCE {

failedCellId-r11 CellGlobalIdEUTRA,

locationInfo-r11 LocationInfo-r10 OPTIONAL,

measResultFailedCell-r11 SEQUENCE {

rsrpResult-r11 RSRP-Range,

rsrqResult-r11 RSRQ-Range OPTIONAL

},

measResultNeighCells-r11 SEQUENCE {

measResultListEUTRA-r11 MeasResultList2EUTRA-r9 OPTIONAL,

measResultListUTRA-r11 MeasResultList2UTRA-r9 OPTIONAL,

measResultListGERAN-r11 MeasResultListGERAN OPTIONAL,

measResultsCDMA2000-r11 MeasResultList2CDMA2000-r9 OPTIONAL

} OPTIONAL,

numberOfPreamblesSent-r11 NumberOfPreamblesSent-r11,

contentionDetected-r11 BOOLEAN,

maxTxPowerReached-r11 BOOLEAN,

timeSinceFailure-r11 TimeSinceFailure-r11,

measResultListEUTRA-v1130 MeasResultList2EUTRA-v9e0 OPTIONAL,

...,

[[ measResultFailedCell-v1250 RSRQ-Range-v1250 OPTIONAL,

failedCellRSRQ-Type-r12 RSRQ-Type-r12 OPTIONAL,

measResultListEUTRA-v1250 MeasResultList2EUTRA-v1250 OPTIONAL

]],

[[ measResultFailedCell-v1360 RSRP-Range-v1360 OPTIONAL

]],

[[ logMeasResultListBT-r15 LogMeasResultListBT-r15 OPTIONAL,

logMeasResultListWLAN-r15 LogMeasResultListWLAN-r15 OPTIONAL

]],

[[ measResultListNR-r16 MeasResultCellListNR-r15 OPTIONAL

]],

[[ measResultListNR-v1640 SEQUENCE {

carrierFreqNR-r16 ARFCN-ValueNR-r15

} OPTIONAL,

measResultListExtNR-r16 MeasResultFreqListNR-r16 OPTIONAL

]]

}

NumberOfPreamblesSent-r11::= INTEGER (1..200)

TimeSinceFailure-r11 ::= INTEGER (0..172800)

TimeUntilReconnection-r16 ::= INTEGER (0..172800)

MobilityHistoryReport-r12 ::= VisitedCellInfoList-r12

FlightPathInfoReport-r15 ::= SEQUENCE {

flightPath-r15 SEQUENCE (SIZE (1..maxWayPoint-r15)) OF WayPointLocation-r15 OPTIONAL,

dummy SEQUENCE {} OPTIONAL

}

WayPointLocation-r15 ::= SEQUENCE {

wayPointLocation-r15 LocationInfo-r10,

timeStamp-r15 AbsoluteTimeInfo-r10 OPTIONAL

}

-- ASN1STOP

| *UEInformationResponse* field descriptions |
| --- |
| ***absoluteTimeStamp***  Indicates the absolute time when the logged measurement configuration logging is provided, as indicated by E-UTRAN within *absoluteTimeInfo*. |
| ***anyCellSelectionDetected***  This field is used to indicate the detection of *any cell selection* state, as defined in TS 36.304 [4]. The UE sets this field when performing the logging of measurement results in RRC\_IDLE and there is no suitable cell or no acceptable cell. |
| ***bler***  Indicates the measured BLER value. The coding of BLER value is defined in TS 36.133 [16]. |
| ***blocksReceived***  Indicates total number of MCH blocks, which were received by the UE and used for the corresponding BLER calculation, within the measurement period as defined in TS 36.133 [16]. |
| ***carrierFreq***  In case the UE includes *carrierFreq-v9e0* and/ or *carrierFreq-v1090*, the UE shall set the corresponding entry of *carrierFreq-r9* and/ or *carrierFreq-r10* respectively to *maxEARFCN*. For E-UTRA and UTRA frequencies, the UE sets the ARFCN according to the band used when obtaining the concerned measurement results. |
| ***carrierFreqNR***  In case the UE includes *measResultListNR*, the UE uses this field to indicate the ARFCN value according to the band used when obtaining the concrned measurement results |
| ***connectionFailureType***  This field is used to indicate whether the connection failure is due to radio link failure or handover failure. |
| ***contentionDetected***  This field is used to indicate that contention was detected for at least one of the transmitted preambles, see TS 36.321 [6]. |
| ***c-RNTI***  This field indicates the C-RNTI used in the PCell upon detecting radio link failure or the C-RNTI used in the source PCell upon handover failure. |
| ***dataBLER-MCH-ResultList***  Includes a BLER result per MCH on subframes using *dataMCS*, with the applicable MCH(s) listed in the same order as in *pmch-InfoList* within *MBSFNAreaConfiguration*. |
| ***drb-EstablishedWithQCI-1***  This field is used to indicate the radio link failure occurred while a bearer with QCI value equal to 1 was configured, see TS 24.301 [35]. |
| ***dummy***  This field is not used in the specification. It shall not be sent by the UE. |
| ***edt-Fallback***  Value TRUE indicates the last successfully completed random access procedure was initiated with EDT PRACH resource and succeeded after receiving EDT fallback indication from lower layers. |
| ***failedCellId***  This field is used to indicate the cell in which connection establishment failed. |
| ***failedPCellId***  This field is used to indicate the PCell in which RLF is detected or the target PCell of the failed handover. The UE sets the EARFCN according to the band used for transmission/ reception when the failure occurred. |
| ***inDeviceCoexDetected***  Indicates that measurement logging is suspended due to IDC problem detection. |
| ***initialCEL***  Indicates the initial CE level used for the last successfully completed random access procedure for BL UEs and UEs in CE. |
| ***logMeasResultListBT***  This field refers to the Bluetooth measurement results. |
| ***logMeasResultListWLAN***  This field refers to the WLAN measurement results. |
| ***maxTxPowerReached***  This field is used to indicate whether or not the maximum power level was used for the last transmitted preamble, see TS 36.321 [6]. |
| ***mch-Index***  Indicates the MCH by referring to the entry as listed in *pmch-InfoList* within *MBSFNAreaConfiguration*. |
| ***measResultFailedCell***  This field refers to the last measurement results taken in the cell, where connection establishment failure happened. For UE supporting CE Mode B, when CE mode B is not restricted by upper layers, *measResultFailedCell-v1360* is reported if the measured RSRP is less than -140 dBm. |
| ***measResultLastServCell***  This field refers to the last measurement results taken in the PCell, where radio link failure or handover failure happened. For BL UEs or UEs in CE, when operating in CE Mode B, *measResultLastServCell-v1360* is reported if the measured RSRP is less than -140 dBm. |
| ***measResultListEUTRA***  If *measResultListEUTRA-v9e0*, *measResultListEUTRA-v1090* or *measResultListEUTRA-v1130* is included, the UE shall include the same number of entries, and listed in the same order, as in *measResultListEUTRA-r9*, *measResultListEUTRA-r10* and/ or *measResultListEUTRA-r11* respectively. |
| ***measResultListEUTRA-v1250***  If included in *RLF-Report-r9* the UE shall include the same number of entries, and listed in the same order, as in *measResultListEUTRA-r9*;  If included in *LogMeasInfo-r10* the UE shall include the same number of entries, and listed in the same order, as in *measResultListEUTRA-r10*;  If included in *ConnEstFailReport-r11* the UE shall include the same number of entries, and listed in the same order, as in *measResultListEUTRA-r11*; |
| ***measResultListIdle***  This field indicates the E-UTRA measurement results done during RRC\_IDLE and RRC\_INACTIVE at network request. |
| ***measResultListIdleNR***  This field indicates the NR measurement results done during RRC\_IDLE and RRC\_INACTIVE at network request. |
| ***measResultListNR, measResultListExtNR***  Includes NR measurement results, with *measResultListNR* including results of a first NR frequency and *measResultListExtNR* including results of additinal NR frequencies, if available. |
| ***measResultServCell***  This field refers to the log measurement results taken in the Serving cell. For UE supporting CE Mode B, when CE mode B is not restricted by upper layers, *measResultServCell-v1360* is reported if the measured RSRP is less than -140 dBm. |
| ***mobilityHistoryReport***  This field is used to indicate the time of stay in 16 most recently visited E-UTRA cells or of stay out of E-UTRA. |
| ***numberOfPreamblesSent***  This field is used to indicate the number of RACH preambles that were transmitted. Corresponds to parameter PREAMBLE\_TRANSMISSION\_COUNTER in TS 36.321 [6]. |
| ***previousPCellId***  This field is used to indicate the source PCell of the last handover (source PCell when the last *RRCConnectionReconfiguration* message including *mobilityControlInfo* was received). |
| ***previousUTRA-CellId***  This field is used to indicate the source UTRA cell of the last successful handover to E-UTRAN, when RLF occurred at the target PCell. The UE sets the ARFCN according to the band used for transmission/ reception on the concerned cell. |
| ***reconnectCellId***  This field is used to indicate the cell in which the UE comes back to connected after connection failure and after failing to perform reestablishment. If the UE comes back to RRC CONNECTED in an NR cell then *nrReconnectCellID* is included and if the UE comes back to RRC CONNECTED in an LTE cell then *eutraReconnectCellID* is included. |
| ***reestablishmentCellId***  This field is used to indicate the cell in which the re-establishment attempt was made after connection failure. |
| ***relativeTimeStamp***  Indicates the time of logging measurement results, measured relative to the *absoluteTimeStamp*. Value in seconds. |
| ***rlf-Cause***  This field is used to indicate the cause of the last radio link failure that was detected. In case of handover failure information reporting (i.e., the *connectionFailureType* is set to '*hof*'), the UE is allowed to set this field to any value. |
| ***selectedUTRA-CellId***  This field is used to indicate the UTRA cell that the UE selects after RLF is detected, while T311 is running. The UE sets the ARFCN according to the band selected for transmission/ reception on the concerned cell. |
| ***signallingBLER-Result***  Includes a BLER result of MBSFN subframes using *signallingMCS*. |
| ***tac-FailedPCell***  This field is used to indicate the Tracking Area Code of the PCell in which RLF is detected. |
| ***tce-Id***  Parameter Trace Collection Entity Id: See TS 32.422 [58]. |
| ***timeConnFailure***  This field is used to indicate the time elapsed since the last HO initialization until connection failure. Actual value = field value \* 100ms. The maximum value 1023 means 102.3s or longer. |
| ***timeSinceFailure***  This field is used to indicate the time that elapsed since the connection (establishment) failure. Value in seconds. The maximum value 172800 means 172800s or longer. |
| ***timeStamp***  Includes time stamps for the waypoints that describe planned locations for the UE. |
| ***timeUntilReconnection***  This field is used to indicate the time that elapsed between the connection (radio link or handover) failure and the next time the UE comes to RRC CONNECTED in an NR or EUTRA cell, after failing to perform reestablishment. Value in seconds. The maximum value 172800 means 172800s or longer. |
| ***traceRecordingSessionRef***  Parameter Trace Recording Session Reference: See TS 32.422 [58]. |
| ***uncomBarPreMeasResult***  This field provides barometric pressure measurements as *Sensor-MeasurementInformation* defined in TS 37.355 [109]. The first/leftmost bit of the first octet contains the most significant bit. |
| ***wayPointLocation***  Includes location coordinates for a UE for Aerial UE operation. The waypoints describe planned locations for the UE. |

### 6.3.1 System information blocks

#### – *SystemInformationBlockType24*

The IE *SystemInformationBlockType24* contains information relevant for inter-RAT cell re-selection (i.e. information about NR frequencies and NR neighbouring cells relevant for cell re-selection), which can also be used for NR idle/inactive measurements. The IE includes cell re-selection parameters common for a frequency.

*SystemInformationBlockType24* information element

-- ASN1START

SystemInformationBlockType24-r15 ::= SEQUENCE {

carrierFreqListNR-r15 CarrierFreqListNR-r15 OPTIONAL, -- Need OR

t-ReselectionNR-r15 T-Reselection,

t-ReselectionNR-SF-r15 SpeedStateScaleFactors OPTIONAL, -- Need OR

lateNonCriticalExtension OCTET STRING OPTIONAL,

...,

[[ carrierFreqListNR-v1610 CarrierFreqListNR-v1610 OPTIONAL -- Need OR

]],

[[ carrierFreqListNR-v1700 CarrierFreqListNR-v1700 OPTIONAL -- Need OR

]]

}

CarrierFreqListNR-r15 ::= SEQUENCE (SIZE (1..maxFreq)) OF CarrierFreqNR-r15

CarrierFreqListNR-v1610 ::= SEQUENCE (SIZE (1..maxFreq)) OF CarrierFreqNR-v1610

CarrierFreqListNR-v1700 ::= SEQUENCE (SIZE (1..maxFreq)) OF CarrierFreqNR-v1700

CarrierFreqNR-r15 ::= SEQUENCE {

carrierFreq-r15 ARFCN-ValueNR-r15,

multiBandInfoList-r15 MultiFrequencyBandListNR-r15 OPTIONAL, -- Need OR

multiBandInfoListSUL-r15 MultiFrequencyBandListNR-r15 OPTIONAL, -- Need OR

measTimingConfig-r15 MTC-SSB-NR-r15 OPTIONAL, -- Need OR

subcarrierSpacingSSB-r15 ENUMERATED {kHz15, kHz30, kHz120, kHz240},

ss-RSSI-Measurement-r15 SS-RSSI-Measurement-r15 OPTIONAL, -- Cond RSRQ2

cellReselectionPriority-r15 CellReselectionPriority OPTIONAL, -- Need OP

cellReselectionSubPriority-r15 CellReselectionSubPriority-r13 OPTIONAL, -- Need OR

threshX-High-r15 ReselectionThreshold,

threshX-Low-r15 ReselectionThreshold,

threshX-Q-r15 SEQUENCE {

threshX-HighQ-r15 ReselectionThresholdQ-r9,

threshX-LowQ-r15 ReselectionThresholdQ-r9

} OPTIONAL, -- Cond RSRQ

q-RxLevMin-r15 INTEGER (-70..-22),

q-RxLevMinSUL-r15 INTEGER (-70..-22) OPTIONAL, -- Need OR

p-MaxNR-r15 P-MaxNR-r15,

ns-PmaxListNR-r15 NS-PmaxListNR-r15 OPTIONAL, -- Need OR

q-QualMin-r15 INTEGER (-43..-12) OPTIONAL, -- Need OP

deriveSSB-IndexFromCell-r15 BOOLEAN,

maxRS-IndexCellQual-r15 MaxRS-IndexCellQualNR-r15 OPTIONAL, -- Need OR

threshRS-Index-r15 ThresholdListNR-r15 OPTIONAL, -- Need OR

...,

[[ multiBandNsPmaxListNR-v1550 MultiBandNsPmaxListNR-1-v1550 OPTIONAL, -- Need OR

multiBandNsPmaxListNR-SUL-v1550 MultiBandNsPmaxListNR-v1550 OPTIONAL, -- Need OR

ssb-ToMeasure-r15 SSB-ToMeasure-r15 OPTIONAL -- Need OR

]]

}

CarrierFreqNR-v1610 ::= SEQUENCE {

smtc2-LP-r16 MTC-SSB2-LP-NR-r16 OPTIONAL, -- Need OR

ssb-PositionQCL-CommonNR-r16 SSB-PositionQCL-RelationNR-r16 OPTIONAL, -- Cond SharedSpectrum2

allowedCellListNR-r16 AllowedCellListNR-r16 OPTIONAL, -- Cond SharedSpectrum

highSpeedCarrierNR-r16 ENUMERATED {true} OPTIONAL -- Need OR

}

CarrierFreqNR-v1700 ::= SEQUENCE {

nr-FreqNeighHSDN-CellList-r17 NR-FreqNeighHSDN-CellList-r17 OPTIONAL -- Need OR

}

MultiBandNsPmaxListNR-1-v1550 ::= SEQUENCE (SIZE (1.. maxMultiBandsNR-1-r15)) OF NS-PmaxListNR-r15

MultiBandNsPmaxListNR-v1550 ::= SEQUENCE (SIZE (1.. maxMultiBandsNR-r15)) OF NS-PmaxListNR-r15

AllowedCellListNR-r16 ::= SEQUENCE (SIZE (1..maxCellAllowedNR-r16)) OF PhysCellIdNR-r15

NR-FreqNeighHSDN-CellList-r17 ::= SEQUENCE (SIZE (1..maxCellNR-r17)) OF PhysCellIdRangeNR-r16

-- ASN1STOP

| *SystemInformationBlockType24* field descriptions |
| --- |
| ***allowedCellListNR***  List of allow-listed neighbouring NR cells. |
| ***carrierFreqListNR***  List of carrier frequencies of NR carriers. These frequencies correspond to GSCN values as specified in TS 38.101 [85]. If the *carrierFreqListNR-v1610* is present, it contains the same number of entries, listed in the same order as in the *carrierFreqListNR* (without suffix). |
| ***cellReselectionPriority***  The field concerns the absolute priority of the concerned carrier frequency as used by the cell reselection procedure. Corresponds with parameter "priority" in TS 36.304 [4]. |
| ***deriveSSB-IndexFromCell***  The field indicates whether the UE may use, to derive the SSB index of a cell on the indicated SSB frequency and subcarrier spacing, the timing of any detected cell with the same SSB frequency and subcarrier spacing. If this field is set to TRUE, the UE assumes SFN and frame boundary alignment across cells on the same NR carrier frequency as specified in TS 36.133 [16]. |
| ***highSpeedCarrierNR***  If the field is present, the UE shall apply the enhanced inter-RAT NR measurement requirements to support high speed up to 500 km/h as specified in TS 36.133 [16] to the NR carrier. |
| ***maxRS-IndexCellQual***  Number of SS blocks to average for cell measurement derivation. Corresponds to the parameter *nrofSS-BlocksToAverage* in TS 38.304 [92]. |
| ***measTimingConfig***  Used to configure measurement timing configurations, i.e., timing occasions at which the UE measures SSBs. If the field is absent, the UE assumes that SSB periodicity is 5ms in this frequency. |
| ***multiBandInfoList***  Indicates the list of frequency bands for which the NR cell reselection parameters apply. The UE shall select the first listed band which it supports in the *multiBandInfoList* field to represent the NR neighbour carrier frequency. The network always includes this field. |
| ***multiBandInfoListSUL***  Indicates the list of frequency bands for which the NR cell reselection parameters apply. The UE shall select the first listed band which it supports in the *multiBandInfoListSUL* field to represent the NR neighbour carrier frequency. |
| ***multiBandNsPmaxListNR***  Indicates the *NS-PmaxListNR* configuration for the NR frequency band(s) listed in *multiBandInfoList*. The first entry corresponds to the second listed band in *multiBandInfoList*, and second entry corresponds to the third listed band in *multiBandInfoList*, and so on. |
| ***multiBandNsPmaxListNR-SUL***  Indicates the *NS-PmaxListNR* configuration for the NR SUL frequency band(s) listed in *multiBandInfoListSUL*. The first entry corresponds to the first listed band in *multiBandInfoListSUL*, and second entry corresponds to the second listed band in *multiBandInfoListSUL*, and so on. |
| ***nr-FreqNeighHSDN-CellList***  List of neighbouring NR HSDN cells as specified in TS 38.304 [92]. |
| ***ns-PmaxListNR***  Indicates a list of *additionalPmax* and *additionalSpectrumEmission*, corresponds to the first listed band in the *multiBandInfoList*. |
| ***p-MaxNR***  Indicates the maximum power for NR (see TS 38.104 [91]) the UE can use in NR SCG. |
| ***q-QualMin***  Parameter "Qqualmin" in TS 36.304 [4], applicable for NR neighbour cells. If the field is not present, the UE applies the (default) value of negative infinity for Qqualmin. The actual value Qqualmin = field value [dB]. |
| ***q-RxLevMin***  Parameter "Qrxlevmin" in TS 38.304 [92], applicable for NR neighbour cells. The actual value Qrxlevmin = field value \* 2 [dBm]. |
| ***q-RxLevMinSUL***  Parameter "Qrxlevmin" in TS 38.304 [92], applicable for NR neighbouring cells. The actual value Qrxlevmin = field value \* 2 [dBm]. |
| ***smtc2-LP***  Measurement timing configuration for inter-RAT neighbour cells in NR with a Long Periodicity (LP) indicated by periodicity in *smtc2-LP*. The timing offset and duration are equal to the offset and duration indicated in *measTimingConfig* in *CarrierFreqNR*. The periodicity in *smtc2-LP* can only be set to a value strictly larger than the periodicity in *measTimingConfig* in *CarrierFreqNR* (e.g. if *measTimingConfig* indicates sf20 the Long Periodicity can only be set to sf40, sf80 or sf160, if *measTimingConfig* indicates sf160, *smtc2-LP* cannot be configured). The *pci-List*, if present, includes the physical cell identities of the inter-RAT neighbour cells with Long Periodicity. If *smtc2-LP* is absent, the UE assumes that there are no inter-RAT neighbour cells with a Long Periodicity. |
| ***ssb-PositionQCL-CommonNR***  Indicates the QCL relationship between SS/PBCH blocks for NR neighbor cells on the indicated frequency as specified in TS 38.213 [88], clause 4.1. |
| ***ssb-ToMeasure***  The set of SS blocks to be measured within the SMTC measurement duration (see TS 38.215 [89]). When the field is absent the UE measures on all SS-blocks. |
| ***ss-RSSI-Measurements***  Indicates the SSB-based RSSI measurement configuration. If the field is absent, the UE behaviour is defined in TS 38.215 [89], clause 5.1.3. |
| ***threshRS-Index***  List of thresholds for consolidation of L1 measurements per RS index. Corresponds to the parameter *absThreshSS-BlocksConsolidation* in TS 38.304 [92]. |
| ***threshX-High***  Parameter "ThreshX, HighP" in TS 36.304 [4]. |
| ***threshX-HighQ***  Parameter "ThreshX, HighQ" in TS 36.304 [4]. |
| ***threshX-Low***  Parameter "ThreshX, LowP" in TS 36.304 [4]. |
| ***threshX-LowQ***  Parameter "ThreshX, LowQ" in TS 36.304 [4]. |
| ***t-ReselectionNR***  Parameter "TreselectionNR" in TS 36.304 [4]. |
| ***t-ReselectionNR-SF***  Parameter "Speed dependent ScalingFactor for TreselectionNR" in TS 36.304 [4]. If the field is not present, the UE behaviour is specified in TS 36.304 [4]. |

| Conditional presence | Explanation |
| --- | --- |
| *RSRQ* | The field is mandatory present if the *threshServingLowQ* is present in *systemInformationBlockType3*; otherwise it is not present. |
| *RSRQ2* | The field is optional Need OP if the *threshServingLowQ* is present in *systemInformationBlockType3*; otherwise it is not present. |
| *SharedSpectrum* | The field is optional Need OP if NR operates with shared spectrum channel access; otherwise, it is not present. |
| *SharedSpectrum2* | The field is mandatory present if NR operates with shared spectrum channel access; otherwise, it is not present. |

### 6.3.6 Other information elements

#### – *UE-EUTRA-Capability*

The IE *UE-EUTRA-Capability* is used to convey the E-UTRA UE Radio Access Capability Parameters, see TS 36.306 [5], and the Feature Group Indicators for mandatory features (defined in Annexes B.1 and C.1) to the network. The IE *UE-EUTRA-Capability* is transferred in E-UTRA or in another RAT.

NOTE 0: For (UE capability specific) guidelines on the use of keyword OPTIONAL, see Annex A.3.5.

*UE-EUTRA-Capability* information element

-- ASN1START

UE-EUTRA-Capability ::= SEQUENCE {

accessStratumRelease AccessStratumRelease,

ue-Category INTEGER (1..5),

pdcp-Parameters PDCP-Parameters,

phyLayerParameters PhyLayerParameters,

rf-Parameters RF-Parameters,

measParameters MeasParameters,

featureGroupIndicators BIT STRING (SIZE (32)) OPTIONAL,

interRAT-Parameters SEQUENCE {

utraFDD IRAT-ParametersUTRA-FDD OPTIONAL,

utraTDD128 IRAT-ParametersUTRA-TDD128 OPTIONAL,

utraTDD384 IRAT-ParametersUTRA-TDD384 OPTIONAL,

utraTDD768 IRAT-ParametersUTRA-TDD768 OPTIONAL,

geran IRAT-ParametersGERAN OPTIONAL,

cdma2000-HRPD IRAT-ParametersCDMA2000-HRPD OPTIONAL,

cdma2000-1xRTT IRAT-ParametersCDMA2000-1XRTT OPTIONAL

},

nonCriticalExtension UE-EUTRA-Capability-v920-IEs OPTIONAL

}

-- Late non critical extensions

UE-EUTRA-Capability-v9a0-IEs ::= SEQUENCE {

featureGroupIndRel9Add-r9 BIT STRING (SIZE (32)) OPTIONAL,

fdd-Add-UE-EUTRA-Capabilities-r9 UE-EUTRA-CapabilityAddXDD-Mode-r9 OPTIONAL,

tdd-Add-UE-EUTRA-Capabilities-r9 UE-EUTRA-CapabilityAddXDD-Mode-r9 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v9c0-IEs OPTIONAL

}

UE-EUTRA-Capability-v9c0-IEs ::= SEQUENCE {

interRAT-ParametersUTRA-v9c0 IRAT-ParametersUTRA-v9c0 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v9d0-IEs OPTIONAL

}

UE-EUTRA-Capability-v9d0-IEs ::= SEQUENCE {

phyLayerParameters-v9d0 PhyLayerParameters-v9d0 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v9e0-IEs OPTIONAL

}

UE-EUTRA-Capability-v9e0-IEs ::= SEQUENCE {

rf-Parameters-v9e0 RF-Parameters-v9e0 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v9h0-IEs OPTIONAL

}

UE-EUTRA-Capability-v9h0-IEs ::= SEQUENCE {

interRAT-ParametersUTRA-v9h0 IRAT-ParametersUTRA-v9h0 OPTIONAL,

-- Following field is only to be used for late REL-9 extensions

lateNonCriticalExtension OCTET STRING OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v10c0-IEs OPTIONAL

}

UE-EUTRA-Capability-v10c0-IEs ::= SEQUENCE {

otdoa-PositioningCapabilities-r10 OTDOA-PositioningCapabilities-r10 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v10f0-IEs OPTIONAL

}

UE-EUTRA-Capability-v10f0-IEs ::= SEQUENCE {

rf-Parameters-v10f0 RF-Parameters-v10f0 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v10i0-IEs OPTIONAL

}

UE-EUTRA-Capability-v10i0-IEs ::= SEQUENCE {

rf-Parameters-v10i0 RF-Parameters-v10i0 OPTIONAL,

-- Following field is only to be used for late REL-10 extensions

lateNonCriticalExtension OCTET STRING (CONTAINING UE-EUTRA-Capability-v10j0-IEs) OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v11d0-IEs OPTIONAL

}

UE-EUTRA-Capability-v10j0-IEs ::= SEQUENCE {

rf-Parameters-v10j0 RF-Parameters-v10j0 OPTIONAL,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

UE-EUTRA-Capability-v11d0-IEs ::= SEQUENCE {

rf-Parameters-v11d0 RF-Parameters-v11d0 OPTIONAL,

otherParameters-v11d0 Other-Parameters-v11d0 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v11x0-IEs OPTIONAL

}

UE-EUTRA-Capability-v11x0-IEs ::= SEQUENCE {

-- Following field is only to be used for late REL-11 extensions

lateNonCriticalExtension OCTET STRING OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v12b0-IEs OPTIONAL

}

UE-EUTRA-Capability-v12b0-IEs ::= SEQUENCE {

rf-Parameters-v12b0 RF-Parameters-v12b0 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v12x0-IEs OPTIONAL

}

UE-EUTRA-Capability-v12x0-IEs ::= SEQUENCE {

-- Following field is only to be used for late REL-12 extensions

lateNonCriticalExtension OCTET STRING OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1370-IEs OPTIONAL

}

UE-EUTRA-Capability-v1370-IEs ::= SEQUENCE {

ce-Parameters-v1370 CE-Parameters-v1370 OPTIONAL,

fdd-Add-UE-EUTRA-Capabilities-v1370 UE-EUTRA-CapabilityAddXDD-Mode-v1370 OPTIONAL,

tdd-Add-UE-EUTRA-Capabilities-v1370 UE-EUTRA-CapabilityAddXDD-Mode-v1370 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1380-IEs OPTIONAL

}

UE-EUTRA-Capability-v1380-IEs ::= SEQUENCE {

rf-Parameters-v1380 RF-Parameters-v1380 OPTIONAL,

ce-Parameters-v1380 CE-Parameters-v1380,

fdd-Add-UE-EUTRA-Capabilities-v1380 UE-EUTRA-CapabilityAddXDD-Mode-v1380,

tdd-Add-UE-EUTRA-Capabilities-v1380 UE-EUTRA-CapabilityAddXDD-Mode-v1380,

nonCriticalExtension UE-EUTRA-Capability-v1390-IEs OPTIONAL

}

UE-EUTRA-Capability-v1390-IEs ::= SEQUENCE {

rf-Parameters-v1390 RF-Parameters-v1390 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v13e0a-IEs OPTIONAL

}

UE-EUTRA-Capability-v13e0a-IEs ::= SEQUENCE {

lateNonCriticalExtension OCTET STRING (CONTAINING UE-EUTRA-Capability-v13e0b-IEs) OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1470-IEs OPTIONAL

}

UE-EUTRA-Capability-v13e0b-IEs ::= SEQUENCE {

phyLayerParameters-v13e0 PhyLayerParameters-v13e0,

-- Following field is only to be used for late REL-13 extensions

nonCriticalExtension SEQUENCE {} OPTIONAL

}

UE-EUTRA-Capability-v1470-IEs ::= SEQUENCE {

mbms-Parameters-v1470 MBMS-Parameters-v1470 OPTIONAL,

phyLayerParameters-v1470 PhyLayerParameters-v1470 OPTIONAL,

rf-Parameters-v1470 RF-Parameters-v1470 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v14a0-IEs OPTIONAL

}

UE-EUTRA-Capability-v14a0-IEs ::= SEQUENCE {

phyLayerParameters-v14a0 PhyLayerParameters-v14a0,

-- Following field is only to be used for late REL-14 extensions

nonCriticalExtension UE-EUTRA-Capability-v14b0-IEs OPTIONAL

}

UE-EUTRA-Capability-v14b0-IEs ::= SEQUENCE {

rf-Parameters-v14b0 RF-Parameters-v14b0 OPTIONAL,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- Regular non critical extensions

UE-EUTRA-Capability-v920-IEs ::= SEQUENCE {

phyLayerParameters-v920 PhyLayerParameters-v920,

interRAT-ParametersGERAN-v920 IRAT-ParametersGERAN-v920,

interRAT-ParametersUTRA-v920 IRAT-ParametersUTRA-v920 OPTIONAL,

interRAT-ParametersCDMA2000-v920 IRAT-ParametersCDMA2000-1XRTT-v920 OPTIONAL,

deviceType-r9 ENUMERATED {noBenFromBatConsumpOpt} OPTIONAL,

csg-ProximityIndicationParameters-r9 CSG-ProximityIndicationParameters-r9,

neighCellSI-AcquisitionParameters-r9 NeighCellSI-AcquisitionParameters-r9,

son-Parameters-r9 SON-Parameters-r9,

nonCriticalExtension UE-EUTRA-Capability-v940-IEs OPTIONAL

}

UE-EUTRA-Capability-v940-IEs ::= SEQUENCE {

lateNonCriticalExtension OCTET STRING (CONTAINING UE-EUTRA-Capability-v9a0-IEs) OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1020-IEs OPTIONAL

}

UE-EUTRA-Capability-v1020-IEs ::= SEQUENCE {

ue-Category-v1020 INTEGER (6..8) OPTIONAL,

phyLayerParameters-v1020 PhyLayerParameters-v1020 OPTIONAL,

rf-Parameters-v1020 RF-Parameters-v1020 OPTIONAL,

measParameters-v1020 MeasParameters-v1020 OPTIONAL,

featureGroupIndRel10-r10 BIT STRING (SIZE (32)) OPTIONAL,

interRAT-ParametersCDMA2000-v1020 IRAT-ParametersCDMA2000-1XRTT-v1020 OPTIONAL,

ue-BasedNetwPerfMeasParameters-r10 UE-BasedNetwPerfMeasParameters-r10 OPTIONAL,

interRAT-ParametersUTRA-TDD-v1020 IRAT-ParametersUTRA-TDD-v1020 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1060-IEs OPTIONAL

}

UE-EUTRA-Capability-v1060-IEs ::= SEQUENCE {

fdd-Add-UE-EUTRA-Capabilities-v1060 UE-EUTRA-CapabilityAddXDD-Mode-v1060 OPTIONAL,

tdd-Add-UE-EUTRA-Capabilities-v1060 UE-EUTRA-CapabilityAddXDD-Mode-v1060 OPTIONAL,

rf-Parameters-v1060 RF-Parameters-v1060 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1090-IEs OPTIONAL

}

UE-EUTRA-Capability-v1090-IEs ::= SEQUENCE {

rf-Parameters-v1090 RF-Parameters-v1090 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1130-IEs OPTIONAL

}

UE-EUTRA-Capability-v1130-IEs ::= SEQUENCE {

pdcp-Parameters-v1130 PDCP-Parameters-v1130,

phyLayerParameters-v1130 PhyLayerParameters-v1130 OPTIONAL,

rf-Parameters-v1130 RF-Parameters-v1130,

measParameters-v1130 MeasParameters-v1130,

interRAT-ParametersCDMA2000-v1130 IRAT-ParametersCDMA2000-v1130,

otherParameters-r11 Other-Parameters-r11,

fdd-Add-UE-EUTRA-Capabilities-v1130 UE-EUTRA-CapabilityAddXDD-Mode-v1130 OPTIONAL,

tdd-Add-UE-EUTRA-Capabilities-v1130 UE-EUTRA-CapabilityAddXDD-Mode-v1130 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1170-IEs OPTIONAL

}

UE-EUTRA-Capability-v1170-IEs ::= SEQUENCE {

phyLayerParameters-v1170 PhyLayerParameters-v1170 OPTIONAL,

ue-Category-v1170 INTEGER (9..10) OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1180-IEs OPTIONAL

}

UE-EUTRA-Capability-v1180-IEs ::= SEQUENCE {

rf-Parameters-v1180 RF-Parameters-v1180 OPTIONAL,

mbms-Parameters-r11 MBMS-Parameters-r11 OPTIONAL,

fdd-Add-UE-EUTRA-Capabilities-v1180 UE-EUTRA-CapabilityAddXDD-Mode-v1180 OPTIONAL,

tdd-Add-UE-EUTRA-Capabilities-v1180 UE-EUTRA-CapabilityAddXDD-Mode-v1180 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v11a0-IEs OPTIONAL

}

UE-EUTRA-Capability-v11a0-IEs ::= SEQUENCE {

ue-Category-v11a0 INTEGER (11..12) OPTIONAL,

measParameters-v11a0 MeasParameters-v11a0 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1250-IEs OPTIONAL

}

UE-EUTRA-Capability-v1250-IEs ::= SEQUENCE {

phyLayerParameters-v1250 PhyLayerParameters-v1250 OPTIONAL,

rf-Parameters-v1250 RF-Parameters-v1250 OPTIONAL,

rlc-Parameters-r12 RLC-Parameters-r12 OPTIONAL,

ue-BasedNetwPerfMeasParameters-v1250 UE-BasedNetwPerfMeasParameters-v1250 OPTIONAL,

ue-CategoryDL-r12 INTEGER (0..14) OPTIONAL,

ue-CategoryUL-r12 INTEGER (0..13) OPTIONAL,

wlan-IW-Parameters-r12 WLAN-IW-Parameters-r12 OPTIONAL,

measParameters-v1250 MeasParameters-v1250 OPTIONAL,

dc-Parameters-r12 DC-Parameters-r12 OPTIONAL,

mbms-Parameters-v1250 MBMS-Parameters-v1250 OPTIONAL,

mac-Parameters-r12 MAC-Parameters-r12 OPTIONAL,

fdd-Add-UE-EUTRA-Capabilities-v1250 UE-EUTRA-CapabilityAddXDD-Mode-v1250 OPTIONAL,

tdd-Add-UE-EUTRA-Capabilities-v1250 UE-EUTRA-CapabilityAddXDD-Mode-v1250 OPTIONAL,

sl-Parameters-r12 SL-Parameters-r12 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1260-IEs OPTIONAL

}

UE-EUTRA-Capability-v1260-IEs ::= SEQUENCE {

ue-CategoryDL-v1260 INTEGER (15..16) OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1270-IEs OPTIONAL

}

UE-EUTRA-Capability-v1270-IEs ::= SEQUENCE {

rf-Parameters-v1270 RF-Parameters-v1270 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1280-IEs OPTIONAL

}

UE-EUTRA-Capability-v1280-IEs ::= SEQUENCE {

phyLayerParameters-v1280 PhyLayerParameters-v1280 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1310-IEs OPTIONAL

}

UE-EUTRA-Capability-v1310-IEs ::= SEQUENCE {

ue-CategoryDL-v1310 ENUMERATED {n17, m1} OPTIONAL,

ue-CategoryUL-v1310 ENUMERATED {n14, m1} OPTIONAL,

pdcp-Parameters-v1310 PDCP-Parameters-v1310,

rlc-Parameters-v1310 RLC-Parameters-v1310,

mac-Parameters-v1310 MAC-Parameters-v1310 OPTIONAL,

phyLayerParameters-v1310 PhyLayerParameters-v1310 OPTIONAL,

rf-Parameters-v1310 RF-Parameters-v1310 OPTIONAL,

measParameters-v1310 MeasParameters-v1310 OPTIONAL,

dc-Parameters-v1310 DC-Parameters-v1310 OPTIONAL,

sl-Parameters-v1310 SL-Parameters-v1310 OPTIONAL,

scptm-Parameters-r13 SCPTM-Parameters-r13 OPTIONAL,

ce-Parameters-r13 CE-Parameters-r13 OPTIONAL,

interRAT-ParametersWLAN-r13IRAT-ParametersWLAN-r13,

laa-Parameters-r13 LAA-Parameters-r13 OPTIONAL,

lwa-Parameters-r13 LWA-Parameters-r13 OPTIONAL,

wlan-IW-Parameters-v1310 WLAN-IW-Parameters-v1310,

lwip-Parameters-r13 LWIP-Parameters-r13,

fdd-Add-UE-EUTRA-Capabilities-v1310 UE-EUTRA-CapabilityAddXDD-Mode-v1310 OPTIONAL,

tdd-Add-UE-EUTRA-Capabilities-v1310 UE-EUTRA-CapabilityAddXDD-Mode-v1310 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1320-IEs OPTIONAL

}

UE-EUTRA-Capability-v1320-IEs ::= SEQUENCE {

ce-Parameters-v1320 CE-Parameters-v1320 OPTIONAL,

phyLayerParameters-v1320 PhyLayerParameters-v1320 OPTIONAL,

rf-Parameters-v1320 RF-Parameters-v1320 OPTIONAL,

fdd-Add-UE-EUTRA-Capabilities-v1320 UE-EUTRA-CapabilityAddXDD-Mode-v1320 OPTIONAL,

tdd-Add-UE-EUTRA-Capabilities-v1320 UE-EUTRA-CapabilityAddXDD-Mode-v1320 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1330-IEs OPTIONAL

}

UE-EUTRA-Capability-v1330-IEs ::= SEQUENCE {

ue-CategoryDL-v1330 INTEGER (18..19) OPTIONAL,

phyLayerParameters-v1330 PhyLayerParameters-v1330 OPTIONAL,

ue-CE-NeedULGaps-r13 ENUMERATED {true} OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1340-IEs OPTIONAL

}

UE-EUTRA-Capability-v1340-IEs ::= SEQUENCE {

ue-CategoryUL-v1340 INTEGER (15) OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1350-IEs OPTIONAL

}

UE-EUTRA-Capability-v1350-IEs ::= SEQUENCE {

ue-CategoryDL-v1350 ENUMERATED {oneBis} OPTIONAL,

ue-CategoryUL-v1350 ENUMERATED {oneBis} OPTIONAL,

ce-Parameters-v1350 CE-Parameters-v1350,

nonCriticalExtension UE-EUTRA-Capability-v1360-IEs OPTIONAL

}

UE-EUTRA-Capability-v1360-IEs ::= SEQUENCE {

other-Parameters-v1360 Other-Parameters-v1360 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1430-IEs OPTIONAL

}

UE-EUTRA-Capability-v1430-IEs ::= SEQUENCE {

phyLayerParameters-v1430 PhyLayerParameters-v1430,

ue-CategoryDL-v1430 ENUMERATED {m2} OPTIONAL,

ue-CategoryUL-v1430 ENUMERATED {n16, n17, n18, n19, n20, m2} OPTIONAL,

ue-CategoryUL-v1430b ENUMERATED {n21} OPTIONAL,

mac-Parameters-v1430 MAC-Parameters-v1430 OPTIONAL,

measParameters-v1430 MeasParameters-v1430 OPTIONAL,

pdcp-Parameters-v1430 PDCP-Parameters-v1430 OPTIONAL,

rlc-Parameters-v1430 RLC-Parameters-v1430,

rf-Parameters-v1430 RF-Parameters-v1430 OPTIONAL,

laa-Parameters-v1430 LAA-Parameters-v1430 OPTIONAL,

lwa-Parameters-v1430 LWA-Parameters-v1430 OPTIONAL,

lwip-Parameters-v1430 LWIP-Parameters-v1430 OPTIONAL,

otherParameters-v1430 Other-Parameters-v1430,

mmtel-Parameters-r14 MMTEL-Parameters-r14 OPTIONAL,

mobilityParameters-r14 MobilityParameters-r14 OPTIONAL,

ce-Parameters-v1430 CE-Parameters-v1430,

fdd-Add-UE-EUTRA-Capabilities-v1430 UE-EUTRA-CapabilityAddXDD-Mode-v1430 OPTIONAL,

tdd-Add-UE-EUTRA-Capabilities-v1430 UE-EUTRA-CapabilityAddXDD-Mode-v1430 OPTIONAL,

mbms-Parameters-v1430 MBMS-Parameters-v1430 OPTIONAL,

sl-Parameters-v1430 SL-Parameters-v1430 OPTIONAL,

ue-BasedNetwPerfMeasParameters-v1430 UE-BasedNetwPerfMeasParameters-v1430 OPTIONAL,

highSpeedEnhParameters-r14 HighSpeedEnhParameters-r14 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1440-IEs OPTIONAL

}

UE-EUTRA-Capability-v1440-IEs ::= SEQUENCE {

lwa-Parameters-v1440 LWA-Parameters-v1440,

mac-Parameters-v1440 MAC-Parameters-v1440,

nonCriticalExtension UE-EUTRA-Capability-v1450-IEs OPTIONAL

}

UE-EUTRA-Capability-v1450-IEs ::= SEQUENCE {

phyLayerParameters-v1450 PhyLayerParameters-v1450 OPTIONAL,

rf-Parameters-v1450 RF-Parameters-v1450 OPTIONAL,

otherParameters-v1450 OtherParameters-v1450,

ue-CategoryDL-v1450 INTEGER (20) OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1460-IEs OPTIONAL

}

UE-EUTRA-Capability-v1460-IEs ::= SEQUENCE {

ue-CategoryDL-v1460 INTEGER (21) OPTIONAL,

otherParameters-v1460 Other-Parameters-v1460,

nonCriticalExtension UE-EUTRA-Capability-v1510-IEs OPTIONAL

}

UE-EUTRA-Capability-v1510-IEs ::= SEQUENCE {

irat-ParametersNR-r15 IRAT-ParametersNR-r15 OPTIONAL,

featureSetsEUTRA-r15 FeatureSetsEUTRA-r15 OPTIONAL,

pdcp-ParametersNR-r15 PDCP-ParametersNR-r15 OPTIONAL,

fdd-Add-UE-EUTRA-Capabilities-v1510 UE-EUTRA-CapabilityAddXDD-Mode-v1510 OPTIONAL,

tdd-Add-UE-EUTRA-Capabilities-v1510 UE-EUTRA-CapabilityAddXDD-Mode-v1510 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1520-IEs OPTIONAL

}

UE-EUTRA-Capability-v1520-IEs ::= SEQUENCE {

measParameters-v1520 MeasParameters-v1520,

nonCriticalExtension UE-EUTRA-Capability-v1530-IEs OPTIONAL

}

UE-EUTRA-Capability-v1530-IEs ::= SEQUENCE {

measParameters-v1530 MeasParameters-v1530 OPTIONAL,

otherParameters-v1530 Other-Parameters-v1530 OPTIONAL,

neighCellSI-AcquisitionParameters-v1530 NeighCellSI-AcquisitionParameters-v1530 OPTIONAL,

mac-Parameters-v1530 MAC-Parameters-v1530 OPTIONAL,

phyLayerParameters-v1530 PhyLayerParameters-v1530 OPTIONAL,

rf-Parameters-v1530 RF-Parameters-v1530 OPTIONAL,

pdcp-Parameters-v1530 PDCP-Parameters-v1530 OPTIONAL,

ue-CategoryDL-v1530 INTEGER (22..26) OPTIONAL,

ue-BasedNetwPerfMeasParameters-v1530 UE-BasedNetwPerfMeasParameters-v1530 OPTIONAL,

rlc-Parameters-v1530 RLC-Parameters-v1530 OPTIONAL,

sl-Parameters-v1530 SL-Parameters-v1530 OPTIONAL,

extendedNumberOfDRBs-r15 ENUMERATED {supported} OPTIONAL,

reducedCP-Latency-r15 ENUMERATED {supported} OPTIONAL,

laa-Parameters-v1530 LAA-Parameters-v1530 OPTIONAL,

ue-CategoryUL-v1530 INTEGER (22..26) OPTIONAL,

fdd-Add-UE-EUTRA-Capabilities-v1530 UE-EUTRA-CapabilityAddXDD-Mode-v1530 OPTIONAL,

tdd-Add-UE-EUTRA-Capabilities-v1530 UE-EUTRA-CapabilityAddXDD-Mode-v1530 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1540-IEs OPTIONAL

}

UE-EUTRA-Capability-v1540-IEs ::= SEQUENCE {

phyLayerParameters-v1540 PhyLayerParameters-v1540 OPTIONAL,

otherParameters-v1540 Other-Parameters-v1540,

fdd-Add-UE-EUTRA-Capabilities-v1540 UE-EUTRA-CapabilityAddXDD-Mode-v1540 OPTIONAL,

tdd-Add-UE-EUTRA-Capabilities-v1540 UE-EUTRA-CapabilityAddXDD-Mode-v1540 OPTIONAL,

sl-Parameters-v1540 SL-Parameters-v1540 OPTIONAL,

irat-ParametersNR-v1540 IRAT-ParametersNR-v1540 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1550-IEs OPTIONAL

}

UE-EUTRA-Capability-v1550-IEs ::= SEQUENCE {

neighCellSI-AcquisitionParameters-v1550 NeighCellSI-AcquisitionParameters-v1550 OPTIONAL,

phyLayerParameters-v1550 PhyLayerParameters-v1550,

mac-Parameters-v1550 MAC-Parameters-v1550,

fdd-Add-UE-EUTRA-Capabilities-v1550 UE-EUTRA-CapabilityAddXDD-Mode-v1550,

tdd-Add-UE-EUTRA-Capabilities-v1550 UE-EUTRA-CapabilityAddXDD-Mode-v1550,

nonCriticalExtension UE-EUTRA-Capability-v1560-IEs OPTIONAL

}

UE-EUTRA-Capability-v1560-IEs ::= SEQUENCE {

pdcp-ParametersNR-v1560 PDCP-ParametersNR-v1560,

irat-ParametersNR-v1560 IRAT-ParametersNR-v1560,

appliedCapabilityFilterCommon-r15 OCTET STRING OPTIONAL,

fdd-Add-UE-EUTRA-Capabilities-v1560 UE-EUTRA-CapabilityAddXDD-Mode-v1560,

tdd-Add-UE-EUTRA-Capabilities-v1560 UE-EUTRA-CapabilityAddXDD-Mode-v1560,

nonCriticalExtension UE-EUTRA-Capability-v1570-IEs OPTIONAL

}

UE-EUTRA-Capability-v1570-IEs ::= SEQUENCE {

rf-Parameters-v1570 RF-Parameters-v1570 OPTIONAL,

irat-ParametersNR-v1570 IRAT-ParametersNR-v1570 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v15a0-IEs OPTIONAL

}

UE-EUTRA-Capability-v15a0-IEs ::= SEQUENCE {

neighCellSI-AcquisitionParameters-v15a0 NeighCellSI-AcquisitionParameters-v15a0,

eutra-5GC-Parameters-r15 EUTRA-5GC-Parameters-r15 OPTIONAL,

fdd-Add-UE-EUTRA-Capabilities-v15a0 UE-EUTRA-CapabilityAddXDD-Mode-v15a0 OPTIONAL,

tdd-Add-UE-EUTRA-Capabilities-v15a0 UE-EUTRA-CapabilityAddXDD-Mode-v15a0 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1610-IEs OPTIONAL

}

UE-EUTRA-Capability-v1610-IEs ::= SEQUENCE {

highSpeedEnhParameters-v1610 HighSpeedEnhParameters-v1610 OPTIONAL,

neighCellSI-AcquisitionParameters-v1610 NeighCellSI-AcquisitionParameters-v1610 OPTIONAL,

mbms-Parameters-v1610 MBMS-Parameters-v1610 OPTIONAL,

pdcp-Parameters-v1610 PDCP-Parameters-v1610 OPTIONAL,

mac-Parameters-v1610 MAC-Parameters-v1610 OPTIONAL,

phyLayerParameters-v1610 PhyLayerParameters-v1610 OPTIONAL,

measParameters-v1610 MeasParameters-v1610 OPTIONAL,

pur-Parameters-r16 PUR-Parameters-r16 OPTIONAL,

eutra-5GC-Parameters-v1610 EUTRA-5GC-Parameters-v1610 OPTIONAL,

otherParameters-v1610 Other-Parameters-v1610 OPTIONAL,

dl-DedicatedMessageSegmentation-r16 ENUMERATED {supported} OPTIONAL,

mmtel-Parameters-v1610 MMTEL-Parameters-v1610,

irat-ParametersNR-v1610 IRAT-ParametersNR-v1610 OPTIONAL,

rf-Parameters-v1610 RF-Parameters-v1610 OPTIONAL,

mobilityParameters-v1610 MobilityParameters-v1610 OPTIONAL,

ue-BasedNetwPerfMeasParameters-v1610 UE-BasedNetwPerfMeasParameters-v1610,

sl-Parameters-v1610 SL-Parameters-v1610 OPTIONAL,

fdd-Add-UE-EUTRA-Capabilities-v1610 UE-EUTRA-CapabilityAddXDD-Mode-v1610 OPTIONAL,

tdd-Add-UE-EUTRA-Capabilities-v1610 UE-EUTRA-CapabilityAddXDD-Mode-v1610 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1630-IEs OPTIONAL

}

UE-EUTRA-Capability-v1630-IEs ::= SEQUENCE {

rf-Parameters-v1630 RF-Parameters-v1630 OPTIONAL,

sl-Parameters-v1630 SL-Parameters-v1630 OPTIONAL,

earlySecurityReactivation-r16 ENUMERATED {supported} OPTIONAL,

mac-Parameters-v1630 MAC-Parameters-v1630,

measParameters-v1630 MeasParameters-v1630 OPTIONAL,

fdd-Add-UE-EUTRA-Capabilities-v1630 UE-EUTRA-CapabilityAddXDD-Mode-v1630,

tdd-Add-UE-EUTRA-Capabilities-v1630 UE-EUTRA-CapabilityAddXDD-Mode-v1630,

nonCriticalExtension UE-EUTRA-Capability-v1650-IEs OPTIONAL

}

UE-EUTRA-Capability-v1650-IEs ::= SEQUENCE {

otherParameters-v1650 Other-Parameters-v1650 OPTIONAL,

nonCriticalExtension UE-EUTRA-Capability-v1660-IEs OPTIONAL

}

UE-EUTRA-Capability-v1660-IEs ::= SEQUENCE {

irat-ParametersNR-v1660 IRAT-ParametersNR-v1660,

nonCriticalExtension UE-EUTRA-Capability-v1700-IEs OPTIONAL

}

UE-EUTRA-Capability-v1700-IEs ::= SEQUENCE {

measParameters-v1700 MeasParameters-v1700 OPTIONAL,

ue-BasedNetwPerfMeasParameters-v1700 UE-BasedNetwPerfMeasParameters-v1700 OPTIONAL,

phyLayerParameters-v1700 PhyLayerParameters-v1700,

ntn-Parameters-r17 NTN-Parameters-r17 OPTIONAL,

irat-ParametersNR-v1700 IRAT-ParametersNR-v1700 OPTIONAL,

mbms-Parameters-v1700 MBMS-Parameters-v1700,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

UE-EUTRA-CapabilityAddXDD-Mode-r9 ::= SEQUENCE {

phyLayerParameters-r9 PhyLayerParameters OPTIONAL,

featureGroupIndicators-r9 BIT STRING (SIZE (32)) OPTIONAL,

featureGroupIndRel9Add-r9 BIT STRING (SIZE (32)) OPTIONAL,

interRAT-ParametersGERAN-r9 IRAT-ParametersGERAN OPTIONAL,

interRAT-ParametersUTRA-r9 IRAT-ParametersUTRA-v920 OPTIONAL,

interRAT-ParametersCDMA2000-r9 IRAT-ParametersCDMA2000-1XRTT-v920 OPTIONAL,

neighCellSI-AcquisitionParameters-r9 NeighCellSI-AcquisitionParameters-r9 OPTIONAL,

...

}

UE-EUTRA-CapabilityAddXDD-Mode-v1060 ::= SEQUENCE {

phyLayerParameters-v1060 PhyLayerParameters-v1020 OPTIONAL,

featureGroupIndRel10-v1060 BIT STRING (SIZE (32)) OPTIONAL,

interRAT-ParametersCDMA2000-v1060 IRAT-ParametersCDMA2000-1XRTT-v1020 OPTIONAL,

interRAT-ParametersUTRA-TDD-v1060 IRAT-ParametersUTRA-TDD-v1020 OPTIONAL,

...,

[[ otdoa-PositioningCapabilities-r10 OTDOA-PositioningCapabilities-r10 OPTIONAL

]]

}

UE-EUTRA-CapabilityAddXDD-Mode-v1130 ::= SEQUENCE {

phyLayerParameters-v1130 PhyLayerParameters-v1130 OPTIONAL,

measParameters-v1130 MeasParameters-v1130 OPTIONAL,

otherParameters-r11 Other-Parameters-r11 OPTIONAL,

...

}

UE-EUTRA-CapabilityAddXDD-Mode-v1180 ::= SEQUENCE {

mbms-Parameters-r11 MBMS-Parameters-r11

}

UE-EUTRA-CapabilityAddXDD-Mode-v1250 ::= SEQUENCE {

phyLayerParameters-v1250 PhyLayerParameters-v1250 OPTIONAL,

measParameters-v1250 MeasParameters-v1250 OPTIONAL

}

UE-EUTRA-CapabilityAddXDD-Mode-v1310 ::= SEQUENCE {

phyLayerParameters-v1310 PhyLayerParameters-v1310 OPTIONAL

}

UE-EUTRA-CapabilityAddXDD-Mode-v1320 ::= SEQUENCE {

phyLayerParameters-v1320 PhyLayerParameters-v1320 OPTIONAL,

scptm-Parameters-r13 SCPTM-Parameters-r13 OPTIONAL

}

UE-EUTRA-CapabilityAddXDD-Mode-v1370 ::= SEQUENCE {

ce-Parameters-v1370 CE-Parameters-v1370 OPTIONAL

}

UE-EUTRA-CapabilityAddXDD-Mode-v1380 ::= SEQUENCE {

ce-Parameters-v1380 CE-Parameters-v1380

}

UE-EUTRA-CapabilityAddXDD-Mode-v1430 ::= SEQUENCE {

phyLayerParameters-v1430 PhyLayerParameters-v1430 OPTIONAL,

mmtel-Parameters-r14 MMTEL-Parameters-r14 OPTIONAL

}

UE-EUTRA-CapabilityAddXDD-Mode-v1510 ::= SEQUENCE {

pdcp-ParametersNR-r15 PDCP-ParametersNR-r15 OPTIONAL

}

UE-EUTRA-CapabilityAddXDD-Mode-v1530 ::= SEQUENCE {

neighCellSI-AcquisitionParameters-v1530 NeighCellSI-AcquisitionParameters-v1530 OPTIONAL,

reducedCP-Latency-r15 ENUMERATED {supported} OPTIONAL

}

UE-EUTRA-CapabilityAddXDD-Mode-v1540 ::= SEQUENCE {

eutra-5GC-Parameters-r15 EUTRA-5GC-Parameters-r15 OPTIONAL,

irat-ParametersNR-v1540 IRAT-ParametersNR-v1540 OPTIONAL

}

UE-EUTRA-CapabilityAddXDD-Mode-v1550 ::= SEQUENCE {

neighCellSI-AcquisitionParameters-v1550 NeighCellSI-AcquisitionParameters-v1550 OPTIONAL

}

UE-EUTRA-CapabilityAddXDD-Mode-v1560 ::= SEQUENCE {

pdcp-ParametersNR-v1560 PDCP-ParametersNR-v1560

}

UE-EUTRA-CapabilityAddXDD-Mode-v15a0 ::= SEQUENCE {

phyLayerParameters-v1530 PhyLayerParameters-v1530 OPTIONAL,

phyLayerParameters-v1540 PhyLayerParameters-v1540 OPTIONAL,

phyLayerParameters-v1550 PhyLayerParameters-v1550 OPTIONAL,

neighCellSI-AcquisitionParameters-v15a0 NeighCellSI-AcquisitionParameters-v15a0

}

UE-EUTRA-CapabilityAddXDD-Mode-v1610 ::= SEQUENCE {

phyLayerParameters-v1610 PhyLayerParameters-v1610 OPTIONAL,

pur-Parameters-r16 PUR-Parameters-r16 OPTIONAL,

measParameters-v1610 MeasParameters-v1610 OPTIONAL,

eutra-5GC-Parameters-v1610 EUTRA-5GC-Parameters-v1610 OPTIONAL,

irat-ParametersNR-v1610 IRAT-ParametersNR-v1610 OPTIONAL,

neighCellSI-AcquisitionParameters-v1610 NeighCellSI-AcquisitionParameters-v1610 OPTIONAL,

mobilityParameters-v1610 MobilityParameters-v1610 OPTIONAL

}

UE-EUTRA-CapabilityAddXDD-Mode-v1630 ::= SEQUENCE {

measParameters-v1630 MeasParameters-v1630

}

AccessStratumRelease ::= ENUMERATED {

rel8, rel9, rel10, rel11, rel12, rel13,

rel14, rel15, ..., rel16, rel17}

FeatureSetsEUTRA-r15 ::= SEQUENCE {

featureSetsDL-r15 SEQUENCE (SIZE (1..maxFeatureSets-r15)) OF FeatureSetDL-r15 OPTIONAL,

featureSetsDL-PerCC-r15 SEQUENCE (SIZE (1..maxPerCC-FeatureSets-r15)) OF FeatureSetDL-PerCC-r15 OPTIONAL,

featureSetsUL-r15 SEQUENCE (SIZE (1..maxFeatureSets-r15)) OF FeatureSetUL-r15 OPTIONAL,

featureSetsUL-PerCC-r15 SEQUENCE (SIZE (1..maxPerCC-FeatureSets-r15)) OF FeatureSetUL-PerCC-r15 OPTIONAL,

...,

[[ featureSetsDL-v1550 SEQUENCE (SIZE (1..maxFeatureSets-r15)) OF FeatureSetDL-v1550 OPTIONAL

]]

}

MobilityParameters-r14 ::= SEQUENCE {

makeBeforeBreak-r14 ENUMERATED {supported} OPTIONAL,

rach-Less-r14 ENUMERATED {supported} OPTIONAL

}

MobilityParameters-v1610 ::= SEQUENCE {

cho-r16 ENUMERATED {supported} OPTIONAL,

cho-FDD-TDD-r16 ENUMERATED {supported} OPTIONAL,

cho-Failure-r16 ENUMERATED {supported} OPTIONAL,

cho-TwoTriggerEvents-r16 ENUMERATED {supported} OPTIONAL

}

DC-Parameters-r12 ::= SEQUENCE {

drb-TypeSplit-r12 ENUMERATED {supported} OPTIONAL,

drb-TypeSCG-r12 ENUMERATED {supported} OPTIONAL

}

DC-Parameters-v1310 ::= SEQUENCE {

pdcp-TransferSplitUL-r13 ENUMERATED {supported} OPTIONAL,

ue-SSTD-Meas-r13 ENUMERATED {supported} OPTIONAL

}

MAC-Parameters-r12 ::= SEQUENCE {

logicalChannelSR-ProhibitTimer-r12 ENUMERATED {supported} OPTIONAL,

longDRX-Command-r12 ENUMERATED {supported} OPTIONAL

}

MAC-Parameters-v1310 ::= SEQUENCE {

extendedMAC-LengthField-r13 ENUMERATED {supported} OPTIONAL,

extendedLongDRX-r13 ENUMERATED {supported} OPTIONAL

}

MAC-Parameters-v1430 ::= SEQUENCE {

shortSPS-IntervalFDD-r14 ENUMERATED {supported} OPTIONAL,

shortSPS-IntervalTDD-r14 ENUMERATED {supported} OPTIONAL,

skipUplinkDynamic-r14 ENUMERATED {supported} OPTIONAL,

skipUplinkSPS-r14 ENUMERATED {supported} OPTIONAL,

multipleUplinkSPS-r14 ENUMERATED {supported} OPTIONAL,

dataInactMon-r14 ENUMERATED {supported} OPTIONAL

}

MAC-Parameters-v1440 ::= SEQUENCE {

rai-Support-r14 ENUMERATED {supported} OPTIONAL

}

MAC-Parameters-v1530 ::= SEQUENCE {

min-Proc-TimelineSubslot-r15 SEQUENCE (SIZE(1..3)) OF ProcessingTimelineSet-r15 OPTIONAL,

skipSubframeProcessing-r15 SkipSubframeProcessing-r15 OPTIONAL,

earlyData-UP-r15 ENUMERATED {supported} OPTIONAL,

dormantSCellState-r15 ENUMERATED {supported} OPTIONAL,

directSCellActivation-r15 ENUMERATED {supported} OPTIONAL,

directSCellHibernation-r15 ENUMERATED {supported} OPTIONAL,

extendedLCID-Duplication-r15 ENUMERATED {supported} OPTIONAL,

sps-ServingCell-r15 ENUMERATED {supported} OPTIONAL

}

MAC-Parameters-v1550 ::= SEQUENCE {

eLCID-Support-r15 ENUMERATED {supported} OPTIONAL

}

MAC-Parameters-v1610 ::= SEQUENCE {

directMCG-SCellActivationResume-r16 ENUMERATED {supported} OPTIONAL,

directSCG-SCellActivationResume-r16 ENUMERATED {supported} OPTIONAL,

earlyData-UP-5GC-r16 ENUMERATED {supported} OPTIONAL,

rai-SupportEnh-r16 ENUMERATED {supported} OPTIONAL

}

MAC-Parameters-v1630 ::= SEQUENCE {

directSCG-SCellActivationNEDC-r16 ENUMERATED {supported} OPTIONAL

}

NTN-Parameters-r17 ::= SEQUENCE {

ntn-Connectivity-EPC-r17 ENUMERATED {supported} OPTIONAL,

ntn-TA-Report-r17 ENUMERATED {supported} OPTIONAL,

ntn-PUR-TimerEnhancement-r17 ENUMERATED {supported} OPTIONAL

}

ProcessingTimelineSet-r15 ::= ENUMERATED {set1, set2}

RLC-Parameters-r12 ::= SEQUENCE {

extended-RLC-LI-Field-r12 ENUMERATED {supported}

}

RLC-Parameters-v1310 ::= SEQUENCE {

extendedRLC-SN-SO-Field-r13 ENUMERATED {supported} OPTIONAL

}

RLC-Parameters-v1430 ::= SEQUENCE {

extendedPollByte-r14 ENUMERATED {supported} OPTIONAL

}

RLC-Parameters-v1530 ::= SEQUENCE {

flexibleUM-AM-Combinations-r15 ENUMERATED {supported} OPTIONAL,

rlc-AM-Ooo-Delivery-r15 ENUMERATED {supported} OPTIONAL,

rlc-UM-Ooo-Delivery-r15 ENUMERATED {supported} OPTIONAL

}

PDCP-Parameters ::= SEQUENCE {

supportedROHC-Profiles ROHC-ProfileSupportList-r15,

maxNumberROHC-ContextSessions ENUMERATED {

cs2, cs4, cs8, cs12, cs16, cs24, cs32,

cs48, cs64, cs128, cs256, cs512, cs1024,

cs16384, spare2, spare1} DEFAULT cs16,

...

}

PDCP-Parameters-v1130 ::= SEQUENCE {

pdcp-SN-Extension-r11 ENUMERATED {supported} OPTIONAL,

supportRohcContextContinue-r11 ENUMERATED {supported} OPTIONAL

}

PDCP-Parameters-v1310 ::= SEQUENCE {

pdcp-SN-Extension-18bits-r13 ENUMERATED {supported} OPTIONAL

}

PDCP-Parameters-v1430 ::= SEQUENCE {

supportedUplinkOnlyROHC-Profiles-r14 SEQUENCE {

profile0x0006-r14 BOOLEAN

},

maxNumberROHC-ContextSessions-r14 ENUMERATED {

cs2, cs4, cs8, cs12, cs16, cs24, cs32,

cs48, cs64, cs128, cs256, cs512, cs1024,

cs16384, spare2, spare1} DEFAULT cs16

}

PDCP-Parameters-v1530 ::= SEQUENCE {

supportedUDC-r15 SupportedUDC-r15 OPTIONAL,

pdcp-Duplication-r15 ENUMERATED {supported} OPTIONAL

}

PDCP-Parameters-v1610 ::= SEQUENCE {

pdcp-VersionChangeWithoutHO-r16 ENUMERATED {supported} OPTIONAL,

ehc-r16 ENUMERATED {supported} OPTIONAL,

continueEHC-Context-r16 ENUMERATED {supported} OPTIONAL,

maxNumberEHC-Contexts-r16 ENUMERATED {cs2, cs4, cs8, cs16, cs32, cs64, cs128, cs256,

cs512, cs1024, cs2048, cs4096, cs8192, cs16384,

cs32768, cs65536} OPTIONAL,

jointEHC-ROHC-Config-r16 ENUMERATED {supported} OPTIONAL

}

SupportedUDC-r15 ::= SEQUENCE {

supportedStandardDic-r15 ENUMERATED {supported} OPTIONAL,

supportedOperatorDic-r15 SupportedOperatorDic-r15 OPTIONAL

}

SupportedOperatorDic-r15 ::= SEQUENCE {

versionOfDictionary-r15 INTEGER (0..15),

associatedPLMN-ID-r15 PLMN-Identity

}

PhyLayerParameters ::= SEQUENCE {

ue-TxAntennaSelectionSupported BOOLEAN,

ue-SpecificRefSigsSupported BOOLEAN

}

PhyLayerParameters-v920 ::= SEQUENCE {

enhancedDualLayerFDD-r9 ENUMERATED {supported} OPTIONAL,

enhancedDualLayerTDD-r9 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-v9d0 ::= SEQUENCE {

tm5-FDD-r9 ENUMERATED {supported} OPTIONAL,

tm5-TDD-r9 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-v1020 ::= SEQUENCE {

twoAntennaPortsForPUCCH-r10 ENUMERATED {supported} OPTIONAL,

tm9-With-8Tx-FDD-r10 ENUMERATED {supported} OPTIONAL,

pmi-Disabling-r10 ENUMERATED {supported} OPTIONAL,

crossCarrierScheduling-r10 ENUMERATED {supported} OPTIONAL,

simultaneousPUCCH-PUSCH-r10 ENUMERATED {supported} OPTIONAL,

multiClusterPUSCH-WithinCC-r10 ENUMERATED {supported} OPTIONAL,

nonContiguousUL-RA-WithinCC-List-r10 NonContiguousUL-RA-WithinCC-List-r10 OPTIONAL

}

PhyLayerParameters-v1130 ::= SEQUENCE {

crs-InterfHandl-r11 ENUMERATED {supported} OPTIONAL,

ePDCCH-r11 ENUMERATED {supported} OPTIONAL,

multiACK-CSI-Reporting-r11 ENUMERATED {supported} OPTIONAL,

ss-CCH-InterfHandl-r11 ENUMERATED {supported} OPTIONAL,

tdd-SpecialSubframe-r11 ENUMERATED {supported} OPTIONAL,

txDiv-PUCCH1b-ChSelect-r11 ENUMERATED {supported} OPTIONAL,

ul-CoMP-r11 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-v1170 ::= SEQUENCE {

interBandTDD-CA-WithDifferentConfig-r11 BIT STRING (SIZE (2)) OPTIONAL

}

PhyLayerParameters-v1250 ::= SEQUENCE {

e-HARQ-Pattern-FDD-r12 ENUMERATED {supported} OPTIONAL,

enhanced-4TxCodebook-r12 ENUMERATED {supported} OPTIONAL,

tdd-FDD-CA-PCellDuplex-r12 BIT STRING (SIZE (2)) OPTIONAL,

phy-TDD-ReConfig-TDD-PCell-r12 ENUMERATED {supported} OPTIONAL,

phy-TDD-ReConfig-FDD-PCell-r12 ENUMERATED {supported} OPTIONAL,

pusch-FeedbackMode-r12 ENUMERATED {supported} OPTIONAL,

pusch-SRS-PowerControl-SubframeSet-r12 ENUMERATED {supported} OPTIONAL,

csi-SubframeSet-r12 ENUMERATED {supported} OPTIONAL,

noResourceRestrictionForTTIBundling-r12 ENUMERATED {supported} OPTIONAL,

discoverySignalsInDeactSCell-r12 ENUMERATED {supported} OPTIONAL,

naics-Capability-List-r12 NAICS-Capability-List-r12 OPTIONAL

}

PhyLayerParameters-v1280 ::= SEQUENCE {

alternativeTBS-Indices-r12 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-v1310 ::= SEQUENCE {

aperiodicCSI-Reporting-r13 BIT STRING (SIZE (2)) OPTIONAL,

codebook-HARQ-ACK-r13 BIT STRING (SIZE (2)) OPTIONAL,

crossCarrierScheduling-B5C-r13 ENUMERATED {supported} OPTIONAL,

fdd-HARQ-TimingTDD-r13 ENUMERATED {supported} OPTIONAL,

maxNumberUpdatedCSI-Proc-r13 INTEGER(5..32) OPTIONAL,

pucch-Format4-r13 ENUMERATED {supported} OPTIONAL,

pucch-Format5-r13 ENUMERATED {supported} OPTIONAL,

pucch-SCell-r13 ENUMERATED {supported} OPTIONAL,

spatialBundling-HARQ-ACK-r13 ENUMERATED {supported} OPTIONAL,

supportedBlindDecoding-r13 SEQUENCE {

maxNumberDecoding-r13 INTEGER(1..32) OPTIONAL,

pdcch-CandidateReductions-r13 ENUMERATED {supported} OPTIONAL,

skipMonitoringDCI-Format0-1A-r13 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

uci-PUSCH-Ext-r13 ENUMERATED {supported} OPTIONAL,

crs-InterfMitigationTM10-r13 ENUMERATED {supported} OPTIONAL,

pdsch-CollisionHandling-r13 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-v1320 ::= SEQUENCE {

mimo-UE-Parameters-r13 MIMO-UE-Parameters-r13 OPTIONAL

}

PhyLayerParameters-v1330 ::= SEQUENCE {

cch-InterfMitigation-RefRecTypeA-r13 ENUMERATED {supported} OPTIONAL,

cch-InterfMitigation-RefRecTypeB-r13 ENUMERATED {supported} OPTIONAL,

cch-InterfMitigation-MaxNumCCs-r13 INTEGER (1.. maxServCell-r13) OPTIONAL,

crs-InterfMitigationTM1toTM9-r13 INTEGER (1.. maxServCell-r13) OPTIONAL

}

PhyLayerParameters-v13e0 ::= SEQUENCE {

mimo-UE-Parameters-v13e0 MIMO-UE-Parameters-v13e0

}

PhyLayerParameters-v1430 ::= SEQUENCE {

ce-PUSCH-NB-MaxTBS-r14 ENUMERATED {supported} OPTIONAL,

ce-PDSCH-PUSCH-MaxBandwidth-r14 ENUMERATED {bw5, bw20} OPTIONAL,

ce-HARQ-AckBundling-r14 ENUMERATED {supported} OPTIONAL,

ce-PDSCH-TenProcesses-r14 ENUMERATED {supported} OPTIONAL,

ce-RetuningSymbols-r14 ENUMERATED {n0, n1} OPTIONAL,

ce-PDSCH-PUSCH-Enhancement-r14 ENUMERATED {supported} OPTIONAL,

ce-SchedulingEnhancement-r14 ENUMERATED {supported} OPTIONAL,

ce-SRS-Enhancement-r14 ENUMERATED {supported} OPTIONAL,

ce-PUCCH-Enhancement-r14 ENUMERATED {supported} OPTIONAL,

ce-ClosedLoopTxAntennaSelection-r14 ENUMERATED {supported} OPTIONAL,

tdd-SpecialSubframe-r14 ENUMERATED {supported} OPTIONAL,

tdd-TTI-Bundling-r14 ENUMERATED {supported} OPTIONAL,

dmrs-LessUpPTS-r14 ENUMERATED {supported} OPTIONAL,

mimo-UE-Parameters-v1430 MIMO-UE-Parameters-v1430 OPTIONAL,

alternativeTBS-Index-r14 ENUMERATED {supported} OPTIONAL,

feMBMS-Unicast-Parameters-r14 FeMBMS-Unicast-Parameters-r14 OPTIONAL

}

PhyLayerParameters-v1450 ::= SEQUENCE {

ce-SRS-EnhancementWithoutComb4-r14 ENUMERATED {supported} OPTIONAL,

crs-LessDwPTS-r14 ENUMERATED {supported} OPTIONAL}

PhyLayerParameters-v1470 ::= SEQUENCE {

mimo-UE-Parameters-v1470 MIMO-UE-Parameters-v1470 OPTIONAL,

srs-UpPTS-6sym-r14 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-v14a0 ::= SEQUENCE {

ssp10-TDD-Only-r14 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-v1530 ::= SEQUENCE {

stti-SPT-Capabilities-r15 SEQUENCE {

aperiodicCsi-ReportingSTTI-r15 ENUMERATED {supported} OPTIONAL,

dmrs-BasedSPDCCH-MBSFN-r15 ENUMERATED {supported} OPTIONAL,

dmrs-BasedSPDCCH-nonMBSFN-r15 ENUMERATED {supported} OPTIONAL,

dmrs-PositionPattern-r15 ENUMERATED {supported} OPTIONAL,

dmrs-SharingSubslotPDSCH-r15 ENUMERATED {supported} OPTIONAL,

dmrs-RepetitionSubslotPDSCH-r15 ENUMERATED {supported} OPTIONAL,

epdcch-SPT-differentCells-r15 ENUMERATED {supported} OPTIONAL,

epdcch-STTI-differentCells-r15 ENUMERATED {supported} OPTIONAL,

maxLayersSlotOrSubslotPUSCH-r15 ENUMERATED {oneLayer,twoLayers,fourLayers}

OPTIONAL,

maxNumberUpdatedCSI-Proc-SPT-r15 INTEGER(5..32) OPTIONAL,

maxNumberUpdatedCSI-Proc-STTI-Comb77-r15 INTEGER(1..32) OPTIONAL,

maxNumberUpdatedCSI-Proc-STTI-Comb27-r15 INTEGER(1..32) OPTIONAL,

maxNumberUpdatedCSI-Proc-STTI-Comb22-Set1-r15 INTEGER(1..32) OPTIONAL,

maxNumberUpdatedCSI-Proc-STTI-Comb22-Set2-r15 INTEGER(1..32) OPTIONAL,

mimo-UE-ParametersSTTI-r15 MIMO-UE-Parameters-r13 OPTIONAL,

mimo-UE-ParametersSTTI-v1530 MIMO-UE-Parameters-v1430 OPTIONAL,

numberOfBlindDecodesUSS-r15 INTEGER(4..32) OPTIONAL,

pdsch-SlotSubslotPDSCH-Decoding-r15 ENUMERATED {supported} OPTIONAL,

powerUCI-SlotPUSCH ENUMERATED {supported} OPTIONAL,

powerUCI-SubslotPUSCH ENUMERATED {supported} OPTIONAL,

slotPDSCH-TxDiv-TM9and10 ENUMERATED {supported} OPTIONAL,

subslotPDSCH-TxDiv-TM9and10 ENUMERATED {supported} OPTIONAL,

spdcch-differentRS-types-r15 ENUMERATED {supported} OPTIONAL,

srs-DCI7-TriggeringFS2-r15 ENUMERATED {supported} OPTIONAL,

sps-cyclicShift-r15 ENUMERATED {supported} OPTIONAL,

spdcch-Reuse-r15 ENUMERATED {supported} OPTIONAL,

sps-STTI-r15 ENUMERATED {slot, subslot, slotAndSubslot}

OPTIONAL,

tm8-slotPDSCH-r15 ENUMERATED {supported} OPTIONAL,

tm9-slotSubslot-r15 ENUMERATED {supported} OPTIONAL,

tm9-slotSubslotMBSFN-r15 ENUMERATED {supported} OPTIONAL,

tm10-slotSubslot-r15 ENUMERATED {supported} OPTIONAL,

tm10-slotSubslotMBSFN-r15 ENUMERATED {supported} OPTIONAL,

txDiv-SPUCCH-r15 ENUMERATED {supported} OPTIONAL,

ul-AsyncHarqSharingDiff-TTI-Lengths-r15 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

ce-Capabilities-r15 SEQUENCE {

ce-CRS-IntfMitig-r15 ENUMERATED {supported} OPTIONAL,

ce-CQI-AlternativeTable-r15 ENUMERATED {supported} OPTIONAL,

ce-PDSCH-FlexibleStartPRB-CE-ModeA-r15 ENUMERATED {supported} OPTIONAL,

ce-PDSCH-FlexibleStartPRB-CE-ModeB-r15 ENUMERATED {supported} OPTIONAL,

ce-PDSCH-64QAM-r15 ENUMERATED {supported} OPTIONAL,

ce-PUSCH-FlexibleStartPRB-CE-ModeA-r15 ENUMERATED {supported} OPTIONAL,

ce-PUSCH-FlexibleStartPRB-CE-ModeB-r15 ENUMERATED {supported} OPTIONAL,

ce-PUSCH-SubPRB-Allocation-r15 ENUMERATED {supported} OPTIONAL,

ce-UL-HARQ-ACK-Feedback-r15 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

shortCQI-ForSCellActivation-r15 ENUMERATED {supported} OPTIONAL,

mimo-CBSR-AdvancedCSI-r15 ENUMERATED {supported} OPTIONAL,

crs-IntfMitig-r15 ENUMERATED {supported} OPTIONAL,

ul-PowerControlEnhancements-r15 ENUMERATED {supported} OPTIONAL,

urllc-Capabilities-r15 SEQUENCE {

pdsch-RepSubframe-r15 ENUMERATED {supported} OPTIONAL,

pdsch-RepSlot-r15 ENUMERATED {supported} OPTIONAL,

pdsch-RepSubslot-r15 ENUMERATED {supported} OPTIONAL,

pusch-SPS-MultiConfigSubframe-r15 INTEGER (0..6) OPTIONAL,

pusch-SPS-MaxConfigSubframe-r15 INTEGER (0..31) OPTIONAL,

pusch-SPS-MultiConfigSlot-r15 INTEGER (0..6) OPTIONAL,

pusch-SPS-MaxConfigSlot-r15 INTEGER (0..31) OPTIONAL,

pusch-SPS-MultiConfigSubslot-r15 INTEGER (0..6) OPTIONAL,

pusch-SPS-MaxConfigSubslot-r15 INTEGER (0..31) OPTIONAL,

pusch-SPS-SlotRepPCell-r15 ENUMERATED {supported} OPTIONAL,

pusch-SPS-SlotRepPSCell-r15 ENUMERATED {supported} OPTIONAL,

pusch-SPS-SlotRepSCell-r15 ENUMERATED {supported} OPTIONAL,

pusch-SPS-SubframeRepPCell-r15 ENUMERATED {supported} OPTIONAL,

pusch-SPS-SubframeRepPSCell-r15 ENUMERATED {supported} OPTIONAL,

pusch-SPS-SubframeRepSCell-r15 ENUMERATED {supported} OPTIONAL,

pusch-SPS-SubslotRepPCell-r15 ENUMERATED {supported} OPTIONAL,

pusch-SPS-SubslotRepPSCell-r15 ENUMERATED {supported} OPTIONAL,

pusch-SPS-SubslotRepSCell-r15 ENUMERATED {supported} OPTIONAL,

semiStaticCFI-r15 ENUMERATED {supported} OPTIONAL,

semiStaticCFI-Pattern-r15 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

altMCS-Table-r15 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-v1540 ::= SEQUENCE {

stti-SPT-Capabilities-v1540 SEQUENCE {

slotPDSCH-TxDiv-TM8-r15 ENUMERATED {supported}

} OPTIONAL,

crs-IM-TM1-toTM9-OneRX-Port-v1540 ENUMERATED {supported} OPTIONAL,

cch-IM-RefRecTypeA-OneRX-Port-v1540 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-v1550 ::= SEQUENCE {

dmrs-OverheadReduction-r15 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-v1610 ::= SEQUENCE {

ce-Capabilities-v1610 SEQUENCE {

ce-CSI-RS-Feedback-r16 ENUMERATED {supported} OPTIONAL,

ce-CSI-RS-FeedbackCodebookRestriction-r16 ENUMERATED {supported} OPTIONAL,

crs-ChEstMPDCCH-CE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

crs-ChEstMPDCCH-CE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

crs-ChEstMPDCCH-CSI-r16 ENUMERATED {supported} OPTIONAL,

crs-ChEstMPDCCH-ReciprocityTDD-r16 ENUMERATED {supported} OPTIONAL,

etws-CMAS-RxInConnCE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

etws-CMAS-RxInConnCE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

mpdcch-InLteControlRegionCE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

mpdcch-InLteControlRegionCE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

pdsch-InLteControlRegionCE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

pdsch-InLteControlRegionCE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

multiTB-Parameters-r16 CE-MultiTB-Parameters-r16 OPTIONAL,

resourceResvParameters-r16 CE-ResourceResvParameters-r16 OPTIONAL

} OPTIONAL,

widebandPRG-Slot-r16 ENUMERATED {supported} OPTIONAL,

widebandPRG-Subslot-r16 ENUMERATED {supported} OPTIONAL,

widebandPRG-Subframe-r16 ENUMERATED {supported} OPTIONAL,

addSRS-r16 SEQUENCE {

addSRS-FrequencyHopping-r16 ENUMERATED {supported} OPTIONAL,

addSRS-AntennaSwitching-r16 ENUMERATED {useBasic} OPTIONAL,

addSRS-CarrierSwitching-r16 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

virtualCellID-BasicSRS-r16 ENUMERATED {supported} OPTIONAL,

virtualCellID-AddSRS-r16 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-v1700 ::= SEQUENCE {

ce-Capabilities-v1700 SEQUENCE {

ce-PDSCH-14HARQProcesses-r17 ENUMERATED {supported} OPTIONAL,

ce-PDSCH-14HARQProcesses-Alt2-r17 ENUMERATED {supported} OPTIONAL,

ce-PDSCH-MaxTBS-r17 ENUMERATED {supported} OPTIONAL

} OPTIONAL

}

MIMO-UE-Parameters-r13 ::= SEQUENCE {

parametersTM9-r13 MIMO-UE-ParametersPerTM-r13 OPTIONAL,

parametersTM10-r13 MIMO-UE-ParametersPerTM-r13 OPTIONAL,

srs-EnhancementsTDD-r13 ENUMERATED {supported} OPTIONAL,

srs-Enhancements-r13 ENUMERATED {supported} OPTIONAL,

interferenceMeasRestriction-r13 ENUMERATED {supported} OPTIONAL

}

MIMO-UE-Parameters-v13e0 ::= SEQUENCE {

mimo-WeightedLayersCapabilities-r13 MIMO-WeightedLayersCapabilities-r13 OPTIONAL

}

MIMO-UE-Parameters-v1430 ::= SEQUENCE {

parametersTM9-v1430 MIMO-UE-ParametersPerTM-v1430 OPTIONAL,

parametersTM10-v1430 MIMO-UE-ParametersPerTM-v1430 OPTIONAL

}

MIMO-UE-Parameters-v1470 ::= SEQUENCE {

parametersTM9-v1470 MIMO-UE-ParametersPerTM-v1470,

parametersTM10-v1470 MIMO-UE-ParametersPerTM-v1470

}

MIMO-UE-ParametersPerTM-r13 ::= SEQUENCE {

nonPrecoded-r13 MIMO-NonPrecodedCapabilities-r13 OPTIONAL,

beamformed-r13 MIMO-UE-BeamformedCapabilities-r13 OPTIONAL,

channelMeasRestriction-r13 ENUMERATED {supported} OPTIONAL,

dmrs-Enhancements-r13 ENUMERATED {supported} OPTIONAL,

csi-RS-EnhancementsTDD-r13 ENUMERATED {supported} OPTIONAL

}

MIMO-UE-ParametersPerTM-v1430 ::= SEQUENCE {

nzp-CSI-RS-AperiodicInfo-r14 SEQUENCE {

nMaxProc-r14 INTEGER(5..32),

nMaxResource-r14 ENUMERATED {n1, n2, n4, n8}

} OPTIONAL,

nzp-CSI-RS-PeriodicInfo-r14 SEQUENCE {

nMaxResource-r14 ENUMERATED {n1, n2, n4, n8}

} OPTIONAL,

zp-CSI-RS-AperiodicInfo-r14 ENUMERATED {supported} OPTIONAL,

ul-dmrs-Enhancements-r14 ENUMERATED {supported} OPTIONAL,

densityReductionNP-r14 ENUMERATED {supported} OPTIONAL,

densityReductionBF-r14 ENUMERATED {supported} OPTIONAL,

hybridCSI-r14 ENUMERATED {supported} OPTIONAL,

semiOL-r14 ENUMERATED {supported} OPTIONAL,

csi-ReportingNP-r14 ENUMERATED {supported} OPTIONAL,

csi-ReportingAdvanced-r14 ENUMERATED {supported} OPTIONAL

}

MIMO-UE-ParametersPerTM-v1470 ::= SEQUENCE {

csi-ReportingAdvancedMaxPorts-r14 ENUMERATED {n8, n12, n16, n20, n24, n28} OPTIONAL

}

MIMO-CA-ParametersPerBoBC-r13 ::= SEQUENCE {

parametersTM9-r13 MIMO-CA-ParametersPerBoBCPerTM-r13 OPTIONAL,

parametersTM10-r13 MIMO-CA-ParametersPerBoBCPerTM-r13 OPTIONAL

}

MIMO-CA-ParametersPerBoBC-r15 ::= SEQUENCE {

parametersTM9-r15 MIMO-CA-ParametersPerBoBCPerTM-r15 OPTIONAL,

parametersTM10-r15 MIMO-CA-ParametersPerBoBCPerTM-r15 OPTIONAL

}

MIMO-CA-ParametersPerBoBC-v1430 ::= SEQUENCE {

parametersTM9-v1430 MIMO-CA-ParametersPerBoBCPerTM-v1430 OPTIONAL,

parametersTM10-v1430 MIMO-CA-ParametersPerBoBCPerTM-v1430 OPTIONAL

}

MIMO-CA-ParametersPerBoBC-v1470 ::= SEQUENCE {

parametersTM9-v1470 MIMO-CA-ParametersPerBoBCPerTM-v1470,

parametersTM10-v1470 MIMO-CA-ParametersPerBoBCPerTM-v1470

}

MIMO-CA-ParametersPerBoBCPerTM-r13 ::= SEQUENCE {

nonPrecoded-r13 MIMO-NonPrecodedCapabilities-r13 OPTIONAL,

beamformed-r13 MIMO-BeamformedCapabilityList-r13 OPTIONAL,

dmrs-Enhancements-r13 ENUMERATED {different} OPTIONAL

}

MIMO-CA-ParametersPerBoBCPerTM-v1430 ::= SEQUENCE {

csi-ReportingNP-r14 ENUMERATED {different} OPTIONAL,

csi-ReportingAdvanced-r14 ENUMERATED {different} OPTIONAL

}

MIMO-CA-ParametersPerBoBCPerTM-v1470 ::= SEQUENCE {

csi-ReportingAdvancedMaxPorts-r14 ENUMERATED {n8, n12, n16, n20, n24, n28} OPTIONAL

}

MIMO-CA-ParametersPerBoBCPerTM-r15 ::= SEQUENCE {

nonPrecoded-r13 MIMO-NonPrecodedCapabilities-r13 OPTIONAL,

beamformed-r13 MIMO-BeamformedCapabilityList-r13 OPTIONAL,

dmrs-Enhancements-r13 ENUMERATED {different} OPTIONAL,

csi-ReportingNP-r14 ENUMERATED {different} OPTIONAL,

csi-ReportingAdvanced-r14 ENUMERATED {different} OPTIONAL

}

MIMO-NonPrecodedCapabilities-r13 ::= SEQUENCE {

config1-r13 ENUMERATED {supported} OPTIONAL,

config2-r13 ENUMERATED {supported} OPTIONAL,

config3-r13 ENUMERATED {supported} OPTIONAL,

config4-r13 ENUMERATED {supported} OPTIONAL

}

MIMO-UE-BeamformedCapabilities-r13 ::= SEQUENCE {

altCodebook-r13 ENUMERATED {supported} OPTIONAL,

mimo-BeamformedCapabilities-r13 MIMO-BeamformedCapabilityList-r13

}

MIMO-BeamformedCapabilityList-r13 ::= SEQUENCE (SIZE (1..maxCSI-Proc-r11)) OF MIMO-BeamformedCapabilities-r13

MIMO-BeamformedCapabilities-r13 ::= SEQUENCE {

k-Max-r13 INTEGER (1..8),

n-MaxList-r13 BIT STRING (SIZE (1..7)) OPTIONAL

}

MIMO-WeightedLayersCapabilities-r13 ::= SEQUENCE {

relWeightTwoLayers-r13 ENUMERATED {v1, v1dot25, v1dot5, v1dot75, v2, v2dot5, v3, v4},

relWeightFourLayers-r13 ENUMERATED {v1, v1dot25, v1dot5, v1dot75, v2, v2dot5, v3, v4} OPTIONAL,

relWeightEightLayers-r13 ENUMERATED {v1, v1dot25, v1dot5, v1dot75, v2, v2dot5, v3, v4} OPTIONAL,

totalWeightedLayers-r13 INTEGER (2..128)

}

NonContiguousUL-RA-WithinCC-List-r10 ::= SEQUENCE (SIZE (1..maxBands)) OF NonContiguousUL-RA-WithinCC-r10

NonContiguousUL-RA-WithinCC-r10 ::= SEQUENCE {

nonContiguousUL-RA-WithinCC-Info-r10 ENUMERATED {supported} OPTIONAL

}

RF-Parameters ::= SEQUENCE {

supportedBandListEUTRA SupportedBandListEUTRA

}

RF-Parameters-v9e0 ::= SEQUENCE {

supportedBandListEUTRA-v9e0 SupportedBandListEUTRA-v9e0 OPTIONAL

}

RF-Parameters-v1020 ::= SEQUENCE {

supportedBandCombination-r10 SupportedBandCombination-r10

}

RF-Parameters-v1060 ::= SEQUENCE {

supportedBandCombinationExt-r10 SupportedBandCombinationExt-r10

}

RF-Parameters-v1090 ::= SEQUENCE {

supportedBandCombination-v1090 SupportedBandCombination-v1090 OPTIONAL

}

RF-Parameters-v10f0 ::= SEQUENCE {

modifiedMPR-Behavior-r10 BIT STRING (SIZE (32)) OPTIONAL

}

RF-Parameters-v10i0 ::= SEQUENCE {

supportedBandCombination-v10i0 SupportedBandCombination-v10i0 OPTIONAL

}

RF-Parameters-v10j0 ::= SEQUENCE {

multiNS-Pmax-r10 ENUMERATED {supported} OPTIONAL

}

RF-Parameters-v1130 ::= SEQUENCE {

supportedBandCombination-v1130 SupportedBandCombination-v1130 OPTIONAL

}

RF-Parameters-v1180 ::= SEQUENCE {

freqBandRetrieval-r11 ENUMERATED {supported} OPTIONAL,

requestedBands-r11 SEQUENCE (SIZE (1.. maxBands)) OF FreqBandIndicator-r11 OPTIONAL,

supportedBandCombinationAdd-r11 SupportedBandCombinationAdd-r11 OPTIONAL

}

RF-Parameters-v11d0 ::= SEQUENCE {

supportedBandCombinationAdd-v11d0 SupportedBandCombinationAdd-v11d0 OPTIONAL

}

RF-Parameters-v1250 ::= SEQUENCE {

supportedBandListEUTRA-v1250 SupportedBandListEUTRA-v1250 OPTIONAL,

supportedBandCombination-v1250 SupportedBandCombination-v1250 OPTIONAL,

supportedBandCombinationAdd-v1250 SupportedBandCombinationAdd-v1250 OPTIONAL,

freqBandPriorityAdjustment-r12 ENUMERATED {supported} OPTIONAL

}

RF-Parameters-v1270 ::= SEQUENCE {

supportedBandCombination-v1270 SupportedBandCombination-v1270 OPTIONAL,

supportedBandCombinationAdd-v1270 SupportedBandCombinationAdd-v1270 OPTIONAL

}

RF-Parameters-v1310 ::= SEQUENCE {

eNB-RequestedParameters-r13 SEQUENCE {

reducedIntNonContCombRequested-r13 ENUMERATED {true} OPTIONAL,

requestedCCsDL-r13 INTEGER (2..32) OPTIONAL,

requestedCCsUL-r13 INTEGER (2..32) OPTIONAL,

skipFallbackCombRequested-r13 ENUMERATED {true} OPTIONAL

} OPTIONAL,

maximumCCsRetrieval-r13 ENUMERATED {supported} OPTIONAL,

skipFallbackCombinations-r13 ENUMERATED {supported} OPTIONAL,

reducedIntNonContComb-r13 ENUMERATED {supported} OPTIONAL,

supportedBandListEUTRA-v1310 SupportedBandListEUTRA-v1310 OPTIONAL,

supportedBandCombinationReduced-r13 SupportedBandCombinationReduced-r13 OPTIONAL

}

RF-Parameters-v1320 ::= SEQUENCE {

supportedBandListEUTRA-v1320 SupportedBandListEUTRA-v1320 OPTIONAL,

supportedBandCombination-v1320 SupportedBandCombination-v1320 OPTIONAL,

supportedBandCombinationAdd-v1320 SupportedBandCombinationAdd-v1320 OPTIONAL,

supportedBandCombinationReduced-v1320 SupportedBandCombinationReduced-v1320 OPTIONAL

}

RF-Parameters-v1380 ::= SEQUENCE {

supportedBandCombination-v1380 SupportedBandCombination-v1380 OPTIONAL,

supportedBandCombinationAdd-v1380 SupportedBandCombinationAdd-v1380 OPTIONAL,

supportedBandCombinationReduced-v1380 SupportedBandCombinationReduced-v1380 OPTIONAL

}

RF-Parameters-v1390 ::= SEQUENCE {

supportedBandCombination-v1390 SupportedBandCombination-v1390 OPTIONAL,

supportedBandCombinationAdd-v1390 SupportedBandCombinationAdd-v1390 OPTIONAL,

supportedBandCombinationReduced-v1390 SupportedBandCombinationReduced-v1390 OPTIONAL

}

RF-Parameters-v12b0 ::= SEQUENCE {

maxLayersMIMO-Indication-r12 ENUMERATED {supported} OPTIONAL

}

RF-Parameters-v1430 ::= SEQUENCE {

supportedBandCombination-v1430 SupportedBandCombination-v1430 OPTIONAL,

supportedBandCombinationAdd-v1430 SupportedBandCombinationAdd-v1430 OPTIONAL,

supportedBandCombinationReduced-v1430 SupportedBandCombinationReduced-v1430 OPTIONAL,

eNB-RequestedParameters-v1430 SEQUENCE {

requestedDiffFallbackCombList-r14 BandCombinationList-r14

} OPTIONAL,

diffFallbackCombReport-r14 ENUMERATED {supported} OPTIONAL

}

RF-Parameters-v1450 ::= SEQUENCE {

supportedBandCombination-v1450 SupportedBandCombination-v1450 OPTIONAL,

supportedBandCombinationAdd-v1450 SupportedBandCombinationAdd-v1450 OPTIONAL,

supportedBandCombinationReduced-v1450 SupportedBandCombinationReduced-v1450 OPTIONAL

}

RF-Parameters-v1470 ::= SEQUENCE {

supportedBandCombination-v1470 SupportedBandCombination-v1470 OPTIONAL,

supportedBandCombinationAdd-v1470 SupportedBandCombinationAdd-v1470 OPTIONAL,

supportedBandCombinationReduced-v1470 SupportedBandCombinationReduced-v1470 OPTIONAL

}

RF-Parameters-v14b0 ::= SEQUENCE {

supportedBandCombination-v14b0 SupportedBandCombination-v14b0 OPTIONAL,

supportedBandCombinationAdd-v14b0 SupportedBandCombinationAdd-v14b0 OPTIONAL,

supportedBandCombinationReduced-v14b0 SupportedBandCombinationReduced-v14b0 OPTIONAL

}

RF-Parameters-v1530 ::= SEQUENCE {

sTTI-SPT-Supported-r15 ENUMERATED {supported} OPTIONAL,

supportedBandCombination-v1530 SupportedBandCombination-v1530 OPTIONAL,

supportedBandCombinationAdd-v1530 SupportedBandCombinationAdd-v1530 OPTIONAL,

supportedBandCombinationReduced-v1530 SupportedBandCombinationReduced-v1530 OPTIONAL,

powerClass-14dBm-r15 ENUMERATED {supported} OPTIONAL

}

RF-Parameters-v1570 ::= SEQUENCE {

dl-1024QAM-ScalingFactor-r15 ENUMERATED {v1, v1dot2, v1dot25},

dl-1024QAM-TotalWeightedLayers-r15 INTEGER (0..10)

}

RF-Parameters-v1610 ::= SEQUENCE {

supportedBandCombination-v1610 SupportedBandCombination-v1610 OPTIONAL,

supportedBandCombinationAdd-v1610 SupportedBandCombinationAdd-v1610 OPTIONAL,

supportedBandCombinationReduced-v1610 SupportedBandCombinationReduced-v1610 OPTIONAL

}

RF-Parameters-v1630 ::= SEQUENCE {

supportedBandCombination-v1630 SupportedBandCombination-v1630 OPTIONAL,

supportedBandCombinationAdd-v1630 SupportedBandCombinationAdd-v1630 OPTIONAL,

supportedBandCombinationReduced-v1630 SupportedBandCombinationReduced-v1630 OPTIONAL

}

SkipSubframeProcessing-r15 ::= SEQUENCE {

skipProcessingDL-Slot-r15 INTEGER (0..3) OPTIONAL,

skipProcessingDL-SubSlot-r15 INTEGER (0..3) OPTIONAL,

skipProcessingUL-Slot-r15 INTEGER (0..3) OPTIONAL,

skipProcessingUL-SubSlot-r15 INTEGER (0..3) OPTIONAL

}

SPT-Parameters-r15 ::= SEQUENCE {

frameStructureType-SPT-r15 BIT STRING (SIZE (3)) OPTIONAL,

maxNumberCCs-SPT-r15 INTEGER (1..32) OPTIONAL

}

STTI-SPT-BandParameters-r15 ::= SEQUENCE {

dl-1024QAM-Slot-r15 ENUMERATED {supported} OPTIONAL,

dl-1024QAM-SubslotTA-1-r15 ENUMERATED {supported} OPTIONAL,

dl-1024QAM-SubslotTA-2-r15 ENUMERATED {supported} OPTIONAL,

simultaneousTx-differentTx-duration-r15 ENUMERATED {supported} OPTIONAL,

sTTI-CA-MIMO-ParametersDL-r15 CA-MIMO-ParametersDL-r15 OPTIONAL,

sTTI-CA-MIMO-ParametersUL-r15 CA-MIMO-ParametersUL-r15,

sTTI-FD-MIMO-Coexistence ENUMERATED {supported} OPTIONAL,

sTTI-MIMO-CA-ParametersPerBoBCs-r15 MIMO-CA-ParametersPerBoBC-r13 OPTIONAL,

sTTI-MIMO-CA-ParametersPerBoBCs-v1530 MIMO-CA-ParametersPerBoBC-v1430 OPTIONAL,

sTTI-SupportedCombinations-r15 STTI-SupportedCombinations-r15 OPTIONAL,

sTTI-SupportedCSI-Proc-r15 ENUMERATED {n1, n3, n4} OPTIONAL,

ul-256QAM-Slot-r15 ENUMERATED {supported} OPTIONAL,

ul-256QAM-Subslot-r15 ENUMERATED {supported} OPTIONAL,

...

}

STTI-SupportedCombinations-r15 ::= SEQUENCE {

combination-22-r15 DL-UL-CCs-r15 OPTIONAL,

combination-77-r15 DL-UL-CCs-r15 OPTIONAL,

combination-27-r15 DL-UL-CCs-r15 OPTIONAL,

combination-22-27-r15 SEQUENCE (SIZE (1..2)) OF DL-UL-CCs-r15 OPTIONAL,

combination-77-22-r15 SEQUENCE (SIZE (1..2)) OF DL-UL-CCs-r15 OPTIONAL,

combination-77-27-r15 SEQUENCE (SIZE (1..2)) OF DL-UL-CCs-r15 OPTIONAL

}

DL-UL-CCs-r15 ::= SEQUENCE {

maxNumberDL-CCs-r15 INTEGER (1..32) OPTIONAL,

maxNumberUL-CCs-r15 INTEGER (1..32) OPTIONAL

}

SupportedBandCombination-r10 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-r10

SupportedBandCombinationExt-r10 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParametersExt-r10

SupportedBandCombination-v1090 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1090

SupportedBandCombination-v10i0 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v10i0

SupportedBandCombination-v1130 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1130

SupportedBandCombination-v1250 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1250

SupportedBandCombination-v1270 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1270

SupportedBandCombination-v1320 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1320

SupportedBandCombination-v1380 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1380

SupportedBandCombination-v1390 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1390

SupportedBandCombination-v1430 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1430

SupportedBandCombination-v1450 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1450

SupportedBandCombination-v1470 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1470

SupportedBandCombination-v14b0 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v14b0

SupportedBandCombination-v1530 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1530

SupportedBandCombination-v1610 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1610

SupportedBandCombination-v1630 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandCombinationParameters-v1630

SupportedBandCombinationAdd-r11 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-r11

SupportedBandCombinationAdd-v11d0 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v10i0

SupportedBandCombinationAdd-v1250 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1250

SupportedBandCombinationAdd-v1270 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1270

SupportedBandCombinationAdd-v1320 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1320

SupportedBandCombinationAdd-v1380 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1380

SupportedBandCombinationAdd-v1390 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1390

SupportedBandCombinationAdd-v1430 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1430

SupportedBandCombinationAdd-v1450 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1450

SupportedBandCombinationAdd-v1470 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1470

SupportedBandCombinationAdd-v14b0 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v14b0

SupportedBandCombinationAdd-v1530 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1530

SupportedBandCombinationAdd-v1610 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1610

SupportedBandCombinationAdd-v1630 ::= SEQUENCE (SIZE (1..maxBandComb-r11)) OF BandCombinationParameters-v1630

SupportedBandCombinationReduced-r13 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-r13

SupportedBandCombinationReduced-v1320 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1320

SupportedBandCombinationReduced-v1380 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1380

SupportedBandCombinationReduced-v1390 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1390

SupportedBandCombinationReduced-v1430 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1430

SupportedBandCombinationReduced-v1450 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1450

SupportedBandCombinationReduced-v1470 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1470

SupportedBandCombinationReduced-v14b0 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v14b0

SupportedBandCombinationReduced-v1530 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1530

SupportedBandCombinationReduced-v1610 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1610

SupportedBandCombinationReduced-v1630 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF BandCombinationParameters-v1630

BandCombinationParameters-r10 ::= SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF BandParameters-r10

BandCombinationParametersExt-r10 ::= SEQUENCE {

supportedBandwidthCombinationSet-r10 SupportedBandwidthCombinationSet-r10 OPTIONAL

}

BandCombinationParameters-v1090 ::= SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF BandParameters-v1090

BandCombinationParameters-v10i0::= SEQUENCE {

bandParameterList-v10i0 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

BandParameters-v10i0 OPTIONAL

}

BandCombinationParameters-v1130 ::= SEQUENCE {

multipleTimingAdvance-r11 ENUMERATED {supported} OPTIONAL,

simultaneousRx-Tx-r11 ENUMERATED {supported} OPTIONAL,

bandParameterList-r11 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF BandParameters-v1130 OPTIONAL,

...

}

BandCombinationParameters-r11 ::= SEQUENCE {

bandParameterList-r11 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

BandParameters-r11,

supportedBandwidthCombinationSet-r11 SupportedBandwidthCombinationSet-r10 OPTIONAL,

multipleTimingAdvance-r11 ENUMERATED {supported} OPTIONAL,

simultaneousRx-Tx-r11 ENUMERATED {supported} OPTIONAL,

bandInfoEUTRA-r11 BandInfoEUTRA,

...

}

BandCombinationParameters-v1250::= SEQUENCE {

dc-Support-r12 SEQUENCE {

asynchronous-r12 ENUMERATED {supported} OPTIONAL,

supportedCellGrouping-r12 CHOICE {

threeEntries-r12 BIT STRING (SIZE(3)),

fourEntries-r12 BIT STRING (SIZE(7)),

fiveEntries-r12 BIT STRING (SIZE(15))

} OPTIONAL

} OPTIONAL,

supportedNAICS-2CRS-AP-r12 BIT STRING (SIZE (1..maxNAICS-Entries-r12)) OPTIONAL,

commSupportedBandsPerBC-r12 BIT STRING (SIZE (1.. maxBands)) OPTIONAL,

...

}

BandCombinationParameters-v1270 ::= SEQUENCE {

bandParameterList-v1270 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

BandParameters-v1270 OPTIONAL

}

BandCombinationParameters-r13 ::= SEQUENCE {

differentFallbackSupported-r13 ENUMERATED {true} OPTIONAL,

bandParameterList-r13 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF BandParameters-r13,

supportedBandwidthCombinationSet-r13 SupportedBandwidthCombinationSet-r10 OPTIONAL,

multipleTimingAdvance-r13 ENUMERATED {supported} OPTIONAL,

simultaneousRx-Tx-r13 ENUMERATED {supported} OPTIONAL,

bandInfoEUTRA-r13 BandInfoEUTRA,

dc-Support-r13 SEQUENCE {

asynchronous-r13 ENUMERATED {supported} OPTIONAL,

supportedCellGrouping-r13 CHOICE {

threeEntries-r13 BIT STRING (SIZE(3)),

fourEntries-r13 BIT STRING (SIZE(7)),

fiveEntries-r13 BIT STRING (SIZE(15))

} OPTIONAL

} OPTIONAL,

supportedNAICS-2CRS-AP-r13 BIT STRING (SIZE (1..maxNAICS-Entries-r12)) OPTIONAL,

commSupportedBandsPerBC-r13 BIT STRING (SIZE (1.. maxBands)) OPTIONAL

}

BandCombinationParameters-v1320 ::= SEQUENCE {

bandParameterList-v1320 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

BandParameters-v1320 OPTIONAL,

additionalRx-Tx-PerformanceReq-r13 ENUMERATED {supported} OPTIONAL

}

BandCombinationParameters-v1380 ::= SEQUENCE {

bandParameterList-v1380 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

BandParameters-v1380 OPTIONAL

}

BandCombinationParameters-v1390 ::= SEQUENCE {

ue-CA-PowerClass-N-r13 ENUMERATED {class2} OPTIONAL

}

BandCombinationParameters-v1430 ::= SEQUENCE {

bandParameterList-v1430 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

BandParameters-v1430 OPTIONAL,

v2x-SupportedTxBandCombListPerBC-r14 BIT STRING (SIZE (1.. maxBandComb-r13)) OPTIONAL,

v2x-SupportedRxBandCombListPerBC-r14 BIT STRING (SIZE (1.. maxBandComb-r13)) OPTIONAL

}

BandCombinationParameters-v1450 ::= SEQUENCE {

bandParameterList-v1450 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

BandParameters-v1450 OPTIONAL

}

BandCombinationParameters-v1470 ::= SEQUENCE {

bandParameterList-v1470 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

BandParameters-v1470 OPTIONAL,

srs-MaxSimultaneousCCs-r14 INTEGER (1..31) OPTIONAL

}

BandCombinationParameters-v14b0 ::= SEQUENCE {

bandParameterList-v14b0 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

BandParameters-v14b0 OPTIONAL

}

BandCombinationParameters-v1530 ::= SEQUENCE {

bandParameterList-v1530 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF BandParameters-v1530 OPTIONAL,

spt-Parameters-r15 SPT-Parameters-r15 OPTIONAL

}

-- If an additional band combination parameter is defined, which is supported for MR-DC,

-- it shall be defined in the IE CA-ParametersEUTRA in TS 38.331 [82].

BandCombinationParameters-v1610 ::= SEQUENCE {

measGapInfoNR MeasGapInfoNR OPTIONAL,

bandParameterList-v1610 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF BandParameters-v1610 OPTIONAL,

interFreqDAPS-r16 SEQUENCE {

interFreqAsyncDAPS-r16 ENUMERATED {supported} OPTIONAL,

interFreqMultiUL-TransmissionDAPS-r16 ENUMERATED {supported} OPTIONAL

} OPTIONAL

}

BandCombinationParameters-v1630 ::= SEQUENCE {

v2x-SupportedTxBandCombListPerBC-v1630 BIT STRING (SIZE (1..maxBandCombSidelinkNR-r16)) OPTIONAL,

v2x-SupportedRxBandCombListPerBC-v1630 BIT STRING (SIZE (1..maxBandCombSidelinkNR-r16)) OPTIONAL,

scalingFactorTxSidelink-r16 SEQUENCE (SIZE (1..maxBandCombSidelinkNR-r16)) OF ScalingFactorSidelink-r16 OPTIONAL,

scalingFactorRxSidelink-r16 SEQUENCE (SIZE (1..maxBandCombSidelinkNR-r16)) OF ScalingFactorSidelink-r16 OPTIONAL,

interBandPowerSharingSyncDAPS-r16 ENUMERATED {supported} OPTIONAL,

interBandPowerSharingAsyncDAPS-r16 ENUMERATED {supported} OPTIONAL

}

ScalingFactorSidelink-r16 ::= ENUMERATED {f0p4, f0p75, f0p8, f1}

SupportedBandwidthCombinationSet-r10 ::= BIT STRING (SIZE (1..maxBandwidthCombSet-r10))

BandParameters-r10 ::= SEQUENCE {

bandEUTRA-r10 FreqBandIndicator,

bandParametersUL-r10 BandParametersUL-r10 OPTIONAL,

bandParametersDL-r10 BandParametersDL-r10 OPTIONAL

}

BandParameters-v1090 ::= SEQUENCE {

bandEUTRA-v1090 FreqBandIndicator-v9e0 OPTIONAL,

...

}

BandParameters-v10i0::= SEQUENCE {

bandParametersDL-v10i0 SEQUENCE (SIZE (1..maxBandwidthClass-r10)) OF CA-MIMO-ParametersDL-v10i0

}

BandParameters-v1130 ::= SEQUENCE {

supportedCSI-Proc-r11 ENUMERATED {n1, n3, n4}

}

BandParameters-r11 ::= SEQUENCE {

bandEUTRA-r11 FreqBandIndicator-r11,

bandParametersUL-r11 BandParametersUL-r10 OPTIONAL,

bandParametersDL-r11 BandParametersDL-r10 OPTIONAL,

supportedCSI-Proc-r11 ENUMERATED {n1, n3, n4} OPTIONAL

}

BandParameters-v1270 ::= SEQUENCE {

bandParametersDL-v1270 SEQUENCE (SIZE (1..maxBandwidthClass-r10)) OF CA-MIMO-ParametersDL-v1270

}

BandParameters-r13 ::= SEQUENCE {

bandEUTRA-r13 FreqBandIndicator-r11,

bandParametersUL-r13 BandParametersUL-r13 OPTIONAL,

bandParametersDL-r13 BandParametersDL-r13 OPTIONAL,

supportedCSI-Proc-r13 ENUMERATED {n1, n3, n4} OPTIONAL

}

BandParameters-v1320 ::= SEQUENCE {

bandParametersDL-v1320 MIMO-CA-ParametersPerBoBC-r13

}

BandParameters-v1380 ::= SEQUENCE {

txAntennaSwitchDL-r13 INTEGER (1..32) OPTIONAL,

txAntennaSwitchUL-r13 INTEGER (1..32) OPTIONAL

}

BandParameters-v1430 ::= SEQUENCE {

bandParametersDL-v1430 MIMO-CA-ParametersPerBoBC-v1430 OPTIONAL,

ul-256QAM-r14 ENUMERATED {supported} OPTIONAL,

ul-256QAM-perCC-InfoList-r14 SEQUENCE (SIZE (2..maxServCell-r13)) OF UL-256QAM-perCC-Info-r14 OPTIONAL,

srs-CapabilityPerBandPairList-r14 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

SRS-CapabilityPerBandPair-r14 OPTIONAL

}

BandParameters-v1450 ::= SEQUENCE {

must-CapabilityPerBand-r14 MUST-Parameters-r14 OPTIONAL

}

BandParameters-v1470 ::= SEQUENCE {

bandParametersDL-v1470 MIMO-CA-ParametersPerBoBC-v1470 OPTIONAL

}

BandParameters-v14b0 ::= SEQUENCE {

srs-CapabilityPerBandPairList-v14b0 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF SRS-CapabilityPerBandPair-v14b0 OPTIONAL

}

BandParameters-v1530 ::= SEQUENCE {

ue-TxAntennaSelection-SRS-1T4R-r15 ENUMERATED {supported} OPTIONAL,

ue-TxAntennaSelection-SRS-2T4R-2Pairs-r15 ENUMERATED {supported} OPTIONAL,

ue-TxAntennaSelection-SRS-2T4R-3Pairs-r15 ENUMERATED {supported} OPTIONAL,

dl-1024QAM-r15 ENUMERATED {supported} OPTIONAL,

qcl-TypeC-Operation-r15 ENUMERATED {supported} OPTIONAL,

qcl-CRI-BasedCSI-Reporting-r15 ENUMERATED {supported} OPTIONAL,

stti-SPT-BandParameters-r15 STTI-SPT-BandParameters-r15 OPTIONAL

}

BandParameters-v1610 ::= SEQUENCE {

intraFreqDAPS-r16 SEQUENCE {

intraFreqAsyncDAPS-r16 ENUMERATED {supported} OPTIONAL,

dummy ENUMERATED {supported} OPTIONAL,

intraFreqTwoTAGs-DAPS-r16 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

addSRS-FrequencyHopping-r16 ENUMERATED {supported} OPTIONAL,

addSRS-AntennaSwitching-r16 SEQUENCE {

addSRS-1T2R-r16 ENUMERATED {supported} OPTIONAL,

addSRS-1T4R-r16 ENUMERATED {supported} OPTIONAL,

addSRS-2T4R-2pairs-r16 ENUMERATED {supported} OPTIONAL,

addSRS-2T4R-3pairs-r16 ENUMERATED {supported} OPTIONAL

} OPTIONAL,

srs-CapabilityPerBandPairList-v1610 SEQUENCE (SIZE (1..maxSimultaneousBands-r10)) OF

SRS-CapabilityPerBandPair-v1610 OPTIONAL

}

V2X-BandParameters-r14 ::= SEQUENCE {

v2x-FreqBandEUTRA-r14 FreqBandIndicator-r11,

bandParametersTxSL-r14 BandParametersTxSL-r14 OPTIONAL,

bandParametersRxSL-r14 BandParametersRxSL-r14 OPTIONAL

}

V2X-BandParameters-v1530 ::= SEQUENCE {

v2x-EnhancedHighReception-r15 ENUMERATED {supported} OPTIONAL

}

BandParametersTxSL-r14 ::= SEQUENCE {

v2x-BandwidthClassTxSL-r14 V2X-BandwidthClassSL-r14,

v2x-eNB-Scheduled-r14 ENUMERATED {supported} OPTIONAL,

v2x-HighPower-r14 ENUMERATED {supported} OPTIONAL

}

BandParametersRxSL-r14 ::= SEQUENCE {

v2x-BandwidthClassRxSL-r14 V2X-BandwidthClassSL-r14,

v2x-HighReception-r14 ENUMERATED {supported} OPTIONAL

}

V2X-BandwidthClassSL-r14 ::= SEQUENCE (SIZE (1..maxBandwidthClass-r10)) OF V2X-BandwidthClass-r14

UL-256QAM-perCC-Info-r14 ::= SEQUENCE {

ul-256QAM-perCC-r14 ENUMERATED {supported} OPTIONAL

}

FeatureSetDL-r15 ::= SEQUENCE {

mimo-CA-ParametersPerBoBC-r15 MIMO-CA-ParametersPerBoBC-r15 OPTIONAL,

featureSetPerCC-ListDL-r15 SEQUENCE (SIZE (1..maxServCell-r13)) OF FeatureSetDL-PerCC-Id-r15

}

FeatureSetDL-v1550 ::= SEQUENCE {

dl-1024QAM-r15 ENUMERATED {supported} OPTIONAL

}

FeatureSetDL-PerCC-r15 ::= SEQUENCE {

fourLayerTM3-TM4-r15 ENUMERATED {supported} OPTIONAL,

supportedMIMO-CapabilityDL-MRDC-r15 MIMO-CapabilityDL-r10 OPTIONAL,

supportedCSI-Proc-r15 ENUMERATED {n1, n3, n4} OPTIONAL

}

FeatureSetUL-r15 ::= SEQUENCE {

featureSetPerCC-ListUL-r15 SEQUENCE (SIZE(1..maxServCell-r13)) OF FeatureSetUL-PerCC-Id-r15

}

FeatureSetUL-PerCC-r15 ::= SEQUENCE {

supportedMIMO-CapabilityUL-r15 MIMO-CapabilityUL-r10 OPTIONAL,

ul-256QAM-r15 ENUMERATED {supported} OPTIONAL

}

FeatureSetDL-PerCC-Id-r15 ::= INTEGER (0..maxPerCC-FeatureSets-r15)

FeatureSetUL-PerCC-Id-r15 ::= INTEGER (0..maxPerCC-FeatureSets-r15)

BandParametersUL-r10 ::= SEQUENCE (SIZE (1..maxBandwidthClass-r10)) OF CA-MIMO-ParametersUL-r10

BandParametersUL-r13 ::= CA-MIMO-ParametersUL-r10

CA-MIMO-ParametersUL-r10 ::= SEQUENCE {

ca-BandwidthClassUL-r10 CA-BandwidthClass-r10,

supportedMIMO-CapabilityUL-r10 MIMO-CapabilityUL-r10 OPTIONAL

}

CA-MIMO-ParametersUL-r15 ::= SEQUENCE {

supportedMIMO-CapabilityUL-r15 MIMO-CapabilityUL-r10 OPTIONAL

}

BandParametersDL-r10 ::= SEQUENCE (SIZE (1..maxBandwidthClass-r10)) OF CA-MIMO-ParametersDL-r10

BandParametersDL-r13 ::= CA-MIMO-ParametersDL-r13

CA-MIMO-ParametersDL-r10 ::= SEQUENCE {

ca-BandwidthClassDL-r10 CA-BandwidthClass-r10,

supportedMIMO-CapabilityDL-r10 MIMO-CapabilityDL-r10 OPTIONAL

}

CA-MIMO-ParametersDL-v10i0 ::= SEQUENCE {

fourLayerTM3-TM4-r10 ENUMERATED {supported} OPTIONAL

}

CA-MIMO-ParametersDL-v1270 ::= SEQUENCE {

intraBandContiguousCC-InfoList-r12 SEQUENCE (SIZE (1..maxServCell-r10)) OF IntraBandContiguousCC-Info-r12

}

CA-MIMO-ParametersDL-r13 ::= SEQUENCE {

ca-BandwidthClassDL-r13 CA-BandwidthClass-r10,

supportedMIMO-CapabilityDL-r13 MIMO-CapabilityDL-r10 OPTIONAL,

fourLayerTM3-TM4-r13 ENUMERATED {supported} OPTIONAL,

intraBandContiguousCC-InfoList-r13 SEQUENCE (SIZE (1..maxServCell-r13)) OF IntraBandContiguousCC-Info-r12

}

CA-MIMO-ParametersDL-r15 ::= SEQUENCE {

supportedMIMO-CapabilityDL-r15 MIMO-CapabilityDL-r10 OPTIONAL,

fourLayerTM3-TM4-r15 ENUMERATED {supported} OPTIONAL,

intraBandContiguousCC-InfoList-r15 SEQUENCE (SIZE (1..maxServCell-r13)) OF

IntraBandContiguousCC-Info-r12 OPTIONAL

}

IntraBandContiguousCC-Info-r12 ::= SEQUENCE {

fourLayerTM3-TM4-perCC-r12 ENUMERATED {supported} OPTIONAL,

supportedMIMO-CapabilityDL-r12 MIMO-CapabilityDL-r10 OPTIONAL,

supportedCSI-Proc-r12 ENUMERATED {n1, n3, n4} OPTIONAL

}

CA-BandwidthClass-r10 ::= ENUMERATED {a, b, c, d, e, f, ...}

V2X-BandwidthClass-r14 ::= ENUMERATED {a, b, c, d, e, f, ..., c1-v1530}

MIMO-CapabilityUL-r10 ::= ENUMERATED {twoLayers, fourLayers}

MIMO-CapabilityDL-r10 ::= ENUMERATED {twoLayers, fourLayers, eightLayers}

MUST-Parameters-r14 ::= SEQUENCE {

must-TM234-UpTo2Tx-r14 ENUMERATED {supported} OPTIONAL,

must-TM89-UpToOneInterferingLayer-r14 ENUMERATED {supported} OPTIONAL,

must-TM10-UpToOneInterferingLayer-r14 ENUMERATED {supported} OPTIONAL,

must-TM89-UpToThreeInterferingLayers-r14 ENUMERATED {supported} OPTIONAL,

must-TM10-UpToThreeInterferingLayers-r14 ENUMERATED {supported} OPTIONAL

}

SupportedBandListEUTRA ::= SEQUENCE (SIZE (1..maxBands)) OF SupportedBandEUTRA

SupportedBandListEUTRA-v9e0::= SEQUENCE (SIZE (1..maxBands)) OF SupportedBandEUTRA-v9e0

SupportedBandListEUTRA-v1250 ::= SEQUENCE (SIZE (1..maxBands)) OF SupportedBandEUTRA-v1250

SupportedBandListEUTRA-v1310 ::= SEQUENCE (SIZE (1..maxBands)) OF SupportedBandEUTRA-v1310

SupportedBandListEUTRA-v1320 ::= SEQUENCE (SIZE (1..maxBands)) OF SupportedBandEUTRA-v1320

SupportedBandEUTRA ::= SEQUENCE {

bandEUTRA FreqBandIndicator,

halfDuplex BOOLEAN

}

SupportedBandEUTRA-v9e0 ::= SEQUENCE {

bandEUTRA-v9e0 FreqBandIndicator-v9e0 OPTIONAL

}

SupportedBandEUTRA-v1250 ::= SEQUENCE {

dl-256QAM-r12 ENUMERATED {supported} OPTIONAL,

ul-64QAM-r12 ENUMERATED {supported} OPTIONAL

}

SupportedBandEUTRA-v1310 ::= SEQUENCE {

ue-PowerClass-5-r13 ENUMERATED {supported} OPTIONAL

}

SupportedBandEUTRA-v1320 ::= SEQUENCE {

intraFreq-CE-NeedForGaps-r13 ENUMERATED {supported} OPTIONAL,

ue-PowerClass-N-r13 ENUMERATED {class1, class2, class4} OPTIONAL

}

MeasParameters ::= SEQUENCE {

bandListEUTRA BandListEUTRA

}

MeasParameters-v1020 ::= SEQUENCE {

bandCombinationListEUTRA-r10 BandCombinationListEUTRA-r10

}

MeasParameters-v1130 ::= SEQUENCE {

rsrqMeasWideband-r11 ENUMERATED {supported} OPTIONAL

}

MeasParameters-v11a0 ::= SEQUENCE {

benefitsFromInterruption-r11 ENUMERATED {true} OPTIONAL

}

MeasParameters-v1250 ::= SEQUENCE {

timerT312-r12 ENUMERATED {supported} OPTIONAL,

alternativeTimeToTrigger-r12 ENUMERATED {supported} OPTIONAL,

incMonEUTRA-r12 ENUMERATED {supported} OPTIONAL,

incMonUTRA-r12 ENUMERATED {supported} OPTIONAL,

extendedMaxMeasId-r12 ENUMERATED {supported} OPTIONAL,

extendedRSRQ-LowerRange-r12 ENUMERATED {supported} OPTIONAL,

rsrq-OnAllSymbols-r12 ENUMERATED {supported} OPTIONAL,

crs-DiscoverySignalsMeas-r12 ENUMERATED {supported} OPTIONAL,

csi-RS-DiscoverySignalsMeas-r12 ENUMERATED {supported} OPTIONAL

}

MeasParameters-v1310 ::= SEQUENCE {

rs-SINR-Meas-r13 ENUMERATED {supported} OPTIONAL,

allowedCellList-r13 ENUMERATED {supported} OPTIONAL,

extendedMaxObjectId-r13 ENUMERATED {supported} OPTIONAL,

ul-PDCP-Delay-r13 ENUMERATED {supported} OPTIONAL,

extendedFreqPriorities-r13 ENUMERATED {supported} OPTIONAL,

multiBandInfoReport-r13 ENUMERATED {supported} OPTIONAL,

rssi-AndChannelOccupancyReporting-r13 ENUMERATED {supported} OPTIONAL

}

MeasParameters-v1430 ::= SEQUENCE {

ceMeasurements-r14 ENUMERATED {supported} OPTIONAL,

ncsg-r14 ENUMERATED {supported} OPTIONAL,

shortMeasurementGap-r14 ENUMERATED {supported} OPTIONAL,

perServingCellMeasurementGap-r14 ENUMERATED {supported} OPTIONAL,

nonUniformGap-r14 ENUMERATED {supported} OPTIONAL

}

MeasParameters-v1520 ::= SEQUENCE {

measGapPatterns-r15 BIT STRING (SIZE (8)) OPTIONAL

}

MeasParameters-v1530 ::= SEQUENCE {

qoe-MeasReport-r15 ENUMERATED {supported} OPTIONAL,

qoe-MTSI-MeasReport-r15 ENUMERATED {supported} OPTIONAL,

ca-IdleModeMeasurements-r15 ENUMERATED {supported} OPTIONAL,

ca-IdleModeValidityArea-r15 ENUMERATED {supported} OPTIONAL,

heightMeas-r15 ENUMERATED {supported} OPTIONAL,

multipleCellsMeasExtension-r15 ENUMERATED {supported} OPTIONAL

}

MeasParameters-v1610 ::= SEQUENCE {

bandInfoNR-v1610 SEQUENCE (SIZE (1..maxBands)) OF MeasGapInfoNR OPTIONAL,

altFreqPriority-r16 ENUMERATED {supported} OPTIONAL,

ce-DL-ChannelQualityReporting-r16 ENUMERATED {supported} OPTIONAL,

ce-MeasRSS-Dedicated-r16 ENUMERATED {supported} OPTIONAL,

eutra-IdleInactiveMeasurements-r16 ENUMERATED {supported} OPTIONAL,

nr-IdleInactiveMeasFR1-r16 ENUMERATED {supported} OPTIONAL,

nr-IdleInactiveMeasFR2-r16 ENUMERATED {supported} OPTIONAL,

idleInactiveValidityAreaList-r16 ENUMERATED {supported} OPTIONAL,

measGapPatterns-NRonly-r16 ENUMERATED {supported} OPTIONAL,

measGapPatterns-NRonly-ENDC-r16 ENUMERATED {supported} OPTIONAL

}

MeasParameters-v1630 ::= SEQUENCE {

nr-IdleInactiveBeamMeasFR1-r16 ENUMERATED {supported} OPTIONAL,

nr-IdleInactiveBeamMeasFR2-r16 ENUMERATED {supported} OPTIONAL,

ce-MeasRSS-DedicatedSameRBs-r16 ENUMERATED {supported} OPTIONAL

}

MeasParameters-v1700 ::= SEQUENCE {

sharedSpectrumMeasNR-EN-DC-r17 SEQUENCE (SIZE (1..maxBandsNR-r15)) OF SharedSpectrumMeasNR-r17 OPTIONAL,

sharedSpectrumMeasNR-SA-r17 SEQUENCE (SIZE (1..maxBandsNR-r15)) OF SharedSpectrumMeasNR-r17 OPTIONAL

}

SharedSpectrumMeasNR-r17 ::= SEQUENCE {

nr-RSSI-ChannelOccupancyReporting-r17 BOOLEAN

}

MeasGapInfoNR ::= SEQUENCE {

interRAT-BandListNR-EN-DC InterRAT-BandListNR OPTIONAL,

interRAT-BandListNR-SA InterRAT-BandListNR OPTIONAL

}

BandListEUTRA ::= SEQUENCE (SIZE (1..maxBands)) OF BandInfoEUTRA

BandCombinationListEUTRA-r10 ::= SEQUENCE (SIZE (1..maxBandComb-r10)) OF BandInfoEUTRA

BandInfoEUTRA ::= SEQUENCE {

interFreqBandList InterFreqBandList,

interRAT-BandList InterRAT-BandList OPTIONAL

}

InterFreqBandList ::= SEQUENCE (SIZE (1..maxBands)) OF InterFreqBandInfo

InterFreqBandInfo ::= SEQUENCE {

interFreqNeedForGaps BOOLEAN

}

InterRAT-BandList ::= SEQUENCE (SIZE (1..maxBands)) OF InterRAT-BandInfo

InterRAT-BandListNR ::= SEQUENCE (SIZE (1..maxBandsNR-r15)) OF InterRAT-BandInfoNR

InterRAT-BandInfo ::= SEQUENCE {

interRAT-NeedForGaps BOOLEAN

}

InterRAT-BandInfoNR ::= SEQUENCE {

interRAT-NeedForGapsNR BOOLEAN

}

IRAT-ParametersNR-r15 ::= SEQUENCE {

en-DC-r15 ENUMERATED {supported} OPTIONAL,

eventB2-r15 ENUMERATED {supported} OPTIONAL,

supportedBandListEN-DC-r15 SupportedBandListNR-r15 OPTIONAL

}

IRAT-ParametersNR-v1540 ::= SEQUENCE {

eutra-5GC-HO-ToNR-FDD-FR1-r15 ENUMERATED {supported} OPTIONAL,

eutra-5GC-HO-ToNR-TDD-FR1-r15 ENUMERATED {supported} OPTIONAL,

eutra-5GC-HO-ToNR-FDD-FR2-r15 ENUMERATED {supported} OPTIONAL,

eutra-5GC-HO-ToNR-TDD-FR2-r15 ENUMERATED {supported} OPTIONAL,

eutra-EPC-HO-ToNR-FDD-FR1-r15 ENUMERATED {supported} OPTIONAL,

eutra-EPC-HO-ToNR-TDD-FR1-r15 ENUMERATED {supported} OPTIONAL,

eutra-EPC-HO-ToNR-FDD-FR2-r15 ENUMERATED {supported} OPTIONAL,

eutra-EPC-HO-ToNR-TDD-FR2-r15 ENUMERATED {supported} OPTIONAL,

ims-VoiceOverNR-FR1-r15 ENUMERATED {supported} OPTIONAL,

ims-VoiceOverNR-FR2-r15 ENUMERATED {supported} OPTIONAL,

sa-NR-r15 ENUMERATED {supported} OPTIONAL,

supportedBandListNR-SA-r15 SupportedBandListNR-r15 OPTIONAL

}

IRAT-ParametersNR-v1560 ::= SEQUENCE {

ng-EN-DC-r15 ENUMERATED {supported} OPTIONAL

}

IRAT-ParametersNR-v1570 ::= SEQUENCE {

ss-SINR-Meas-NR-FR1-r15 ENUMERATED {supported} OPTIONAL,

ss-SINR-Meas-NR-FR2-r15 ENUMERATED {supported} OPTIONAL

}

IRAT-ParametersNR-v1610 ::= SEQUENCE {

nr-HO-ToEN-DC-r16 ENUMERATED {supported} OPTIONAL,

ce-EUTRA-5GC-HO-ToNR-FDD-FR1-r16 ENUMERATED {supported} OPTIONAL,

ce-EUTRA-5GC-HO-ToNR-TDD-FR1-r16 ENUMERATED {supported} OPTIONAL,

ce-EUTRA-5GC-HO-ToNR-FDD-FR2-r16 ENUMERATED {supported} OPTIONAL,

ce-EUTRA-5GC-HO-ToNR-TDD-FR2-r16 ENUMERATED {supported} OPTIONAL

}

IRAT-ParametersNR-v1660 ::= SEQUENCE {

extendedBand-n77-r16 ENUMERATED {supported} OPTIONAL

}

IRAT-ParametersNR-v1700 ::= SEQUENCE {

eutra-5GC-HO-ToNR-TDD-FR2-2-r17 ENUMERATED {supported} OPTIONAL,

eutra-EPC-HO-ToNR-TDD-FR2-2-r17 ENUMERATED {supported} OPTIONAL,

ce-EUTRA-5GC-HO-ToNR-TDD-FR2-2-r17 ENUMERATED {supported} OPTIONAL,

ims-VoiceOverNR-FR2-2-r17 ENUMERATED {supported} OPTIONAL

}

EUTRA-5GC-Parameters-r15 ::= SEQUENCE {

eutra-5GC-r15 ENUMERATED {supported} OPTIONAL,

eutra-EPC-HO-EUTRA-5GC-r15 ENUMERATED {supported} OPTIONAL,

ho-EUTRA-5GC-FDD-TDD-r15 ENUMERATED {supported} OPTIONAL,

ho-InterfreqEUTRA-5GC-r15 ENUMERATED {supported} OPTIONAL,

ims-VoiceOverMCG-BearerEUTRA-5GC-r15 ENUMERATED {supported} OPTIONAL,

inactiveState-r15 ENUMERATED {supported} OPTIONAL,

reflectiveQoS-r15 ENUMERATED {supported} OPTIONAL

}

EUTRA-5GC-Parameters-v1610 ::= SEQUENCE {

ce-InactiveState-r16 ENUMERATED {supported} OPTIONAL,

ce-EUTRA-5GC-r16 ENUMERATED {supported} OPTIONAL

}

PDCP-ParametersNR-r15 ::= SEQUENCE {

rohc-Profiles-r15 ROHC-ProfileSupportList-r15,

rohc-ContextMaxSessions-r15 ENUMERATED {

cs2, cs4, cs8, cs12, cs16, cs24, cs32,

cs48, cs64, cs128, cs256, cs512, cs1024,

cs16384, spare2, spare1} DEFAULT cs16,

rohc-ProfilesUL-Only-r15 SEQUENCE {

profile0x0006-r15 BOOLEAN

},

rohc-ContextContinue-r15 ENUMERATED {supported} OPTIONAL,

outOfOrderDelivery-r15 ENUMERATED {supported} OPTIONAL,

sn-SizeLo-r15 ENUMERATED {supported} OPTIONAL,

ims-VoiceOverNR-PDCP-MCG-Bearer-r15 ENUMERATED {supported} OPTIONAL,

ims-VoiceOverNR-PDCP-SCG-Bearer-r15 ENUMERATED {supported} OPTIONAL

}

PDCP-ParametersNR-v1560 ::= SEQUENCE {

ims-VoNR-PDCP-SCG-NGENDC-r15 ENUMERATED {supported} OPTIONAL

}

ROHC-ProfileSupportList-r15 ::= SEQUENCE {

profile0x0001-r15 BOOLEAN,

profile0x0002-r15 BOOLEAN,

profile0x0003-r15 BOOLEAN,

profile0x0004-r15 BOOLEAN,

profile0x0006-r15 BOOLEAN,

profile0x0101-r15 BOOLEAN,

profile0x0102-r15 BOOLEAN,

profile0x0103-r15 BOOLEAN,

profile0x0104-r15 BOOLEAN

}

SupportedBandListNR-r15 ::= SEQUENCE (SIZE (1..maxBandsNR-r15)) OF SupportedBandNR-r15

SupportedBandNR-r15 ::= SEQUENCE {

bandNR-r15 FreqBandIndicatorNR-r15

}

IRAT-ParametersUTRA-FDD ::= SEQUENCE {

supportedBandListUTRA-FDD SupportedBandListUTRA-FDD

}

IRAT-ParametersUTRA-v920 ::= SEQUENCE {

e-RedirectionUTRA-r9 ENUMERATED {supported}

}

IRAT-ParametersUTRA-v9c0 ::= SEQUENCE {

voiceOverPS-HS-UTRA-FDD-r9 ENUMERATED {supported} OPTIONAL,

voiceOverPS-HS-UTRA-TDD128-r9 ENUMERATED {supported} OPTIONAL,

srvcc-FromUTRA-FDD-ToUTRA-FDD-r9 ENUMERATED {supported} OPTIONAL,

srvcc-FromUTRA-FDD-ToGERAN-r9 ENUMERATED {supported} OPTIONAL,

srvcc-FromUTRA-TDD128-ToUTRA-TDD128-r9 ENUMERATED {supported} OPTIONAL,

srvcc-FromUTRA-TDD128-ToGERAN-r9 ENUMERATED {supported} OPTIONAL

}

IRAT-ParametersUTRA-v9h0 ::= SEQUENCE {

mfbi-UTRA-r9 ENUMERATED {supported}

}

SupportedBandListUTRA-FDD ::= SEQUENCE (SIZE (1..maxBands)) OF SupportedBandUTRA-FDD

SupportedBandUTRA-FDD ::= ENUMERATED {

bandI, bandII, bandIII, bandIV, bandV, bandVI,

bandVII, bandVIII, bandIX, bandX, bandXI,

bandXII, bandXIII, bandXIV, bandXV, bandXVI, ...,

bandXVII-8a0, bandXVIII-8a0, bandXIX-8a0, bandXX-8a0,

bandXXI-8a0, bandXXII-8a0, bandXXIII-8a0, bandXXIV-8a0,

bandXXV-8a0, bandXXVI-8a0, bandXXVII-8a0, bandXXVIII-8a0,

bandXXIX-8a0, bandXXX-8a0, bandXXXI-8a0, bandXXXII-8a0}

IRAT-ParametersUTRA-TDD128 ::= SEQUENCE {

supportedBandListUTRA-TDD128 SupportedBandListUTRA-TDD128

}

SupportedBandListUTRA-TDD128 ::= SEQUENCE (SIZE (1..maxBands)) OF SupportedBandUTRA-TDD128

SupportedBandUTRA-TDD128 ::= ENUMERATED {

a, b, c, d, e, f, g, h, i, j, k, l, m, n,

o, p, ...}

IRAT-ParametersUTRA-TDD384 ::= SEQUENCE {

supportedBandListUTRA-TDD384 SupportedBandListUTRA-TDD384

}

SupportedBandListUTRA-TDD384 ::= SEQUENCE (SIZE (1..maxBands)) OF SupportedBandUTRA-TDD384

SupportedBandUTRA-TDD384 ::= ENUMERATED {

a, b, c, d, e, f, g, h, i, j, k, l, m, n,

o, p, ...}

IRAT-ParametersUTRA-TDD768 ::= SEQUENCE {

supportedBandListUTRA-TDD768 SupportedBandListUTRA-TDD768

}

SupportedBandListUTRA-TDD768 ::= SEQUENCE (SIZE (1..maxBands)) OF SupportedBandUTRA-TDD768

SupportedBandUTRA-TDD768 ::= ENUMERATED {

a, b, c, d, e, f, g, h, i, j, k, l, m, n,

o, p, ...}

IRAT-ParametersUTRA-TDD-v1020 ::= SEQUENCE {

e-RedirectionUTRA-TDD-r10 ENUMERATED {supported}

}

IRAT-ParametersGERAN ::= SEQUENCE {

supportedBandListGERAN SupportedBandListGERAN,

interRAT-PS-HO-ToGERAN BOOLEAN

}

IRAT-ParametersGERAN-v920 ::= SEQUENCE {

dtm-r9 ENUMERATED {supported} OPTIONAL,

e-RedirectionGERAN-r9 ENUMERATED {supported} OPTIONAL

}

SupportedBandListGERAN ::= SEQUENCE (SIZE (1..maxBands)) OF SupportedBandGERAN

SupportedBandGERAN ::= ENUMERATED {

gsm450, gsm480, gsm710, gsm750, gsm810, gsm850,

gsm900P, gsm900E, gsm900R, gsm1800, gsm1900,

spare5, spare4, spare3, spare2, spare1, ...}

IRAT-ParametersCDMA2000-HRPD ::= SEQUENCE {

supportedBandListHRPD SupportedBandListHRPD,

tx-ConfigHRPD ENUMERATED {single, dual},

rx-ConfigHRPD ENUMERATED {single, dual}

}

SupportedBandListHRPD ::= SEQUENCE (SIZE (1..maxCDMA-BandClass)) OF BandclassCDMA2000

IRAT-ParametersCDMA2000-1XRTT ::= SEQUENCE {

supportedBandList1XRTT SupportedBandList1XRTT,

tx-Config1XRTT ENUMERATED {single, dual},

rx-Config1XRTT ENUMERATED {single, dual}

}

IRAT-ParametersCDMA2000-1XRTT-v920 ::= SEQUENCE {

e-CSFB-1XRTT-r9 ENUMERATED {supported},

e-CSFB-ConcPS-Mob1XRTT-r9 ENUMERATED {supported} OPTIONAL

}

IRAT-ParametersCDMA2000-1XRTT-v1020 ::= SEQUENCE {

e-CSFB-dual-1XRTT-r10 ENUMERATED {supported}

}

IRAT-ParametersCDMA2000-v1130 ::= SEQUENCE {

cdma2000-NW-Sharing-r11 ENUMERATED {supported} OPTIONAL

}

SupportedBandList1XRTT ::= SEQUENCE (SIZE (1..maxCDMA-BandClass)) OF BandclassCDMA2000

IRAT-ParametersWLAN-r13 ::= SEQUENCE {

supportedBandListWLAN-r13 SEQUENCE (SIZE (1..maxWLAN-Bands-r13)) OF WLAN-BandIndicator-r13 OPTIONAL

}

CSG-ProximityIndicationParameters-r9 ::= SEQUENCE {

intraFreqProximityIndication-r9 ENUMERATED {supported} OPTIONAL,

interFreqProximityIndication-r9 ENUMERATED {supported} OPTIONAL,

utran-ProximityIndication-r9 ENUMERATED {supported} OPTIONAL

}

NeighCellSI-AcquisitionParameters-r9 ::= SEQUENCE {

intraFreqSI-AcquisitionForHO-r9 ENUMERATED {supported} OPTIONAL,

interFreqSI-AcquisitionForHO-r9 ENUMERATED {supported} OPTIONAL,

utran-SI-AcquisitionForHO-r9 ENUMERATED {supported} OPTIONAL

}

NeighCellSI-AcquisitionParameters-v1530 ::= SEQUENCE {

reportCGI-NR-EN-DC-r15 ENUMERATED {supported} OPTIONAL,

reportCGI-NR-NoEN-DC-r15 ENUMERATED {supported} OPTIONAL

}

NeighCellSI-AcquisitionParameters-v1550 ::= SEQUENCE {

eutra-CGI-Reporting-ENDC-r15 ENUMERATED {supported} OPTIONAL,

utra-GERAN-CGI-Reporting-ENDC-r15 ENUMERATED {supported} OPTIONAL

}

NeighCellSI-AcquisitionParameters-v15a0 ::= SEQUENCE {

eutra-CGI-Reporting-NEDC-r15 ENUMERATED {supported} OPTIONAL

}

NeighCellSI-AcquisitionParameters-v1610 ::= SEQUENCE {

eutra-SI-AcquisitionForHO-ENDC-r16 ENUMERATED {supported} OPTIONAL,

nr-AutonomousGaps-ENDC-FR1-r16 ENUMERATED {supported} OPTIONAL,

nr-AutonomousGaps-ENDC-FR2-r16 ENUMERATED {supported} OPTIONAL,

nr-AutonomousGaps-FR1-r16 ENUMERATED {supported} OPTIONAL,

nr-AutonomousGaps-FR2-r16 ENUMERATED {supported} OPTIONAL

}

SON-Parameters-r9 ::= SEQUENCE {

rach-Report-r9 ENUMERATED {supported} OPTIONAL

}

PUR-Parameters-r16 ::= SEQUENCE {

pur-CP-5GC-CE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

pur-CP-5GC-CE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

pur-UP-5GC-CE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

pur-UP-5GC-CE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

pur-CP-EPC-CE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

pur-CP-EPC-CE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

pur-UP-EPC-CE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

pur-UP-EPC-CE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

pur-CP-L1Ack-r16 ENUMERATED {supported} OPTIONAL,

pur-FrequencyHopping-r16 ENUMERATED {supported} OPTIONAL,

pur-PUSCH-NB-MaxTBS-r16 ENUMERATED {supported} OPTIONAL,

pur-RSRP-Validation-r16 ENUMERATED {supported} OPTIONAL,

pur-SubPRB-CE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

pur-SubPRB-CE-ModeB-r16 ENUMERATED {supported} OPTIONAL

}

UE-BasedNetwPerfMeasParameters-r10 ::= SEQUENCE {

loggedMeasurementsIdle-r10 ENUMERATED {supported} OPTIONAL,

standaloneGNSS-Location-r10 ENUMERATED {supported} OPTIONAL

}

UE-BasedNetwPerfMeasParameters-v1250 ::= SEQUENCE {

loggedMBSFNMeasurements-r12 ENUMERATED {supported}

}

UE-BasedNetwPerfMeasParameters-v1430 ::= SEQUENCE {

locationReport-r14 ENUMERATED {supported} OPTIONAL

}

UE-BasedNetwPerfMeasParameters-v1530 ::= SEQUENCE {

loggedMeasBT-r15 ENUMERATED {supported} OPTIONAL,

loggedMeasWLAN-r15 ENUMERATED {supported} OPTIONAL,

immMeasBT-r15 ENUMERATED {supported} OPTIONAL,

immMeasWLAN-r15 ENUMERATED {supported} OPTIONAL

}

UE-BasedNetwPerfMeasParameters-v1610 ::= SEQUENCE {

ul-PDCP-AvgDelay-r16 ENUMERATED {supported} OPTIONAL

}

UE-BasedNetwPerfMeasParameters-v1700 ::= SEQUENCE {

loggedMeasIdleEventL1-r17 ENUMERATED {supported} OPTIONAL,

loggedMeasIdleEventOutOfCoverage-r17 ENUMERATED {supported} OPTIONAL,

loggedMeasUncomBarPre-r17 ENUMERATED {supported} OPTIONAL,

immMeasUncomBarPre-r17 ENUMERATED {supported} OPTIONAL

}

OTDOA-PositioningCapabilities-r10 ::= SEQUENCE {

otdoa-UE-Assisted-r10 ENUMERATED {supported},

interFreqRSTD-Measurement-r10 ENUMERATED {supported} OPTIONAL

}

Other-Parameters-r11 ::= SEQUENCE {

inDeviceCoexInd-r11 ENUMERATED {supported} OPTIONAL,

powerPrefInd-r11 ENUMERATED {supported} OPTIONAL,

ue-Rx-TxTimeDiffMeasurements-r11 ENUMERATED {supported} OPTIONAL

}

Other-Parameters-v11d0 ::= SEQUENCE {

inDeviceCoexInd-UL-CA-r11 ENUMERATED {supported} OPTIONAL

}

Other-Parameters-v1360 ::= SEQUENCE {

inDeviceCoexInd-HardwareSharingInd-r13 ENUMERATED {supported} OPTIONAL

}

Other-Parameters-v1430 ::= SEQUENCE {

bwPrefInd-r14 ENUMERATED {supported} OPTIONAL,

rlm-ReportSupport-r14 ENUMERATED {supported} OPTIONAL

}

OtherParameters-v1450 ::= SEQUENCE {

overheatingInd-r14 ENUMERATED {supported} OPTIONAL

}

Other-Parameters-v1460 ::= SEQUENCE {

nonCSG-SI-Reporting-r14 ENUMERATED {supported} OPTIONAL

}

Other-Parameters-v1530 ::= SEQUENCE {

assistInfoBitForLC-r15 ENUMERATED {supported} OPTIONAL,

timeReferenceProvision-r15 ENUMERATED {supported} OPTIONAL,

flightPathPlan-r15 ENUMERATED {supported} OPTIONAL

}

Other-Parameters-v1540 ::= SEQUENCE {

inDeviceCoexInd-ENDC-r15 ENUMERATED {supported} OPTIONAL

}

Other-Parameters-v1610 ::= SEQUENCE {

resumeWithStoredMCG-SCells-r16 ENUMERATED {supported} OPTIONAL,

resumeWithMCG-SCellConfig-r16 ENUMERATED {supported} OPTIONAL,

resumeWithStoredSCG-r16 ENUMERATED {supported} OPTIONAL,

resumeWithSCG-Config-r16 ENUMERATED {supported} OPTIONAL,

mcgRLF-RecoveryViaSCG-r16 ENUMERATED {supported} OPTIONAL,

overheatingIndForSCG-r16 ENUMERATED {supported} OPTIONAL

}

Other-Parameters-v1650 ::= SEQUENCE {

mpsPriorityIndication-r16 ENUMERATED {supported} OPTIONAL

}

MBMS-Parameters-r11 ::= SEQUENCE {

mbms-SCell-r11 ENUMERATED {supported} OPTIONAL,

mbms-NonServingCell-r11 ENUMERATED {supported} OPTIONAL

}

MBMS-Parameters-v1250 ::= SEQUENCE {

mbms-AsyncDC-r12 ENUMERATED {supported} OPTIONAL

}

MBMS-Parameters-v1430 ::= SEQUENCE {

fembmsDedicatedCell-r14 ENUMERATED {supported} OPTIONAL,

fembmsMixedCell-r14 ENUMERATED {supported} OPTIONAL,

subcarrierSpacingMBMS-khz7dot5-r14 ENUMERATED {supported} OPTIONAL,

subcarrierSpacingMBMS-khz1dot25-r14 ENUMERATED {supported} OPTIONAL

}

MBMS-Parameters-v1470 ::= SEQUENCE {

mbms-MaxBW-r14 CHOICE {

implicitValue NULL,

explicitValue INTEGER(2..20)

},

mbms-ScalingFactor1dot25-r14 ENUMERATED {n3, n6, n9, n12} OPTIONAL,

mbms-ScalingFactor7dot5-r14 ENUMERATED {n1, n2, n3, n4} OPTIONAL

}

MBMS-Parameters-v1610 ::= SEQUENCE {

mbms-ScalingFactor2dot5-r16 ENUMERATED {n2, n4, n6, n8} OPTIONAL,

mbms-ScalingFactor0dot37-r16 ENUMERATED {n12, n16, n20, n24} OPTIONAL,

mbms-SupportedBandInfoList-r16 SEQUENCE (SIZE (1..maxBands)) OF MBMS-SupportedBandInfo-r16

}

MBMS-Parameters-v1700 ::= SEQUENCE {

mbms-SupportedBandInfoList-v1700 SEQUENCE (SIZE (1..maxBands)) OF MBMS-SupportedBandInfo-v1700 OPTIONAL

}

MBMS-SupportedBandInfo-r16 ::= SEQUENCE {

subcarrierSpacingMBMS-khz2dot5-r16 ENUMERATED {supported} OPTIONAL,

subcarrierSpacingMBMS-khz0dot37-r16 SEQUENCE {

timeSeparationSlot2-r16 ENUMERATED {supported} OPTIONAL,

timeSeparationSlot4-r16 ENUMERATED {supported} OPTIONAL

} OPTIONAL

}

MBMS-SupportedBandInfo-v1700 ::= SEQUENCE {

pmch-Bandwidth-n40-r17 ENUMERATED {supported} OPTIONAL,

pmch-Bandwidth-n35-r17 ENUMERATED {supported} OPTIONAL,

pmch-Bandwidth-n30-r17 ENUMERATED {supported} OPTIONAL

}

FeMBMS-Unicast-Parameters-r14 ::= SEQUENCE {

unicast-fembmsMixedSCell-r14 ENUMERATED {supported} OPTIONAL,

emptyUnicastRegion-r14 ENUMERATED {supported} OPTIONAL

}

SCPTM-Parameters-r13 ::= SEQUENCE {

scptm-ParallelReception-r13 ENUMERATED {supported} OPTIONAL,

scptm-SCell-r13 ENUMERATED {supported} OPTIONAL,

scptm-NonServingCell-r13 ENUMERATED {supported} OPTIONAL,

scptm-AsyncDC-r13 ENUMERATED {supported} OPTIONAL

}

CE-Parameters-r13 ::= SEQUENCE {

ce-ModeA-r13 ENUMERATED {supported} OPTIONAL,

ce-ModeB-r13 ENUMERATED {supported} OPTIONAL

}

CE-Parameters-v1320 ::= SEQUENCE {

intraFreqA3-CE-ModeA-r13 ENUMERATED {supported} OPTIONAL,

intraFreqA3-CE-ModeB-r13 ENUMERATED {supported} OPTIONAL,

intraFreqHO-CE-ModeA-r13 ENUMERATED {supported} OPTIONAL,

intraFreqHO-CE-ModeB-r13 ENUMERATED {supported} OPTIONAL

}

CE-Parameters-v1350 ::= SEQUENCE {

unicastFrequencyHopping-r13 ENUMERATED {supported} OPTIONAL

}

CE-Parameters-v1370 ::= SEQUENCE {

tm9-CE-ModeA-r13 ENUMERATED {supported} OPTIONAL,

tm9-CE-ModeB-r13 ENUMERATED {supported} OPTIONAL

}

CE-Parameters-v1380 ::= SEQUENCE {

tm6-CE-ModeA-r13 ENUMERATED {supported} OPTIONAL

}

CE-Parameters-v1430 ::= SEQUENCE {

ce-SwitchWithoutHO-r14 ENUMERATED {supported} OPTIONAL

}

CE-MultiTB-Parameters-r16 ::= SEQUENCE {

pdsch-MultiTB-CE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

pdsch-MultiTB-CE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

pusch-MultiTB-CE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

pusch-MultiTB-CE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

ce-MultiTB-64QAM-r16 ENUMERATED {supported} OPTIONAL,

ce-MultiTB-EarlyTermination-r16 ENUMERATED {supported} OPTIONAL,

ce-MultiTB-FrequencyHopping-r16 ENUMERATED {supported} OPTIONAL,

ce-MultiTB-HARQ-AckBundling-r16 ENUMERATED {supported} OPTIONAL,

ce-MultiTB-Interleaving-r16 ENUMERATED {supported} OPTIONAL,

ce-MultiTB-SubPRB-r16 ENUMERATED {supported} OPTIONAL

}

CE-ResourceResvParameters-r16 ::= SEQUENCE {

subframeResourceResvDL-CE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

subframeResourceResvDL-CE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

subframeResourceResvUL-CE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

subframeResourceResvUL-CE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

slotSymbolResourceResvDL-CE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

slotSymbolResourceResvDL-CE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

slotSymbolResourceResvUL-CE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

slotSymbolResourceResvUL-CE-ModeB-r16 ENUMERATED {supported} OPTIONAL,

subcarrierPuncturingCE-ModeA-r16 ENUMERATED {supported} OPTIONAL,

subcarrierPuncturingCE-ModeB-r16 ENUMERATED {supported} OPTIONAL

}

LAA-Parameters-r13 ::= SEQUENCE {

crossCarrierSchedulingLAA-DL-r13 ENUMERATED {supported} OPTIONAL,

csi-RS-DRS-RRM-MeasurementsLAA-r13 ENUMERATED {supported} OPTIONAL,

downlinkLAA-r13 ENUMERATED {supported} OPTIONAL,

endingDwPTS-r13 ENUMERATED {supported} OPTIONAL,

secondSlotStartingPosition-r13 ENUMERATED {supported} OPTIONAL,

tm9-LAA-r13 ENUMERATED {supported} OPTIONAL,

tm10-LAA-r13 ENUMERATED {supported} OPTIONAL

}

LAA-Parameters-v1430 ::= SEQUENCE {

crossCarrierSchedulingLAA-UL-r14 ENUMERATED {supported} OPTIONAL,

uplinkLAA-r14 ENUMERATED {supported} OPTIONAL,

twoStepSchedulingTimingInfo-r14 ENUMERATED {nPlus1, nPlus2, nPlus3} OPTIONAL,

uss-BlindDecodingAdjustment-r14 ENUMERATED {supported} OPTIONAL,

uss-BlindDecodingReduction-r14 ENUMERATED {supported} OPTIONAL,

outOfSequenceGrantHandling-r14 ENUMERATED {supported} OPTIONAL

}

LAA-Parameters-v1530 ::= SEQUENCE {

aul-r15 ENUMERATED {supported} OPTIONAL,

laa-PUSCH-Mode1-r15 ENUMERATED {supported} OPTIONAL,

laa-PUSCH-Mode2-r15 ENUMERATED {supported} OPTIONAL,

laa-PUSCH-Mode3-r15 ENUMERATED {supported} OPTIONAL

}

WLAN-IW-Parameters-r12 ::= SEQUENCE {

wlan-IW-RAN-Rules-r12 ENUMERATED {supported} OPTIONAL,

wlan-IW-ANDSF-Policies-r12 ENUMERATED {supported} OPTIONAL

}

LWA-Parameters-r13 ::= SEQUENCE {

lwa-r13 ENUMERATED {supported} OPTIONAL,

lwa-SplitBearer-r13 ENUMERATED {supported} OPTIONAL,

wlan-MAC-Address-r13 OCTET STRING (SIZE (6)) OPTIONAL,

lwa-BufferSize-r13 ENUMERATED {supported} OPTIONAL

}

LWA-Parameters-v1430 ::= SEQUENCE {

lwa-HO-WithoutWT-Change-r14 ENUMERATED {supported} OPTIONAL,

lwa-UL-r14 ENUMERATED {supported} OPTIONAL,

wlan-PeriodicMeas-r14 ENUMERATED {supported} OPTIONAL,

wlan-ReportAnyWLAN-r14 ENUMERATED {supported} OPTIONAL,

wlan-SupportedDataRate-r14 INTEGER (1..2048) OPTIONAL

}

LWA-Parameters-v1440 ::= SEQUENCE {

lwa-RLC-UM-r14 ENUMERATED {supported} OPTIONAL

}

WLAN-IW-Parameters-v1310 ::= SEQUENCE {

rclwi-r13 ENUMERATED {supported} OPTIONAL

}

LWIP-Parameters-r13 ::= SEQUENCE {

lwip-r13 ENUMERATED {supported} OPTIONAL

}

LWIP-Parameters-v1430 ::= SEQUENCE {

lwip-Aggregation-DL-r14 ENUMERATED {supported} OPTIONAL,

lwip-Aggregation-UL-r14 ENUMERATED {supported} OPTIONAL

}

NAICS-Capability-List-r12 ::= SEQUENCE (SIZE (1..maxNAICS-Entries-r12)) OF NAICS-Capability-Entry-r12

NAICS-Capability-Entry-r12 ::= SEQUENCE {

numberOfNAICS-CapableCC-r12 INTEGER(1..5),

numberOfAggregatedPRB-r12 ENUMERATED {

n50, n75, n100, n125, n150, n175,

n200, n225, n250, n275, n300, n350,

n400, n450, n500, spare},

...

}

SL-Parameters-r12 ::= SEQUENCE {

commSimultaneousTx-r12 ENUMERATED {supported} OPTIONAL,

commSupportedBands-r12 FreqBandIndicatorListEUTRA-r12 OPTIONAL,

discSupportedBands-r12 SupportedBandInfoList-r12 OPTIONAL,

discScheduledResourceAlloc-r12 ENUMERATED {supported} OPTIONAL,

disc-UE-SelectedResourceAlloc-r12 ENUMERATED {supported} OPTIONAL,

disc-SLSS-r12 ENUMERATED {supported} OPTIONAL,

discSupportedProc-r12 ENUMERATED {n50, n400} OPTIONAL

}

SL-Parameters-v1310 ::= SEQUENCE {

discSysInfoReporting-r13 ENUMERATED {supported} OPTIONAL,

commMultipleTx-r13 ENUMERATED {supported} OPTIONAL,

discInterFreqTx-r13 ENUMERATED {supported} OPTIONAL,

discPeriodicSLSS-r13 ENUMERATED {supported} OPTIONAL

}

SL-Parameters-v1430 ::= SEQUENCE {

zoneBasedPoolSelection-r14 ENUMERATED {supported} OPTIONAL,

ue-AutonomousWithFullSensing-r14 ENUMERATED {supported} OPTIONAL,

ue-AutonomousWithPartialSensing-r14 ENUMERATED {supported} OPTIONAL,

sl-CongestionControl-r14 ENUMERATED {supported} OPTIONAL,

v2x-TxWithShortResvInterval-r14 ENUMERATED {supported} OPTIONAL,

v2x-numberTxRxTiming-r14 INTEGER(1..16) OPTIONAL,

v2x-nonAdjacentPSCCH-PSSCH-r14 ENUMERATED {supported} OPTIONAL,

slss-TxRx-r14 ENUMERATED {supported} OPTIONAL,

v2x-SupportedBandCombinationList-r14 V2X-SupportedBandCombination-r14 OPTIONAL

}

SL-Parameters-v1530 ::= SEQUENCE {

slss-SupportedTxFreq-r15 ENUMERATED {single, multiple} OPTIONAL,

sl-64QAM-Tx-r15 ENUMERATED {supported} OPTIONAL,

sl-TxDiversity-r15 ENUMERATED {supported} OPTIONAL,

ue-CategorySL-r15 UE-CategorySL-r15 OPTIONAL,

v2x-SupportedBandCombinationList-v1530 V2X-SupportedBandCombination-v1530 OPTIONAL

}

SL-Parameters-v1540 ::= SEQUENCE {

sl-64QAM-Rx-r15 ENUMERATED {supported} OPTIONAL,

sl-RateMatchingTBSScaling-r15 ENUMERATED {supported} OPTIONAL,

sl-LowT2min-r15 ENUMERATED {supported} OPTIONAL,

v2x-SensingReportingMode3-r15 ENUMERATED {supported} OPTIONAL

}

SL-Parameters-v1610 ::= SEQUENCE {

sl-ParameterNR-r16 OCTET STRING OPTIONAL,

dummy V2X-SupportedBandCombinationEUTRA-NR-r16 OPTIONAL

}

SL-Parameters-v1630 ::= SEQUENCE {

v2x-SupportedBandCombinationListEUTRA-NR-r16 V2X-SupportedBandCombinationEUTRA-NR-v1630 OPTIONAL

}

UE-CategorySL-r15 ::= SEQUENCE {

ue-CategorySL-C-TX-r15 INTEGER(1..5),

ue-CategorySL-C-RX-r15 INTEGER(1..4)

}

V2X-SupportedBandCombination-r14 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF V2X-BandCombinationParameters-r14

V2X-SupportedBandCombination-v1530 ::= SEQUENCE (SIZE (1..maxBandComb-r13)) OF V2X-BandCombinationParameters-v1530

V2X-BandCombinationParameters-r14 ::= SEQUENCE (SIZE (1.. maxSimultaneousBands-r10)) OF V2X-BandParameters-r14

V2X-BandCombinationParameters-v1530 ::= SEQUENCE (SIZE (1.. maxSimultaneousBands-r10)) OF V2X-BandParameters-v1530

V2X-SupportedBandCombinationEUTRA-NR-r16 ::= SEQUENCE (SIZE (1..maxBandCombSidelinkNR-r16)) OF V2X-BandParametersEUTRA-NR-r16

V2X-SupportedBandCombinationEUTRA-NR-v1630 ::= SEQUENCE (SIZE (1..maxBandCombSidelinkNR-r16)) OF V2X-BandCombinationParametersEUTRA-NR-v1630

V2X-BandCombinationParametersEUTRA-NR-v1630 ::= SEQUENCE {

bandListSidelinkEUTRA-NR-r16 SEQUENCE (SIZE (1.. maxSimultaneousBands-r10)) OF V2X-BandParametersEUTRA-NR-r16,

bandListSidelinkEUTRA-NR-v1630 SEQUENCE (SIZE (1.. maxSimultaneousBands-r10)) OF V2X-BandParametersEUTRA-NR-v1630

}

V2X-BandParametersEUTRA-NR-r16 ::= CHOICE {

eutra SEQUENCE {

v2x-BandParameters1-r16 V2X-BandParameters-r14 OPTIONAL,

v2x-BandParameters2-r16 V2X-BandParameters-v1530 OPTIONAL

},

nr SEQUENCE {

v2x-BandParametersNR-r16 OCTET STRING OPTIONAL

}

}

V2X-BandParametersEUTRA-NR-v1630 ::= CHOICE {

eutra NULL,

nr SEQUENCE {

tx-Sidelink-r16 ENUMERATED {supported} OPTIONAL,

rx-Sidelink-r16 ENUMERATED {supported} OPTIONAL

}

}

SupportedBandInfoList-r12 ::= SEQUENCE (SIZE (1..maxBands)) OF SupportedBandInfo-r12

SupportedBandInfo-r12 ::= SEQUENCE {

support-r12 ENUMERATED {supported} OPTIONAL

}

FreqBandIndicatorListEUTRA-r12 ::= SEQUENCE (SIZE (1..maxBands)) OF FreqBandIndicator-r11

MMTEL-Parameters-r14 ::= SEQUENCE {

delayBudgetReporting-r14 ENUMERATED {supported} OPTIONAL,

pusch-Enhancements-r14 ENUMERATED {supported} OPTIONAL,

recommendedBitRate-r14 ENUMERATED {supported} OPTIONAL,

recommendedBitRateQuery-r14 ENUMERATED {supported} OPTIONAL

}

MMTEL-Parameters-v1610 ::= SEQUENCE {

recommendedBitRateMultiplier-r16 ENUMERATED {supported} OPTIONAL

}

SRS-CapabilityPerBandPair-r14 ::= SEQUENCE {

retuningInfo SEQUENCE {

rf-RetuningTimeDL-r14 ENUMERATED {n0, n0dot5, n1, n1dot5, n2, n2dot5, n3,

n3dot5, n4, n4dot5, n5, n5dot5, n6, n6dot5,

n7, spare1} OPTIONAL,

rf-RetuningTimeUL-r14 ENUMERATED {n0, n0dot5, n1, n1dot5, n2, n2dot5, n3,

n3dot5, n4, n4dot5, n5, n5dot5, n6, n6dot5,

n7, spare1} OPTIONAL

}

}

SRS-CapabilityPerBandPair-v14b0 ::= SEQUENCE {

srs-FlexibleTiming-r14 ENUMERATED {supported} OPTIONAL,

srs-HARQ-ReferenceConfig-r14 ENUMERATED {supported} OPTIONAL

}

SRS-CapabilityPerBandPair-v1610::= SEQUENCE {

addSRS-CarrierSwitching-r16 ENUMERATED {supported} OPTIONAL

}

HighSpeedEnhParameters-r14 ::= SEQUENCE {

measurementEnhancements-r14 ENUMERATED {supported} OPTIONAL,

demodulationEnhancements-r14 ENUMERATED {supported} OPTIONAL,

prach-Enhancements-r14 ENUMERATED {supported} OPTIONAL

}

HighSpeedEnhParameters-v1610 ::= SEQUENCE {

measurementEnhancementsSCell-r16 ENUMERATED {supported} OPTIONAL,

measurementEnhancements2-r16 ENUMERATED {supported} OPTIONAL,

demodulationEnhancements2-r16 ENUMERATED {supported} OPTIONAL,

interRAT-enhancementNR-r16 ENUMERATED {supported} OPTIONAL

}

-- ASN1STOP

| *UE-EUTRA-Capability* field descriptions | | *FDD/ TDD diff* |
| --- | --- | --- |
| ***accessStratumRelease***  Set to rel17 in this version of the specification. NOTE 7. | | - |
| ***additionalRx-Tx-PerformanceReq***  Indicates whether the UE supports the additional Rx and Tx performance requirement for a given band combination as specified in TS 36.101 [42]. | | - |
| ***addSRS***  Presence of this field indicates the UE supports the additional SRS symbol(s) within the normal UL subframes in TDD as described in TS 36.213 [23]. | | - |
| ***addSRS-1T2R***  Indicates whether the UE supports selecting one antenna among two antennas to transmit additional SRS symbol(s) for the corresponding band of the band combination as described in TS 36.213 [23]. | | - |
| ***addSRS-1T4R***  Indicates whether the UE supports selecting one antenna among four antennas to transmit additional SRS symbol(s) for the corresponding band of the band combination as described in TS 36.213 [23]. | | - |
| ***addSRS-2T4R-2Pairs***  Indicates whether the UE supports selecting one antenna pair between two antenna pairs to transmit additional SRS symbol(s) simultaneously for the corresponding band of the band combination as described in TS 36.213 [23]. | | - |
| ***addSRS-2T4R-3Pairs***  Indicates whether the UE supports selecting one antenna pair among three antenna pairs to transmit additional SRS symbol(s) simultaneously for the corresponding band of the band combination as described in TS 36.213 [23]. | | - |
| ***addSRS-AntennaSwitching (in addSRS)***  Value *useBasic* indicates the antenna switching capabilities for additional SRS symbol(s) for a band of band combination for which the capability is not signalled in *bandParameterList-v1610* is the same as indicated by *bandParameterList-v1380* and/or *bandParameterList-v1530* for the concerned band of band combination. | | - |
| ***addSRS-AntennaSwitching (in bandParameterList-v1610)***  If signalled, the field indicates the antenna switching capabilities for additional SRS symbol(s) for the concerned band of band combination. | | - |
| ***addSRS-CarrierSwitching (in addSRS)***  Indicates whether carrier switching is supported for additional SRS symbol(s) for all band pairs of band combinations for which UE supports SRS carrier switching. This field is included only if *srs-CapabilityPerBandPairList-r14* is included. If this field is included, *addSRS-CarrierSwitching* (in *bandParameterList-v1610*) is not included. | | - |
| ***addSRS-CarrierSwitching (in bandParameterList-v1610)***  Indicates whether carrier switching is supported for additional SRS symbol(s) for the concerned band pair of band combination. This field is included only if *srs-CapabilityPerBandPairList-r14* is included.If this field is included, *addSRS-CarrierSwitching* (in *addSRS*) is not included. | | - |
| ***addSRS-FrequencyHopping (in addSRS)***  Indicates whether frequency hopping is supported for additional SRS symbol(s) for all bands of band combinations for which the capability is not signalled in *bandParameterList-v1610*. | | - |
| ***addSRS-FrequencyHopping (in bandParameterList-v1610)***  If signalled, the field indicates whether frequency hopping is supported for additional SRS symbol(s) for the concerned band of band combination. | | - |
| ***allowedCellList***  Indicates whether the UE supports EUTRA allowed-cell listing to limit the set of cells applicable for measurements. | | - |
| ***alternativeTBS-Indices***  Indicates whether the UE supports alternative TBS indices *I*TBS 26A and 33A as specified in TS 36.213 [23]. | | - |
| ***alternativeTBS-Index***  Indicates whether the UE supports alternative TBS index ITBS 33B as specified in TS 36.213 [23]. | | No |
| ***alternativeTimeToTrigger***  Indicates whether the UE supports alternativeTimeToTrigger. | | No |
| ***altFreqPriority***  Indicates whether the UE supports alternative cell reselection priority. | | No |
| ***altMCS-Table***  Indicates whether the UE supports the 6-bit MCS table as specified in TS 36.212 [22] and TS 36.213 [23]. | | Yes |
| ***aperiodicCSI-Reporting***  Indicates whether the UE supports aperiodic CSI reporting with 3 bits of the CSI request field size as specified in TS 36.213 [23], clause 7.2.1 and/or aperiodic CSI reporting mode 1-0 and mode 1-1 as specified in TS 36.213 [23], clause 7.2.1. The first bit is set to "1" if the UE supports the aperiodic CSI reporting with 3 bits of the CSI request field size. The second bit is set to "1" if the UE supports the aperiodic CSI reporting mode 1-0 and mode 1-1. | | No |
| ***aperiodicCsi-ReportingSTTI***  Indicates whether the UE supports aperiodic CSI reporting for short TTI as specified in TS 36.213 [23], clause 7.2.1. | | Yes |
| ***appliedCapabilityFilterCommon***  Contains the filter, applied by the UE, common for all MR-DC related capability containers that are requested and as defined by *UE-CapabilityRequestFilterCommon* IE in TS 38.331 [82]. | | - |
| ***assistInfoBitForLC***  Indicates whether the UE supports assistance information bit for local cache. | | - |
| ***aul***  Indicates whether the UE supports AUL as specified n TS 36.321 [6]. | | - |
| ***bandCombinationListEUTRA***  One entry corresponding to each supported band combination listed in the same order as in *supportedBandCombination.* | | - |
| ***BandCombinationParameters-v1090, BandCombinationParameters-v10i0, BandCombinationParameters-v1270***  If included, the UE shall include the same number of entries, and listed in the same order, as in *BandCombinationParameters-r10*. | | - |
| ***BandCombinationParameters-v1130***  The field is applicable to each supported CA bandwidth class combination (i.e. CA configuration in TS 36.101 [42], clause 5.6A.1) indicated in the corresponding band combination. If included, the UE shall include the same number of entries, and listed in the same order, as in *BandCombinationParameters-r10*. | | - |
| ***bandEUTRA***  E‑UTRA band as defined in TS 36.101 [42]. In case the UE includes *bandEUTRA-v9e0* or *bandEUTRA-v1090*, the UE shall set the corresponding entry of *bandEUTRA* (i.e. without suffix) or *bandEUTRA-r10* respectively to *maxFBI*. | | - |
| ***bandInfoNR-v1610***  One entry corresponding to each supported E-UTRA band listed in the same order as in *supportedBandListEUTRA*. If absent, network assumes gap is required when measurement is performed on any NR bands while UE is served by cell(s) belongs to a E-UTRA band listed in *supportedBandListEUTRA* except for the FR2 inter-RAT measurement which depends on the support of *independentGapConfig*. | | - |
| ***bandListEUTRA***  One entry corresponding to each supported E‑UTRA band listed in the same order as in *supportedBandListEUTRA*. | | - |
| ***bandParameterList-v1380***  If included, the UE shall include the same number of entries listed in the same order as the band entries in the corresponding band combination. | | - |
| ***bandParametersUL, bandParametersDL***  Indicates the supported parameters for the band. Each of *CA-MIMO-ParametersUL* and *CA-MIMO-ParametersDL* can be included only once for one band in a single band combination entry. | | - |
| ***beamformed (in MIMO-CA-ParametersPerBoBCPerTM)***  If signalled, the field indicates for a particular transmission mode, the UE capabilities concerning beamformed EBF/ FD-MIMO operation (class B) applicable for the concerned band combination. | | - |
| ***beamformed (in MIMO-UE-ParametersPerTM)***  Indicates for a particular transmission mode, the UE capabilities concerning beamformed EBF/ FD-MIMO operation (class B) applicable for band combinations for which the concerned capabilities are not signalled. | | Yes |
| ***benefitsFromInterruption***  Indicates whether the UE power consumption would benefit from being allowed to cause interruptions to serving cells when performing measurements of deactivated SCell carriers for *measCycleSCell* of less than 640ms, as specified in TS 36.133 [16]. | | No |
| ***bwPrefInd***  Indicates whether the UE supports maximum PDSCH/PUSCH bandwidth preference indication. | | - |
| ***ca-BandwidthClass***  The CA bandwidth class supported by the UE as defined in TS 36.101 [42], Table 5.6A-1.  The UE explicitly includes all the supported CA bandwidth class combinations in the band combination signalling. Support for one CA bandwidth class does not implicitly indicate support for another CA bandwidth class. | | - |
| ***ca-IdleModeMeasurements***  Indicates whether UE supports reporting measurements performed during RRC\_IDLE. | | - |
| ***ca-IdleModeValidityArea***  Indicates whether UE supports validity area for IDLE measurements during RRC\_IDLE. | | - |
| ***cch-IM-RefRecTypeA-OneRX-Port***  This field defines whether the DL Category 1bis or the DL Category M2 UE supports Type A downlink control channel interference mitigation (CCH-IM) receiver "LMMSE-IRC + CRS-IC" for PDCCH/PCFICH/PHICH/EPDCCH receive processing (Enhanced downlink control channel performance requirements Type A in TS 36.101 [6]). | | No |
| ***cch-InterfMitigation-RefRecTypeA, cch-InterfMitigation-RefRecTypeB, cch-InterfMitigation-MaxNumCCs***  The field *cch-InterfMitigation-RefRecTypeA* defines whether the UE supports Type A downlink control channel interference mitigation (CCH-IM) receiver "LMMSE-IRC + CRS-IC" for PDCCH/PCFICH/PHICH/EPDCCH receive processing (Enhanced downlink control channel performance requirements Type A in the TS 36.101 [6]). The field *cch-InterfMitigation-RefRecTypeB* defines whether the UE supports Type B downlink CCH-IM receiver "E-LMMSE-IRC + CRS-IC" for PDCCH/PCFICH/PHICH receive processing in synchronous networks (Enhanced downlink control channel performance requirements Type B in the TS 36.101 [6]). The UE supporting the capability defined by *cch-InterfMitigation-RefRecTypeB-r13* shall also support the capability defined by *cch-InterfMitigation-RefRecTypeA-r13*.  If the UE sets one or more of the fields *cch-InterfMitigation-RefRecTypeA* and *cch-InterfMitigation-RefRecTypeB* to "supported", the UE shall include the parameter *cch-InterfMitigation-MaxNumCCs* to indicate that the UE supports CCH-IM on at least one arbitrary downlink CC for up to *cch-InterfMitigation-MaxNumCCs* downlink CC CA configuration. The UE shall not include the parameter *cch-InterfMitigation-MaxNumCCs* if neither *cch-InterfMitigation-RefRecTypeA* nor *cch-InterfMitigation-RefRecTypeB* is present. The UE may not perform CCH-IM on more than 1 DL CCs. For example, the UE sets "*cch-InterfMitigation-MaxNumCCs* = 3"to indicate that UE supports CCH-IM on at least one DL CC for supported non-CA, 2DL CA and 3DL CA configurations. For CA scenarios, the CCH-IM is guaranteed to be supported on at least one arbitrary component carrier. | | - |
| ***cdma2000-NW-Sharing***  Indicates whether the UE supports network sharing for CDMA2000. | | - |
| ***ce-ClosedLoopTxAntennaSelection***  Indicates whether the UE supports UL closed-loop Tx antenna selection in CE mode A, as specified in TS 36.212 [22]. | | Yes |
| ***ce-CQI-AlternativeTable***  Indicates whether the UE supports alternative CQI table in CE mode A. See TS 36.213 [22]. | | Yes |
| ***ce-CRS-IntfMitig***  Indicates whether UE supports CRS interference mitigation, i.e., value *supported* indicates UE does not rely on the CRS outside certain PRBs and subframes as defined in TS 36.133 [16], clauses 3.6.1.2 and 3.6.1.3, and TS 36.213 [23] when operating in coverage enhancement mode. | | Yes |
| ***ce-CSI-RS-Feedback***  Indicates whether the UE supports CSI-RS based feedback when the UE is operating in CE mode A, as specified in TS 36.213 [23]. | | Yes |
| ***ce-CSI-RS-FeedbackCodebookRestriction***  Indicates whether the UE supports CSI-RS based feedback with codebook subset restriction when the UE in CE is operating in CE mode A, as specified in TS 36.213 [23]. | | Yes |
| ***ce-DL-ChannelQualityReporting***  Indicates whether UE operating in CE mode supports aperiodic DL channel quality reporting in RRC\_CONNECTED. | | Yes |
| ***ce-EUTRA-5GC***  Indicates whether the UE operating in CE mode A or B supports E-UTRA/5GC. | | Yes |
| ***ce-EUTRA-5GC-HO-ToNR-FDD-FR1***  Indicates whether the UE operating in CE mode A or B supports handover from E-UTRA/5GC to NR FDD FR1. | | Yes |
| ***ce-EUTRA-5GC-HO-ToNR-TDD-FR1***  Indicates whether the UE operating in CE mode A or B supports handover from E-UTRA/5GC to NR TDD FR1. | | Yes |
| ***ce-EUTRA-5GC-HO-ToNR-FDD-FR2***  Indicates whether the UE operating in CE mode A or B supports handover from E-UTRA/5GC to NR FDD FR2. | | Yes |
| ***ce-EUTRA-5GC-HO-ToNR-TDD-FR2***  Indicates whether the UE operating in CE mode A or B supports handover from E-UTRA/5GC to NR TDD FR2-1 as specified in TS 38.101-x [xx]. | | Yes |
| ***ce-EUTRA-5GC-HO-ToNR-TDD-FR2-2***  Indicates whether the UE operating in CE mode A or B supports handover from E-UTRA/5GC to NR TDD FR2-2 as specified in TS 38.101-x [xx]. | | - |
| ***ce-HARQ-AckBundling***  Indicates whether the UE supports HARQ-ACK bundling in half duplex FDD in CE mode A, as specified in TS 36.212 [22] and TS 36.213 [23]. | | - |
| ***ce-InactiveState***  Indicates whether UE operating in CE mode supports RRC\_INACTIVE when connected to 5GC. A UE including this field also supports short eDRX cycles in RRC\_INACTIVE when connected to 5GC. | | No |
| ***ce-MeasRSS-Dedicated, ce-MeasRSS-DedicatedSameRBs***  Indicates whether the UE operating in CE mode A/B supports receiving neighbour cell RSS information in dedicated signalling and performing serving cell and neighbour cell measurements based on RSS in RRC\_CONNECTED as specified in TS 36.306 [5] and TS 36.133 [16]. | | Yes |
| ***ce-ModeA, ce-ModeB***  Indicates whether the UE supports operation in CE mode A and/or B, as specified in TS 36.211 [21] and TS 36.213 [23]. | | - |
| ***crs-ChEstMPDCCH-CE-ModeA, crs-ChEstMPDCCH-CE-ModeB***  Indicates whether UE operating in CE mode A/B supports using CRS for improving MPDCCH channel estimation. | | Yes |
| ***crs-ChEstMPDCCH-CSI***  Indicates whether UE operating in CE mode A supports CSI-based mapping for improving MPDCCH channel estimation. | | Yes |
| ***crs-ChEstMPDCCH-ReciprocityTDD***  Indicates whether UE operating in CE mode A supports using CRS for improving MPDCCH channel estimation with reciprocity-based candidates in TDD. | | No |
| ***ceMeasurements***  Indicates whether the UE supports intra-frequency RSRQ measurements and inter-frequency RSRP and RSRQ measurements in RRC\_CONNECTED, as specified in TS 36.133 [16] and TS 36.304 [4]. | | - |
| ***ce-MultiTB-64QAM***  Indicates whether the UE supports downlink 64QAM for multiple TB scheduling in connected mode for PDSCH when operating in CE mode A, as specified in TS 36.211 [21] and TS 36.213 [23]. This field can be included only if *ce-PUSCH-SubPRB-Allocation* is included. | | Yes |
| ***ce-MultiTB-EarlyTermination***  Indicates whether the UE supports early termination of PUSCH transmission for multiple TB scheduling in connected mode, as specified in TS 36.211 [21] and TS 36.213 [23]. | | Yes |
| ***ce-MultiTB-FrequencyHopping***  Indicates whether the UE supports frequency hopping for multiple TB scheduling for PDSCH/PUSCH in connected mode, as specified in TS 36.211 [21] and TS 36.213 [23]. | | Yes |
| ***ce-MultiTB-HARQ-AckBundling***  Indicates whether the UE supports downlink HARQ-ACK bundling for multiple TB scheduling in connected mode when operating in CE mode A, as specified in TS 36.211 [21] and TS 36.213 [23]. | | Yes |
| ***ce-MultiTB-Interleaving***  Indicates whether the UE supports TB interleaving for multiple TB scheduling in connected mode for PDSCH/PUSCH when operating in CE mode A or B, as specified in TS 36.211 [21] and TS 36.213 [23]. | | Yes |
| ***ce-MultiTB-SubPRB***  Indicates whether the UE supports sub-PRB allocation for multiple TB scheduling for PUSCH in connected mode, as specified in TS 36.211 [21] and TS 36.213 [23]. This field can be included only if *ce-PUSCH-SubPRB-Allocation* is included. | | Yes |
| ***ce-PDSCH-14HARQProcesses, ce-PDSCH-14HARQProcesses-Alt2***  Indicates whether the UE supports 14-HARQ processes, as specified in TS 36.212 [22]. | | - |
| ***ce-PDSCH-64QAM***  Indicates whether the UE supports 64QAM for non-repeated unicast PDSCH in CE mode A. | | Yes |
| ***ce-PDSCH-FlexibleStartPRB-CE-ModeA*, *ce-PDSCH-FlexibleStartPRB-CE-ModeB*,**  ***ce-PUSCH-FlexibleStartPRB-CE-ModeA*, *ce-PUSCH-FlexibleStartPRB-CE-ModeB***  This field indicates whether UE supports flexible starting PRB for PDSCH/PUSCH when operating in coverage enhancement mode A/B, as specified in TS 36.211 [21] and TS 36.213 [22]. | | Yes |
| ***ce-PDSCH-MaxTBS***  Indicates whether the UE supports downlink TBS of 1736 bits, as specified in TS 36.212 [22]. | | - |
| ***ce-PDSCH-PUSCH-Enhancement***  Indicates whether the UE supports new numbers of repetitions for PUSCH and modulation restrictions for PDSCH/PUSCH in CE mode A as specified in TS 36.212 [22] and TS 36.213 [23]. | | No |
| ***ce-PDSCH-PUSCH-MaxBandwidth***  Indicates the maximum supported PDSCH/PUSCH channel bandwidth in CE mode A and B, as specified in TS 36.212 [22] and TS 36.213 [23]. Value bw5 corresponds to 5 MHz and value bw20 corresponds to 20 MHz. If the field is absent the maximum PDSCH/PUSCH channel bandwidth in CE mode A and B is 1.4 MHz. If the setting of this parameter is 20 MHz, the max supported PUSCH channel bandwidth in CE mode A is 5 MHz. The maximum PUSCH channel bandwidth in CE mode B is 1.4 MHz regardless of the setting of this parameter. Parameter: transmission bandwidth configuration, see TS 36.101 [42], table 5.6-1. | | Yes |
| ***ce-PDSCH-TenProcesses***  Indicates whether the UE supports 10 DL HARQ processes in FDD in CE mode A. | | Yes |
| ***ce-PUCCH-Enhancement***  Indicates whether the UE supports repetition levels 64 and 128 for PUCCH in CE Mode B, as specified in TS 36.211 [21] and in TS 36.213 [23]. | | No |
| ***ce-PUSCH-NB-MaxTBS***  Indicates whether the UE supports 2984 bits max UL TBS in 1.4 MHz in CE mode A operation, as specified in TS 36.212 [22] and TS 36.213 [23]. | | Yes |
| ***ce-PUSCH-SubPRB-Allocation***  Indicates whether the UE supports sub-PRB resource allocation for PUSCH in CE mode A or B, as specified in TS 36.211 [21], TS 36.212 [22] and TS 36.213 [23]. | | Yes |
| ***ce-RetuningSymbols***  Indicates the number of retuning symbols in CE mode A and B as specified in TS 36.211 [21]. Value n0 corresponds to 0 retuning symbols and value n1 corresponds to 1 retuning symbol. If the field is absent the number of retuning symbols in CE mode A and B is 2. | | No |
| ***ce-SchedulingEnhancement***  Indicates whether the UE supports dynamic HARQ-ACK delay for HD-FDD in CE mode A as specified in TS 36.212 [22] and TS 36.213 [23]. | | No |
| ***ce-SRS-Enhancement***  Indicates whether the UE supports SRS coverage enhancement in TDD with support of SRS combs 2 and 4 as specified in TS 36.213 [23]. This field can be included only if *ce-SRS-EnhancementWithoutComb4* is not included. | | Yes |
| ***ce-SRS-EnhancementWithoutComb4***  Indicates whether the UE supports SRS coverage enhancement in TDD with support of SRS comb 2 but without support of SRS comb 4 as specified in TS 36.213 [23]. This field can be included only if *ce-SRS-Enhancement* is not included. | | - |
| ***ce-SwitchWithoutHO***  Indicates whether the UE supports switching between normal mode and enhanced coverage mode without handover. | | - |
| ***ce-UL-HARQ-ACK-Feedback***  This field indicates whether UE supports uplink HARQ ACK feedback when operating in coverage enhancement, as specified in TS36.213 [22]. | | Yes |
| ***channelMeasRestriction***  Indicates for a particular transmission mode whether the UE supports channel measurement restriction. | | Yes |
| ***cho***  Indicates whether the UE supports conditional handover including execution condition, candidate cell configuration and maximum 8 candidate cells. | | Yes |
| ***cho-Failure***  Indicates whether the UE supports conditional handover during re-establishment procedure when the selected cell is configured as candidate cell for condition handover. | | Yes |
| ***cho-FDD-TDD***  Indicates whether the UE supports conditional handover between FDD and TDD cells. | | No |
| ***cho-TwoTriggerEvents***  Indicates whether the UE supports 2 trigger events for same execution condition. It is mandatory supported if the UE suppors *cho*. | | Yes |
| ***codebook-HARQ-ACK***  Indicates whether the UE supports determining HARQ ACK codebook size based on the DAI-ased solution and/or the number of configured CCs. The first bit is set to "1" if the UE supports the DAI-based codebook size determination. The second bit is set to "1" if the UE supports the codebook determination based on the number of configured CCs. | | No |
| ***commMultipleTx***  Indicates whether the UE supports multiple transmissions of sidelink communication to different destinations in one SC period. If *commMultipleTx-r13* is set to supported then the UE support 8 transmitting sidelink processes. | | - |
| ***commSimultaneousTx***  Indicates whether the UE supports simultaneous transmission of EUTRA and sidelink communication (on different carriers) in all bands for which the UE indicated sidelink support in a band combination (using *commSupportedBandsPerBC*). | | - |
| ***commSupportedBands***  Indicates the bands on which the UE supports sidelink communication, by an independent list of bands i.e. separate from the list of supported E-UTRA band, as indicated in *supportedBandListEUTRA*. | | - |
| ***commSupportedBandsPerBC***  Indicates, for a particular band combination, the bands on which the UE supports simultaneous reception of EUTRA and sidelink communication. If the UE indicates support simultaneous transmission (using *commSimultaneousTx*), it also indicates, for a particular band combination, the bands on which the UE supports simultaneous transmission of EUTRA and sidelink communication. The first bit refers to the first band included in *commSupportedBands*, with value 1 indicating sidelink is supported. | | - |
| ***configN (in MIMO-CA-ParametersPerBoBCPerTM)***  If signalled, the field indicates for a particular transmission mode whether the UE supports non-precoded EBF/ FD-MIMO (class A) related configuration N for the concerned band combination. | | - |
| ***configN (in MIMO-UE-ParametersPerTM)***  Indicates for a particular transmission mode whether the UE supports non-precoded EBF/ FD-MIMO (class A) related configuration N for band combinations for which the concerned capabilities are not signalled. | | Yes |
| ***continueEHC-Context***  Indicates that the UE supports EHC context continuation operation where the UE keeps the established EHC context(s) upon PDCP re-establishment, as specified in TS 36.323 [8]. | | No |
| ***crossCarrierScheduling*** | | Yes |
| ***crossCarrierScheduling-B5C***  Indicates whether the UE supports cross carrier scheduling beyond 5 DL CCs. | | No |
| ***crossCarrierSchedulingLAA-DL***  Indicates whether the UE supports cross-carrier scheduling from a licensed carrier for LAA cell(s) for downlink. This field can be included only if *downlinkLAA* is included. | | - |
| ***crossCarrierSchedulingLAA-UL***  Indicates whether the UE supports cross-carrier scheduling from a licensed carrier for LAA cell(s) for uplink. This field can be included only if *uplinkLAA* is included. | | - |
| ***crs-DiscoverySignalsMeas***  Indicates whether the UE supports CRS based discovery signals measurement, and PDSCH/EPDCCH RE mapping with zero power CSI-RS configured for discovery signals. | | Yes |
| ***crs-IM-TM1-toTM9-OneRX-Port***  Indicates whether the DL Cateogry 1bis UE ot the DL Category M2 UE supports CRS interference mitigation (IM) while operating in the following transmission modes (TM): TM 1, TM 2, …, TM 8 and TM 9. | | No |
| ***crs-InterfHandl***  Indicates whether the UE supports CRS interference handling. | | Yes |
| ***crs-InterfMitigationTM10***  The field defines whether the UE supports CRS interference mitigation in transmission mode 10. The UE supporting the *crs-InterfMitigationTM10* capability shall also support the *crs-InterfHandl* capability. | | No |
| ***crs-InterfMitigationTM1toTM9***  Indicates whether the UE supports CRS interference mitigation (IM) while operating in the following transmission modes (TM): TM 1, TM 2, …, TM 8 and TM 9. The UE shall not include the field if it does not support CRS IM in TMs 1-9. If the field is present, the UE supports CRS-IM on at least one arbitrary downlink CC for up to *crs-InterfMitigationTM1toTM9-r13* downlink CC CA configuration. The UE signals *crs-InterfMitigationTM1toTM9-r13* value to indicate the maximum *crs-InterfMitigationTM1toTM9-r13* downlink CC CA configuration where UE may apply CRS IM. For example, the UE sets "*crs-InterfMitigationTM1toTM9-r13* = 3" to indicate that the UE supports CRS-IM on at least one DL CC for supported non-CA, 2DL CA and 3DL CA configurations. The UE supporting the *crs-InterfMitigationTM1toTM9-r13* capability shall also support the *crs-InterfHandl-r11* capability. | | - |
| ***crs-IntfMitig***  Indicate whether the UE supports CRS interference mitigation as specified in TS 36.133 [16], clause 3.6.1.1. | | Yes |
| ***crs-LessDwPTS***  Indicates whether the UE supports TDD special subframe configuration 10 without CRS transmission on the 5th symbol of DwPTS, i.e. *ssp10-CRS-LessDwPTS*, as specified in TS 36.211 [17]*.* | | - |
| ***csi-ReportingAdvanced, csi-ReportingAdvancedMaxPorts (in MIMO-CA-ParametersPerBoBCPerTM)***  If signalled, the field indicates that for a particular transmission mode, the maximum number of CSI-RS ports supported by the UE for advanced CSI reporting is different in the concerned band of band combination than the value indicated by the field *csi-ReportingAdvanced* or *csi-ReportingAdvancedMaxPorts* in *MIMO-UE-ParametersPerTM*. The UE shall not include both *csi-ReportingAdvanced* and *csi-ReportingAdvancedMaxPorts* for a particular transmission mode in the concerned band of band combination. | | - |
| ***csi-ReportingAdvanced (in MIMO-UE-ParametersPerTM)***  Indicates for a particular transmission mode the maximum number of CSI-RS ports supported by the UE for advanced CSI reporting. The field *csi-ReportingAdvanced* indicates 32 CSI-RS ports. The UE shall not include both *csi-ReportingAdvanced* and *csi-ReportingAdvancedMaxPorts* for a particular transmission mode. | | Yes |
| ***csi-ReportingAdvancedMaxPorts (in MIMO-UE-ParametersPerTM)***  Indicates for a particular transmission mode the maximum number of CSI-RS ports supported by the UE for advanced CSI reporting. The field *csi-ReportingAdvancedMaxPorts* indicates 8, 12, 16, 20, 24 or 28 CSI-RS ports. The UE shall not include both *csi-ReportingAdvanced* and *csi-ReportingAdvancedMaxPorts* for a particular transmission mode. | | - |
| ***csi-ReportingNP (in MIMO-CA-ParametersPerBoBCPerTM)***  If signalled, value *different* indicates that for a particular transmission mode, the CSI reporting on non-precoded CSI-RS with 20, 24, 28 or 32 antenna ports for the concerned band of band combination is different than the value indicated by field *csi-ReportingNP* in *MIMO-UE-ParametersPerTM*. | | - |
| ***csi-ReportingNP (in MIMO-UE-ParametersPerTM)***  Indicates for a particular transmission mode whether the UE supports CSI reporting on non-precoded CSI-RS with 20, 24, 28, or 32 antenna ports for band combinations for which the concerned capabilities are not signalled in *MIMO-CA-ParametersPerBoBCPerTM*, and the FD-MIMO processing capability condition as described in NOTE 8 is satisfied. | | Yes |
| ***csi-RS-DiscoverySignalsMeas***  Indicates whether the UE supports CSI-RS based discovery signals measurement. If this field is included, the UE shall also include *crs-DiscoverySignalsMeas*. | | Yes |
| ***csi-RS-DRS-RRM-MeasurementsLAA***  Indicates whether the UE supports performing RRM measurements on LAA cell(s) based on CSI-RS-based DRS. This field can be included only if *downlinkLAA* is included. | | - |
| ***csi-RS-EnhancementsTDD***  Indicates for a particular transmission mode whether the UE supports CSI-RS enhancements applicable for TDD. | | Yes |
| ***csi-SubframeSet***  Indicates whether the UE supports REL-12 DL CSI subframe set configuration, REL-12 DL CSI subframe set dependent CSI measurement/feedback, configuration of up to 2 CSI-IM resources for a CSI process with no more than 4 CSI-IM resources for all CSI processes of one frequency if the UE supports tm10, configuration of two ZP-CSI-RS for tm1 to tm9, PDSCH RE mapping with two ZP-CSI-RS configurations, and EPDCCH RE mapping with two ZP-CSI-RS configurations if the UE supports EPDCCH. This field is only applicable for UEs supporting TDD. | | Yes |
| ***dataInactMon***  Indicates whether the UE supports the data inactivity monitoring as specified in TS 36.321 [6]. | | - |
| ***dc-Support***  Including this field indicates that the UE supports synchronous DC and power control mode 1. Including this field for a band combination entry comprising of single band entry indicates that the UE supports intra-band contiguous DC. Including this field for a band combination entry comprising of two or more band entries, indicates that the UE supports DC for these bands and that the serving cells corresponding to a band entry shall belong to one cell group (i.e. MCG or SCG). Including field *asynchronous* indicates that the UE supports asynchronous DC and power control mode 2. Including this field for a TDD/FDD band combination indicates that the UE supports TDD/FDD DC for this band combination. | | - |
| ***delayBudgetReporting***  Indicates whether the UE supports delay budget reporting. | | No |
| ***demodulationEnhancements***  This field defines whether the UE supports advanced receiver in SFN scenario (350 km/h) as specified in TS 36.101 [42]. | | - |
| ***demodulationEnhancements2***  This field defines whether the UE supports further enhanced receiver in HST-SFN scenario (up to 500 km/h velocity) as specified in TS 36.101 [42]. | | - |
| ***densityReductionNP, densityReductionBF***  Indicates whether the UE supports CSI-RS density reduction with values 1, 1/2 and 1/3 for non-precoded CSI-RS and beamformed CSI-RS respectively. | | Yes |
| ***deviceType***  UE may set the value to "*noBenFromBatConsumpOpt*" when it does not foresee to particularly benefit from NW-based battery consumption optimisation. Absence of this value means that the device does benefit from NW-based battery consumption optimisation. | | - |
| ***diffFallbackCombReport***  Indicates that the UE supports reporting of UE radio access capabilities for the CA band combinations asked by the eNB as well as, if any, reporting of different UE radio access capabilities for their fallback band combination as specified in TS 36.306 [5]. The UE does not report fallback combinations if their UE radio access capabilities are the same as the ones for the CA band combination asked by the eNB. | | - |
| ***differentFallbackSupported***  Indicates that the UE supports different capabilities for at least one fallback case of this band combination. | | - |
| ***directMCG-SCellActivationResume***  Indicates whether the UE supports having an E-UTRA MCG SCell configured in activated SCell state. | | - |
| ***directSCellActivation***  Indicates whether the UE supports having an E-UTRA SCell configured in activated SCell state in the *RRCConnectionReconfiguration* message. This field is applicable to both LTE standalone and LTE-DC. | | - |
| ***directSCellHibernation***  Indicates whether the UE supports having an SCell configured in dormant SCell state. | | - |
| ***directSCG-SCellActivationNEDC***  Indicates whether the UE supports having an E-UTRA SCG SCell configured in activated SCell state in the *RRCConnectionReconfiguration* message contained in the NR *RRCReconfiguration* message, as defined in TS 36.321 [6] and TS 38.331 [82].  If the UE indicates support of *directSCG-SCellActivationNEDC-r16*, the UE shall also indicate support of *ne-dc* as specified in TS 38.331 [82]. | | - |
| ***directSCG-SCellActivationResume***  Indicates whether the UE supports having an E-UTRA SCG SCell configured in activated SCell state. | | - |
| ***discInterFreqTx***  Indicates whether the UE support sidelink discovery announcements either a) on the primary frequency only or b) on other frequencies also, regardless of the UE configuration (e.g. CA, DC). The UE may set discInterFreqTx to supported when having a separate transmitter or if it can request sidelink discovery transmission gaps. | | - |
| ***discoverySignalsInDeactSCell***  Indicates whether the UE supports the behaviour on DL signals and physical channels when SCell is deactivated and discovery signals measurement is configured as specified in TS 36.211 [21], clause 6.11A. This field is included only if UE supports carrier aggregation and includes *crs-DiscoverySignalsMeas*. | | Yes |
| ***discPeriodicSLSS***  Indicates whether the UE supports periodic (i.e. not just one time before sidelink discovery announcement) Sidelink Synchronization Signal (SLSS) transmission and reception for sidelink discovery. | | - |
| ***discScheduledResourceAlloc***  Indicates whether the UE supports transmission of discovery announcements based on network scheduled resource allocation. | | - |
| ***disc-UE-SelectedResourceAlloc***  Indicates whether the UE supports transmission of discovery announcements based on UE autonomous resource selection. | | - |
| ***disc***-***SLSS***  Indicates whether the UE supports Sidelink Synchronization Signal (SLSS) transmission and reception for sidelink discovery. | | - |
| ***discSupportedBands***  Indicates the bands on which the UE supports sidelink discovery. One entry corresponding to each supported E-UTRA band, listed in the same order as in *supportedBandListEUTRA*. | | - |
| ***discSupportedProc***  Indicates the number of processes supported by the UE for sidelink discovery. | | - |
| ***discSysInfoReporting***  Indicates whether the UE supports reporting of system information for inter-frequency/PLMN sidelink discovery. | | - |
| ***dl-256QAM***  Indicates whether the UE supports 256QAM in DL on the band. | | - |
| ***dl-1024QAM***  Indicates whether the UE supports 1024QAM in DL on the band or on the band within the band combination. When *dl-1024QAM-ScalingFactor* and *dl-1024QAM-TotalWeightedLayers* are included, the UE supports 1024QAM in a set of CCs in a band combination if the CCs belong to bands indicated to support 1024QAM in that band combination and the 1024QAM processing capability condition as specified in equation 4.3.5.31-1 in TS 36.306 [5] is satisfied. | | - |
| ***dl-1024QAM-ScalingFactor***  Indicates scaling factor for processing a CC configured with 1024QAM with respect to a CC not configured with 1024QAM as described in 4.3.5.31 in TS 36.306 [5]. Value *v1* indicates 1, value *v1dot2* indicates 1.2 and value *v1dot25* indicates 1.25. | | - |
| ***dl-1024QAM-TotalWeightedLayers***  Indicates total number of weighted layers the UE can process for 1024QAM as described in 4.3.5.31 in TS 36.306 [5]. Actual value = (10 + indicated value x 2), i.e., value 0 indicates 10 layers, value 1 indicates 12 layers and so on. | | - |
| ***dl-1024QAM-Slot***  Indicates whether the UE supports 1024QAM in DL on the band for slot TTI operation. | | - |
| ***dl-1024QAM-SubslotTA-1***  Indicates whether the UE supports 1024QAM in DL on the band for subslot TTI operation with TA set 1. | | - |
| ***dl-1024QAM-SubslotTA-2***  Indicates whether the UE supports 1024QAM in DL on the band for subslot TTI operation with TA set 2, dmrsBasedSPDCCH-nonMBSFN | | - |
| ***dl-DedicatedMessageSegmentation***  Indicates whether the UE supports reception of segmented DL RRC messages. | | - |
| ***dmrs-BasedSPDCCH-MBSFN***  Indicates whether the UE supports sDCI monitoring in DMRS based SPDCCH for MBSFN subframe. If UE supports this, it also provides the corresponding DMRS based SPDCCH capability in *min-Proc-TimelineSubslot.* | | Yes |
| ***dmrs-BasedSPDCCH-nonMBSFN***  Indicates whether the UE supports sDCI monitoring in DMRS based SPDCCH for non-MBSFN subframe. If UE supports this, it also provides the corresponding DMRS based SPDCCH capability in *min-Proc-TimelineSubslot.* | | Yes |
| ***dmrs-Enhancements (in MIMO-CA-ParametersPerBoBCPerTM)***  If signalled, the field indicates for a particular transmission mode, that for the concerned band combination the DMRS enhancements are different than the value indicated by field *dmrs-Enhancements* in *MIMO-UE-ParametersPerTM*. | | - |
| ***dmrs-Enhancements (in MIMO-UE-ParametersPerTM)***  Indicates for a particular transmission mode whether the UE supports DMRS enhancements for the indicated transmission mode. | | Yes |
| ***dmrs-LessUpPTS***  Indicates whether the UE supports not to transmit DMRS for PUSCH in UpPTS. | | No |
| ***dmrs-OverheadReduction***  Indicates whether the UE supports OCC4 for rank 3 and 4 transmission as specified in clause 5.3.3.1.5C of TS 36.212 [22]. | | Yes |
| ***dmrs-PositionPattern***  Indicates whether the UE supports uplink DMRS position pattern 'D D D' in subslot #5 with application of the 1/6 as the TBS scaling factor. | | Yes |
| ***dmrs-RepetitionSubslotPDSCH***  Indicates whether the UE supports back-to-back 3/4-layer DMRS reception in two consecutive subslots across subframe boundary for subslot-PDSCH. | | Yes |
| ***dmrs-SharingSubslotPDSCH***  Indicates whether the UE supports DMRS sharing in two consecutive subslots across subframe boundary for subslot-PDSCH. | | Yes |
| ***dormantSCellState***  Indicates whether UE supports Dormant SCell state (i.e. SCell state with CQI and RRM measurement reporting but no PDCCH monitoring). | | - |
| ***downlinkLAA***  Presence of the field indicates that the UE supports downlink LAA operation including identification of downlink transmissions on LAA cell(s) for full downlink subframes, decoding of common downlink control signalling on LAA cell(s), CSI feedback for LAA cell(s), RRM measurements on LAA cell(s) based on CRS-based DRS. | | - |
| ***drb-TypeSCG***  Indicates whether the UE supports SCG bearer. | | - |
| ***drb-TypeSplit***  Indicates whether the UE supports split bearer except for PDCP data transfer in UL. | | - |
| ***dtm***  Indicates whether the UE supports DTM in GERAN. | | - |
| ***dummy***  This field is not used in the specification. It shall not be sent by the UE. | | - |
| ***earlyData-UP***  Indicates whether the UE supports UP-EDT when connected to EPC. | | - |
| ***earlyData-UP-5GC***  Indicates whether the UE supports UP-EDT when connected to 5GC. | | - |
| ***earlySecurityReactivation***  Indicates whether the UE supports early security reactivation when resuming a suspended RRC connection. | | - |
| ***e-CSFB-1XRTT***  Indicates whether the UE supports enhanced CS fallback to CDMA2000 1xRTT or not. | | Yes |
| ***e-CSFB-ConcPS-Mob1XRTT***  Indicates whether the UE supports concurrent enhanced CS fallback to CDMA2000 1xRTT and PS handover/ redirection to CDMA2000 HRPD. | | Yes |
| ***e-CSFB-dual-1XRTT***  Indicates whether the UE supports enhanced CS fallback to CDMA2000 1xRTT for dual Rx/Tx configuration. This bit can only be set to supported if *tx-Config1XRTT* and *rx-Config1XRTT* are both set to dual. | | Yes |
| ***e-HARQ-Pattern-FDD***  Indicates whether the UE supports enhanced HARQ pattern for TTI bundling operation for FDD. | | Yes |
| ***ehc***  Indicates that the UE supports Ethernet header compression and decompression using EHC protocol, as specified in TS 36.323 [8] and in Annex A of TS 38.323 [83]. The UE indicating this capability and indicating support for at least one ROHC profile, shall support simultaneous configuration of EHC and ROHC on different DRBs. | | No |
| ***eLCID-Support***  Indicates whether the UE supports LCID "10000" and MAC PDU subheader containing the eLCID field as described in TS 36.321 [6]. | | - |
| ***emptyUnicastRegion***  Indicates whether the UE supports unicast reception in subframes with empty unicast control region as described in TS 36.213 [23] clause 12. This field can be included only if *unicast-fembmsMixedSCell* and *crossCarrierScheduling* are included. | | No |
| ***en-DC***  Indicates whether the UE supports EN-DC. | | - |
| ***endingDwPTS***  Indicates whether the UE supports reception ending with a subframe occupied for a DwPTS-duration as described in TS 36.211 [21] and TS 36.213 [23]. This field can be included only if *downlinkLAA* is included. | | - |
| ***Enhanced-4TxCodebook***  Indicates whether the UE supports enhanced 4Tx codebook*.* | | No |
| ***enhancedDualLayerTDD***  Indicates whether the UE supports enhanced dual layer (PDSCH transmission mode 8) for TDD or not. | | - |
| ***ePDCCH***  Indicates whether the UE can receive DCI on UE specific search space on Enhanced PDCCH. | | Yes |
| ***epdcch-SPT-differentCells***  Indicates whether the UE supports EPDCCH and short processing time on different serving cells. | | Yes |
| ***epdcch-STTI-differentCells***  Indicates whether the UE supports EPDCCH and sTTI on different serving cells. | | Yes |
| ***e-RedirectionUTRA*** | | Yes |
| ***e-RedirectionUTRA-TDD***  Indicates whether the UE supports enhanced redirection to UTRA TDD to multiple carrier frequencies both with and without using related SIB provided by *RRCConnectionRelease* or not. | | Yes |
| ***etws-CMAS-RxInConnCE-ModeA, etws-CMAS-RxInConn***  Indicates whether the UE operating in CE mode A/B supports reception of ETWS/CMAS indication in RRC\_CONNECTED mode as specified in TS 36.212 [22]. | | - |
| ***eutra-5GC***  Indicates whether the UE supports E-UTRA/5GC. | | Yes |
| ***eutra-5GC-HO-ToNR-FDD-FR1***  Indicates whether the UE supports handover from E-UTRA/5GC to NR FDD FR1. | | Yes |
| ***eutra-5GC-HO-ToNR-TDD-FR1***  Indicates whether the UE supports handover from E-UTRA/5GC to NR TDD FR1. | | Yes |
| ***eutra-5GC-HO-ToNR-FDD-FR2***  Indicates whether the UE supports handover from E-UTRA/5GC to NR FDD FR2. | | Yes |
| ***eutra-5GC-HO-ToNR-TDD-FR2***  Indicates whether the UE supports handover from E-UTRA/5GC to NR TDD FR2-1 as specified in TS 38.101-x [xx]. | | Yes |
| ***eutra-5GC-HO-ToNR-TDD-FR2-2***  Indicates whether the UE supports handover from E-UTRA/5GC to NR TDD FR2-2 as specified in TS 38.101-x [xx]. | | - |
| ***eutra-CGI-Reporting-ENDC***  Indicates whether the UE supports Intra-RAT report CGI procedure when it is configured with (NG) EN-DC wherein either MN and SN have different DRX cycles, or on-duration configured by MN does not contain on-duration configured by SN if their DRX cycles are same. | | Yes |
| ***eutra-CGI-Reporting-NEDC***  Indicates whether the UE supports acquisition of relevant information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell and reporting the acquired information to the network when the NE-DC is configured. | | Yes |
| ***eutra-EPC-HO-ToNR-FDD-FR1***  Indicates whether the UE supports handover from E-UTRA/EPC to NR FDD FR1. | | Yes |
| ***eutra-EPC-HO-ToNR-TDD-FR1***  Indicates whether the UE supports handover from E-UTRA/EPC to NR TDD FR1. | | Yes |
| ***eutra-EPC-HO-ToNR-FDD-FR2***  Indicates whether the UE supports handover from E-UTRA/EPC to NR FDD FR2. | | Yes |
| ***eutra-EPC-HO-ToNR-TDD-FR2***  Indicates whether the UE supports handover from E-UTRA/EPC to NR TDD FR2-1 as specified in TS 38.101-x [xx]. | | Yes |
| ***eutra-EPC-HO-ToNR-TDD-FR2-2***  Indicates whether the UE supports handover from E-UTRA/EPC to NR TDD FR2-2 as specified in TS 38.101-x [xx]. | | - |
| ***eutra-EPC-HO-EUTRA-5GC***  Indicates whether the UE supports handover between E-UTRA/EPC and E-UTRA/5GC. | | Yes |
| ***eutra-IdleInactiveMeasurements***  Indicates whether UE supports reporting measurements performed during RRC\_IDLE or RRC\_INACTIVE. | | No |
| ***eutra-SI-AcquisitionForHO-ENDC***  Indicates whether the UE supports, upon configuration of *si-RequestForHO* by the network, acquisition of relevant information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell using autonomous gaps and reporting the acquired information to the network. | | Yes |
| ***eventB2***  Indicates whether the UE supports event B2. A UE supporting NR SA operation shall set this bit to *supported*. | | - |
| ***extendedBand-n77***  This field is only applicable for UEs that indicate support for band n77. If present, the UE supports the restriction to 3450 - 3550 MHz and 3700 - 3980 MHz ranges of band n77 in the USA as specified in Note 12 of Table 5.2-1 in TS 38.101-1 [85]. If absent, the UE supports only restriction to the 3700 - 3980 MHz range of band n77 in the USA. A UE that indicates this field shall support NS value 55 as specified in TS 38.101-1 [85]. | | - |
| ***extendedFreqPriorities***  Indicates whether the UE supports extended E-UTRA frequency priorities indicated by *cellReselectionSubPriority* field. A UE supporting NR SA operation shall set this bit to *supported*. | | - |
| ***extendedLCID-Duplication***  Indicates whether the UE supports use of extended LCIDs 32-38 for PDCP duplication. | | - |
| ***extendedLongDRX***  Indicates whether the UE supports extended long DRX cycle values of 5.12s and 10.24s in RRC\_CONNECTED. | | - |
| ***extendedMAC-LengthField***  Indicates whether the UE supports the MAC header with L field of size 16 bits as specified in TS 36.321 [6], clause 6.2.1. | | - |
| ***extendedMaxMeasId***  Indicates whether the UE supports extended number of measurement identies as defined by *maxMeasId-r12*. | | No |
| ***extendedMaxObjectId***  Indicates whether the UE supports extended number of measurement object identies as defined by *maxObjectId-r13*. | | No |
| ***extendedNumberOfDRBs***  Indicates whether the UE supports up to 15 DRBs. The UE shall support any combination of RLC AM and RLC UM entities for the configured DRBs. | | - |
| ***extendedPollByte***  Indicates whether the UE supports extended pollByte values as defined by *pollByte-r14*. | | - |
| ***extended-RLC-LI-Field***  Indicates whether the UE supports 15 bit RLC length indicator. | | - |
| ***extendedRLC-SN-SO-Field***  Indicates whether the UE supports 16 bits of RLC sequence number and segmentation offset. | | - |
| ***extendedRSRQ-LowerRange***  Indicates whether the UE supports the extended RSRQ lower value range from -34dB to -19.5dB in measurement configuration and reporting as specified in TS 36.133 [16]. | | No |
| ***fdd-HARQ-TimingTDD***  Indicates whether UE supports FDD HARQ timing for TDD SCell when configured with TDD PCell. | | Yes |
| ***featureGroupIndicators, featureGroupIndRel9Add, featureGroupIndRel10***  The definitions of the bits in the bit string are described in Annex B.1 (for *featureGroupIndicators* and *featureGroupIndRel9Add*) and in Annex C.1 (for *featureGroupIndRel10*). | | Yes |
| ***featureSetsDL-PerCC***  In MR-DC, indicates a set of features that the UE supports on one component carrier in a bandwidth class for a band in a given band combination. The UE shall hence include at least as many *FeatureSetDL-PerCC-Id* in this list as the number of carriers it supports according to the *ca-bandwidthClassDL*, except if indicating additional functionality by reducing the number of *FeatureSetDownlinkPerCC-Id* in the feature set. The order of the elements in this list is not relevant, i.e., the network may configure any of the carriers in accordance with any of the *FeatureSetDL-PerCC-Id* in this list. | | - |
| ***FeatureSetDL-PerCC-Id***  In MR-DC, indicates the index position of the *FeatureSetDL-PerCC-r15* in the *featureSetsDL-PerCC-r15* list. Value 0 corresponds to the first element in the list, value 1 corresponds to the second element in the list, and so on. Value 32 is not used. | | - |
| ***featureSetsUL-PerCC***  In MR-DC, indicates a set of features that the UE supports on one component carrier in a bandwidth class for a band in a given band combination. The UE shall hence include at least as many *FeatureSetUL-PerCC-Id* in this list as the number of carriers it supports according to the *ca-bandwidthClassUL*, except if indicating additional functionality by reducing the number of *FeatureSetDownlinkPerCC-Id* in the feature set. The order of the elements in this list is not relevant, i.e., the network may configure any of the carriers in accordance with any of the *FeatureSetUL-PerCC-Id* in this list. | | - |
| ***FeatureSetUL-PerCC-Id***  In MR-DC, indicates the index position of the *FeatureSetUL-PerCC-r15* in the *featureSetsUL-PerCC-r15* list. Value 0 corresponds to the first element in the list, value 1 corresponds to the second element in the list, and so on. Value 32 is not used. | | - |
| ***fembmsMixedCell***  Indicates whether the UE in RRC\_CONNECTED supports MBMS reception with 15 kHz subcarrier spacings via MBSFN from FeMBMS/Unicast mixed cells on a frequency indicated in an *MBMSInterestIndication* message. | |  |
| ***fembmsDedicatedCell***  Indicates whether the UE in RRC\_CONNECTED supports MBMS reception with 15 kHz subcarrier spacings via MBSFN from MBMS-dedicated cells on a frequency indicated in an *MBMSInterestIndication* message. | |  |
| ***flexibleUM-AM-Combinations***  Indicates whether the UE supports any combination of RLC UM and RLC AM bearers as long as the total number of bearers is at most 8, regardless of what FGI20 indicates. | | - |
| ***flightPathPlan***  Indicates whether UE supports reporting of flight path plan information. | | - |
| ***fourLayerTM3-TM4***  Indicates whether the UE supports 4-layer spatial multiplexing for TM3 and TM4. | | - |
| ***fourLayerTM3-TM4 (in FeatureSetDL-PerCC)***  Indicates whether the UE supports 4-layer spatial multiplexing for TM3 and TM4 for MR-DC within the indicated feature set. If this field is absent, UE supports two layer MIMO for TM3/TM4. | | - |
| ***fourLayerTM3-TM4-perCC***  Indicates whether the UE supports 4-layer spatial multiplexing for TM3 and TM4 for the component carrier. | | - |
| ***frameStructureType-SPT***  This field indicates the supported FS-type(s) for short processing time. The UE capability is reported per band combination. The reported FS-type(s) apply to the reported *maxNumberCCs-SPT-r15* for the given band combination. | | - |
| ***freqBandPriorityAdjustment***  Indicates whether the UE supports the prioritization of frequency bands in *multiBandInfoList* over the band in *freqBandIndicator* as defined by *freqBandIndicatorPriority-r12*. | | - |
| ***freqBandRetrieval***  Indicates whether the UE supports reception of *requestedFrequencyBands.* | | - |
| ***halfDuplex***  If *halfDuplex* is set to true, only half duplex operation is supported for the band, otherwise full duplex operation is supported. | | - |
| ***heightMeas***  Indicates whether UE supports the measurement events H1/H2. | | - |
| ***ho-EUTRA-5GC-FDD-TDD***  Indicates whether the UE supports handover between E-UTRA/5GC FDD and E-UTRA/5GC TDD. | | No |
| ***ho-InterfreqEUTRA-5GC***  Indicates whether the UE supports inter frequency handover within E-UTRA/5GC. | | Yes |
| ***hybridCSI***  Indicates whether the UE supports hybrid CSI transmission as described in TS 36.213 [23]. | | Yes |
| ***idleInactiveValidityAreaList***  Indicates whether the UE supports list of validity areas for measurements during RRC\_IDLE and RRC\_INACTIVE. | | No |
| ***immMeasBT***  Indicates whether the UE supports Bluetooth measurements in RRC connected mode. | | - |
| ***immMeasUnComBarPre***  Indicates whether the UE supports uncompensated barometric pressure measurements in RRC connected mode. | | - |
| ***immMeasWLAN***  Indicates whether the UE supports WLAN measurements in RRC connected mode. | | - |
| ***ims-VoiceOverMCG-BearerEUTRA-5GC***  Indicates whether the UE supports IMS voice over NR PDCP for MCG bearer for E-UTRA/5GC. | | No |
| ***ims-VoiceOverNR-FR1***  Indicates whether the UE supports IMS voice over NR FR1. | | No |
| ***ims-VoiceOverNR-FR2***  Indicates whether the UE supports IMS voice over NR FR2-1 as specified in TS 38.101-x [xx]. | | No |
| ***ims-VoiceOverNR-FR2-2***  Indicates whether the UE supports IMS voice over NR FR2-2 as specified in TS 38.101-x [xx]. | | - |
| ***ims-VoiceOverNR-PDCP-MCG-Bearer***  Indicates whether the UE supports IMS voice over NR PDCP with only MCG RLC bearer. | | Yes |
| ***ims-VoiceOverNR-PDCP-SCG-Bearer***  Indicates whether the UE supports IMS voice over NR PDCP with only SCG RLC bearer when configured with EN-DC. | | Yes |
| ***ims-VoNR-PDCP-SCG-NGENDC***  Indicates whether the UE supports IMS voice over NR PDCP with only SCG RLC bearer when configured with NGEN-DC. | | Yes |
| ***inactiveState***  Indicates whether the UE supports RRC\_INACTIVE. | | No |
| ***incMonEUTRA***  Indicates whether the UE supports increased number of E-UTRA carrier monitoring in RRC\_IDLE and RRC\_CONNECTED, as specified in TS 36.133 [16]. | | No |
| ***incMonUTRA***  Indicates whether the UE supports increased number of UTRA carrier monitoring in RRC\_IDLE and RRC\_CONNECTED, as specified in TS 36.133 [16]. | | No |
| ***inDeviceCoexInd***  Indicates whether the UE supports in-device coexistence indication as well as autonomous denial functionality. | | Yes |
| ***inDeviceCoexInd-ENDC***  Indicates whether the UE supports in-device coexistence indication for (NG)EN-DC operation. This field can be included only if *inDeviceCoexInd* is included. The UE supports *inDeviceCoexInd-ENDC* in the same duplexing modes as it supports *inDeviceCoexInd*. | | - |
| ***inDeviceCoexInd-HardwareSharingInd***  Indicates whether the UE supports indicating hardware sharing problems when sending the *InDeviceCoexIndication*, as well as omitting the TDM assistance information. A UE that supports hardware sharing indication shall also indicate support of LAA operation. | | - |
| ***inDeviceCoexInd-UL-CA***  Indicates whether the UE supports UL CA related in-device coexistence indication. This field can be included only if *inDeviceCoexInd* is included. The UE supports *inDeviceCoexInd-UL-CA* in the same duplexing modes as it supports *inDeviceCoexInd*. | | - |
| ***interBandTDD-CA-WithDifferentConfig***  Indicates whether the UE supports inter-band TDD carrier aggregation with different UL/DL configuration combinations. The first bit indicates UE supports the configuration combination of SCell DL subframes are a subset of PCell and PSCell by SIB1 configuration and the configuration combination of SCell DL subframes are a superset of PCell and PSCell by SIB1 configuration; the second bit indicates UE supports the configuration combination of SCell DL subframes are neither superset nor subset of PCell and PSCell by SIB1 configuration. This field is included only if UE supports inter-band TDD carrier aggregation. | | - |
| ***interBandPowerSharingAsyncDAPS***  Indicates whether the UE supports power sharing for asynchronous inter-band DAPS handovers. | | - |
| ***interBandPowerSharingSyncDAPS***  Indicates whether the UE supports power sharing for synchronous inter-band DAPS handovers. | | - |
| ***interferenceMeasRestriction***  Indicates whether the UE supports interference measurement restriction. | | Yes |
| ***interFreqAsyncDAPS***  Indicates whether the UE supports asynchronous DAPS handover in source PCell and inter-frequency target PCell. | | - |
| ***interFreqBandList***  One entry corresponding to each supported E‑UTRA band listed in the same order as in *supportedBandListEUTRA*. | | - |
| ***interFreqDAPS***  Indicates whether the UE supports DAPS handover in source PCell and inter-frequency target PCell, i.e. support of simultaneous DL reception of PDCCH and PDSCH from source and target cell. For a BC, the capability applies to every carrier pair for source and target. A UE indicating this capability shall also support synchronous DAPS handover, and single UL transmission for inter-frequency DAPS handover. | | - |
| ***interFreqMultiUL-TransmissionDAPS***  Indicates that the UE supports simultaneous UL transmission in source PCell and inter-frequency target PCell. | | - |
| ***interFreqNeedForGaps***  Indicates need for measurement gaps when operating on the E‑UTRA band given by the entry in *bandListEUTRA* or on the E-UTRA band combination given by the entry in *bandCombinationListEUTRA* and measuring on the E‑UTRA band given by the entry in *interFreqBandList*. | | - |
| ***interFreqProximityIndication***  Indicates whether the UE supports proximity indication for inter-frequency E-UTRAN CSG member cells*.* | | - |
| ***interFreqRSTD-Measurement***  Indicates whether the UE supports inter-frequency RSTD measurements for OTDOA positioning, as specified in TS 36.355 [54]. | | Yes |
| ***interFreqSI-AcquisitionForHO***  Indicates whether the UE supports, upon configuration of si-RequestForHO by the network, acquisition and reporting of relevant information using autonomous gaps by reading the SI from a neighbouring inter-frequency cell. | | Yes |
| ***interRAT-BandList***  One entry corresponding to each supported band of another RAT listed in the same order as in the *interRAT-Parameters*. The NR bands reported in *SupportedBandListNR* are excluded from this list. | | - |
| ***interRAT-BandListNR-EN-DC***  One entry corresponding to each supported NR band listed in the same order as in the *supportedBandListEN-DC-r15*. If both *interRAT-BandListNR-EN-DC* and *interRAT-BandListNR-SA* are included, the UE shall set the same *interRAT-NeedForGapsNR* value for the same NR band. | | - |
| ***interRAT-BandListNR-SA***  One entry corresponding to each supported NR band listed in the same order as in the *supportedBandListNR-SA*. If both *interRAT-BandListNR-EN-DC* and *interRAT-BandListNR-SA* are included, the UE shall set the same *interRAT-NeedForGapsNR* value for the same NR band. | | - |
| ***interRAT-enhancementNR***  Indicates whether the UE supports enhanced inter-RAT NR measurement requirements to support high speed up to 500 km/h as specified in TS 36.133 [16], when EN-DC is not configured and when EN-DC is configured. | | - |
| ***interRAT-NeedForGaps***  Indicates need for DL measurement gaps when operating on the E‑UTRA band given by the entry in *bandListEUTRA or on the E-UTRA band combination given by the entry in bandCombinationListEUTRA* and measuring on the inter-RAT band given by the entry in the *interRAT-BandList*. | | - |
| ***interRAT-NeedForGapsNR***  Indicates need for measurement gaps when operating on the E‑UTRA band given by the entry in *supportedBandListEUTRA or on the E-UTRA band combination given by the entry in supportedBandCombination-r10 or supportedBandCombinationAdd-r11* or *supportedBandCombinationReduced-r13* and measuring on the NR band given by the entry in the *InterRAT-BandListNR*. | | - |
| ***interRAT-ParametersWLAN***  Indicates whether the UE supports WLAN measurements configured by *MeasObjectWLAN* with corresponding quantity and report configuration in the supported WLAN bands. | | - |
| ***interRAT-PS-HO-ToGERAN***  Indicates whether the UE supports inter-RAT PS handover to GERAN or not. | | Yes |
| ***intraBandContiguousCC-InfoList***  Indicates, per serving carrier of which the corresponding bandwidth class includes multiple serving carriers (i.e. bandwidth class B, C, D and so on), the maximum number of supported layers for spatial multiplexing in DL and the maximum number of CSI processes supported. The number of entries is equal to the number of component carriers in the corresponding bandwidth class. The UE shall support the setting indicated in each entry of the list regardless of the order of entries in the list.The UE shall include the field only if it supports 4-layer spatial multiplexing in transmission mode3/4 for a subset of component carriers in the corresponding bandwidth class, or if the maximum number of supported layers for at least one component carrier is higher than *supportedMIMO-CapabilityDL-r10* in the corresponding bandwidth class, or if the number of CSI processes for at least one component carrier is higher than *supportedCSI-Proc-r11* in the corresponding band.  This field may also be included for bandwidth class A but in such a case without including any sub-fields in *IntraBandContiguousCC-Info-r12* (see NOTE 6). | | - |
| ***intraFreqA3-CE-ModeA***  Indicates whether the UE when operating in CE Mode A supports *eventA3* for intra-frequency neighbouring cells. | | - |
| ***intraFreqA3-CE-ModeB***  Indicates whether the UE when operating in CE Mode B supports *eventA3* for intra-frequency neighbouring cells. | | - |
| ***intraFreq-CE-NeedForGaps***  Indicates need for measurement gaps when operating in CE on the E‑UTRA band given by the entry in *supportedBandListEUTRA.* | |  |
| ***intraFreqAsyncDAPS***  Indicates whether the UE supports asynchronous DAPS handover in source PCell and intra-frequency target PCell. | | - |
| ***intraFreqDAPS***  Indicates whether UE supports DAPS handover in source PCell and intra-frequency target PCell, i.e. support of simultaneous DL reception of PDCCH and PDSCH from source and target cell. A UE indicating this capability shall also support synchronous DAPS handover, and single UL transmission for intra-frequency DAPS handover. | | - |
| ***intraFreqHO-CE-ModeA***  Indicates whether the UE when operating in CE Mode A supports intra-frequency handover. | | - |
| ***intraFreqHO-CE-ModeB***  Indicates whether the UE when operating in CE Mode B supports intra-frequency handover. | | - |
| ***intraFreqProximityIndication***  Indicates whether the UE supports proximity indication for intra-frequency E-UTRAN CSG member cells. | | - |
| ***intraFreqSI-AcquisitionForHO***  Indicates whether the UE supports, upon configuration of si-RequestForHO by the network, acquisition and reporting of relevant information using autonomous gaps by reading the SI from a neighbouring intra-frequency cell. | | Yes |
| ***intraFreqTwoTAGs-DAPS***  Indicates whether the UE supports different timing advance groups in source PCell and intra-frequency target PCell. It is mandatory for *intraFreqDAPS* capable UE. | | - |
| ***jointEHC-ROHC-Config***  Indicates whether the UE supports simultaneous configuration of EHC and ROHC protocols for the same DRB. | | No |
| ***k-Max (in MIMO-CA-ParametersPerBoBCPerTM)***  If signalled, the field indicates for a particular transmission mode the maximum number of NZP CSI RS resource configurations supported within a CSI process applicable for the concerned band combination. | | No |
| ***k-Max (in MIMO-UE-ParametersPerTM)***  Indicates for a particular transmission mode the maximum number of NZP CSI RS resource configurations supported within a CSI process applicable for band combinations for which the concerned capabilities are not signalled. | | Yes |
| ***laa-PUSCH-Mode1***  Indicates whether the UE supports LAA PUSCH mode 1as defined in TS 36.213 [23]. | | - |
| ***laa-PUSCH-Mode2***  Indicates whether the UE supports LAA PUSCH mode 2as defined in TS 36.213 [23]*.* | | - |
| ***laa-PUSCH-Mode3***  Indicates whether the UE supports LAA PUSCH mode 3as defined in TS 36.213 [23]*.* | | - |
| ***locationReport***  Indicates whether the UE supports reporting of its geographical location information to eNB. | | - |
| ***loggedMBSFNMeasurements***  Indicates whether the UE supports logged measurements for MBSFN. A UE indicating support for logged measurements for MBSFN shall also indicate support for logged measurements in Idle mode. | | - |
| ***loggedMeasBT***  Indicates whether the UE supports Bluetooth measurements in RRC idle mode. | | - |
| ***loggedMeasIdleEventL1***  Indicates whether the UE supports event triggered logged measurements for *eventL1* in *camped normally* state. | | - |
| ***loggedMeasIdleEventOutOfCoverage***  Indicates whether the UE supports event triggered logged measurements for *outOfCoverage* in *any cell selection* state. | | - |
| ***loggedMeasUnComBarPre***  Indicates whether the UE supports uncompensated barometric pressure measurements in RRC\_IDLE mode. | | - |
| ***loggedMeasurementsIdle***  Indicates whether the UE supports logged measurements in Idle mode. | | - |
| ***loggedMeasWLAN***  Indicates whether the UE supports WLAN measurements in RRC idle mode. | | - |
| ***logicalChannelSR-ProhibitTimer***  Indicates whether the UE supports the *logicalChannelSR-ProhibitTimer* as defined in TS 36.321 [6]. | | - |
| ***longDRX-Command***  Indicates whether the UE supports Long DRX Command MAC Control Element. | | - |
| ***lwa***  Indicates whether the UE supports LTE-WLAN Aggregation (LWA). The UE which supports LWA shall also indicate support of *interRAT-ParametersWLAN-r13*. | | - |
| ***lwa-BufferSize***  Indicates whether the UE supports the layer 2 buffer sizes for "with support for split bearers" as defined in Table 4.1-3 and 4.1A-3 of TS 36.306 [5] for LWA. | | - |
| ***lwa-HO-WithoutWT-Change***  Indicates whether the UE supports handover where LWA configuration is retained without WT change and using LWA end-marker for PDCP key change indication for LWA operation. | | - |
| ***lwa-RLC-UM***  Indicates whether the UE supports RLC UM for LWA bearer. | | - |
| ***lwa-SplitBearer***  Indicates whether the UE supports the split LWA bearer (as defined in TS 36.300 [9]). | | - |
| ***lwa-UL***  Indicates whether the UE supports UL transmission over WLAN for LWA bearer. | | - |
| ***lwip***  Indicates whether the UE supports LTE/WLAN Radio Level Integration with IPsec Tunnel (LWIP). The UE which supports LWIP shall also indicate support of *interRAT-ParametersWLAN-r13*. | | - |
| ***lwip-Aggregation-DL, lwip-Aggregation-UL***  Indicates whether the UE supports aggregation of LTE and WLAN over DL/UL LWIP. The UE that indicates support of LWIP aggregation over DL or UL shall also indicate support of *lwip*. | | - |
| ***makeBeforeBreak***  Indicates whether the UE supports intra-frequency Make-Before-Break handover, and whether the UE which indicates *dc-Parameters* supports intra-frequency Make-Before-Break SeNB change, as defined in TS 36.300 [9]. | | - |
| ***measGapPatterns-NRonly***  Indicates whether the UE supports gap patterns 2, 3 and 11 in LTE standalone when the frequencies to be measured within this measurement gap are all NR frequencies. | | No |
| ***measGapPatterns-NRonly-ENDC***  Indicates whether the UE supports gap patterns 2, 3 and 11 in (NG)EN-DC when the frequencies to be measured within this measurement gap are all NR frequencies. | | No |
| ***maximumCCsRetrieval***  Indicates whether UE supports reception of *requestedMaxCCsDL* and *requestedMaxCCsUL*. | | - |
| ***maxLayersMIMO-Indication***  Indicates whether the UE supports the network configuration of *maxLayersMIMO*. If the UE supports *fourLayerTM3-TM4* or *intraBandContiguousCC-InfoList* or *FeatureSetDL-PerCC* for MR-DC, UE supports the configuration of *maxLayersMIMO* for these cases regardless of indicating *maxLayersMIMO-Indication*. | | - |
| ***maxLayersSlotOrSubslotPUSCH***  Indicates the maxiumum number of layers for slot-PUSCH or subslot-PUSCH transmission. | | Yes |
| ***maxNumberCCs-SPT***  Indicates the maximum number of supported CCs for short processing time. The UE capability is reported per band combination. The reported number of carriers applies to all the FS-type(s) *frameStructureType-SPT-r15* supported in a given band combination. Absence of the field indicates that 0 number of CCs are supported for short processing time. | | - |
| ***maxNumberDL-CCs, maxNumberUL-CCs***  Indicates for each TTI combination "sTTI-SupportedCombinations", the maximum number of supported DL CCs/UL CCs for short TTI. Absence of the field indicates that 0 number of CCs are supported for short TTI. | | - |
| ***maxNumberDecoding***  Indicates the maximum number of blind decodes in UE-specific search space per UE in one subframe for CA with more than 5 CCs as defined in TS 36.213 [23] which is supported by the UE. The number of blind decodes supported by the UE is the field value \* 32. Only values 5 to 32 can be used in this version of the specification. | | No |
| ***maxNumberEHC-Contexts***  Defines the maximum number of Ethernet header compression contexts supported by the UE across all DRBs and across UE's EHC compressor and EHC decompressor. The indicated number defines the number of contexts in addition to CID = "all zeros" as specified in Annex A of TS 38.323 [83]. | | No |
| ***maxNumberROHC-ContextSessions***  Set to the maximum number of concurrently active ROHC contexts supported by the UE, excluding context sessions that leave all headers uncompressed. cs2 corresponds with 2 (context sessions), cs4 corresponds with 4 and so on. The network ignores this field if the UE supports none of the ROHC profiles in *supportedROHC-Profiles*. If the UE indicates both *maxNumberROHC-ContextSessions* and *maxNumberROHC-ContextSessions-r14*, same value shall be indicated. | | - |
| ***maxNumberUpdatedCSI-Proc, maxNumberUpdatedCSI-Proc-SPT***  Indicates the maximum number of CSI processes to be updated across CCs. | | No |
| ***maxNumberUpdatedCSI-Proc-STTI-Comb77, maxNumberUpdatedCSI-Proc-STTI-Comb27, maxNumberUpdatedCSI-Proc-STTI-Comb22-Set1, maxNumberUpdatedCSI-Proc-STTI-Comb22-Set2***  Indicates the maximum number of CSI processes to be updated across CCs. Comb77 is applicable for {slot, slot}, Comb27 for {subslot, slot}, Comb22-Set1 for  {subslot, subslot} processing timeline set 1 and the Comb22-Set2 for {subslot, subslot} processing timeline set 2. | |  |
| ***mbms-AsyncDC***  Indicates whether the UE in RRC\_CONNECTED supports MBMS reception via MRB on a frequency indicated in an *MBMSInterestIndication* message, where (according to *supportedBandCombination*) the carriers that are or can be configured as serving cells in the MCG and the SCG are not synchronized. If this field is included, the UE shall also include *mbms-SCell* and *mbms-NonServingCell*. The field indicates that the UE supports the feature for xDD if *mbms-SCell* and *mbms-NonServingCell* are supported for xDD. | | - |
| ***mbms-MaxBW***  Indicates maximum supported bandwidth (T) for MBMS reception, see TS 36.213 [23]. clause 11.1. If the value is set to *implicitValue*, the corresponding value of T is calculated as specified in TS 36.213 [23], clause 11.1. If the value is set to *explicitValue*, the actual value of T = *explicitValue* \* 40 MHz. | | - |
| ***mbms-NonServingCell***  Indicates whether the UE in RRC\_CONNECTED supports MBMS reception via MRB on a frequency indicated in an *MBMSInterestIndication* message, where (according to *supportedBandCombination* and to network synchronization properties) a serving cell may be additionally configured. If this field is included, the UE shall also include the *mbms-SCell* field. | | Yes |
| ***mbms-ScalingFactor1dot25, mbms-ScalingFactor7dot5***  Indicates parameter A(1.25 / A(7.5, i.e., scaling factor for processing one unit of bandwidth corresponding to subcarrier spacing of 1.25 kHz / 7.5 kHz, with respect to one unit of bandwidth corresponding to subcarrier spacing of 15 kHz. See TS 36.213 [23], clause 11.1. This field is included only if *subcarrierSpacingMBMS-khz1dot25 / subcarrierSpacingMBMS-khz7dot5* is included. This field shall be included if *mbms-MaxBW* and *subcarrierSpacingMBMS-khz1dot25 / subcarrierSpacingMBMS-khz7dot5* are included. | | - |
| ***mbms-ScalingFactor0dot37, mbms-ScalingFactor2dot5***  Indicates parameter A(0.37 / A(2..5, i.e., scaling factor for processing one unit of bandwidth corresponding to subcarrier spacing of 0.37 kHz / 2.5 kHz, with respect to one unit of bandwidth corresponding to subcarrier spacing of 15 kHz. See TS 36.213 [23], clause 11.1. This field is included only if *fembmsMixedCell* or *fembmsDedicatedCell* is included. This field shall be included if *subcarrierSpacingMBMS-khz0dot37 / subcarrierSpacingMBMS-khz2dot5* is included for at least one E-UTRA band in *mbms-SupportedBandInfoList*. | | - |
| ***mbms-SCell***  Indicates whether the UE in RRC\_CONNECTED supports MBMS reception via MRB on a frequency indicated in an *MBMSInterestIndication* message, when an SCell is configured on that frequency (regardless of whether the SCell is activated or deactivated). | | Yes |
| ***mbms-SupportedBandInfoList***  One entry corresponding to each supported E-UTRA band listed in the same order as in *supportedBandListEUTRA*. This list is included only if *fembmsMixedCell* or *fembmsDedicatedCell* is included. If *mbms-SupportedBandInfoList-v1700* is included, the UE shall include the same number of entries, and listed in the same order, as in *mbms-SupportedBandInfoList-r16*. | | - |
| ***mcgRLF-RecoveryViaSCG***  Indicates whether the UE supports recovery from MCG RLF via split SRB1 (if supported) and via SRB3 (if supported). | | - |
| ***measGapPatterns-NRonly***  Indicates whether the UE supports gap patterns 2, 3 and 11 in LTE standalone when the frequencies to be measured within this measurement gap are all NR frequencies. | | No |
| ***measGapPatterns-NRonly-ENDC***  Indicates whether the UE supports gap patterns 2, 3 and 11 in (NG)EN-DC when the frequencies to be measured within this measurement gap are all NR frequencies. | | No |
| ***measurementEnhancements***  This field defines whether UE supports measurement enhancements in high speed scenario (350 km/h) as specified in TS 36.133 [16]. | | - |
| ***measurementEnhancements2***  This field defines whether UE supports measurement enhancements in high speed scenario (up to 500 km/h velocity) as specified in TS 36.133 [16]. | | - |
| ***measurementEnhancementsSCell***  This field defines whether UE supports SCell measurement enhancements in high speed scenario (350 km/h) as specified in TS 36.133 [16]. | | - |
| ***measGapPatterns***  Indicates whether the UE that supports NR supports gap patterns 4 to 11 in LTE standalone as specified in TS 36.133 [16], and for independent measurement gap configuration on FR1 and per-UE gap in (NG)EN-DC as specified in TS 38.133 [84]. The first/ leftmost bit covers pattern 4, and so on. Value 1 indicates that the UE supports the concerned gap pattern. | | - |
| ***mfbi-UTRA***  It indicates if the UE supports the signalling requirements of multiple radio frequency bands in a UTRA FDD cell, as defined in TS 25.307 [65]. | | - |
| ***MIMO-BeamformedCapabilityList***  A list of pairs of {k-Max, n-MaxList} values with the nth entry indicating the values that the UE supports for each CSI process in case n CSI processes would be configured. | | No |
| ***MIMO-CapabilityDL***  The number of supported layers for spatial multiplexing in DL. The field may be absent for category 0 and category 1 UE in which case the number of supported layers is 1. | | - |
| ***MIMO-CapabilityUL***  The number of supported layers for spatial multiplexing in UL. Absence of the field means that the number of supported layers is 1. | | - |
| ***MIMO-CA-ParametersPerBoBC***  A set of MIMO parameters provided per band of a band combination. In case a subfield is absent, the concerned capabilities are the same as indicated at the per UE level (i.e. by MIMO-UE-ParametersPerTM). | | - |
| ***mimo-CBSR-AdvancedCSI***  Indicates whether UE supports CBSR for advanced CSI reporting with and without amplitude restriction as defined in TS 36.213 [23], clause 7.2. | | Yes |
| ***min-Proc-TimelineSubslot***  Minimum processing timeline for subslot operation. The minimum processing timeline can belong to one of two sets of associated processing and maximum TA operation. The sets supported can be different for 1os CRS-based SPDCCH, 2os CRS-based SPDCCH and DMRS-based SPDCCH. The sequence applies to:  1. 1os CRS based SPDCCH  2. 2os CRS based SPDCCH  3. DMRS based SPDCCH | | - |
| ***modifiedMPR-Behavior***  Field encoded as a bit map, where at least one bit N is set to "1" if UE supports modified MPR/A-MPR behaviour N, see TS 36.101 [42]. All remaining bits of the field are set to "0". The leading / leftmost bit (bit 0) corresponds to modified MPR/A-MPR behaviour 0, the next bit corresponds to modified MPR/A-MPR behaviour 1 and so on.  Absence of this field means that UE does not support any modified MPR/A-MPR behaviour. | | - |
| ***mpdcch-InLteControlRegionCE-ModeA,*** ***mpdcch-InLteControlRegionCE-ModeB***  Indicates whether UE operating in CE mode A/B supports MPDCCH reception in LTE control channel region as specified in TS 36.211 [21]. | | Yes |
| ***mpsPriorityIndication***  Indicates whether the UE supports *mpsPriorityIndication* on release with redirect. | | - |
| ***multiACK-CSI-reporting***  Indicates whether the UE supports multi-cell HARQ ACK and periodic CSI reporting and SR on PUCCH format 3. | | Yes |
| ***multiBandInfoReport***  Indicates whether the UE supports the acquisition and reporting of multi band information for *reportCGI*. | | - |
| ***multiClusterPUSCH-WithinCC*** | | Yes |
| ***multiNS-Pmax***  Indicates whether the UE supports the mechanisms defined for cells broadcasting *NS-PmaxList*. | | - |
| ***multipleCellsMeasExtension***  Indicates whether the UE supports numberOfTriggeringCells in the report configuration. | | - |
| ***multipleTimingAdvance***  Indicates whether the UE supports multiple timing advances for each band combination listed in *supportedBandCombination*. If the band combination comprised of more than one band entry (i.e., inter-band or intra-band non-contiguous band combination), the field indicates that the same or different timing advances on different band entries are supported. If the band combination comprised of one band entry (i.e., intra-band contiguous band combination), the field indicates that the same or different timing advances across component carriers of the band entry are supported. It is mandatory for UEs to support 2 TAGs for inter frequency DAPS handover. | | - |
| ***multipleUplinkSPS***  Indicates whether the UE supports multiple uplink SPS and reporting SPS assistance information. A UE indicating *multipleUplinkSPS* shall also support V2X communication via Uu, as defined in TS 36.300 [9]. | | - |
| ***must-CapabilityPerBand***  Indicates that UE supports MUST, as specified in 36.212 [22], clause 5.3.3.1, on the band in the band combination. | | - |
| ***must-TM234-UpTo2Tx-r14***  Indicates that the UE supports MUST operation for TM2/3/4 using up to 2Tx. | | - |
| ***must-TM89-UpToOneInterferingLayer-r14***  Indicates that the UE supports MUST operation for TM8/9 with assistance information for up to 1 interfering layer. | | - |
| ***must-TM89-UpToThreeInterferingLayers-r14***  Indicates that the UE supports MUST operation for TM8/9 with assistance information for up to 3 interfering layers. | | - |
| ***must-TM10-UpToOneInterferingLayer-r14***  Indicates that the UE supports MUST operation for TM10 with assistance information for up to 1 interfering layer. | | - |
| ***must-TM10-UpToThreeInterferingLayers-r14***  Indicates that the UE supports MUST operation for TM10 with assistance information for up to 3 interfering layers. | | - |
| ***naics-Capability-List***  Indicates that UE supports NAICS, i.e. receiving assistance information from serving cell and using it to cancel or suppress interference of neighbouring cell(s) for at least one band combination. If not present, UE does not support NAICS for any band combination. The field *numberOfNAICS-CapableCC* indicates the number of component carriers where the NAICS processing is supported and the field *numberOfAggregatedPRB* indicates the maximum aggregated bandwidth across these of component carriers (expressed as a number of PRBs) with the restriction that NAICS is only supported over the full carrier bandwidth. The UE shall indicate the combination of {*numberOfNAICS-CapableCC, numberOfNAICS-CapableCC*} for every supported *numberOfNAICS-CapableCC*, e.g. if a UE supports {x CC, y PRBs} and {x-n CC, y-m PRBs} where n>=1 and m>=0, the UE shall indicate both.  - For *numberOfNAICS-CapableCC* = 1, UE signals one value for *numberOfAggregatedPRB* from the range {50, 75, 100};  - For *numberOfNAICS-CapableCC* = 2, UE signals one value for *numberOfAggregatedPRB* from the range {50, 75, 100, 125, 150, 175, 200};  - For *numberOfNAICS-CapableCC* = 3, UE signals one value for *numberOfAggregatedPRB* from the range {50, 75, 100, 125, 150, 175, 200, 225, 250, 275, 300};  - For *numberOfNAICS-CapableCC* = 4, UE signals one value for *numberOfAggregatedPRB* from the range {50, 100, 150, 200, 250, 300, 350, 400};  - For *numberOfNAICS-CapableCC* = 5, UE signals one value for *numberOfAggregatedPRB* from the range {50, 100, 150, 200, 250, 300, 350, 400, 450, 500}. | | No |
| ***ncsg***  Indicates whether the UE supports measurement NCSG Pattern Id 0, 1, 2 and 3, as specified in TS 36.133 [16]. If this field is included and the UE supports asynchronous DC, the UE shall support NCSG Pattern Id 0, 1, 2 and 3. If this field is included but the UE does not support asynchronous DC, only NCSG Pattern Id 0 and 1 shall be supported | | No |
| ***ng-EN-DC***  Indicates whether the UE supports NGEN-DC. | | - |
| ***n-MaxList (in MIMO-UE-ParametersPerTM)***  Indicates for a particular transmission mode the maximum number of NZP CSI RS ports supported within a CSI process applicable for band combinations for which the concerned capabilities are not signalled. For *k-Max* values exceeding 1, the UE shall include the field and signal *k-Max* minus 1 bits. The first bit indicates *n-Max2*, with value 0 indicating 8 and value 1 indicating 16. The second bit indicates *n-Max3*, with value 0 indicating 8 and value 1 indicating 16. The third bit indicates *n-Max4*, with value 0 indicating 8 and value 1 indicating 32. The fourth bit indicates *n-Max5*, with value 0 indicating 16 and value 1 indicating 32. The fifth bit indicates *n-Max6*, with value 0 indicating 16 and value 1 indicating 32. The sixt bit indicates *n-Max7*, with value 0 indicating 16 and value 1 indicating 32. The seventh bit indicates *n-Max8*, with value 0 indicating 16 and value 1 indicating 64. | | Yes |
| ***n-MaxList (in MIMO-CA-ParametersPerBoBCPerTM)***  If signalled, the field indicates for a particular transmission mode the maximum number of NZP CSI RS ports supported within a CSI process applicable for band the concerned combination. Further details are as indicated for *n-MaxList* in *MIMO-UE-ParametersPerTM*. | | No |
| ***NonContiguousUL-RA-WithinCC-List***  One entry corresponding to each supported E-UTRA band listed in the same order as in *supportedBandListEUTRA*. | | No |
| ***nonPrecoded (in MIMO-UE-ParametersPerTM)***  Indicates for a particular transmission mode the UE capabilities concerning non-precoded EBF/ FD-MIMO operation (class A) for band combinations for which the concerned capabilities are not signalled in *MIMO-CA-ParametersPerBoBCPerTM*, and the FD-MIMO processing capability condition as described in NOTE 8 is satisfied. | | Yes |
| ***nonPrecoded (in MIMO-CA-ParametersPerBoBCPerTM)***  If signalled, the field indicates for a particular transmission mode, the UE capabilities concerning non-precoded EBF/ FD-MIMO operation (class A) applicable for the concerned band combination. | | - |
| ***nonUniformGap***  Indicates whether the UE supports measurement non uniform Pattern Id 1, 2, 3 and 4 in LTE standalone as specified in TS 36.133 [16]. | | No |
| ***noResourceRestrictionForTTIBundling***  Indicate whether the UE supports TTI bundling operation without resource allocation restriction. | | No |
| ***nonCSG-SI-Reporting***  Indicates whether UE will report PLMN list from non-CSG cells. | | - |
| ***nr-AutonomousGaps-ENDC-FR1***  Indicates whether the UE supports, upon configuration of *useAutonomousGapsNR* by the network, acquisition of relevant information from a neighbouring NR cell by reading the SI of the neighbouring cell on FR1 using autonomous gaps and reporting the acquired information to the network when it is configured with (NG)EN-DC. | | Yes |
| ***nr-AutonomousGaps-ENDC-FR2***  Indicates whether the UE supports, upon configuration of *useAutonomousGapsNR* by the network, acquisition of relevant information from a neighbouring NR cell by reading the SI of the neighbouring cell on FR2 using autonomous gaps and reporting the acquired information to the network when it is configured with (NG)EN-DC. | | Yes |
| ***nr-AutonomousGaps-FR1***  Indicates whether the UE supports, upon configuration of *useAutonomousGapsNR* by the network, acquisition of relevant information from a neighbouring NR cell by reading the SI of the neighbouring cell on FR1 using autonomous gaps and reporting the acquired information to the network when it is not configured with (NG)EN-DC. | | Yes |
| ***nr-AutonomousGaps-FR2***  Indicates whether the UE supports, upon configuration of *useAutonomousGapsNR* by the network, acquisition of relevant information from a neighbouring NR cell by reading the SI of the neighbouring cell on FR2 using autonomous gaps and reporting the acquired information to the network when it is not configured with (NG)EN-DC. | | Yes |
| ***nr-HO-ToEN-DC***  Indicates whether the UE supports inter-RAT handover from NR to EN-DC while NR-DC or NE-DC is not configured. This field is mandatory present if EN-DC is supported. | | - |
| ***nr-IdleInactiveBeamMeasFR1***  Indicates whether the UE supports performing eNB-configured SSB-based beam level RRM measurements for configured NR FR1 carrier(s) in RRC\_IDLE and in RRC\_INACTIVE as specified in TS 36.306 [5], clause 4.3.6.46. | | No |
| ***nr-IdleInactiveBeamMeasFR2***  Indicates whether the UE supports performing eNB-configured SSB-based beam level RRM measurements for configured NR FR2 carrier(s) in RRC\_IDLE and in RRC\_INACTIVE as specified in TS 36.306 [5], clause 4.3.6.47. | | No |
| ***nr-IdleInactiveMeasFR1***  Indicates whether UE supports reporting measurements performed on NR FR1 carrier(s) during RRC\_IDLE and RRC\_INACTIVE. | | No |
| ***nr-IdleInactiveMeasFR2***  Indicates whether UE supports reporting measurements performed on NR FR2 carrier(s) during RRC\_IDLE and RRC\_INACTIVE. | | No |
| ***nr-RSSI-ChannelOccupancyReporting***  Indicates whether the UE supports performing measurements and reporting of RSSI and channel occupancy on the corresponding NR band. | | - |
| ***ntn-Connectivity-EPC***  Indicates whether the UE supports NTN access when connected to EPC. If the UE indicates this capability, the UE shall support all NTN essential features as specified in TS 36.306 [5]. | | - |
| ***ntn-PUR-TimerEnhancement***  Indicates whether the UE supports PUR timer enhancement for NTN, see TS 36.321 [6]. | | - |
| ***ntn-TA-report***  Indicates whether the UE supports time advance reporting in RRC\_CONNECTED, see TS 36.321 [6]. | | - |
| ***numberOfBlindDecodesUSS***  Indicates the maximum number of blind decodes in UE specific search space in one subframe for CCs configured with sTTI operation supported by the UE. The number of blind decodes supported by the UE is the field value X\*68. Field value ranges from 4 to 32. | | Yes |
| ***nzp-CSI-RS-AperiodicInfo***  Indicates whether the UE supports aperiodic NZP CSI-RS transmission for the indicated transmission mode. | | Yes |
| ***nzp-CSI-RS-PeriodicInfo***  Indicates whether the UE supports periodic NZP CSI-RS transmission for the indicated transmission mode. | | Yes |
| ***otdoa-UE-Assisted***  Indicates whether the UE supports UE-assisted OTDOA positioning, as specified in TS 36.355 [54]. | | Yes |
| ***outOfOrderDelivery***  Same as "*outOfOrderDelivery*" defined in TS 38.306 [87]. | | No |
| ***outOfSequenceGrantHandling***  Indicates whether the UE supports PUSCH transmissions with out of sequence UL grants as defined in TS 36.213 [23]. This field can be included only if uplinkLAA is included. | | - |
| ***overheatingInd***  Indicates whether the UE supports overheating assistance information. | | No |
| ***overheatingIndForSCG***  Indicates whether the UE supports the inclusion of NR SCG reduced configuration in the overheating assistance information. The UE which indicates support of *overheatingIndForSCG* shall also indicate support of *overheatingInd*. | | - |
| ***pdcch-CandidateReductions***  Indicates whether the UE supports PDCCH candidate reduction on UE specific search space as specified in TS 36.213 [23], clause 9.1.1. | | No |
| ***pdcp-Duplication***  Indicates whether the UE supports PDCP duplication. | | - |
| ***pdcp-SN-Extension***  Indicates whether the UE supports 15 bit length of PDCP sequence number. | | - |
| ***pdcp-SN-Extension-18bits***  Indicates whether the UE supports 18 bit length of PDCP sequence number. | | - |
| ***pdcp-TransferSplitUL***  Indicates whether the UE supports PDCP data transfer split in UL for the *drb-TypeSplit* as specified in TS 36.323 [8]. | | - |
| ***pdcp-VersionChangeWithoutHO***  Indicates whether, the UE supports changing the PDCP version of DRBs, from LTE PDCP to NR PDCP and vice versa, with and without handover. A UE supporting PDCP version change shall signal field *pdcp-Parameters-v1610*. When the field *pdcp-VersionChangeWithoutHO* is not included and *pdcp-Parameters-v1610* is included, it implies the UE supports PDCP version change only with handover. | | - |
| ***pdsch-CollisionHandling***  Indicates whether the UE supports PDSCH collision handling as specified in TS 36.213 [23]. | | No |
| ***pdsch-InLteControlRegionCE-ModeA, pdsch-InLteControlRegionCE-ModeB***  Indicates whether UE operating in CE mode A/B supports PDSCH reception in LTE control channel region as specified in TS 36.211 [21]. | | Yes |
| ***pdsch-MultiTB-CE-ModeA, pdsch-MultiTB-CE-ModeB***  Indicates whether the UE supports multiple TB scheduling in connected mode for PDSCH when operating in CE mode A/B, as specified in TS 36.211 [21] and TS 36.213 [23]. | | Yes |
| ***pdsch-RepSubframe***  Indicates whether the UE supports subframe PDSCH repetition. | | Yes |
| ***pdsch-RepSlot***  Indicates whether the UE supports slot PDSCH repetition. | | Yes |
| ***pdsch-RepSubslot***  Indicates whether the UE supports subslot PDSCH repetition. This field is only applicable for UEs supporting FDD. | | - |
| ***pdsch-SlotSubslotPDSCH-Decoding***  Indicates whether the UE supports decoding of PDSCH and slot-PDSCH/subslot-PDSCH assigned with C-RNTI/SPS C-RNTI in the same subframe for a given carrier. | | Yes |
| ***perServingCellMeasurementGap***  Indicates whether the UE supports per serving cell measurement gap indication, as specified in TS 36.133 [16]. | | - |
| ***phy-TDD-ReConfig-FDD-PCell***  Indicates whether the UE supports TDD UL/DL reconfiguration for TDD serving cell(s) via monitoring PDCCH with eIMTA-RNTI on a FDD PCell, and HARQ feedback according to UL and DL HARQ reference configurations. This bit can only be set to supported only if the UE supports FDD PCell and *phy-TDD-ReConfig-TDD-PCell* is set to supported. | | No |
| ***phy-TDD-ReConfig-TDD-PCell***  Indicates whether the UE supports TDD UL/DL reconfiguration for TDD serving cell(s) via monitoring PDCCH with eIMTA-RNTI on a TDD PCell, and HARQ feedback according to UL and DL HARQ reference configurations, and PUCCH format 3. | | Yes |
| ***pmch-Bandwidth-n40, pmch-Bandwidth-n35, pmch-Bandwidth-n30***  Indicates, for the E‑UTRA band corresponding to the entry in *mbms-SupportedBandInfoList-v1700*, whether the UE in RRC\_CONNECTED supports MBMS reception via MBSFN from MBMS-dedicated cells in an MBSFN area with PMCH bandwidth of 40/ 35/ 30 PRBs as described in TS 36.211 [21] and TS 36.213 [23]. | - | |
| ***pmi-Disabling*** | | Yes |
| ***powerClass-14dBm***  Indicates whether the UE supports power class 14 dBm when operating in CE mode A or B for all the bands that are supported by the UE, as specified in TS 36.101 [42]. | | - |
| ***powerPrefInd***  Indicates whether the UE supports power preference indication. | | No |
| ***powerUCI-SlotPUSCH, powerUCI-SubslotPUSCH***  Indicates whether the UE supports BPRE derivation based on the actual derived O\_CQI. The parameter *uplinkPower-CSIPayload* configures the UE to derive BPRE based on either the actual value of O\_CQI or the largest value of O\_CQI across all RI values. If the UE does not support the capability, the UE will derive BPRE based on the largest value of O\_CQI across all RI values. | | Yes |
| ***prach-Enhancements***  This field defines whether the UE supports random access preambles generated from restricted set type B in high speed scenoario as specified in TS 36.211 [21]. | | - |
| ***processingTimelineSet***  Indicates, for each SPDCCH configuration, support for a set of TA values. Each set consists of two different processing timelines and associated maximum TA. Set 1 indicates support for n+4 and n+6 and set 2 indicates support for n+6 and n+8, see TS 36.211 [21], clause 8.1, The minimum processing timeline to use, out of the two options for a given set is configured by parameter *proc-Timeline*. Support of Set 1 implicitly means support of Set 2. | | - |
| ***pucch-Format4***  Indicates whether the UE supports PUCCH format 4. | | Yes |
| ***pucch-Format5***  Indicates whether the UE supports PUCCH format 5. | | Yes |
| ***pucch-SCell***  Indicates whether the UE supports PUCCH on SCell. | | No |
| ***pur-CP-EPC-CE-ModeA, pur-CP-EPC-CE-ModeB, pur-CP-5GC-CE-ModeA, pur-CP-5GC-CE-ModeB***  Indicates whether UE operating in CE mode A/B supports CP transmission using PUR when connected to EPC/ 5GC. | | Yes |
| ***pur-CP-L1Ack***  Indicates whether UE supports L1 acknowledgement in response to CP transmission using PUR when connected to EPC/ 5GC. | | Yes |
| ***pur-FrequencyHopping***  Indicates whether UE supports frequency hopping for transmission using PUR. | | Yes |
| ***pur-PUSCH-NB-MaxTBS***  Indicates whether the UE supports 2984 bits max UL TBS in 1.4 MHz for transmission using PUR when operating in CE mode A, as specified in TS 36.212 [22] and TS 36.213 [23]. | | Yes |
| ***pur-RSRP-Validation***  Indicates whether UE supports serving cell RSRP for TA validation for transmission using PUR when connected to EPC/ 5GC. | | Yes |
| ***pur-SubPRB-CE-ModeA, pur-SubPRB-CE-ModeB***  Indicates whether UE supports subPRB resource allocation for PUSCH for transmission using PUR when operating in CE mode A/B. | | Yes |
| ***pur-UP-EPC-CE-ModeA, pur-UP-EPC-CE-ModeB, pur-UP-5GC-CE-ModeA, pur-UP-5GC-CE-ModeB***  Indicates whether UE operating in CE mode A/B supports UP transmission using PUR when connected to EPC/ 5GC. | | Yes |
| ***pusch-Enhancements***  Indicates whether the UE supports the PUSCH enhancement mode as specified in TS 36.211 [21] and TS 36.213 [23]. | | Yes |
| ***pusch-FeedbackMode***  Indicates whether the UE supports PUSCH feedback mode 3-2. | | No |
| ***pusch-MultiTB-CE-ModeA, pusch-MultiTB-CE-ModeB***  Indicates whether the UE supports multiple TB scheduling in connected mode for PUSCH when operating in CE mode A/B, as specified in TS 36.211 [21] and TS 36.213 [23]. | | Yes |
| ***pusch-SPS-MaxConfigSlot***  Indicates the max number of SPS configurations across all cells for slot PUSCH. | | Yes |
| ***pusch-SPS-MultiConfigSlot***  Indicates the number of multiple SPS configurations of slot PUSCH for each serving cell. | | Yes |
| ***pusch-SPS-MaxConfigSubframe***  Indicates the max number of SPS configurations across all cells for subframe PUSCH. | | Yes |
| ***pusch-SPS-MultiConfigSubframe***  Indicates the number of multiple SPS configurations of subframe PUSCH for each serving cell. | | Yes |
| ***pusch-SPS-MaxConfigSubslot***  Indicates the max number of SPS configurations across all cells for subslot PUSCH. | | - |
| ***pusch-SPS-MultiConfigSubslot***  Indicates the number of multiple SPS configurations of subslot PUSCH for each serving cell. This field is only applicable for UEs supporting FDD. | | - |
| ***pusch-SPS-SlotRepPCell***  Indicates whether the UE supports SPS repetition for slot PUSCH for PCell. | | Yes |
| ***pusch-SPS-SlotRepPSCell***  Indicates whether the UE supports SPS repetition for slot PUSCH for PSCell. | | Yes |
| ***pusch-SPS-SlotRepSCell***  Indicates whether the UE supports SPS repetition for slot PUSCH for serving cells other than SpCell. | | Yes |
| ***pusch-SPS-SubframeRepPCell***  Indicates whether the UE supports SPS repetition for subframe PUSCH for PCell. | | Yes |
| ***pusch-SPS-SubframeRepPSCell***  Indicates whether the UE supports SPS repetition for subframe PUSCH for PSCell. | | Yes |
| ***pusch-SPS-SubframeRepSCell***  Indicates whether the UE supports SPS repetition for subframe PUSCH for serving cells other than SpCell. | | Yes |
| ***pusch-SPS-SubslotRepPCell***  Indicates whether the UE supports SPS repetition for subslot PUSCH for PCell. This field is only applicable for UEs supporting FDD. | | - |
| ***pusch-SPS-SubslotRepPSCell***  Indicates whether the UE supports SPS repetition for subslot PUSCH for PSCell. This field is only applicable for UEs supporting FDD. | | - |
| ***pusch-SPS-SubslotRepSCell***  Indicates whether the UE supports SPS repetition for subslot PUSCH for serving cells other than SpCell. This field is only applicable for UEs supporting FDD. | | - |
| ***pusch-SRS-PowerControl-SubframeSet***  Indicates whether the UE supports subframe set dependent UL power control for PUSCH and SRS. This field is only applicable for UEs supporting TDD. | | Yes |
| ***qcl-CRI-BasedCSI-Reporting***  Indicates whether the UE supports CRI based CSI feedback for the FeCoMP feature as specified in TS 36.213 [23], clause 7.1.10. | | - |
| ***qcl-TypeC-Operation***  The UE uses this field to indicate the support of all of the following three features: QCL Type-C operation for FeCoMP, the capability to support separate PDSCH RE mapping for different PDSCH CWs in non-coherent joint transmission and the capability to support handling new DMRS port to MIMO layer mapping for the CWs, as specified in TS 36.213 [23], clause 7.1.10. | | - |
| ***qoe-MeasReport***  Indicates whether the UE supports QoE Measurement Collection for streaming services. | | - |
| ***qoe-MTSI-MeasReport***  Indicates whether the UE supports QoE Measurement Collection for MTSI services. | |  |
| ***rach-Less***  Indicates whether the UE supports RACH-less handover, and whether the UE which indicates *dc-Parameters* supports RACH-less SeNB change, as defined in TS 36.300 [9]. | | - |
| ***rach-Report***  Indicates whether the UE supports delivery of *rach-Report.* | | - |
| ***rai-Support***  Defines whether the UE supports release assistance indication (RAI) as specified in TS 36.321 [6] for BL UEs. | | No |
| ***rai-SupportEnh***  Indicates whether the UE supports 2-bit RAI when connected to EPC as specified in TS 36.321 [6]. | | - |
| ***rclwi***  Indicates whether the UE supports RCLWI, i.e. reception of *rclwi-Configuration*. The UE which supports RLCWI shall also indicate support of *interRAT-ParametersWLAN-r13*. The UE which supports RCLWI and *wlan-IW-RAN-Rules* shall also support applying WLAN identifiers received in *rclwi-Configuration* for the access network selection and traffic steering rules when in RRC\_IDLE. | | - |
| ***recommendedBitRate***  Indicates whether the UE supports the bit rate recommendation message from the eNB to the UE as specified in TS 36.321 [6], clause 6.1.3.13*.* | | No |
| ***recommendedBitRateMultiplier***  Indicates whether the UE supports the bit rate multiplier for recommended bit rate MAC CE as specified in TS 36.321 [6], clause 6.1.3.13. If this field is included, the UE shall also include the *recommendedBitRate* field. | | - |
| ***recommendedBitRateQuery***  Indicates whether the UE supports the bit rate recommendation query message from the UE to the eNB as specified in TS 36.321 [6], clause 6.1.3.13. If this field is included, the UE shall also include the *recommendedBitRate* field. | | No |
| ***reducedCP-Latency***  Indicates whether the UE supports reduced CP latency. | | Yes |
| ***reducedIntNonContComb***  Indicates whether the UE supports receiving *requestReducedIntNonContComb* that requests the UE to exclude supported intra-band non-contiguous CA band combinations other than included in capability signalling as specified in TS 36.306 [5], clause 4.3.5.21. | | - |
| ***reducedIntNonContCombRequested***  Indicates that the UE excluded supported intra-band non-contiguous CA band combinations other than included in capability signalling as specified in TS 36.306 [5,] clause 4.3.5.21. | | - |
| ***reflectiveQoS***  Indicates whether the UE supports AS reflective QoS. | | No |
| ***relWeightTwoLayers/ relWeightFourLayers/ relWeightEightLayers***  Indicates relative weight of processing FD-MIMO with 2/ 4/ 8 layers with respect to non-FD-MIMO with the same number of layers, see NOTE 8. Value v1 corresponds to relative weight of 1, value v1dot25 corresponds to relative weight of 1.25 and so on. This field can be included only if the UE supports the corresponding number of layers (i.e., 2/ 4/ 8 layers). | | - |
| ***reportCGI-NR-EN-DC***  Indicates whether the UE supports Inter-RAT report CGI procedure towards NR cell when it is configured with (NG)EN-DC. | | Yes |
| ***reportCGI-NR-NoEN-DC***  Indicates whether the UE supports Inter-RAT report CGI procedure towards NR cell when it is not configured with (NG)EN-DC. | | Yes |
| ***resumeWithMCG-SCellConfig***  Indicates whether the UE supports (re-)configuration of E-UTRA MCG SCells. | | - |
| ***resumeWithSCG-Config***  Indicates whether the UE supports (re-)configuration of an NR SCG. | | - |
| ***resumeWithStoredMCG-SCells***  Indicates whether the UE supports not deleting the stored E-UTRA MCG SCell configuration when initiating the resume procedure. | | - |
| ***resumeWithStoredSCG***  Indicates whether the UE supports not deleting the stored NR SCG configuration when initiating the resume procedure. | | - |
| ***srs-CapabilityPerBandPairList***  Indicates, for a particular pair of bands, the SRS carrier switching parameters when switching between the band pair to transmit SRS on a PUSCH-less SCell as specified in TS 36.212 [22] and TS 36.213 [23]. If included, the UE shall include a number of entries as indicated in the following, and listed in the same order, as in *bandParameterList* for the concerned band combination:  - For the first band, the UE shall include the same number of entries as in *bandParameterList* i.e. first entry corresponds to first band in *bandParameterList* and so on,  - For the second band, the UE shall include one entry less i.e. first entry corresponds to the second band in *bandParameterList* and so on  - And so on. | | - |
| ***requestedBands***  Indicates the frequency bands requested by E-UTRAN. | | - |
| ***requestedCCsDL, requestedCCsUL***  Indicates the maximum number of CCs requested by E-UTRAN. | | - |
| ***requestedDiffFallbackCombList***  Indicates the CA band combinations for which report of different UE capabilities is requested by E-UTRAN. | | - |
| ***rf-RetuningTimeDL***  Indicates the interruption time on DL reception within a band pair during the RF retuning for switching between the band pair to transmit SRS on a PUSCH-less SCell. n0 represents 0 OFDM symbols, n0dot5 represents 0.5 OFDM symbols, n1 represents 1 OFDM symbol and so on. This field is mandatory present if switching between the band pair is supported. | | - |
| ***rf-RetuningTimeUL***  Indicates the interruption time on UL transmission within a band pair during the RF retuning for switching between the band pair to transmit SRS on a PUSCH-less SCell. n0 represents 0 OFDM symbols, n0dot5 represents 0.5 OFDM symbols, n1 represents 1 OFDM symbol and so on. This field is mandatory present if switching between the band pair is supported. | | - |
| ***rlc-AM-Ooo-Delivery***  Indicates whether the UE supports out-of-order delivery from RLC to PDCP for RLC AM*.* | | - |
| ***rlc-UM-Ooo-Delivery***  Indicates whether the UE supports out-of-order delivery from RLC to PDCP for RLC UM*.* | | - |
| ***rlm-ReportSupport***  Indicates whether the UE supports RLM event and information reporting. | | - |
| ***rohc-ContextContinue***  Same as "*continueROHC-Context*" defined in TS 38.306 [87]. | | No |
| ***rohc-ContextMaxSessions***  Same as "*maxNumberROHC-ContextSessions*" defined in TS 38.306 [87]. | | No |
| ***rohc-Profiles***  Same as "*supportedROHC-Profiles*" defined in TS 38.306 [87]. | | No |
| ***rohc-ProfilesUL-Only***  Same as "*uplinkOnlyROHC-Profiles*" defined in TS 38.306 [87]. | | No |
| ***rsrqMeasWideband***  Indicates whether the UE can perform RSRQ measurements with wider bandwidth. | | Yes |
| ***rsrq-OnAllSymbols***  Indicates whether the UE can perform RSRQ measurement on all OFDM symbols and also support the extended RSRQ upper value range from -3dB to 2.5dB in measurement configuration and reporting as specified in TS 36.133 [16]. | | No |
| ***rs-SINR-Meas***  Indicates whether the UE can perform RS-SINR measurements in RRC\_CONNECTED as specified in TS 36.214 [48]. | | - |
| ***rssi-AndChannelOccupancyReporting***  Indicates whether the UE supports performing measurements and reporting of RSSI and channel occupancy. This field can be included only if *downlinkLAA* is included. | | - |
| ***sa-NR***  Indicates whether the UE supports standalone NR as specified in TS 38.331 [82]. | | No |
| ***scalingFactorTxSidelink, scalingFactorRxSidelink***  Indicates, for a particular band combination of EUTRA, the scaling facor, as defined in TS 38.306 [87], for the PC5 band combination(s) *v2x-SupportedBandCombinationListEUTRA-NR* on which the UE supports simultaneous transmission/reception of EUTRA and NR sidelink communication respectively, or simultaneous transmission or reception of EUTRA and joint V2X sidelink communication and NR sidelink communication respectively (as indicated by *v2x-SupportedTxBandCombListPerBC-v1630 /* *v2x-SupportedRxBandCombListPerBC-v1630*). The leading / leftmost value corresponds to the first band combination included in *v2x-SupportedBandCombinationListEUTRA-NR* which is indicated with value 1 by *v2x-SupportedTxBandCombListPerBC-v1630 /* *v2x-SupportedRxBandCombListPerBC-v1630*, the next value corresponds to the second band combination included in *v2x-SupportedBandCombinationListEUTRA-NR* which is indicated with value 1 by *v2x-SupportedTxBandCombListPerBC-v1630 /* *v2x-SupportedRxBandCombListPerBC-v1630* and so on. For each value of *ScalingFactorSidelink-r16*, value f0p4 indicates the scaling factor 0.4, f0p75 indicates 0.75, and so on. | | - |
| ***scptm-AsyncDC***  Indicates whether the UE in RRC\_CONNECTED supports MBMS reception via SC-MRB on a frequency indicated in an *MBMSInterestIndication* message, where (according to *supportedBandCombination*) the carriers that are or can be configured as serving cells in the MCG and the SCG are not synchronized. If this field is included, the UE shall also include *scptm-SCell* and *scptm-NonServingCell*. | | Yes |
| ***scptm-NonServingCell***  Indicates whether the UE in RRC\_CONNECTED supports MBMS reception via SC-MRB on a frequency indicated in an *MBMSInterestIndication* message, where (according to *supportedBandCombination* and to network synchronization properties) a serving cell may be additionally configured. If this field is included, the UE shall also include the *scptm-SCell* field. | | Yes |
| ***scptm-Parameters***  Presence of the field indicates that the UE supports SC-PTM reception as specified in TS 36.306 [5]. | | Yes |
| ***scptm-SCell***  Indicates whether the UE in RRC\_CONNECTED supports MBMS reception via SC-MRB on a frequency indicated in an *MBMSInterestIndication* message, when an SCell is configured on that frequency (regardless of whether the SCell is activated or deactivated). | | Yes |
| ***scptm-ParallelReception***  Indicates whether the UE in RRC\_CONNECTED supports parallel reception in the same subframe of DL-SCH transport blocks transmitted using C-RNTI/Semi-Persistent Scheduling C-RNTI and using SC-RNTI/G-RNTI as specified in TS 36.306 [5]. | | Yes |
| ***secondSlotStartingPosition***  Indicates whether the UE supports reception of subframes with second slot starting position as described in TS 36.211 [21] and TS 36.213 [23]. This field can be included only if *downlinkLAA* is included. | | - |
| ***semiOL***  Indicates whether the UE supports semi-open-loop transmission for the indicated transmission mode. | | Yes |
| ***semiStaticCFI***  Indicates whether the UE supports the semi-static configuration of CFI for subframe/slot/sub-slot operation. | | Yes |
| ***semiStaticCFI-Pattern***  Indicates whether the UE supports the semi-static configuration of CFI pattern for subframe/slot/sub-slot operation. This field is only applicable for UEs supporting TDD. | | - |
| ***sharedSpectrumMeasNR-EN-DC***  Indicates whether the UE supports performing measurements and reporting of RSSI and channel occupancy on each supported NR band in EN-DC. If included, the UE shall include the same number of entries, and listed in the same order as in *supportedBandListEN-DC-r15*. | | - |
| ***sharedSpectrumMeasNR-SA***  Indicates whether the UE supports performing measurements and reporting of RSSI and channel occupancy on each supported NR band in NR SA. If included, the UE shall include the same number of entries, and listed in the same order as in *supportedBandListNR-SA-r15*. | | - |
| ***shortCQI-ForSCellActivation***  Indicates whether the UE supports additional CQI reporting periodicity after SCell activation. | | Yes |
| ***shortMeasurementGap*** Indicates whether the UE supports shorter measurement gap length (i.e. *gp2* and *gp3*) in LTE standalone as specified in TS 36.133 [16], and for independent measurement gap configuration on FR1 and per-UE gap in (NG)EN-DC as specified in TS38.133 [84]. | | No |
| ***shortSPS-IntervalFDD***  Indicates whether the UE supports uplink SPS intervals shorter than 10 subframes in FDD mode. | | - |
| ***shortSPS-IntervalTDD***  Indicates whether the UE supports uplink SPS intervals shorter than 10 subframes in TDD mode. | | - |
| ***simultaneousPUCCH-PUSCH***  Indicates whether the UE supports simultaneous transmission of PUSCH/PUCCH and SlotOrSubslotPUSCH/SPUCCH (if supported). | | Yes |
| ***simultaneousRx-Tx***  Indicates whether the UE supports simultaneous reception and transmission on different bands for each band combination listed in *supportedBandCombination*. This field is only applicable for inter-band TDD band combinations. A UE indicating support of *simultaneousRx-Tx* and *dc-Support-r12* shall support different UL/DL configurations between PCell and PSCell. | | - |
| ***simultaneousTx-DifferentTx-Duration***  Indicates whether the UE supports simultaneous transmission of different transmission durations over different carriers. The different transmission durations can be of subframe, slot or subslot duration. | | - |
| ***skipFallbackCombinations***  Indicates whether UE supports receiving *requestSkipFallbackComb* that requests UE to exclude fallback band combinations from capability signalling. | | - |
| ***skipFallbackCombRequested***  Indicates whether *requestSkipFallbackComb* is requested by E-UTRAN. | | - |
| ***skipMonitoringDCI-Format0-1A***  Indicates whether UE supports blind decoding reduction on UE specific search space by not monitoring DCI Format 0 and 1A as specified in TS 36.213 [23], clause 9.1.1. | | No |
| ***skipSubframeProcessing***  This fields defines whether the UE supports aborting reception of PDSCH if the UE receives slot-PDSCH/subslot-PDSCH during an ongoing PDSCH reception and instead starts receiving the slot-PDSCH/subslot-PDSCH, as well as whether the UE supports aborting a PUSCH transmission if the UE gets a grant for a slot-PUSCH/ subslot-PUSCH transmission that overlaps with a grant received for a PUSCH transmission. The capability indicates the number of subframes that the UE may drop prior to the subframe in which it prioritizes the processing of slot/subslot PDSCH/PUSCH as described in TS 36.213 [23], clauses 7.1 and 8.0. Separate capability for UL and DL and per sTTI length in each direction*: skipProcessingDL-Slot, skipProcessingDL-Subslot, skipProcessingUL-Slot* and *skipProcessingUL-Subslot.* | | - |
| ***skipUplinkDynamic***  Indicates whether the UE supports skipping of UL transmission for an uplink grant indicated on PDCCH if no data is available for transmission as described in TS 36.321 [6]. | | - |
| ***skipUplinkSPS***  Indicates whether the UE supports skipping of UL transmission for a configured uplink grant if no data is available for transmission as described in TS 36.321 [6]. | | - |
| ***sl-64QAM-Rx***  Indicates whether the UE supports 64QAM for the reception of V2X sidelink communication. | | - |
| ***sl-64QAM-Tx***  Indicates whether the UE supports 64QAM for the transmission of V2X sidelink communication. | | - |
| ***sl-CongestionControl***  Indicates whether the UE supports Channel Busy Ratio measurement and reporting of Channel Busy Ratio measurement results to eNB for V2X sidelink communication. | | - |
| ***sl-LowT2min***  Indicates whether the UE supports 10ms as minimum value of T2 for resource selection procedure of V2X sidelink communication. | | - |
| ***sl-ParameterNR***  Includes the *SidelinkParametersNR* IE as specified in TS 38.331 [82]. The field includes the sidelink capability for NR-PC5, where *multipleSR-ConfigurationsSidelink* and *logicalChannelSR-DelayTimerSidelink* is not applicable. | | - |
| ***sl-RateMatchingTBSScaling***  Indicates whether the UE supports rate matching and TBS scalling for V2X sidelink communication. | | - |
| ***slotPDSCH-TxDiv-TM8***  Indicates whether the UE supports TX diversity transmission using ports 7 and 8 for TM8 for slot PDSCH. | | - |
| ***slotPDSCH-TxDiv-TM9and10***  Indicates whether the UE supports TX diversity transmission using ports 7 and 8 for TM9/10 for slot PDSCH. | | Yes |
| ***slotSymbolResourceResvDL-CE-ModeA, slotSymbolResourceResvDL-CE-ModeB, slotSymbolResourceResvUL-CE-ModeA, slotSymbolResourceResvUL-CE-ModeB***  Indicates whether the UE supports slot/symbol-level time-domain resource reservation in downlink/uplink when operating in CE mode A/B, as specified in TS 36.211 [21] and TS 36.213 [23]. | | Yes |
| ***slss-SupportedTxFreq***  Indicates whether the UE supports the SLSS transmission on single carrier or on multiple carriers in the case of sidelink carrier aggregation. | | - |
| ***slss-TxRx***  Indicates whether the UE supports SLSS/PSBCH transmission and reception in UE autonomous resource selection mode and eNB scheduled mode in a band for V2X sidelink communication. | | - |
| ***sl-TxDiversity***  Indicates whether the UE supports transmit diversity for V2X sidelink communication. See TS 36.101 [42]. | | - |
| ***sn-SizeLo***  Same as "*shortSN*" defined in TS 38.306 [87]. | | No |
| ***spatialBundling-HARQ-ACK***  Indicates whether UE supports HARQ-ACK spatial bundling on PUCCH or PUSCH as specified in TS 36.213 [23], clauses 7.3.1 and 7.3.2. | | No |
| ***spdcch-differentRS-types***  Indicates whether the UE supports monitoring of sPDCCH on RB sets with different RS types within a TTI. | | Yes |
| ***spdcch-Reuse***  Indicates whether the UE supports L1 based SPDCCH reuse. | | Yes |
| ***sps-CyclicShift***  Indicates whether the UE supports RRC configuration of cyclic shift for DMRS for UL SPS using 1ms TTI. | | Yes |
| ***sps-ServingCell***  Indicates whether the UE supports multiple UL/DL SPS configurations simultaneously active on different serving cells as specified in TS 36.321 [6]. | | - |
| ***sps-STTI***  Indicates whether the UE supports SPS in DL and/or UL for slot or subslot based PDSCH and PUSCH, respectively. | | Yes |
| ***srs-DCI7-TriggeringFS2***  Indicates whether the UE supports SRS triggerring via DCI format 7 for FS2. | | - |
| ***srs-Enhancements***  Indicates whether the UE supports SRS enhancements. | | Yes |
| ***srs-EnhancementsTDD***  Indicates whether the UE supports TDD specific SRS enhancements. | | Yes |
| ***srs-FlexibleTiming***  Indicates whether the UE supports configuration of *soundingRS-FlexibleTiming-r14* for the corresponding band pair. For a TDD-TDD band pair, UE shall include at least one of *srs-FlexibleTiming* and/or *srs-HARQ-ReferenceConfig* when *rf-RetuningTimeDL* or *rf-RetuningTimeUL* corresponding to the band pair is larger than 1 OFDM symbol. | | - |
| ***srs-HARQ-ReferenceConfig***  Indicates whether the UE supports configuration of *harq-ReferenceConfig-r14* for the corresponding band pair. For a TDD-TDD band pair, UE shall include at least one of *srs-FlexibleTiming* and/or *srs-HARQ-ReferenceConfig* when *rf-RetuningTimeDL* or *rf-RetuningTimeUL* corresponding to the band pair is larger than 1 OFDM symbol. | | - |
| ***srs-MaxSimultaneousCCs***  Indicates the maximum number of simultaneously configurable target CCs for SRS switching (i.e., CCs for which srs-SwitchFromServCellIndex is configured) supported by the UE. | | - |
| ***srs-UpPTS-6sym***  Indicates whether the UE supports up to 6-symbol SRS in UpPTS. | | - |
| ***srvcc-FromUTRA-FDD-ToGERAN***  Indicates whether UE supports SRVCC handover from UTRA FDD PS HS to GERAN CS. | | - |
| ***srvcc-FromUTRA-FDD-ToUTRA-FDD***  Indicates whether UE supports SRVCC handover from UTRA FDD PS HS to UTRA FDD CS. | | - |
| ***srvcc-FromUTRA-TDD128-ToGERAN***  Indicates whether UE supports SRVCC handover from UTRA TDD 1.28Mcps PS HS to GERAN CS. | | - |
| ***srvcc-FromUTRA-TDD128-ToUTRA-TDD128***  Indicates whether UE supports SRVCC handover from UTRA TDD 1.28Mcps PS HS to UTRA TDD 1.28Mcps CS. | | - |
| ***ss-CCH-InterfHandl***  Indicates whether the UE supports synchronisation signal and common channel interference handling. | | Yes |
| ***ss-SINR-Meas-NR-FR1, ss-SINR-Meas-NR-FR2***  Indicates whether the UE can perform NR SS-SINR measurement for a frequency range (i.e. FR1 or FR2) as specified in TS 38.215 [89]. | | - |
| ***ssp10-TDD-Only***  Indicates the UE supports special subframe configuration 10 when operating only in TDD carriers (i.e., not in TDD/FDD CA or TDD/FS3 CA). A UE including this field shall not include *tdd-SpecialSubframe-r14*. | | - |
| ***standaloneGNSS-Location***  Indicates whether the UE is equipped with a standalone GNSS receiver that may be used to provide detailed location information in RRC measurement report and logged measurements. | | - |
| ***sTTI-SPT-Supported***  Indicates whether the UE supports the features STTI and/or SPT. If the UE supports STTI and/or SPT features, the UE shall report the field *sTTI-SPT-Supported* set to *supported* in capability signalling, irrespective of whether *requestSTTI-SPT-Capability* field is present or not. | | - |
| ***sTTI-FD-MIMO-Coexistence***  Indicates whether the UE supports CSI feedback for more than 8 NZP CSI-RS ports on subframe based PUSCH in any serving cell and supporting STTI in any serving cell. | | - |
| ***sTTI-SupportedCombinations***  Indicates the different combinations of short TTI lengths, see field description for *dl-STTI-Length* and *ul-STTI-Length*, that the UE supports in a single PUCCH group or in two PUCCH groups. A short TTI length combination is reported for DL first followed by UL. In case of two PUCCH groups the support for the primary PUCCH group is indicated first. | | - |
| ***subcarrierPuncturingCE-ModeA, subcarrierPuncturingCE-ModeB***  Indicates whether the UE supports subcarrier puncturing in downlink when operating in CE mode A/B, as specified in TS 36.211 [21] and TS 36.213 [23]. | | Yes |
| ***subcarrierSpacingMBMS-khz7dot5, subcarrierSpacingMBMS-khz1dot25***  Indicates the supported subcarrier spacings for MBSFN subframes in addition to 15 kHz subcarrier spacing. *subcarrierSpacingMBMS-khz1dot25* and *subcarrierSpacingMBMS-khz7dot5* indicates that the UE supports 1.25 and 7.5 kHz respectively for MBSFN subframes as described in TS 36.211 [21], clause 6.12. This field is included only if *fembmsMixedCell* or *fembmsDedicatedCell* is included. | | - |
| ***subcarrierSpacingMBMS-khz2dot5, subcarrierSpacingMBMS-khz0dot37***  Presence of this field indicates the supported subcarrier spacings of 2.5kHz / 0.37kHz for MBSFN subframes in addition to 15 kHz subcarrier spacing when operating on the E-UTRA band given by the entry in *mbms-SupportedBandInfoList* as described in TS 36.211 [21], clause 6.12. | | - |
| ***subframeResourceResvDL-CE-ModeA, subframeResourceResvDL-CE-ModeB, subframeResourceResvUL-CE-ModeA, subframeResourceResvUL-CE-ModeB***  Indicates whether the UE supports Subframe-level time-domain resource reservation in downlink/uplink when operating in CE mode A/B, as specified in TS 36.211 [21] and TS 36.213 [23]. | | Yes |
| ***subslotPDSCH-TxDiv-TM9and10***  Indicates whether the UE supports TX diversity transmission using ports 7 and 8 for TM9/10 for subslot PDSCH. | | Yes |
| ***supportedBandCombination***  Includes the supported CA band combinations, if any, and may include all the supported non-CA bands. | | - |
| ***supportedBandCombinationAdd-r11***  Includes additional supported CA band combinations in case maximum number of CA band combinations of *supportedBandCombination* is exceeded. | | - |
| ***SupportedBandCombinationAdd-v11d0,*** ***SupportedBandCombinationAdd-v1250,*** ***SupportedBandCombinationAdd-v1270, SupportedBandCombinationAdd-v1320, SupportedBandCombinationAdd-v1380, SupportedBandCombinationAdd-v1390, SupportedBandCombinationAdd-v1430, SupportedBandCombinationAdd-v1450, SupportedBandCombinationAdd-v1470, SupportedBandCombinationAdd-v14b0, SupportedBandCombinationAdd-v1530, SupportedBandCombinationAdd-v1630***  If included, the UE shall include the same number of entries, and listed in the same order, as in *SupportedBandCombinationAdd-r11*. | | - |
| ***SupportedBandCombinationAdd-v1610***  If included, the UE shall include the same number of entries, and listed in the same order, as in *SupportedBandCombinationAdd-r11*. If absent, network assumes gap is required when measurement is performed on any NR bands while UE is served by cell(s) belongs to an E-UTRA CA band combinations listed in *SupportedBandCombinationAdd-r11* except for the FR2 inter-RAT measurement which depends on the support of *independentGapConfig.* | | - |
| ***SupportedBandCombinationExt, SupportedBandCombination-v1090, SupportedBandCombination-v10i0, SupportedBandCombination-v1130, SupportedBandCombination-v1250, SupportedBandCombination-v1270, SupportedBandCombination-v1320, SupportedBandCombination-v1380, SupportedBandCombination-v1390, SupportedBandCombination-v1430, SupportedBandCombination-v1450, SupportedBandCombination-v1470, SupportedBandCombination-v14b0, SupportedBandCombination-v1530, SupportedBandCombination-v1630***  If included, the UE shall include the same number of entries, and listed in the same order, as in *supportedBandCombination-r10*. | | - |
| ***SupportedBandCombination-v1610***  If included, the UE shall include the same number of entries, and listed in the same order, as in *supportedBandCombination-r10*. If absent, network assumes gap is required when measurement is performed on any NR bands while UE is served by cell(s) belongs to an E-UTRA CA band combinations listed in *supportedBandCombination-r10* except for the FR2 inter-RAT measurement which depends on the support of *independentGapConfig.* | | - |
| ***supportedBandCombinationReduced***  Includes the supported CA band combinations, and may include the fallback CA combinations specified in TS 36.101 [42], clause 4.3A. This field also indicates whether the UE supports reception of *requestReducedFormat*. | | - |
| ***SupportedBandCombinationReduced-v1320, SupportedBandCombinationReduced-v1380, SupportedBandCombinationReduced-v1390, SupportedBandCombinationReduced-v1430, SupportedBandCombinationReduced-v1450, SupportedBandCombinationReduced-v1470, SupportedBandCombinationReduced-v14b0, SupportedBandCombinationReduced-v1530, SupportedBandCombinationReduced-v1630***  If included, the UE shall include the same number of entries, and listed in the same order, as in *supportedBandCombinationReduced-r13*. | | - |
| ***SupportedBandCombinationReduced-v1610***  If included, the UE shall include the same number of entries, and listed in the same order, as in *supportedBandCombinationReduced-r13*. If absent, network assumes gap is required when measurement is performed on any NR bands while UE is served by cell(s) belongs to an E-UTRA CA band combinations listed in *supportedBandCombinationReduced-r13* except for the FR2 inter-RAT measurement which depends on the support of *independentGapConfig.* | | - |
| ***SupportedBandGERAN***  GERAN band as defined in TS 45.005 [20]. | | No |
| ***SupportedBandList1XRTT***  One entry corresponding to each supported CDMA2000 1xRTT band class. | | - |
| ***SupportedBandListEUTRA***  Includes the supported E-UTRA bands. This field shall include all bands which are indicated in *BandCombinationParameters*. | | - |
| ***SupportedBandListEUTRA-v9e0, SupportedBandListEUTRA-v1250, SupportedBandListEUTRA-v1310, SupportedBandListEUTRA-v1320***  If included, the UE shall include the same number of entries, and listed in the same order, as in *supportedBandListEUTRA* (i.e. without suffix). | | - |
| ***SupportedBandListGERAN*** | | No |
| ***SupportedBandListHRPD***  One entry corresponding to each supported CDMA2000 HRPD band class. | | - |
| ***SupportedBandListNR-SA***  Includes the NR bands supported by the UE in NR-SA (for handover and redirection). The field is included in case the UE supports NR SA as specified in TS 38.331 [32] and not otherwise. The presence of this field also indicates that the UE can perform both NR SS-RSRP and SS-RSRQ measurement in the included NR band(s) as specified in TS 38.215 [89]. | | No |
| ***supportedBandListEN-DC***  Includes the NR bands supported by the UE in (NG)EN-DC. The field is included in case the parameter *en-DC* or *ng-EN-DC* is present and set to *supported* and not otherwise. The presence of this field also indicates that the UE can perform both NR SS-RSRP and SS-RSRQ measurement in the included NR band(s) as specified in TS 38.215 [89]. | | - |
| ***supportedBandListWLAN***  Indicates the supported WLAN bands by the UE. | | - |
| ***SupportedBandUTRA-FDD***  UTRA band as defined in TS 25.101 [17]. | | - |
| ***SupportedBandUTRA-TDD128***  UTRA band as defined in TS 25.102 [18]. | | - |
| ***SupportedBandUTRA-TDD384***  UTRA band as defined in TS 25.102 [18]. | | - |
| ***SupportedBandUTRA-TDD768***  UTRA band as defined in TS 25.102 [18]. | | - |
| ***supportedBandwidthCombinationSet***  The *supportedBandwidthCombinationSet* indicated for a band combination is applicable to all bandwidth classes indicated by the UE in this band combination.  Field encoded as a bit map, where bit N is set to "1" if UE support Bandwidth Combination Set N for this band combination, see 36.101 [42]. The leading / leftmost bit (bit 0) corresponds to the Bandwidth Combination Set 0, the next bit corresponds to the Bandwidth Combination Set 1 and so on. The UE shall neither include the field for a non-CA band combination, nor for a CA band combination for which the UE only supports Bandwidth Combination Set 0. | | - |
| ***supportedCellGrouping***  This field indicates for which mapping of serving cells to cell groups (i.e. MCG or SCG) the UE supports asynchronous DC. This field is only present for a band combination with more than two but less than six band entries where the UE supports asynchronous DC. If this field is not present but asynchronous operation is supported, the UE supports all possible mappings of serving cells to cell groups for the band combination. The bitmap size is selected based on the number of entries in the combinations, i.e., in case of three entries, the bitmap corresponding to *threeEntries* is selected and so on.  A bit in the bit string set to 1 indicates that the UE supports asynchronous DC for the cell grouping option represented by the concerned bit position. Each bit position represents a different cell grouping option, as illustrated by a table, see NOTE 5. A cell grouping option is represented by a number of bits, each representing a particular band entry in the band combination with the left-most bit referring to the band listed first in the band combination, etc. Value 0 indicates that the carriers of the corresponding band entry are mapped to a first cell group, while value 1 indicates that the carriers of the corresponding band entry are mapped to a second cell group.  It is noted that the mapping table does not include entries with all bits set to the same value (0 or 1) as this does not represent a DC scenario (i.e. indicating that the UE supports that all carriers of the corresponding band entry are in one cell group). | | - |
| ***supportedCSI-Proc, sTTI-SupportedCSI-Proc***  Indicates the maximum number of CSI processes supported on a component carrier within a band. Value n1 corresponds to 1 CSI process, value n3 corresponds to 3 CSI processes, and value n4 corresponds to 4 CSI processes. If this field is included, the UE shall include the same number of entries listed in the same order as in *BandParameters/STTI-SPT-BandParameters*. If the UE supports at least 1 CSI process on any component carrier, then the UE shall include this field in all bands in all band combinations. | | - |
| ***supportedCSI-Proc (in FeatureSetDL-PerCC)***  In MR-DC, indicates the number of CSI processes for the component carrier in the corresponding bandwidth class. If the UE supports at least 1 CSI process, then the UE shall include this field. | | - |
| ***supportedMIMO-CapabilityDL-MRDC (in FeatureSetDL-PerCC)***  In MR-DC, indicates the maximum number of supported layers in TM9/10 for the component carrier in the corresponding bandwidth class. | | - |
| ***supportedNAICS-2CRS-AP***  If included, the UE supports NAICS for the band combination. The UE shall include a bitmap of the same length, and in the same order, as in *naics-Capability-List,* to indicate 2 CRS AP NAICS capability of the band combination. The first/ leftmost bit points to the first entry of *naics-Capability-List*, the second bit points to the second entry of *naics-Capability-List*, and so on.  For band combinations with a single component carrier, UE is only allowed to indicate {*numberOfNAICS-CapableCC*, *numberOfAggregatedPRB*} = {1, 100} if NAICS is supported. | | - |
| ***supportedOperatorDic***  Indicates whether the UE supports operator defined dictionary. If UE supports operator defined dictionary, the UE shall report *versionOfDictionary* and *associatedPLMN-ID* of the stored operator defined dictionary. This parameter is not required to be present if the UE is in VPLMN. In this release of the specification, UE can only support one operator defined dictionary. The *associatedPLMN-ID* is only associated to the operator defined dictionary which has no relationship with UE's HPLMN ID. | | - |
| ***supportRohcContextContinue***  Indicates whether the UE supports ROHC context continuation operation where the UE does not reset the current ROHC context upon handover. | | - |
| ***supportedROHC-Profiles***  Indicates the ROHC profiles that UE supports in both uplink and downlink. | | - |
| ***supportedUplinkOnlyROHC-Profiles***  Indicates the ROHC profiles that UE supports in uplink and not in downlink, see TS 36.323 [8] | | - |
| ***supportedStandardDic***  Indicates whether the UE supports standard dictionary for SIP and SDP as specified in TS 36.323 [8]. | | - |
| ***supportedUDC***  Indicates whether the UE supports UL data compression, see TS 36.323 [8]. | | - |
| ***tdd-SpecialSubframe***  Indicates whether the UE supports TDD special subframe defined in TS 36.211 [21]. A UE shall indicate *tdd-SpecialSubframe-r11* if it supports the TDD special subframes ssp7 and ssp9. A UE shall indicate *tdd-SpecialSubframe-r14* if it supports the TDD special subframe ssp10, except when *ssp10-TDD-Only-r14* is included. | | Yes |
| ***tdd-FDD-CA-PCellDuplex***  The presence of this field indicates that the UE supports TDD/FDD CA in any supported band combination including at least one FDD band with *bandParametersUL* and at least one TDD band with *bandParametersUL*. The first bit is set to "1" if UE supports the TDD PCell. The second bit is set to "1" if UE supports FDD PCell. This field is included only if the UE supports band combination including at least one FDD band with *bandParametersUL* and at least one TDD band with *bandParametersUL*. If this field is included, the UE shall set at least one of the bits as "1". If this field is included with DC, then it is applicable within a CG, and the presence of this field indicates the capability of the UE to support TDD/FDD CA with at least one FDD band and at least one TDD band in the same CG, with the value indicating the support for TDD/FDD PCell (PSCell). | | No |
| ***tdd-TTI-Bundling***  The presence of this field indicates whether the UE supporting TDD special subframe configuration 10 also supports TTI bundling for TDD configuration 2 and 3 when PUSCH transimission in UpPTS is configured, see TS 36.213 [23], clause 8.0. If this field is present, the *tdd-SpecialSubframe-r14* or *ssp10-TDD-Only-r14* shall be present. | | Yes |
| ***timeReferenceProvision***  Indicates whether the UE supports provision of time reference in *DLInformationTransfer* message. | | - |
| ***timeSeparationSlot2, timeSeparationSlot4***  Indicates whether the UE supports time staggering length of 2 slots (MBSFN reference signal pattern type 2) / 4 slots (MBSFN reference signal pattern type 1) for MBSFN-RS associated with PMCH with subcarrier spacing of 0.37 kHz for MBSFN subframes when operating on the E‑UTRA band given by the entry in *mbms-SupportedBandInfoList* as described in TS 36.211 [21], clause 6.10.2.2.4. | | - |
| ***timerT312***  Indicates whether the UE supports T312. | | No |
| ***tm5-FDD***  Indicates whether the UE supports the PDSCH transmission mode 5 in FDD. | | - |
| ***tm5-TDD***  Indicates whether the UE supports the PDSCH transmission mode 5 in TDD. | | - |
| ***tm6-CE-ModeA***  Indicates whether the UE supports tm6 operation in CE mode A, see TS 36.213 [23], clause 7.2.3. This field can be included only if *ce-ModeA* is included. | | Yes |
| ***tm8-slotPDSCH***  Indicates whether the UE supports configuration and decoding of TM8 for slot PDSCH in TDD. | | - |
| ***tm9-CE-ModeA***  Indicates whether the UE supports tm9 operation in CE mode A, see TS 36.213 [23], clause 7.2.3. This field can be included only if *ce-ModeA* is included. | | Yes |
| ***tm9-CE-ModeB***  Indicates whether the UE supports tm9 operation in CE mode B, see TS 36.213 [23], clause 7.2.3. This field can be included only if *ce-ModeB* is included. | | Yes |
| ***tm9-LAA***  Indicates whether the UE supports tm9 operation on LAA cell(s). This field can be included only if *downlinkLAA* is included. | | - |
| ***tm9-slotSubslot***  Indicates whether the UE supports configuration and decoding of TM9 for slot and/or subslot PDSCH for non-MBSFN. | | Yes |
| ***tm9-slotSubslotMBSFN***  Indicates whether the UE supports configuration and decoding of TM9 for slot and/or subslot PDSCH for MBSFN. | | Yes |
| ***tm9-With-8Tx-FDD***  Indicates whether the UE supports PDSCH transmission mode 9 with 8 CSI reference signal ports for FDD when not operating in CE mode. | | Yes |
| ***tm10-LAA***  Indicates whether the UE supports tm10 operation on LAA cell(s). This field can be included only if *downlinkLAA* is included. | | - |
| ***tm10-slotSubslot***  Indicates whether the UE supports configuration and decoding of TM10 for slot and/or subslot PDSCH for non-MBSFN. | | Yes |
| ***tm10-slotSubslotMBSFN***  Indicates whether the UE supports configuration and decoding of TM10 for slot and/or subslot PDSCH for MBSFN. | | Yes |
| ***totalWeightedLayers***  Indicates total number of weighted layers the UE can process for FD-MIMO. See NOTE 8. | | - |
| ***twoAntennaPortsForPUCCH*** | | No |
| ***twoStepSchedulingTimingInfo***  Presence of this field indicates that the UE supports uplink scheduling using PUSCH trigger A and PUSCH trigger B (as defined in TS 36.213 [23]).  This field also indicates the timing between the PUSCH trigger B and the earliest time the UE supports performing the associated UL transmission. For reception of PUSCH trigger B in subframe N, value *nPlus1* indicates that the UE supports performing the UL transmission in subframe N+1, value *nPlus2* indicates that the UE supports performing the UL transmission in subframe N+2, and so on.  This field can be included only if *uplinkLAA* is included. | | - |
| ***txAntennaSwitchDL, txAntennaSwitchUL***  The presence of *txAntennaSwitchUL* indicates the UE supports transmit antenna selection for this UL band in the band combination as described in TS 36.213 [23], clauses 8.2 and 8.7.  The field *txAntennaSwitchDL* indicates the entry number of the first-listed band with UL in the band combination that affects this DL. The field *txAntennaSwitchUL* indicates the entry number of the first-listed band with UL in the band combination that switches together with this UL. Value 1 means first entry, value 2 means second entry and so on. All DL and UL that switch together indicate the same entry number.  For the case of carrier switching, the antenna switching capability for the target carrier configuration is indicated as follows:  For UE configured with a set of component carriers belonging to a band combination Cbaseline = {b1(1),…,bx(1),…,by(0),…}, where "1/0" denotes whether the corresponding band has an uplink, if a component carrier in bx is to be switched to a component carrier in by (according to *srs-SwitchFromServCellIndex*), the antenna switching capability is derived based on band combination Ctarget = {b1(1),…,bx(0),…,by(1),…}. | | - |
| ***txDiv-PUCCH1b-ChSelect***  Indicates whether the UE supports transmit diversity for PUCCH format 1b with channel selection. | | Yes |
| ***txDiv-SPUCCH***  Indicates whether the UE supports Tx diversity on SPUCCH format 1/1a/1b/3. | | Yes |
| ***tx-Sidelink, rx-Sidelink***  Indicates that the UE supports sidelink transmission/reception on the band in the band combination.  For NR sidelink transmission, *tx-Sidelink* is only applicable if the UE supports at least one of *sl-TransmissionMode1-r16* and *sl-TransmissionMode2-r16* on the band as specified in TS 38.331 [82].  For NR sidelink reception, *rx-Sidelink* is only applicable if the UE supports *sl-Reception-r16* on the band as specified in TS 38.331 [82]. | | - |
| ***uci-PUSCH-Ext***  Indicates whether the UE supports an extension of UCI delivering more than 22 HARQ-ACK bits on PUSCH as specified in TS 36.212 [22], clause 5.2.2.6 and TS 36.213 [23], clause 8.6.3. | | No |
| ***ue-AutonomousWithFullSensing***  Indicates whether the UE supports transmitting PSCCH/PSSCH using UE autonomous resource selection mode with full sensing (i.e., continuous channel monitoring) for V2X sidelink communication and the UE supports maximum transmit power associated with Power class 3 V2X UE, see TS 36.101 [42]. | | - |
| ***ue-AutonomousWithPartialSensing***  Indicates whether the UE supports transmitting PSCCH/PSSCH using UE autonomous resource selection mode with partial sensing (i.e., channel monitoring in a limited set of subframes) for V2X sidelink communication and the UE supports maximum transmit power associated with Power class 3 V2X UE, see TS 36.101 [42]. | | - |
| ***ue-Category***  UE category as defined in TS 36.306 [5]. Set to values 1 to 12 in this version of the specification. | | - |
| ***ue-CategoryDL***  UE DL category as defined in TS 36.306 [5]. Value *n17* corresponds to UE category 17, value *m1* corresponds to UE category M1, value *oneBis* corresponds to UE category 1bis, value m2 corresponds to UE category M2. For ASN.1 compatibility, a UE indicating DL category 0, m1 or m2 shall also indicate any of the categories (1..5) in *ue-Category* (without suffix), which is ignored by the eNB, a UE indicating UE category oneBis shall also indicate UE category 1 in *ue-Category* (without suffix), and a UE indicating UE category m2 shall also indicate UE category m1. The field *ue-CategoryDL* is set to values 0, m1, oneBis, m2, 4, 6, 7, 9 to 16, n17, 18, 19, 20, 21, 22, 23, 24, 25, 26 in this version of the specification. | | - |
| ***ue-CategorySL-C-TX***  UE SL category for V2X transmission as defined in TS 36.306 [5]. Set to values 1 to 5 in this version of the specification. | | - |
| ***ue-CategorySL-C-RX***  UE SL category for V2X reception as defined in TS 36.306 [5]. Set to values 1 to 4 in this version of the specification. | | - |
| ***ue-CategoryUL***  UE UL category as defined in TS 36.306 [5]. Value *n14* corresponds to UE category 14, value *n16* corresponds to UE category 16 and so on. Value *m1* corresponds to UE category M1, value *m2* corresponds to UE category M2, value *oneBis* corresponds to UE category 1bis. The field *ue-CategoryUL* is set to values m1, m2, 0, oneBis, 3, 5, 7, 8, 13, n14, 15, n16 to n21 or 22 to 26 in this version of the specification. | | - |
| ***ue-CA-PowerClass-N***  Indicates whether the UE supports UE power class N in the E-UTRA band combination, see TS 36.101 [42] and TS 36.307 [78]. If *ue-CA-PowerClass-N* is not included, UE supports the default UE power class in the E-UTRA band combination, see TS 36.101 [42]. | | - |
| ***ue-CE-NeedULGaps***  Indicates whether the UE needs uplink gaps during continuous uplink transmission in FDD as specified in TS 36.211 [21] and TS 36.306 [5]. | | - |
| ***ue-PowerClass-N, ue-PowerClass-5***  Indicates whether the UE supports UE power class 1, 2, 4 or 5 in the E-UTRA band, see TS 36.101 [42] and TS 36.307 [79]. UE includes either *ue-PowerClass-N* or *ue-PowerClass-5*. If neither *ue-PowerClass-N* nor *ue-PowerClass-5* is included, UE supports the default UE power class in the E-UTRA band, see TS 36.101 [42]. | | - |
| ***ue-Rx-TxTimeDiffMeasurements***  Indicates whether the UE supports Rx - Tx time difference measurements. | | No |
| ***ue-SpecificRefSigsSupported*** | | No |
| ***ue-SSTD-Meas***  Indicates whether the UE supports SSTD measurements between the PCell and the PSCell as specified in TS 36.214 [48] and TS 36.133 [16]. | | - |
| ***ue-TxAntennaSelectionSupported***  Except for the supported band combinations for which *bandParameterList-v1380* is included, TRUE indicates that the UE is capable of supporting UE transmit antenna selection such that all the supported bands in the band combination are affected by transmit antenna switching, as described in TS 36.213 [23], clause 8.7. E-UTRAN ignores this field for band combinations for which *bandParameterList-v1380* is included. | | Yes |
| ***ue-TxAntennaSelection-SRS-1T4R***  Indicates whether the UE supports selecting one antenna among four antennas to transmit SRS for the corresponding band of the band combination as described in TS 36.213 [23]. | | - |
| ***ue-TxAntennaSelection-SRS-2T4R-2Pairs***  Indicates whether the UE supports selecting one antenna pair between two antenna pairs to transmit SRS simultaneously for the corresponding band of the band combination as described in TS 36.213 [23]. | | - |
| ***ue-TxAntennaSelection-SRS-2T4R-3Pairs***  Indicates whether the UE supports selecting one antenna pair among three antenna pairs to transmit SRS simultaneously for the corresponding band of the band combination as described in TS 36.213 [23]. | | - |
| ***ul-64QAM***  Indicates whether the UE supports 64QAM in UL on the band. This field is only present when the field ue*-CategoryUL* indicates UL UE category that supports UL 64QAM, see TS 36.306 [5], Table 4.1A-2. If the field is present for one band, the field shall be present for all bands including downlink only bands. | | - |
| ***ul-256QAM***  Indicates whether the UE supports 256QAM in UL on the band in the band combination. This field is only present when the field ue*-CategoryUL* indicates UL UE category that supports 256QAM in UL, see TS 36.306 [5], Table 4.1A-2. The UE includes this field only if the field *ul-256QAM-perCC-InfoLis*t is not included. | | - |
| ***ul-256QAM (in FeatureSetUL-PerCC)***  Indicates whether the UE supports 256QAM in UL for MR-DC within the indicated feature set. This field is only present when the field ue-CategoryUL indicates UL UE category that supports 256QAM in UL, see TS 36.306 [5], Table 4.1A-2. | | - |
| ***ul-256QAM-perCC-InfoList***  Indicates, per serving carrier of which the corresponding bandwidth class includes multiple serving carriers (i.e. bandwidth class B, C, D and so on), whether the UE supports 256QAM in the band combination. The number of entries is equal to the number of component carriers in the corresponding bandwidth class. The UE shall support the setting indicated in each entry of the list regardless of the order of entries in the list. This field is only present when the field *ue-CategoryUL* indicates UL UE category that supports 256QAM in UL, see TS 36.306 [5], Table 4.1A-2. The UE includes this field only if the field *ul-256QAM* is not included. | | - |
| ***ul-256QAM-Slot***  Indicates whether the UE supports 256QAM in UL for slot TTI operation on the band. | | - |
| ***ul-256QAM-Subslot***  Indicates whether the UE supports 256QAM in UL for subslot TTI operation on the band. | | - |
| ***ul-AsyncHarqSharingDiff-TTI-Lengths***  Indicates whether the UE supports UL asynchronous HARQ sharing between different TTI lengths for an UL serving cell. | | Yes |
| ***ul-CoMP***  Indicates whether the UE supports UL Coordinated Multi-Point operation. | | No |
| ***ul-dmrs-Enhancements***  Indicates whether the UE supports UL DMRS enhancements as defined in TS 36.211 [21], clause 6.10.3A. | | Yes |
| ***ul-PDCP-AvgDelay***  Indicates whether the UE supports UL PDCP Packet Average Delay measurement (as specified in TS 38.314 [103]) and reporting in RRC\_CONNECTED. | | - |
| ***ul-PDCP-Delay***  Indicates whether the UE supports UL PDCP Packet Delay per QCI measurement as specified in TS 36.314 [71]. | | - |
| ***ul-powerControlEnhancements***  Indicates whether UE supports UplinkPowerControlDedicated. | | Yes |
| ***uplinkLAA***  Presence of the field indicates that the UE supports uplink LAA operation. | | - |
| ***uss-BlindDecodingAdjustment***  Indicates whether the UEsupports blind decoding adjustment on UE specific search space as defined in TS 36.213 [22]. This field can be included only if uplinkLAA is included. | | - |
| ***uss-BlindDecodingReduction***  Indicates whether the UE supports blind decoding reduction on UE specific search space by not monitoring DCI format 0A/0B/4A/4B as defined in TS 36.213 [22]. This field can be included only if uplinkLAA is included. | | - |
| ***unicastFrequencyHopping***  Indicates whether the UE supports frequency hopping for unicast MPDCCH/PDSCH (configured by *mpdcch-pdsch-HoppingConfig*) and unicast PUSCH (configured by *pusch-HoppingConfig*). | | - |
| ***unicast-fembmsMixedSCell***  Indicates whether the UE supports unicast reception from FeMBMS/Unicast mixed cell. This field is included only if UE supports carrier aggregation. | | No |
| ***utra-GERAN-CGI-Reporting-ENDC***  Indicates whether the UE supports Inter-RAT report CGI procedure towards GERAN/UTRA cell when it is configured with (NG)EN-DC wherein either MN and SN have different DRX cycles, or on-duration configured by MN does not contain on-duration configured by SN if their DRX cycles are same. | | Yes |
| ***utran-ProximityIndication***  Indicates whether the UE supports proximity indication for UTRAN CSG member cells. | | - |
| ***utran-SI-AcquisitionForHO***  Indicates whether the UE supports, upon configuration of si-RequestForHO by the network, acquisition and reporting of relevant information using autonomous gaps by reading the SI from a neighbouring UMTS cell. | | Yes |
| ***v2x-BandParametersNR***  Includes the NR *BandParametersSidelink-r16* IE as specified in TS 38.331 [82]. The field includes the per-band sidelink capability for NR-PC5. | | - |
| ***v2x-BandwidthClassTxSL, v2x-BandwidthClassRxSL***  The bandwidth class for V2X sidelink transmission and reception supported by the UE as defined in TS 36.101 [42], Table 5.6G.1-3.  The UE explicitly includes all the supported bandwidth class combinations for V2X sidelink transmission or reception in the band combination signalling. Support for one bandwidth class does not implicitly indicate support for another bandwidth class. | | - |
| ***v2x-eNB-Scheduled***  Indicates whether the UE supports transmitting PSCCH/PSSCH using dynamic scheduling, SPS in eNB scheduled mode for V2X sidelink communication, reporting SPS assistance information and the UE supports maximum transmit power associated with Power class 3 V2X UE, see TS 36.101 [42] in a band. | | - |
| ***v2x-EnhancedHighReception***  Indicates whether the UE supports reception of 30 PSCCH in a subframe and decoding of 204 RBs per subframe counting both PSCCH and PSSCH in a band for V2X sidelink communication. | | - |
| ***v2x-HighPower***  Indicates whether the UE supports maximum transmit power associated with Power class 2 V2X UE for V2X sidelink transmission in a band, see TS 36.101 [42]. | | - |
| ***v2x-HighReception***  Indicates whether the UE supports reception of 20 PSCCH in a subframe and decoding of 136 RBs per subframe counting both PSCCH and PSSCH in a band for V2X sidelink communication. | | - |
| ***v2x-nonAdjacentPSCCH-PSSCH***  Indicates whether the UE supports transmission and reception in the configuration of non-adjacent PSCCH and PSSCH for V2X sidelink communication. | | - |
| ***v2x-numberTxRxTiming***  Indicates the number of multiple reference TX/RX timings counted over all the configured sidelink carriers for V2X sidelink communication. | | - |
| ***v2x-SensingReportingMode3***  Indicates whether the UE supports sensing measurements and reporting of measurement results in eNB scheduled mode for V2X sidelink communication. | | - |
| ***v2x-SupportedBandCombinationList***  Indicates the supported band combination list on which the UE supports simultaneous transmission and/or reception of V2X sidelink communication. | |  |
| ***v2x-SupportedBandCombinationListEUTRA-NR***  Indicates the supported band combination list on which the UE supports simultaneous transmission and/or reception of NR sidelink communication only, or joint V2X sidelink communication and NR sidelink communication. | | - |
| ***v2x-SupportedTxBandCombListPerBC, v2x-SupportedRxBandCombListPerBC***  Indicates, for a particular band combination of EUTRA, the supported band combination list among *v2x-SupportedBandCombinationList* on which the UE supports simultaneous transmission or reception of EUTRA and V2X sidelink communication respectively. The first bit refers to the first entry of *v2x-SupportedBandCombinationList*, with value 1 indicating V2X sidelink transmission/reception is supported. | | - |
| ***v2x-SupportedTxBandCombListPerBC-v1630, v2x-SupportedRxBandCombListPerBC-v1630***  Indicates, for a particular band combination of EUTRA, the supported band combination list among *v2x-SupportedBandCombinationListEUTRA-NR* on which the UE supports simultaneous transmission or reception of EUTRA and NR sidelink communication respectively, or simultaneous transmission or reception of EUTRA and joint V2X sidelink communication and NR sidelink communication respectively. The first bit refers to the first entry of *v2x-SupportedBandCombinationListEUTRA-NR*, with value 1 indicating V2X sidelink transmission/reception is supported. | | - |
| ***v2x-TxWithShortResvInterval***  Indicates whether the UE supports 20 ms and 50 ms resource reservation periods for UE autonomous resource selection and eNB scheduled resource allocation for V2X sidelink communication. | | - |
| ***virtualCellID-BasicSRS***  Indicates whether the UE supports virtual cell ID for basic SRS symbol(s). | | - |
| ***virtualCellID-AddSRS***  This field indicates whether the UE supports virtual cell ID for additional SRS symbol(s). | | - |
| ***voiceOverPS-HS-UTRA-FDD***  Indicates whether UE supports IMS voice according to GSMA IR.58 profile in UTRA FDD. | | - |
| ***voiceOverPS-HS-UTRA-TDD128***  Indicates whether UE supports IMS voice in UTRA TDD 1.28Mcps. | | - |
| ***widebandPRG-Slot, widebandPRG-Subslot, widebandPRG-Subframe***  Indicates whether the UE supports wideband precoding resource block group size for slot/subslot/subframe operation as specified in TS 36.213 [23]. | | - |
| ***wlan-IW-RAN-Rules***  Indicates whether the UE supports RAN-assisted WLAN interworking based on access network selection and traffic steering rules. | | - |
| ***wlan-IW-ANDSF-Policies***  Indicates whether the UE supports RAN-assisted WLAN interworking based on ANDSF policies. | | - |
| ***wlan-MAC-Address***  Indicates the WLAN MAC address of this UE. | | - |
| ***wlan-PeriodicMeas***  Indicates whether the UE supports periodic reporting of WLAN measurements. | | - |
| ***wlan-ReportAnyWLAN***  Indicates whether the UE supports reporting of WLANs not listed in the *measObjectWLAN*. | | - |
| ***wlan-SupportedDataRate***  Indicates the maximum WLAN data rate supported by the UE over all LWA bearers. Actual value of supported data rate is field value \* 10 Mbps (i.e., value 1 corresponds to 10 Mbps, value 2 corresponds to 20 Mbps and so on). | | - |
| ***zp-CSI-RS-AperiodicInfo***  Indicates whether the UE supports aperiodic ZP-CSI-RS transmission for the indicated transmission mode. | | Yes |

NOTE 1: The IE *UE-EUTRA-Capability* does not include AS security capability information, since these are the same as the security capabilities that are signalled by NAS. Consequently, AS need not provide "man-in-the-middle" protection for the security capabilities.

NOTE 2: The column FDD/ TDD diff indicates if the UE is allowed to signal, as part of the additional capabilities for an XDD mode i.e. within *UE-EUTRA-CapabilityAddXDD-Mode-xNM*, a different value compared to the value signalled elsewhere within *UE-EUTRA-Capability* (i.e. the common value, supported for both XDD modes). A '-' is used to indicate that it is not possible to signal different values (used for fields for which the field description is provided for other reasons). Annex E specifies for which TDD and FDD serving cells a UE supporting TDD/FDD CA shall support a capability for which it indicates support within the capability signalling.

NOTE 2a: From REL-15 onwards, the UE is not allowed to signal different values for FDD and TDD unless yes is indicated in column FDD/ TDD diff (i.e. no need to introduce field description solely for the purpose of indicate no).

NOTE 3: The *BandCombinationParameters* for the same band combination can be included more than once.

NOTE 4: UE CA and measurement capabilities indicate the combinations of frequencies that can be configured as serving frequencies.

NOTE 5: The grouping of the cells to the first and second cell group, as indicated by *supportedCellGrouping*, is shown in the table below. The leading / leftmost bit of *supportedCellGrouping* corresponds to the Bit String Position 1.

|  |  |  |  |
| --- | --- | --- | --- |
| Nr of Band Entries: | 5 | 4 | 3 |
| Length of Bit-String: | 15 | 7 | 3 |
| Bit String Position | Cell grouping option (0= first cell group, 1= second cell group) | | |
| 1 | 00001 | 0001 | 001 |
| 2 | 00010 | 0010 | 010 |
| 3 | 00011 | 0011 | 011 |
| 4 | 00100 | 0100 |  |
| 5 | 00101 | 0101 |  |
| 6 | 00110 | 0110 |  |
| 7 | 00111 | 0111 |  |
| 8 | 01000 |  |  |
| 9 | 01001 |  |  |
| 10 | 01010 |  |  |
| 11 | 01011 |  |  |
| 12 | 01100 |  |  |
| 13 | 01101 |  |  |
| 14 | 01110 |  |  |
| 15 | 01111 |  |  |

NOTE 6: UE includes the *intraBandContiguousCC-InfoList-r12* also for bandwidth class A because of the presence conditions in *BandCombinationParameters-v1270*. For example, if UE supports CA\_1A\_41D band combination, if UE includes the field *intraBandContiguousCC-InfoList-r12* for band 41, the UE includes *intraBandContiguousCC-InfoList-r12* also for band 1.

NOTE 6a: For multiple *BandParameters* entries with the same *bandEUTRA* and same *ca-BandwidthClassDL* in a supported band combination, the UE capabilities indicated by *BandParameters* are agnostic to the order in which they are indicated in the *bandParameterList*, under the condition that the set of the capabilities indicated for the concerned *bandEUTRA* (e.g. *bandParametersDL* and *bandParametersUL)* are used together, and the concerned *BandParameters* correspond to the *supportedBandwithCombinationSet* for which set of channel bandwidths for carrier(s) is the same among sub-blocks, as defined in TS 36.101 [42], Table 5.6A.1-3, Table 5.6A.1-4, Table 5.6A.1-5.

NOTE 7: For a UE that indicates release X in field *accessStratumRelease* but supports a feature specified in release X+ N (i.e. early UE implementation), the ASN.1 comprehension requirement are specified in Annex F.

NOTE 8: For a UE that does not include *mimo-WeightedLayersCapabilities-r13*, or for the case with no CC configured with FD-MIMO, the FD-MIMO processing capability condition is not applicable (i.e. considered as satisfied). For a UE that includes *mimo-WeightedLayersCapabilities-r13*, the FD-MIMO processing capability condition is satisfied if the equation 4.3.28.13-1 in TS 36.306 [5] is satisfied.

#### – *UE-RadioPagingInfo*

The *UE-RadioPagingInfo* IE contains UE capability information needed for paging.

*UE-RadioPagingInfo* information element

-- ASN1START

UE-RadioPagingInfo-r12 ::= SEQUENCE {

ue-Category-v1250 INTEGER (0) OPTIONAL,

...,

[[ ue-CategoryDL-v1310 ENUMERATED {m1} OPTIONAL,

ce-ModeA-r13 ENUMERATED {true} OPTIONAL,

ce-ModeB-r13 ENUMERATED {true} OPTIONAL

]],

[[ wakeUpSignal-r15 ENUMERATED {true} OPTIONAL,

wakeUpSignal-TDD-r15 ENUMERATED {true} OPTIONAL,

wakeUpSignalMinGap-eDRX-r15 ENUMERATED {ms40, ms240, ms1000, ms2000} OPTIONAL,

wakeUpSignalMinGap-eDRX-TDD-r15 ENUMERATED {ms40, ms240, ms1000, ms2000} OPTIONAL

]],

[[ ue-CategoryDL-v1610 ENUMERATED {m2} OPTIONAL,

groupWakeUpSignal-r16 ENUMERATED {true} OPTIONAL,

groupWakeUpSignalTDD-r16 ENUMERATED {true} OPTIONAL,

groupWakeUpSignalAlternation-r16 ENUMERATED {true} OPTIONAL,

groupWakeUpSignalAlternationTDD-r16 ENUMERATED {true} OPTIONAL

]],

[[

inactiveStatePO-Determination-r17 ENUMERATED {true} OPTIONAL

]]

}

-- ASN1STOP

| *UE-RadioPagingInfo* field descriptions |
| --- |
| ***ce-ModeA, ce-ModeB***  Indicates whether the UE supports operation in CE mode A and/or B, as specified in TS 36.211 [21] and TS 36.213 [23]. |
| ***groupWakeUpSignal, groupWakeUpSignalTDD***  Indicates whether the UE supports GWUS for paging in RRC\_IDLE as specified in TS 36.211 [21], TS 36.213 [23] and TS 36.304 [4]. If this field is included, the minimum gap between GWUS and associated PO for DRX is fixed as 40 ms. |
| ***groupWakeUpSignalAlternation, groupWakeUpSignalAlternationTDD***  Indicates whether the UE supports GWUS with group resource alternation for paging in RRC\_IDLE as specified in TS 36.211 [21], TS 36.213 [23] and TS 36.304 [4]. If this field is included, the minimum gap between GWUS and associated PO for DRX is fixed as 40 ms. |
| ***inactiveStatePO-Determination***  Indicates whether the UE other than BL UE or UE in CE supports to use the same i\_s in RRC\_INACTIVE state as in RRC\_IDLE state, as specified in TS 36.304 [4]. |
| ***ue-Category, ue-CategoryDL***  UE category as defined in TS 36.306 [5]. A category M2 UE shall also include the field *ue-CategoryDL-v1310* in this version of the specification. |
| ***wakeUpSignal, wakeUpSignal-TDD***  Indicates whether the UE supports WUS for paging in RRC\_IDLE as specified in TS 36.213 [22] and TS 36.304 [4]. If this field is included, the minimum gap between WUS and associated PO for DRX is fixed as 40 ms. |
| ***wakeUpSignalMinGap-eDRX, wakeUpSignalMinGap-eDRX-TDD***  Indicates the minimum gap the UE supports between WUS and associated PO for eDRX as specified in TS 36.213 [22] and TS 36.304 [4]. Value ms40 corresponds to 40 ms, ms240 corresponds to 240 ms and so on. If this field is included, the UE shall also indicate support of WUS or GWUS for paging. |

### 6.3.7 MBMS information elements

#### – *MBSFN-AreaInfoList*

The IE *MBSFN-AreaInfoList* contains the information required to acquire the MBMS control information associated with one or more MBSFN areas.

*MBSFN-AreaInfoList* information element

-- ASN1START

MBSFN-AreaInfoList-r9 ::= SEQUENCE (SIZE(1..maxMBSFN-Area)) OF MBSFN-AreaInfo-r9

MBSFN-AreaInfo-r9 ::= SEQUENCE {

mbsfn-AreaId-r9 MBSFN-AreaId-r12,

non-MBSFNregionLength ENUMERATED {s1, s2},

notificationIndicator-r9 INTEGER (0..7),

mcch-Config-r9 SEQUENCE {

mcch-RepetitionPeriod-r9 ENUMERATED {rf32, rf64, rf128, rf256},

mcch-Offset-r9 INTEGER (0..10),

mcch-ModificationPeriod-r9 ENUMERATED {rf512, rf1024},

sf-AllocInfo-r9 BIT STRING (SIZE(6)),

signallingMCS-r9 ENUMERATED {n2, n7, n13, n19}

},

...,

[[ mcch-Config-r14 SEQUENCE {

mcch-RepetitionPeriod-v1430 ENUMERATED {rf1, rf2, rf4, rf8,

rf16 } OPTIONAL, -- Need OR

mcch-ModificationPeriod-v1430 ENUMERATED {rf1, rf2, rf4, rf8, rf16, rf32, rf64, rf128,

rf256, spare7} OPTIONAL -- Need OR

} OPTIONAL, -- Need OR

subcarrierSpacingMBMS-r14 ENUMERATED {kHz7dot5, kHz1dot25} OPTIONAL -- Need OR

]]

}

MBSFN-AreaInfoList-r16 ::= SEQUENCE (SIZE(1..maxMBSFN-Area)) OF MBSFN-AreaInfo-r16

MBSFN-AreaInfo-r16 ::= SEQUENCE {

mbsfn-AreaId-r16 MBSFN-AreaId-r12,

notificationIndicator-r16 INTEGER (0..7),

mcch-Config-r16 SEQUENCE {

mcch-RepetitionPeriod-r16 ENUMERATED {rf1, rf2, rf4, rf8, rf16, rf32, rf64,

rf128, rf256, spare7, spare6, spare5,

spare4, spare3, spare2, spare1},

mcch-ModificationPeriod-r16 ENUMERATED {rf1, rf2, rf4, rf8, rf16, rf32, rf64, rf128,

rf256, rf512, rf1024, spare5, spare4,

spare3,spare2, spare1},

mcch-Offset-r16 INTEGER (0..10),

sf-AllocInfo-r16 BIT STRING (SIZE(10)),

signallingMCS-r16 ENUMERATED {n2, n7, n13, n19}

},

subcarrierSpacingMBMS-r16 ENUMERATED {kHz7dot5, kHz2dot5, kHz1dot25, kHz0dot37,

kHz15-v17xy, spare3, spare2, spare1},

timeSeparation-r16 ENUMERATED {sl2, sl4} OPTIONAL, -- Need OR

...

}

MBSFN-AreaInfoList-r17 ::= SEQUENCE (SIZE(1..maxMBSFN-Area)) OF MBSFN-AreaInfo-r17

MBSFN-AreaInfo-r17 ::= SEQUENCE {

mbsfn-AreaInfo-r17 MBSFN-AreaInfo-r16,

pmch-Bandwidth-r17 ENUMERATED {n40, n35, n30, spare1},

...

}

-- ASN1STOP

| *MBSFN-AreaInfoList* field descriptions |
| --- |
| ***mcch-ModificationPeriod***  Defines periodically appearing boundaries, i.e. radio frames for which SFN mod *mcch-ModificationPeriod* = 0. The contents of different transmissions of MCCH information can only be different if there is at least one such boundary in-between them. In case *mcch-ModificationPeriod-v1430* is configured, the UE shall ignore the *mcch-ModificationPeriod-r9*. |
| ***mcch-Offset***  Indicates, together with the *mcch-RepetitionPeriod*, the radio frames in which MCCH is scheduled i.e. MCCH is scheduled in radio frames for which: SFN mod *mcch-RepetitionPeriod* = *mcch-Offset*. |
| ***mcch-RepetitionPeriod***  Defines the interval between transmissions of MCCH information, in radio frames, Value rf32 corresponds to 32 radio frames, rf64 corresponds to 64 radio frames and so on. In case *mcch-RepetitionPeriod-v1430* is configured, the UE shall ignore the *mcch-RepetitionPeriod-r9*. |
| ***non-MBSFNregionLength***  Indicates how many symbols from the beginning of the subframe constitute the non-MBSFN region. This value applies in all subframes of the MBSFN area used for PMCH transmissions as indicated in the MSI. The values s1 and s2 correspond with 1 and 2 symbols, respectively: see TS 36.211 [21], Table 6.7-1. |
| ***notificationIndicator***  Indicates which PDCCH bit is used to notify the UE about change of the MCCH applicable for this MBSFN area. Value 0 corresponds with the least significant bit as defined in TS 36.212 [22], clause 5.3.3.1 and so on. |
| ***pmch-Bandwidth***  Indicates the PMCH and corresponding MBSFN-RS bandwidth applicable for this MBSFN area (parameter in TS 36.211 [ 21] and TS 36.213 [23]). Value n40 corresponds to 40 PRBs, n35 corresponds to 35 PRBs and so on. |
| ***sf-AllocInfo-r9***  Indicates the subframes of the radio frames indicated by the *mcch-RepetitionPeriod* and the *mcch-Offset*, that may carry MCCH. Value "1" indicates that the corresponding subframe is allocated. If the bitmap is set to all zeros, the corresponding MBSFN area is considered as not configured.  The following mapping applies:  FDD: The first/ leftmost bit defines the allocation for subframe #1 of the radio frame indicated by *mcch-RepetitionPeriod* and *mcch-Offset*, the second bit for #2, the third bit for #3, the fourth bit for #6, the fifth bit for #7 and the sixth bit for #8.  TDD: The first/leftmost bit defines the allocation for subframe #3 of the radio frame indicated by *mcch-RepetitionPeriod* and *mcch-Offset*, the second bit for #4, third bit for #7, fourth bit for #8, fifth bit for #9. Uplink subframes are not allocated. The last bit is not used. |
| ***sf-AllocInfo-r16***  Indicates the subframes of the radio frames indicated by the *mcch-RepetitionPeriod* and the *mcch-Offset*, that may carry MCCH. Value "1" indicates that the corresponding subframe is allocated. The first/ leftmost bit defines the allocation for subframe #0 of the radio frame indicated by *mcch-RepetitionPeriod* and *mcch-Offset*, the second bit for #1 and so on. When *subcarrierSpacingMBMS* indicates 0.37 kHz subcarrier spacing, a valid MBMS slot can carry MCCH if any subframe corresponding to the slot is configured to carry MCCH. |
| ***signallingMCS***  Indicates the MCS applicable for the subframes indicated by the field *sf-AllocInfo* and for each (P)MCH that is configured for this MBSFN area, for the first subframe allocated to the (P)MCH within each MCH scheduling period (which may contain the MCH scheduling information provided by MAC). Value n2 corresponds with the value 2 for parameter in TS 36.213 [23], Table 7.1.7.1-1, and so on. |
| ***subcarrierSpacingMBMS***  The value indicates subcarrier spacing for MBSFN subframes, kHz7dot5 refers to 7.5 kHz subcarrier spacing, kHz2dot5 refers to 2.5 kHz subcarrier spacing and so on as defined in TS 36.211 [21], clause 6.12. These subframes do not have non-MBSFN region. If *subcarrierSpacingMBMS-r14* is present, then *non-MBSFNregionLength* shall be ignored. EUTRAN configures parameter *subcarrierSpacingMBMS* only when the MBSFN subframes have subcarrier spacing other than 15 kHz or when included in *mbsfn-AreaInfo-r17*. Value kHz15-r17 is applicable only when the field is included in *mbsfn-AreaInfo-r17*. If *subcarrierSpacingMBMS* indicates 0.37 kHz subcarrier spacing, the slot as defined in TS 36.211 [21], clause 4.1 is valid only when all the corresponding subframes are configured as MBSFN subframes in this slot. |
| ***timeSeparation***  Indicates the staggering length for MBSFN-RS associated with PMCH as defined in TS 36.211 [21], clause 6.10.2.2.4. Value sl2 refers to staggering length of 2 slots (MBSFN reference signal pattern type 2) and sl4 refers to staggering length of 4 slots (MBSFN reference signal pattern type 1). E-UTRAN always configures this field when *subcarrierSpacingMBMS* indicates 0.37 kHz subcarrier spacing. Othewise the field is not configured. |

#### 6.7.3.6 NB-IoT Other information elements

#### – *UE-Capability-NB*

The IE *UE-Capability-NB* is used to convey the NB-IoT UE Radio Access Capability Parameters, see TS 36.306 [5]. The IE *UE-Capability-NB* is transferred in NB-IoT only.

*UE-Capability-NB* information element

-- ASN1START

UE-Capability-NB-r13 ::= SEQUENCE {

accessStratumRelease-r13 AccessStratumRelease-NB-r13,

ue-Category-NB-r13 ENUMERATED {nb1} OPTIONAL,

multipleDRB-r13 ENUMERATED {supported} OPTIONAL,

pdcp-Parameters-r13 PDCP-Parameters-NB-r13 OPTIONAL,

phyLayerParameters-r13 PhyLayerParameters-NB-r13,

rf-Parameters-r13 RF-Parameters-NB-r13,

dummy SEQUENCE {} OPTIONAL

}

UE-Capability-NB-Ext-r14-IEs ::= SEQUENCE {

ue-Category-NB-r14 ENUMERATED {nb2} OPTIONAL,

mac-Parameters-r14 MAC-Parameters-NB-r14 OPTIONAL,

phyLayerParameters-v1430 PhyLayerParameters-NB-v1430 OPTIONAL,

rf-Parameters-v1430 RF-Parameters-NB-v1430,

nonCriticalExtension UE-Capability-NB-v1440-IEs OPTIONAL

}

UE-Capability-NB-v1440-IEs ::= SEQUENCE {

phyLayerParameters-v1440 PhyLayerParameters-NB-v1440 OPTIONAL,

nonCriticalExtension UE-Capability-NB-v14x0-IEs OPTIONAL

}

UE-Capability-NB-v14x0-IEs ::= SEQUENCE {

-- Following field is only to be used for late REL-14 extensions

lateNonCriticalExtension OCTET STRING OPTIONAL,

nonCriticalExtension UE-Capability-NB-v1530-IEs OPTIONAL

}

UE-Capability-NB-v1530-IEs ::= SEQUENCE {

earlyData-UP-r15 ENUMERATED {supported} OPTIONAL,

rlc-Parameters-r15 RLC-Parameters-NB-r15,

mac-Parameters-v1530 MAC-Parameters-NB-v1530,

phyLayerParameters-v1530 PhyLayerParameters-NB-v1530 OPTIONAL,

tdd-UE-Capability-r15 TDD-UE-Capability-NB-r15 OPTIONAL,

nonCriticalExtension UE-Capability-NB-v15x0-IEs OPTIONAL

}

UE-Capability-NB-v15x0-IEs ::= SEQUENCE {

-- Following field is only to be used for late REL-15 extensions

lateNonCriticalExtension OCTET STRING OPTIONAL,

nonCriticalExtension UE-Capability-NB-v1610-IEs OPTIONAL

}

UE-Capability-NB-v1610-IEs ::= SEQUENCE {

earlySecurityReactivation-r16 ENUMERATED {supported} OPTIONAL,

earlyData-UP-5GC-r16 ENUMERATED {supported} OPTIONAL,

pur-Parameters-r16 PUR-Parameters-NB-r16 OPTIONAL,

mac-Parameters-v1610 MAC-Parameters-NB-v1610,

phyLayerParameters-v1610 PhyLayerParameters-NB-v1610 OPTIONAL,

son-Parameters-r16 SON-Parameters-NB-r16 OPTIONAL,

measParameters-r16 MeasParameters-NB-r16,

tdd-UE-Capability-v1610 TDD-UE-Capability-NB-v1610 OPTIONAL,

nonCriticalExtension UE-Capability-NB-v16x0-IEs OPTIONAL

}

UE-Capability-NB-v16x0-IEs ::= SEQUENCE {

-- Following field is only to be used for late REL-16 extensions

lateNonCriticalExtension OCTET STRING OPTIONAL,

nonCriticalExtension UE-Capability-NB-v1700-IEs OPTIONAL

}

UE-Capability-NB-v1700-IEs ::= SEQUENCE {

connModeMeasIntraFreq-r17 ENUMERATED {supported} OPTIONAL,

connModeMeasInterFreq-r17 ENUMERATED {supported} OPTIONAL,

coverageBasedPaging-r17 ENUMERATED {supported} OPTIONAL,

phyLayerParameters-v1700 PhyLayerParameters-NB-v1700 OPTIONAL,

ntn-Parameters-r17 NTN-Parameters-NB-r17 OPTIONAL,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

TDD-UE-Capability-NB-r15 ::= SEQUENCE {

ue-Category-NB-r15 ENUMERATED {nb2} OPTIONAL,

phyLayerParametersRel13-r15 PhyLayerParameters-NB-r13 OPTIONAL,

phyLayerParametersRel14-r15 PhyLayerParameters-NB-v1430 OPTIONAL,

phyLayerParameters-v1530 PhyLayerParameters-NB-v1530 OPTIONAL,

...

}

TDD-UE-Capability-NB-v1610 ::= SEQUENCE {

slotSymbolResourceResvDL-r16 ENUMERATED {supported} OPTIONAL,

slotSymbolResourceResvUL-r16 ENUMERATED {supported} OPTIONAL,

subframeResourceResvDL-r16 ENUMERATED {supported} OPTIONAL,

subframeResourceResvUL-r16 ENUMERATED {supported} OPTIONAL

}

AccessStratumRelease-NB-r13 ::= ENUMERATED {rel13, rel14, rel15, rel16, rel17, spare3, spare2, spare1, ...}

PDCP-Parameters-NB-r13 ::= SEQUENCE {

supportedROHC-Profiles-r13 SEQUENCE {

profile0x0002 BOOLEAN,

profile0x0003 BOOLEAN,

profile0x0004 BOOLEAN,

profile0x0006 BOOLEAN,

profile0x0102 BOOLEAN,

profile0x0103 BOOLEAN,

profile0x0104 BOOLEAN

},

maxNumberROHC-ContextSessions-r13 ENUMERATED {cs2, cs4, cs8, cs12} DEFAULT cs2,

...

}

RLC-Parameters-NB-r15 ::= SEQUENCE {

rlc-UM-r15 ENUMERATED {supported} OPTIONAL

}

MAC-Parameters-NB-r14 ::= SEQUENCE {

dataInactMon-r14 ENUMERATED {supported} OPTIONAL,

rai-Support-r14 ENUMERATED {supported} OPTIONAL

}

MAC-Parameters-NB-v1530 ::= SEQUENCE {

sr-SPS-BSR-r15 ENUMERATED {supported} OPTIONAL

}

MAC-Parameters-NB-v1610 ::= SEQUENCE {

rai-SupportEnh-r16 ENUMERATED {supported} OPTIONAL

}

NTN-Parameters-NB-r17 ::= SEQUENCE {

ntn-Connectivity-EPC-r17 ENUMERATED {supported} OPTIONAL,

ntn-TA-Report-r17 ENUMERATED {supported} OPTIONAL,

ntn-PUR-TimerEnhancement-r17 ENUMERATED {supported} OPTIONAL

}

MeasParameters-NB-r16 ::= SEQUENCE {

dl-ChannelQualityReporting-r16 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-NB-r13 ::= SEQUENCE {

multiTone-r13 ENUMERATED {supported} OPTIONAL,

multiCarrier-r13 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-NB-v1430 ::= SEQUENCE {

multiCarrier-NPRACH-r14 ENUMERATED {supported} OPTIONAL,

twoHARQ-Processes-r14 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-NB-v1440 ::= SEQUENCE {

interferenceRandomisation-r14 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-NB-v1530 ::= SEQUENCE {

mixedOperationMode-r15 ENUMERATED {supported} OPTIONAL,

sr-WithHARQ-ACK-r15 ENUMERATED {supported} OPTIONAL,

sr-WithoutHARQ-ACK-r15 ENUMERATED {supported} OPTIONAL,

nprach-Format2-r15 ENUMERATED {supported} OPTIONAL,

additionalTransmissionSIB1-r15 ENUMERATED {supported} OPTIONAL,

npusch-3dot75kHz-SCS-TDD-r15 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-NB-v1610 ::= SEQUENCE {

npdsch-MultiTB-r16 ENUMERATED {supported} OPTIONAL,

npdsch-MultiTB-Interleaving-r16 ENUMERATED {supported} OPTIONAL,

npusch-MultiTB-r16 ENUMERATED {supported} OPTIONAL,

npusch-MultiTB-Interleaving-r16 ENUMERATED {supported} OPTIONAL,

multiTB-HARQ-AckBundling-r16 ENUMERATED {supported} OPTIONAL,

slotSymbolResourceResvDL-r16 ENUMERATED {supported} OPTIONAL,

slotSymbolResourceResvUL-r16 ENUMERATED {supported} OPTIONAL,

subframeResourceResvDL-r16 ENUMERATED {supported} OPTIONAL,

subframeResourceResvUL-r16 ENUMERATED {supported} OPTIONAL

}

PUR-Parameters-NB-r16 ::= SEQUENCE {

pur-CP-EPC-r16 ENUMERATED {supported} OPTIONAL,

pur-CP-5GC-r16 ENUMERATED {supported} OPTIONAL,

pur-UP-EPC-r16 ENUMERATED {supported} OPTIONAL,

pur-UP-5GC-r16 ENUMERATED {supported} OPTIONAL,

pur-NRSRP-Validation-r16 ENUMERATED {supported} OPTIONAL,

pur-CP-L1Ack-r16 ENUMERATED {supported} OPTIONAL

}

PhyLayerParameters-NB-v1700 ::= SEQUENCE {

npdsch-16QAM-r17 ENUMERATED {supported} OPTIONAL,

npusch-16QAM-r17 ENUMERATED {supported} OPTIONAL

}

RF-Parameters-NB-r13 ::= SEQUENCE {

supportedBandList-r13 SupportedBandList-NB-r13,

multiNS-Pmax-r13 ENUMERATED {supported} OPTIONAL

}

RF-Parameters-NB-v1430 ::= SEQUENCE {

powerClassNB-14dBm-r14 ENUMERATED {supported} OPTIONAL

}

SupportedBandList-NB-r13 ::= SEQUENCE (SIZE (1..maxBands)) OF SupportedBand-NB-r13

SupportedBand-NB-r13 ::= SEQUENCE {

band-r13 FreqBandIndicator-NB-r13,

powerClassNB-20dBm-r13 ENUMERATED {supported} OPTIONAL

}

SON-Parameters-NB-r16 ::= SEQUENCE {

anr-Report-r16 ENUMERATED {supported} OPTIONAL,

rach-Report-r16 ENUMERATED {supported} OPTIONAL

}

-- ASN1STOP

| *UE-Capability-NB* field descriptions | *FDD/TDD appl* | *FDD/TDD diff* |
| --- | --- | --- |
| ***accessStratumRelease***  Set to rel17 in this version of the specification. | FDD/TDD | No |
| ***additionalTransmissionSIB1***  Indicates whether the UE supports additional SIB1 transmission as specified in TS 36.213 [23]. | FDD | - |
| ***anr-Report***  Indicates whether the UE supports ANR measurements in RRC\_IDLE. | FDD/TDD | No |
| ***connModeMeasIntraFreq, connModeMeasInterFreq***  Indicates whether the UE in RRC\_CONNECTED supports neighbour cell measurements. | FDD/TDD | No |
| ***coverageBasedPaging***  Indicates whether the UE in RRC\_IDLE supports coverage based paging carrier selection as defined in TS 36.304 [4]. | FDD/TDD | No |
| ***dataInactMon***  Indicates whether the UE supports the data inactivity monitoring as specified in TS 36.321 [6]. | FDD/TDD | No |
| ***dl-ChannelQualityReporting-r16***  Indicates whether the UE supports DL channel quality reporting in connected mode as specified in TS 36.321 [6]. | FDD | - |
| ***dummy***  This field is not used in the specification. It shall not be sent by the UE. | NA | NA |
| ***earlyData-UP, earlyData-UP-5GC***  Indicates whether the UE supports EDT for User plane CIoT EPS/5GS optimisations, as defined in TS 24.301 [35] and 24.501 [95] respectively. | FDD | - |
| ***earlySecurityReactivation***  Indicates whether the UE supports early security reactivation when resuming a suspended RRC connection. | FDD/TDD | No |
| ***interferenceRandomisation***  For FDD: Indicates whether the UE supports interference randomisation in connected mode as defined in TS.36.211 [21]. | FDD | - |
| ***maxNumberROHC-ContextSessions***  Set to the maximum number of concurrently active ROHC contexts supported by the UE, excluding context sessions that leave all headers uncompressed. cs2 corresponds with 2 (context sessions), cs4 corresponds with 4 and so on. The network ignores this field if the UE supports none of the ROHC profiles in *supportedROHC-Profiles*. | FDD/TDD | No |
| ***mixedOperationMode***  Defines whether the UE supports multi-carrier operation with mixed operation mode, standalone or inband/guardband, between the anchor carrier and the non-anchor carrier for unicast, paging, and random access as specified in TS 36.300 [9]. | FDD | - |
| ***multiCarrier***  Defines whether the UE supports multi -carrier operation. | FDD/TDD | Yes |
| ***multicarrier-NPRACH***  Defines whether the UE supports NPRACH on non-anchor carrier as specified in TS 36.321 [6]. | FDD/TDD | Yes |
| ***multipleDRB***  Defines whether the UE supports multiple DRBs. | FDD/TDD | No |
| ***multiNS-Pmax***  Defines whether the UE supports the mechanisms defined for NB-IoT cells broadcasting *NS-PmaxList-NB*. | FDD/TDD | No |
| ***multiTB-HARQ-AckBundling***  Indicates whether the UE supports HARQ ACK bundling for interleaved transmission for DL.  If *multiTB-HARQ-AckBundling* is included, the UE shall also indicate support for *npdsch-MultiTB-Interleaving*. | FDD | - |
| ***multiTone***  Defines whether the UE supports UL multi-tone transmissions on NPUSCH. | FDD/TDD | Yes |
| ***npdsch-16QAM***  Indicates whether the UE supports 16QAM for DL unicast as defined in TS 36.213 [23]. | TBD | TBD |
| ***npdsch-MultiTB***  Indicates whether the UE supports multiple TBs scheduling in RRC\_CONNECTED for DL.  If *npdsch-MultiTB* is included, the UE shall also indicate support for *twoHARQ-Processes*. | FDD | - |
| ***npdsch-MultiTB-Interleaving***  Indicates whether the UE supports interleaved transmission when multiple TBs is scheduled in RRC\_CONNECTED for DL. | FDD | - |
| ***nprach-Format2***  Defines whether the UE supports NPRACH resources using preamble format 2. | FDD | - |
| ***npusch-16QAM***  Indicates whether the UE supports 16QAM for UL unicast as defined in TS 36.213 [23]. | TBD | TBD |
| ***npusch-3dot75kHz-SCS-TDD***  Indicates whether the UE supports NPUSCH with 3.75kHz SCS for TDD. | TDD | - |
| ***npusch-MultiTB***  Indicates whether the UE supports multiple TBs scheduling in RRC\_CONNECTED for UL.  If *npusch-MultiTB* is included, the UE shall also indicate support for *twoHARQ-Processes*. | FDD | - |
| ***npusch-MultiTB-Interleaving***  Indicates whether the UE supports interleaved transmission when multiple TBs is scheduled in RRC\_CONNECTED for UL. | FDD | - |
| ***ntn-Connectivity-EPC***  Indicates whether the UE supports NTN access when connected to EPC. If the UE indicates this capability, the UE shall support all NTN essential features as specified in TS 36.306 [5]. | FDD | - |
| ***ntn-PUR-TimerEnhancement***  Indicates whether the UE supports PUR timer enhancement for NTN, see TS 36.321 [6]. | - |  |
| ***ntn-TA-report***  Indicates whether the UE supports time advance reporting in RRC\_CONNECTED, see TS 36.321 [6]. | FDD | - |
| ***powerClassNB-14dBm***  Defines whether the UE supports power class 14dBm in all the bands supported by the UE as specified in TS 36.101 [42].  If *powerClassNB-20dBm* is included, the UE shall not include the field *powerClassNB-14dBm*. | FDD/TDD | No |
| ***powerClassNB-20dBm***  Defines whether the UE supports power class 20dBm in NB-IoT for the band, as specified in TS 36.101 [42]. If neither *powerClassNB-14dBm* nor *powerClassNB-20dBm* is included, UE supports power class 23 dBm in the NB-IoT band. | FDD/TDD | No |
| ***pur-CP-EPC*, *pur-CP-5GC***  Indicates whether the UE supports transmission using PUR for Control plane CIoT EPS/5GS optimisations, as defined in TS 24.301 [35] and TS 24.501 [95] respectively. | FDD | - |
| ***pur-CP-L1Ack***  Indicates whether UE supports L1 acknowledgement in response to CP transmission using PUR.  If *pur-CP-L1Ack* is included, the UE shall also indicate support for *pur-CP-EPC* or *pur-CP-5GC*. | FDD | - |
| ***pur-NRSRP-Validation***  Indicates whether UE supports serving cell NRSRP for TA validation for transmission using PUR.  If *pur-NRSRP-Validation* is included, the UE shall also indicate support for *pur-CP-EPC*, *pur-CP-5GC*, *pur-UP-EPC* or *pur-CP-5GC*. | FDD | - |
| ***pur-UP-EPC*, *pur-UP-5GC***  Indicates whether the UE supports transmission using PUR for User plane CIoT EPS/5GS optimisations, as defined in TS 24.301 [35] and TS 24.501 [95] repectively. | FDD | - |
| ***rach-Report***  Indicates whether the UE supports delivery of *rach-Report*. | FDD/TDD | No |
| ***rai-Support***  Defines whether the UE supports release assistance indication (RAI) as specified in TS 36.321 [6]. | FDD/TDD | No |
| ***rai-SupportEnh***  Indicates whether the UE supports AS Release Assistance Indication via the DCQR and AS RAI MAC CE when connected to EPC as specified in TS 36.321 [6]. | FDD/TDD | No |
| ***rlc-UM***  Defines whether the UE supports RLC UM as specified in TS 36.322 [7]. | FDD/TDD | No |
| ***slotSymbolResourceResvDL***  Indicates whether the UE supports slot/symbol-level time-domain DL resource reservation, e.g. for NB-IoT coexistence with NR.  If *slotSymbolResourceResvDL* is included, the UE shall also indicate support for *subframeResourceResvDL*. | FDD/TDD | Yes |
| ***slotSymbolResourceResvUL***  Indicates whether the UE supports slot/symbol-level time-domain UL resource reservation, e.g. for NB-IoT coexistence with NR.  If *slotSymbolResourceResvUL* is included, the UE shall also indicate support for *subframeResourceResvUL*. | FDD/TDD | Yes |
| ***supportedBandList***  Includes the supported NB-IoT bands as defined in TS 36.101 [42]. | FDD/TDD | No |
| ***sr-SPS-BSR***  Defines whether the UE supports SR using SPS BSR as specified in TS 36.321 [6]. | FDD | - |
| ***sr-withHARQ-ACK***  Defines whether the UE supports physical layer SR with HARQ ACK as specified in TS 36.213 [23]. | FDD | - |
| ***sr-withoutHARQ-ACK***  Defines whether the UE supports physical layer SR without HARQ ACK as specified in TS 36.211 [21] and TS 36.213 [23]. | FDD | - |
| ***subframeResourceResvDL***  Indicates whether the UE supports subframe-level time-domain DL resource reservation, e.g. for NB-IoT coexistence with NR. | FDD/TDD | Yes |
| ***subframeResourceResvUL***  Indicates whether the UE supports subframe-level time-domain UL resource reservation, e.g. for NB-IoT coexistence with NR. | FDD/TDD | Yes |
| ***supportedROHC-Profiles***  List of supported ROHC profiles as defined in TS 36.323 [8]. | FDD/TDD | No |
| ***twoHARQ-Processes***  Defines whether the UE supports two HARQ processes operation in DL and UL as specified in TS 36.212 [22] and TS 36.213 [23]. | FDD/TDD | Yes |
| ***ue-Category-NB***  UE category as defined in TS 36.306 [5]. Value nb1 corresponds to UE category NB1, value nb2 corresponds to UE category NB2.  A UE shall always include the field *ue-Category-NB-r13* in this version of the specification. | FDD/TDD | Yes |

NOTE 1: The IE *UE-Capability-NB* does not include AS security capability information, since these are the same as the security capabilities that are signalled by NAS. Consequently AS need not provide "man-in-the-middle" protection for the security capabilities.

NOTE 2: The column 'FDD/TDD appl' indicates the applicability to the xDD mode: 'FDD' means applicable to FDD only, 'TDD' means applicable to TDD only and 'FDD/TDD' means applicable to FDD and TDD.

NOTE 3: The column 'FDD/TDD diff' indicates if the UE is allowed to signal a different value for FDD and TDD when the capability applies to both FDD and TDD modes. '-' is used when the capability applies to one mode only, 'No' is used for dual mode capabilities where a common value is signalled for both modes, and 'Yes' is used for dual mode capabilities where a separate value is signalled for each mode. Common capabilities and FDD capabilities are reported in the fields of *UE-Capability-NB* except field *tdd-UE-Capability.* TDD capabilities are reported in *tdd-UE-Capability*.

Editor's Note: RAN1 has sent an LS to RAN4 in R1-2202893 asking for their view on whether 16-QAM capability should be per-band.

### 7.3.1 Timers (Informative)

| Timer | Start | Stop | At expiry |
| --- | --- | --- | --- |
| T300  NOTE1 | Transmission of *RRCConnectionRequest* or *RRCConnectionResumeRequest* or *RRCEarlyDataRequest* | Reception of *RRCConnectionSetup*, *RRCConnectionReject* or *RRCConnectionResume* or *RRCEarlyDataComplete* or *RRCConnectionRelease* for UP-EDT, cell re-selection and upon abortion of connection establishment by upper layers | Perform the actions as specified in 5.3.3.6 |
| T301  NOTE1 | Transmission of *RRCConnectionReestabilshmentRequest* | Reception of *RRCConnectionReestablishment* or *RRCConnectionReestablishmentReject* message as well as when the selected cell becomes unsuitable | Go to RRC\_IDLE |
| T302 | Reception of *RRCConnectionReject* while performing RRC connection establishment or reception of *RRCConnectionRelease* including *waitTime* | Upon entering RRC\_CONNECTED and upon cell re-selection, or upon reception of *RRCEarlyDataComplete* or *RRCConnectionRelease* for UP-EDT or *RRCConnectionRelease* for UP transmission using PUR, or upon reception of *RRCConnectionReject* message for E-UTRA/5GC. | Inform upper layers about barring alleviation as specified in 5.3.3.7 |
| T303 | Access barred while performing RRC connection establishment for mobile originating calls | Upon entering RRC\_CONNECTED and upon cell re-selection, or upon reception of *RRCEarlyDataComplete* or *RRCConnectionRelease* for UP-EDT or *RRCConnectionRelease* for UP transmission using PUR. | Inform upper layers about barring alleviation as specified in 5.3.3.7 |
| T304 | Reception of *RRCConnectionReconfiguration* message including the *MobilityControl Info* or  reception of *MobilityFromEUTRACommand* message including *CellChangeOrder* or upon conditional reconfiguration execution i.e. when applying a stored *RRCConnectionReconfiguration* message including the *MobilityControl Info*. | Criterion for successful completion of handover within E-UTRA, handover to E-UTRA or cell change order is met (the criterion is specified in the target RAT in case of inter-RAT) | In case of cell change order from E-UTRA or intra E-UTRA handover, initiate the RRC connection re-establishment procedure; In case of handover to E-UTRA, perform the actions defined in the specifications applicable for the source RAT; If any DAPS bearer is configured and if there is no RLF in source PCell, initiate the failure information procedure. |
| T305 | Access barred while performing RRC connection establishment for mobile originating signalling | Upon entering RRC\_CONNECTED and upon cell re-selection, or upon reception of *RRCEarlyDataComplete* or *RRCConnectionRelease* for UP-EDT or *RRCConnectionRelease* for UP transmission using PUR. | Inform upper layers about barring alleviation as specified in 5.3.3.7 |
| T306 | Access barred while performing RRC connection establishment for mobile originating CS fallback. | Upon entering RRC\_CONNECTED and upon cell re-selection, or upon reception of *RRCEarlyDataComplete* or *RRCConnectionRelease* for UP-EDT or *RRCConnectionRelease* for UP transmission using PUR. | Inform upper layers about barring alleviation as specified in 5.3.3.7 |
| T307 | Reception of *RRCConnectionReconfiguration* message including *MobilityControlInfoSCG* | Successful completion of random access on the PSCell, upon initiating re-establishment and upon SCG release | Initiate the SCG failure information procedure as specified in 5.6.13. |
| T308 | Access barred due to ACDC while performing RRC connection establishment subject to ACDC | Upon entering RRC\_CONNECTED and upon cell re-selection, or upon reception of *RRCEarlyDataComplete* or *RRCConnectionRelease* for UP-EDT or *RRCConnectionRelease* for UP transmission using PUR. | Inform upper layers about barring alleviation for ACDC as specified in 5.3.3.7 |
| T309  NOTE1 | When access attempt is barred at access barring check for an Access Category. The UE shall maintain one instance of this timer per Access Category. | Upon entering RRC\_CONNECTED, upon cell (re)selection, upon reception of *RRCConnectionRelease,* upon change of PCell while in RRC\_CONNECTED, or upon reception of *MobilityFromEUTRACommand*. | Perform the actions as specified in 5.3.16.4. |
| T310  NOTE1  NOTE2 | Upon detecting physical layer problems for the PCell i.e. upon receiving N310 consecutive out-of-sync indications from lower layers | Upon receiving N311 consecutive in-sync indications from lower layers for the PCell, upon triggering the handover procedure, upon initiating the connection re-establishment procedure, and upon initiating the MCG failure information procedure. | If security is not activated and the UE is not a NB-IoT UE that supports RRC connection re-establishment for the Control Plane CIoT EPS/5GS optimisation: go to RRC\_IDLE else: initiate the MCG failure information procedure as specified in 5.6.26 or the connection re-establishment procedure as specified in 5.3.7. |
| T311  NOTE1 | Upon initiating the RRC connection re-establishment procedure | Selection of a suitable E-UTRA cell or a cell using another RAT. | Go to RRC\_IDLE |
| T312  NOTE2 | Upon triggering a measurement report for a measurement identity for which T312 has been configured and *useT312* has been set to true, while T310 is running | Upon receiving N311 consecutive in-sync indications from lower layers, upon triggering the handover procedure, upon initiating the connection re-establishment procedure, upon initiating the MCG failure information procedure, and upon the expiry of T310 | Initiate the MCG failure information procedure as specified in 5.6.26 or the connection re-establishment procedure as specified in 5.3.7. |
| T313  NOTE2 | Upon detecting physical layer problems for the PSCell i.e. upon receiving N313 consecutive out-of-sync indications from lower layers | Upon receiving N314 consecutive in-sync indications from lower layers for the PSCell, upon initiating the connection re-establishment procedure, upon SCG release and upon receiving *RRCConnectionReconfiguration* including *MobilityControlInfoSCG* | Inform E-UTRAN about the SCG radio link failure by initiating the SCG failure information procedure as specified in 5.6.13. |
| T314  NOTE2 | Upon early detecting physical layer problems for the PCell i.e. upon receiving N310 consecutive "early-out-of-sync" indications from lower layers. | Upon receiving N311 consecutive in-sync indications from lower layers for the PCell, upon triggering the handover procedure and upon initiating the connection re-establishment procedure | Initiate the UE Assistance Information procedure to report early detection of physical layer problems in accordance with 5.6.10. |
| T315  NOTE2 | Upon detecting physical layer improvements of the PCell i.e. upon receiving N311 consecutive "early-in-sync" indications from lower layers. | Upon receiving N310 consecutive "early-out-of-sync" indications from lower layers for the PCell. | Initiate the UE Assistance Information procedure to report detection of physical layer improvements in accordance with 5.6.10. |
| T316 | Upon transmission of the *MCGFailureInformation* message | Upon receiving *RRCConnectionRelease*, *RRCConnectionReconfiguration* with *mobilityControlInfo, MobilityFromEUTRACommand*, or upon initiaitng the re-establishment procedure, | Perform the actions as specified in 5.6.26.5. |
| T317  NOTE1 | Upon acquisition of *SystemInformationBlockType31* |  | In RRC\_CONNECTED mode, initiate acquisition of *SystemInformationBlockType31* in accordance with 5.3.3.21. |
| T318  NOTE1 | Upon starting acquisition of *SystemInformationBlockType31* in RRC\_CONNECTED | Upon successful acquisition of *SystemInformationBlockType31*in RRC\_CONNECTED | If security is not activated and the UE is not a NB-IoT UE that supports RRC connection re-establishment for the Control Plane CIoT EPS optimisation: go to RRC\_IDLE else: initiate the connection re-establishment procedure as specified in 5.3.7. |
| T320 | Upon receiving *t320* or upon cell (re)selection to E-UTRA from another RAT with validity time configured for dedicated priorities (in which case the remaining validity time is applied). | Upon entering RRC\_CONNECTED, when PLMN selection is performed on request by NAS, when the UE enters RRC\_IDLE from RRC\_INACTIVE, or upon cell (re)selection to another RAT (in which case the timer is carried on to the other RAT), or upon reception of *RRCEarlyDataComplete* or *RRCConnectionRelease* for UP-EDT or *RRCConnectionRelease* for UP transmission using PUR. | Discard the cell reselection priority information provided by dedicated signalling. |
| T321 | Upon receiving *measConfig* including a *reportConfig* with the *purpose* set to *reportCGI* | Upon acquiring the information needed to set all fields of *cellGlobalId* for the requested cell, upon receiving *measConfig* that includes removal of the *reportConfig* with the *purpose* set to *reportCGI* and upon detecting that a cell is not broadcasting SIB1. | Initiate the measurement reporting procedure, stop performing the related measurements and remove the corresponding *measId* |
| T322  NOTE1 | Upon receiving *redirectedCarrierOffsetDedicated* included in *RedirectedCarrierInfo* | Upon entering RRC\_CONNECTED, when PLMN selection is performed on request by NAS, or upon cell (re)selection to another frequency or RAT, or upon reception of *RRCEarlyDataComplete* or *RRCConnectionRelease* for UP-EDT or *RRCConnectionRelease* for UP transmission using PUR. | Release *redirectedCarrierOffsetDedicated*. |
| T323 | Upon receiving *t323*. | Upon entering RRC\_CONNECTED, when PLMN selection is performed on request by NAS, when the UE enters RRC\_IDLE from RRC\_INACTIVE, or upon cell (re)selection to another RAT, or upon reception of *RRCEarlyDataComplete* or *RRCConnectionRelease* for UP-EDT or *RRCConnectionRelease* for UP transmission using PUR. | Discard the *altFreqPriorities* provided by dedicated signalling. UE shall apply the cell reselection priority information broadcast in the system information via *cellReselectionPriority* and *cellReselectionSubPriority*. |
| T325 | Timer (re)started upon receiving *RRCConnectionReject* message with *deprioritisationTimer*. |  | Stop deprioritisation of all frequencies or E-UTRA signalled by *RRCConnectionReject.* |
| T326  NOTE1 | Upon entering RRC\_CONNECTED, upon update to NRSRPRef . | Upon leaving RRC\_CONNECTED. | Stop performing neighbour cell measurement while in RRC\_CONNECTED. |
| T330 | Upon receiving *LoggedMeasurementConfiguration* message | Upon log volume exceeding the suitable UE memory, upon initiating the release of *LoggedMeasurementConfiguration* procedure | Perform the actions specified in 5.6.6.4 |
| T331 | Upon receiving *RRCConnectionRelease* message including *measIdleConfig.* | Upon receiving *RRCConnectionSetup, RRCConnectionResume, RRCConnectionRelease* with an idle/inactive measurement configuration or indication to release the configuration, if *validityArea* is configured, upon cell selection/reselection to a cell that does not belong to the *validityArea* (if configured)*,* or upon reselecting to an inter-RAT cell. | Perform the actions specified in 5.6.20.3. |
| T340  NOTE2 | Upon transmitting *UEAssistanceInformation* message with *powerPrefIndication* set to *normal* | Upon releasing *powerPrefIndication* during the connection re-establishment procedure | No action. |
| T341  NOTE2 | Upon transmitting *UEAssistanceInformation* message with *bw-Preference.* | Upon resuming an RRC connection or upon releasing *bw-Preference* during the connection re-establishment procedure | No action. |
| T342  NOTE2 | Upon transmitting *UEAssistanceInformation* message with *delayBudgetReport*. | Upon releasing *delayBudgetReportingConfig* during the connection re-establishment and connection resume procedures | No action. |
| T343  NOTE2 | Upon transmitting *UEAssistanceInformation* message with *RLM-Report* including *earlyOutOfSync*. | Upon initiating the connection re-establishment procedure | No action. |
| T344  NOTE2 | Upon transmitting *UEAssistanceInformation* message with *RLM-Report* including *earlyInSync*. | Upon initiating the connection re-establishment procedure | No action. |
| T345 | Upon transmitting *UEAssistanceInformation* message with *overheatingAssistance* | Upon releasing *overheatingAssistance* during the connection re-establishment procedure, or connection resume procedure. | No action. |
| T346 | Upon transmitting UEAssistanceInformation message with *scg-DeactivationPreference* | Upon releasing *scg-DeactivationPreferenceConfig* during the RRC connection establishment or re-establishment procedures, or upon reconfiguration of *scg-DeactivationPreferenceConfig* to *release*. | No action. |
| T350 | Upon entering RRC\_IDLE if *t350* has been received in wlan-OffloadInfo. | Upon entering RRC\_CONNECTED, or upon cell reselection. | Perform the actions specified in 5.6.12.4. |
| T351 | Reception of *RRCConnectionReconfiguration* message including the association*Timer* in *WLAN-MobilityConfig*. | Upon successful connection to WLAN, upon WLAN connection failure, upon leaving RRC\_CONNECTED, upon triggering the handover procedure, or upon initiating the connection re-establishment procedure. | Perform WLAN Connection Status Reporting specified in 5.6.15.2. |
| T360 | Upon performing the redistribution target selection as specified in TS 36.304 [4]. | Upon entering RRC\_CONNECTED, upon receiving a Paging message including *redistributionIndication*; upon reselecting a cell not belonging to the redistribution target. | Stop considering a frequency or cell to be redistribution target, and perform the redistribution target selection if the condition specified in TS 36.304 [4] is met. |
| T370 | Upon receiving *SL-DiscConfig* including a *discSysInfoToReportConfig* set to *setup.* | Upon initiating the transmission of *SidelinkUEInformation* including *discSysInfoReportFreqList*, upon receiving *SL-DiscConfig* including *discSysInfoToReportConfig* set to *release*, upon handover and re-establishment*.* | Release *discSysInfoToReportConfig*. |
| T380 | Upon reception of *periodic-RNAU-timer* in RRCConnectionRelease. | Upon reception of *RRCConnectionResume*, *RRCConnectionRelease* or *RRCConnectionSetup*. | Initiate the RAN notification area update procedure |
| NOTE1: Only the timers marked with "NOTE1" are applicable to NB-IoT.  NOTE2: The behaviour as specified in 7.3.2 applies. | | | |